3GPP TSG-RAN WG2 Meeting #118 Electronic R2-2206184

09 – 20 May 2022

**Agenda item: 6.8.1**

**Source: Nokia (Rapporteur)**

**Title: Report from [AT118-e][241][Slicing] Finalizing Stage-2 for RAN slicing (Nokia)**

**WID/SID: NR\_Slice -Core - Release 17**

**Document for: Discussion and Decision**

# 1 Introduction

This document is the report of the following email discussion:

* [AT118-e][241][Slicing] Finalizing Stage-2 for RAN slicing (Nokia)

      Scope: Finalize Stage-2 CR for RAN slicing based on meeting decisions.

      Intended outcome: Discussion report in [R2-2206184](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2206184.zip) and agreeable CR in [R2-2205491](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205491.zip).

      Deadline: Deadline 5

This email discussion covers the changes from the following tdocs:

[R2-2205975](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip) Resolving open issues Ericsson draftCR Rel-17 38.300 17.0.0 NR\_slice-Core

[R2-2205492](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip) Clarifications on slice groups and other corrections Nokia, Nokia Shanghai Bell draftCR Rel-17 38.300 17.0.0 NR\_slice-Core

[R2-2205077](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205077.zip) Corrections on TS 38.300 for RAN Slicing Huawei, HiSilicon CR Rel-17 38.300 17.0.0 0454 - F NR\_slice-Core

(**Deadline 5 (discussions for 2nd week Thu/Fri online):**

* **Comment deadline:** Wednesday W2, 0400 UTC (for collecting views)
* **Rapporteur proposals:** Wednesday W2, 0800 UTC (proposed resolution of issues)
* **Document deadline:** Wednesday W2, 1600 UTC (report or agreed CRs)
	+ No extensions to this deadline for regular discussions. Discussions handling CRs may continue to short post-meeting email (based on chair decision).

# 2 Contact Points

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Nokia (Rapporteur) | Gyuri Wolfner | gyorgy.wolfner@nokia.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion

## 3.1 Introduction of NSAG terminology

It is proposed to introduce "NSAG" in [R2-2205975](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip) and in [R2-2205492](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip):

NSAG Network Slice AS Group

**Rapporteur's comments:** It is desired to harmonize terminology in 38.300 with SA2 specifications.

**Question 1**: Do you agree to use "NSAG" for slice groups in 38.300? (This impacts other changes below.)

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 1: TBD**

## 3.2 Correction in 7.3.1

The following is proposed in [R2-2205492](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip):

- *SIB16* contains slice specific cell reselection information;

**Rapporteur's comments:** description of SIB16 is missing from 38.300.

**Question 2**: Do you agree to add the missing SIB16 description into 7.3.1?

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 2: TBD**

## 3.3 Clarification in 8.2

The following is proposed in [R2-2205492](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip):

- Network Slice Access stratum Group (NSAG): identifies a set of S-NSSAI within a Tracking Area that can be used for slice specific cell reselection or slice specific RACH configuration.

**Rapporteur's comments:** this clarification is useful in 38.300.

**Question 3**: Do you agree to add this clarification into 8.2?

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 3: TBD**

## 3.4 Clarification in 9.2.1.2

The following clarification is proposed in [R2-2205077](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205077.zip):

- Slice specific cell reselection information can be provided to facilitate the UE to reselect a cell that supports specific slice group(s).

**Rapporteur's comments:** Even if the cell reselection information is slice group specific, the purpose of the enhancement is to facilitate the reselection of a cell that support some specific slice(s).

**Question 4**: Do you agree with this change in 9.2.1.2?

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 4: TBD**

## 3.5 Clarifications in 16.3.1

The following clarification is proposed in [R2-2205077](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205077.zip):

**Resource isolation between slices**

- The NG-RAN supports resource isolation between slices. NG-RAN resource isolation may be achieved by means of RRM policies and protection mechanisms that should avoid that shortage of shared resources in one slice breaks the service level agreement for another slice. It should be possible to fully dedicate NG-RAN resources to a certain slice. Some RACH resources can be associated to specific slice group(s). Other aspects how NG-RAN supports resource isolation is implementation dependent.

**Rapporteur's comments:** This clarification is useful as RACH resources are associated to slice groups. If the use of NSAG is accepted, then the rapporteur proposes to use NSAG instead of "slice groups" here.

**Question 5a**: Do you agree with this change in 16.3.1?

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 5a: TBD**

The following clarification is proposed in [R2-2205975](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip)

**Slice Availability**

- Some slices may be available only in part of the network, within one or a few TAs, while other slices may be available in the entire network. The NG-RAN supported S-NSSAI(s) is configured by OAM. Awareness in the NG-RAN of the slices supported in the cells of its neighbours may be beneficial for inter-frequency mobility in connected mode. It is assumed that the slice availability does not change within the UE's registration area.

**Rapporteur's comments:** This clarification is not directly connected to the enhancements introduced in RAN slicing.

**Question 5b**: Do you agree to add this clarification into 16.3.1?

|  |  |  |
| --- | --- | --- |
| Company | YES/NO | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 5b: TBD**

## 3.6 Clarifications/corrections in 16.3.3.1

The following changes are proposed in [R2-2205077](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205077.zip):

Slice group specific RACH configuration for RA partitioning and prioritization can be included in SIB1 message. The slice specific RACH configurations are associated to specific slice groups, and if not provided for a slice group that UE considers for selecting the RACH configuration, then the UE does not consider the slice(s) for selecting the slice specific RACH configuration, i.e., the UE uses the common RACH configuration. In the UE, NAS provides the slice group information to be considered during RA to AS.

Editor's Note: Details of slice grouping and how it is provided to the UE are FFS, depends on SA2.

The following changes are proposed in [R2-2205492](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip):

Slice specific RACH configuration for RA isolation and prioritization can be included in SIB1 messages. The slice specific RACH configurations are associated to specific Network Slice AS Groups (NSAGs), and if not provided for a NSAG that UE considers for selecting the RACH configuration, then the UE does not consider the slice(s) for selecting the slice specific RACH configuration, i.e., the UE uses the common RACH configuration. In the UE, NAS provides the NSAG to be considered during RA to AS.

The following changes are proposed in [R2-2205975](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip)

Slice specific RACH configuration for RA isolation and prioritization can be included in SIB1 messages. The slice specific RACH configurations are associated to specific slice groups, and if not provided for a slice or slice group that UE considers for selecting the RACH configuration, then the UE does not consider the slice(s) for selecting the slice specific RACH configuration, i.e., the UE uses the common RACH configuration. In the UE, NAS provides the NSAGs to be considered during RA to AS.

UE is configured with NSAG mappings per TA for some or all configured slices.

Editor's Note: Details of slice grouping and how it is provided to the UE are FFS, depends on SA2.

**Rapporteur's comments:**

* If the use of NSAG is accepted, then it is proposed to use NSAG here.
* The Editor's Note can be removed, as clarification from SA2 has been received.
* The added sentence in [R2-2205975](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip) is a clarification.

**Question 6**: Which proposals do you support/accept from the following changes in 16.3.3.1?

A) Using NSAG instead of slice groups

B) Changing "RA isolation" to "RA "partitioning"

C) Removing the Editor's Note

D) Adding the clarification "UE is configured with NSAG mappings per TA for some or all configured slices"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Company | Support | Accept | Not Accept | Comments |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Summary 6: TBD**

## 3.7 Clarifications/corrections in 16.3.3a

**The following changes are proposed in** [**R2-2205077**](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205077.zip)**:**

Slice group specific cell reselection information can be included in SIB messages and in *RRCRelease* message. The slice group specific cell reselection information provides information about the frequencies where slice group(s) are supported. It may include reselection priorities per slice group per frequency and corresponding list(s) of cells where the slice group(s) are supported or not supported. In the UE, NAS provides the slice(s) or slice group(s) and their priorities to be considered during cell reselection.

When a UE supports slice aware cell reselection, and when slice specific cell reselection information is provided to the UE, then the UE uses the slice specific cell reselection information. Valid cell reselection information provided in *RRCRelease* always has a priority over cell reselection information provided in SIB messages. When no slice specific reselection information is provided for any slice or slice group that UE AS received from NAS to be considered during cell reselection, then the UE uses the general cell reselection information, i.e., without considering the slice priorities.

Editor's Note: Details of slice grouping and how it is provided to the UE are FFS, depends on SA2.

**The following changes are proposed in** [**R2-2205492**](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205492.zip)**:**

Slice specific cell reselection information can be included in SIB16 and in *RRCRelease* messages. The slice specific cell reselection information may include reselection priorities per NSAG(s) per frequency and corresponding list(s) of cells where the NSAG(s) are supported or not supported. In the UE, NAS provides the NSAG(s) and their priorities to be considered during cell reselection.

When a UE supports slice aware cell reselection, and when slice specific cell reselection information is provided to the UE, then the UE uses the slice specific cell reselection information. Valid cell reselection information provided in *RRCRelease* always has a priority over cell reselection information provided in SIB messages. When no slice specific reselection information is provided for any NSAG(s) that UE AS received from NAS to be considered during cell reselection, then the UE uses the general cell reselection information without considering the NSAG(s) and their priorities.

**The following changes are proposed in** [**R2-2205975**](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_118-e/Docs/R2-2205975.zip)

Slice specific cell reselection information can be included in SIB messages and in *RRCRelease* message. The slice specific cell reselection information provides information about the frequencies where slice group(s) are supported. It may include reselection priorities per slice group per frequency and corresponding list(s) of cells where the slice group(s) are supported or not supported. The UE is over NAS provided with slice group mappings and priorities. The UEs NAS layer provides the slice group(s) and their priorities to be considered during cell reselection.

When a UE supports slice aware cell reselection, and when slice specific cell reselection information is provided to the UE, then the UE uses the slice specific cell reselection information. Valid cell reselection information provided in *RRCRelease* always has a priority over cell reselection information provided in SIB messages. When no slice specific reselection information is provided in SIB or *RRCRelease* message for any slice group that UE AS received from NAS to be considered during cell reselection, then the UE uses the general cell reselection information, i.e., without considering the slice priorities.

Editor's Note: Details of how the UE’s slice priorities are provided to the RAN are FFS, depends on RAN3 and SA2.

**Rapporteur's comments:**

* Removing "slice" from "slice or slice group" is necessary as only slice groups as used. If the use of NSAG is accepted, then it is proposed to use NSAG here.
* The Editor's Note can be removed, as clarification from SA2 has been received. Adding a new Editor's is not needed.
* Other proposed clarifications may be useful

**Question 7**: Which proposals do you support/accept from the following changes in 16.3.3a?

A) Removing "slice" from "slice or slice group"

B) Using NSAG instead of slice groups

C) Removing details on slice specific cell reselection information ""

D) Adding clarification "The UE is over NAS provided with slice group mappings and priorities."

E) Adding clarification " is provided in SIB or *RRCRelease* message for any"

F) Removing the Editor's Note

G) Adding the new Editor's Note "Details of how the UE’s slice priorities are provided to the RAN are FFS, depends on RAN3 and SA2"

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Company | Support | Accept | Not Accept | Comments |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Summary 7: TBD.**

# 4 Conclusion

TBD.