**3GPP TSG-RAN WG2 Meeting #118 Electronic *R2-220xxxx***

**Elbonia, 09 – 20 May 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.300** | **CR** | **0466** | **rev** | **1** | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of RACH partitioning |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_SmallData\_INACTIVE-CoreNR\_Slice -CoreNR\_redcap-CoreNR\_cov\_enh-Core |  | ***Date:*** | 2022-05 |
|  |  |  |  |  |
| ***Category:*** | **Cat F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | RACH partitioning introduction into Stage-2. |
|  |  |
| ***Summary of change:*** | Introduce a description of RACH partitioning into 9.2.6.**Impact analysis**Impacted functionality: Random Access Procedure.Inter-operability: 1. If the network is implemented according to the CR and the UE is not, no inter-operability issues.
2. If the UE is implemented according to the CR and the network is not, no inter-operability issues.
 |
|  |  |
| ***Consequences if not approved:*** | RACH partitioning concept not introduced in Stage-2. |
|  |  |
| ***Clauses affected:*** | 9.2.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*First Modified Subclause*

9.2.6 Random Access Procedure

The random access procedure is triggered by a number of events:

- Initial access from RRC\_IDLE;

- RRC Connection Re-establishment procedure;

- DL or UL data arrival during RRC\_CONNECTED when UL synchronisation status is "non-synchronised";

- UL data arrival during RRC\_CONNECTED when there are no PUCCH resources for SR available;

- SR failure;

- Request by RRC upon synchronous reconfiguration (e.g. handover);

- RRC Connection Resume procedure from RRC\_INACTIVE;

- To establish time alignment for a secondary TAG;

- Request for Other SI (see clause 7.3);

- Beam failure recovery;

- Consistent UL LBT failure on SpCell;

- SDT in RRC\_INACTIVE (see clause 18);

- Positioning purpose during RRC\_CONNECTED requiring random access procedure, e.g., when timing advance is needed for UE positioning.

Two types of random access procedure are supported: 4-step RA type with MSG1 and 2-step RA type with MSGA. Both types of RA procedure support contention-based random access (CBRA) and contention-free random access (CFRA) as shown on Figure 9.2.6-1 below.

The UE selects the type of random access at initiation of the random access procedure based on network configuration:

- when CFRA resources are not configured, an RSRP threshold is used by the UE to select between 2-step RA type and 4-step RA type;

- when CFRA resources for 4-step RA type are configured, UE performs random access with 4-step RA type;

- when CFRA resources for 2-step RA type are configured, UE performs random access with 2-step RA type.

The network does not configure CFRA resources for 4-step and 2-step RA types at the same time for a Bandwidth Part (BWP). CFRA with 2-step RA type is only supported for handover.

The MSG1 of the 4-step RA type consists of a preamble on PRACH. After MSG1 transmission, the UE monitors for a response from the network within a configured window. For CFRA, dedicated preamble for MSG1 transmission is assigned by the network and upon receiving random access response from the network, the UE ends the random access procedure as shown in Figure 9.2.6-1(c). For CBRA, upon reception of the random access response, the UE sends MSG3 using the UL grant scheduled in the response and monitors contention resolution as shown in Figure 9.2.6-1(a). If contention resolution is not successful after MSG3 (re)transmission(s), the UE goes back to MSG1 transmission.

The MSGA of the 2-step RA type includes a preamble on PRACH and a payload on PUSCH. After MSGA transmission, the UE monitors for a response from the network within a configured window. For CFRA, dedicated preamble and PUSCH resource are configured for MSGA transmission and upon receiving the network response, the UE ends the random access procedure as shown in Figure 9.2.6-1(d). For CBRA, if contention resolution is successful upon receiving the network response, the UE ends the random access procedure as shown in Figure 9.2.6-1(b); while if fallback indication is received in MSGB, the UE performs MSG3 transmission using the UL grant scheduled in the fallback indication and monitors contention resolution as shown in Figure 9.2.6-2. If contention resolution is not successful after MSG3 (re)transmission(s), the UE goes back to MSGA transmission.

If the random access procedure with 2-step RA type is not completed after a number of MSGA transmissions, the UE can be configured to switch to CBRA with 4-step RA type.

** **

**(a) CBRA with 4-step RA type (b) CBRA with 2-step RA type**

** **

**(c) CFRA with 4-step RA type (d) CFRA with 2-step RA type**

**Figure 9.2.6-1: Random Access Procedures**

****

**Figure 9.2.6-2: Fallback for CBRA with 2-step RA type**

For random access in a cell configured with SUL, the network can explicitly signal which carrier to use (UL or SUL). Otherwise, the UE selects the SUL carrier if and only if the measured quality of the DL is lower than a broadcast threshold. UE performs carrier selection before selecting between 2-step and 4-step RA type. The RSRP threshold for selecting between 2-step and 4-step RA type can be configured separately for UL and SUL. Once started, all uplink transmissions of the random access procedure remain on the selected carrier.

The network can associate a set of RA resources with feature(s) triggering the Random Access procedure: Network Slicing (see clause 16.3), RedCap (see clause 16.13), SDT (see clause 18), and NR coverage enhancement (see clause 19). A set of RA resources associated with a feature is only valid for random access procedures for that feature; and a set of RA resources associated with several features is only valid for random access procedures having all these features. The UE selects the applicable RA resources set(s), after uplink carrier and BWP selection and before selecting the RA type, according to *one* of the following criteria, listed in priority order:

1. if CFRA resources are available to the current RA procedure or the RA procedure is not initated for any feature, only the sets of RA resources not associated with any feature can be used.

2. if a set of RA resources associated with all the features applicable to the current RA procedure exists, that set of RA resources is used.

3. if the features applicable at initiation of the current RA procedure has no RA resources associated, the UE considers features subset and their associated RA resource sets based on a priority order configured for the features by the network. The first subset in priority order for which there are RA resources set associated, is selected.

4. if there is no RA resources associated with any of the features applicable to the current RA procedure, the sets of RA resources not associated with any feature are used.

When CA is configured, random access procedure with 2-step RA type is only performed on PCell while contention resolution can be cross-scheduled by the PCell.

When CA is configured, for random access procedure with 4-step RA type, the first three steps of CBRA always occur on the PCell while contention resolution (step 4) can be cross-scheduled by the PCell. The three steps of a CFRA started on the PCell remain on the PCell. CFRA on SCell can only be initiated by the gNB to establish timing advance for a secondary TAG: the procedure is initiated by the gNB with a PDCCH order (step 0) that is sent on a scheduling cell of an activated SCell of the secondary TAG, preamble transmission (step 1) takes place on the indicated SCell, and Random Access Response (step 2) takes place on PCell.

*End of Changes*