3GPP RAN WG2 Meeting #119bis-e R2-2210853

eMeeting October 10th – 19th, 2022

Agenda Item: 6.10.3

Source: InterDigital

Title: [DRAFT] Report of [AT119bis-e][111][NR NTN] UP corrections

Document for: Discussion, Decision

# Introduction

This document is intended to address general corrections and address proposals from contributions in AI 6.10.3 as per the following discussion guidelines:

**[AT119bis-e][111][NR NTN] UP corrections (InterDigital)**

* **Initial scope: Discuss UP corrections based on contributions in 6.10.3**
* **Initial intended outcome: Summary of the offline discussion with e.g.:**
	+ **List of proposals for agreement (if any)**
	+ **List of proposals that require online discussions**
	+ **List of proposals that should not be pursued (if any)**

**Please note the following deadlines:**

* **Initial deadline (for companies' feedback): Thursday 2022-10-13 18:00 UTC**
* **Initial deadline (for rapporteur's summary in R2-2210853): Thursday 2022-10-13 22:00 UTC**

**Please also note the following chair guidance:**

Proposals marked "for agreement" in R2-2210853 not challenged until Friday 2022-10-14 10:00 UTC will be declared as agreed via email by the session chair (for the rest the discussion might continue online).

# Remaining corrections from RAN2#119e

## Cancellation of pending SR for TA report

As noted in [2], RAN2 agreed that UE can select between any available SR configuration for SR triggered by Timing Advance Report MAC CE. However, the cancellation of pending SR for TA report is not curently defined in MAC specification.

The following text proposal has been agreed in RAN2#119bis-e to be taken as baseline, with detailed wording to be fine-tuned:

**Baseline text proposal from R2-2210087**

|  |
| --- |
| The MAC entity shall for each pending SR not triggered according to the BSR procedure (clause 5.4.5) for a Serving Cell:…1. if this SR was triggered by consistent LBT failure recovery (see clause 5.21) of an SCell and all the triggered consistent LBT failure(s) for this SCell are cancelled; or

1> if this SR was triggered by Timing Advance report (see clause 5.4.8) and a MAC PDU is transmitted and the MAC PDU includes a Timing Advance Report MAC CE:2> cancel the pending SR and stop the corresponding *sr-ProhibitTimer*, if running. |

The following alternative text proposals have been provided in [2-4]:

**Alternative 1:** [2][R2-2210641](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210641.zip)

|  |
| --- |
| …1> if this SR was triggered by Timing Advance reporting (see clause 5.4.8) and all the triggered Timing Advance reports are cancelled:2> cancel the pending SR and stop the corresponding *sr-ProhibitTimer*, if running. |

**Alternative 2:** [3][R2-2210708](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210708.zip)

|  |
| --- |
| …1> if this SR was triggered by Timing Advance Report procedure (see clause 5.4.8) prior to the MAC PDU assembly and a MAC PDU containing the relevant Timing Advance Report MAC CE is transmitted:2> cancel the pending SR and stop the corresponding *sr-ProhibitTimer*, if running. |

**Alternative 3:** [4][R2-2210768](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210768.zip)

|  |
| --- |
| …1> if the SR is triggered by Timing Advance Reporting (see clause 5.4.8) and the Timing Advance Report MAC CE that triggers the SR has already been cancelled; or2> cancel the pending SR and stop the corresponding *sr-ProhibitTimer*, if running. |

Unless technical justification is provided demonstrating the baseline text from R2-2210087 is insufficient and/or incorrect, Rapporteur suggests the baseline text proposal be agreed and included in NTN MAC corrections CR.

**Question 1: Do you agree to the baseline text proposal for SR cancellation in** [**R2-2210087**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210087.zip)**? If ‘Disagree’, please: 1) indicate which of the above alternatives is preferred; and 2) provide technical justification why the baseline is insufficient.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Cancellation of RACH due to pending SR for TA report

[2] Further notes that the ongoing Random Access procedure due to a pending SR for Timing Advance Report MAC CE should be stopped if the MAC CE is included in a transmitted MAC PDU. This is also not currently captured in MAC specification.

The following text proposal has been agreed in RAN2#119bis-e to be taken as baseline, with detailed wording to be fine-tuned:

**Baseline text proposal from R2-2210087**

|  |
| --- |
| …The MAC entity may stop, if any, ongoing Random Access procedure due to a pending SR for positioning measurement gap activation/deactivation request, which has no valid PUCCH resources configured, if:- the Positioning Measurement Gap Activation/Deactivation Request MAC CE that triggers the SR corresponding to the Random Access procedure has already been cancelled.The MAC entity may stop, if any, ongoing Random Access procedure due to a pending SR for Timing Advance report, which has no valid PUCCH resources configured, if:- a MAC PDU is transmitted using a UL grant other than a UL grant provided by Random Access Response or a UL grant determined as specified in clause 5.1.2a for the transmission of the MSGA payload, and this PDU includes a Timing Advance Report MAC CE. |

The following alternative text proposals have been provided in [2] and [3]:

**Alternative 1:** [2][R2-2210641](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210641.zip)

|  |
| --- |
| The MAC entity may stop, if any, ongoing Random Access procedure due to a pending SR for Timing Advance Report MAC CE, which has no valid PUCCH resources configured, if:- a MAC PDU is transmitted using a UL grant other than a UL grant provided by Random Access Response or a UL grant determined as specified in clause 5.1.2a for the transmission of the MSGA payload, and this PDU contains a Timing Advance Report MAC CE which includes the latest available estimate of the UE’s Timing Advance value prior to the MAC PDU assembly. |

**Alternative 2:** [3][R2-2210708](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210708.zip)

|  |
| --- |
| The MAC entity may stop, if any, ongoing Random Access procedure due to a pending SR for Timing Advance report, which has no valid PUCCH resources configured, if:- the Timing Advance Report MAC CE that triggers the SR corresponding to the Random Access procedure has already been cancelled. |

Unless technical justification is provided demonstrating the baseline text from R2-2210087 is insufficient and/or incorrect, Rapporteur suggests the baseline text proposal be agreed and included in NTN MAC corrections CR.

**Question 2: Do you agree to the baseline text proposal for RACH cancellation in** [**R2-2210087**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210087.zip)**? If ‘Disagree’, please: 1) indicate which of the above alternatives is preferred; and 2) provide technical justification why the baseline is insufficient.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Other corrections

Contributions [4-6] also provide additional corrections and text proposals. A summary of main issues and proposed resolutions is provided below, however companies are encouraged to review referenced papers for detailed discussion.

### Corrections to Random Access

As noted in [5], RAN1 has specified in TS 38.213 that UE pre-compensates the RTT between UE and the reference point for the uplink timing adjustment in NTN. Currently, the related UE behaviour on how this pre-compensation is considered during PRACH occasion selection is not captured in the latest MAC spec.

[5] notes that a clear UE behaviour to clarify such a procedure specific for NTN is preferable, thus, it is proposed to add the description in the TS 38.321 clause 5.1.2 that if Random Access Preamble is transmitted on a non-terrestrial network, the MAC entity shall take into account the UE-RP RTT when determining the next available PRACH occasion.

**Question 3a: Do you agree to specify that if Random Access Preamble is transmitted in the non-terrestrial network, the MAC entity shall take into account the RTT between UE and the reference point when determining the next available PRACH occasion?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 3b: If ‘Agree’ to Question 3a, do you agree to the text proposal from** [**R2-2209503**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209503.zip) **as baseline?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Corrections on reported value for event-triggered TA report

As noted in [6], in the previous meeting it was agreed that the TAR MAC CE shall be generated based on the latest available estimate of the UE’s Timing Advance value prior to the MAC PDU assembly. However, the time between when a TA report is triggered and the TA report is generated may be long. For the case that the TA report is triggered due to the variation between current TA and the last reported TA becoming larger than *offsetThresholdTA*, it may result in that the TA value to be reported doesn’t fulfil the condition of triggering the TA report (e.g. the current TA at time of assembly may have fallen back below the threshold).

[6] notes that in this case, it may make sense to re-evaluate the offsetThresholdTA when the TAR MAC CE is to be generated if corresponding TA report is triggered by offsetThresholdTA. If the TA value to be reported doesn’t fulfil the condition of the trigger, the TA report is cancelled.

**Question 4a: Do you agree to cancel the TA report if the variation between the latest TA value prior to the MAC PDU assembly and the last reported TA becomes lower than *offsetThresholdTA*?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 4b: If ‘Agree’ to Question 4a, do you agree to the text proposal from** [**R2-2209849**](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209849.zip) **as baseline?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments**  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Editorial corrections

Several editorial corrections have additionally been captured in [4]. Companies are encouraged to review the draft CR provided within the Offline discussion folder and provide comments (if any) within that document.

If a company does not question an editorial correction, it is assumed agreeable.

# Summary

<To be generated based on company input>

# Conclusions

<To be generated based on company input>

# References

1. [R2-2210087](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210087.zip) – Correction to TA report triggered SR and DRX – OPPO
2. [R2-2210641](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210641.zip) – Correction on SR cancellation and Random Access procedure stop for NTN – Nokia, Nokia Shanghai Bell
3. [R2-2210708](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210708.zip) – Correction on SR triggered by TAR – ZTE Corporation, Sanechips
4. [R2-2210768](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210768.zip) – Corrections to TS 38.321 for Rel-17 NR NTN – Samsung Research America
5. [R2-2209503](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209503.zip) – On corrections on random access procedure in NR NTN – vivo
6. [R2-2209849](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209849.zip) – Discussion on reported value for event-triggered TA report – ASUSTek