**3GPP T****SG-RAN WG2 Meeting #119bis-e R2-2210860**

**E-Meeting, Oct 10 – 19, 2022**

**Agenda item:**  **8.7.4**

**Source: Intel Corporation**

**Title: Report of [AT119bis-e][117][NR NTN Enh] cell reselection enhancements (Intel)**

**Document for: Discussion and Decision**

# Introduction

This is the report of the following offline discussion on cell reselection enhancements:

* [AT119bis-e][117][NR NTN Enh] cell reselection enhancements (Intel)

Scope: Discuss NTN-NTN and NTN-TN cell reselection enhancements based on remaining proposals in [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) and [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx)

Initial intended outcome: Summary of the offline discussion with e.g.:

* List of proposals for agreement (if any)
* List of proposals that require online discussions
* List of proposals that should not be pursued (if any)

Initial deadline (for companies' feedback): Tuesday 2022-10-18 0600 UTC

Initial deadline (for rapporteur's summary in R2-2210860): Tuesday 2022-10-18 0800 UTC

And according to session chair’s guidance, “Regarding [117] and [118], please note that, besides those in the listed papers, the offlines may also consider alternative proposals from other papers, if they are on the same issues as covered in the selected papers. But additional issues/completely separate proposals should be excluded for now (as otherwise the discussions will explode).”

# Discussion

## 2.1 NTN-NTN cell reselection

During the online discussion in first week, the following agreement was achieved as high level guideline:

Agreements:

1. For NTN-NTN cell reselection with earth moving cell, RAN2 will consider providing parameters of serving cell to UE, for UE to estimate when the serving cell stops providing coverage at the present UE location (FFS whether this will be an optional UE feature) (this does not exclude any time-based or location-based approach) (other solutions can also be considered)

In the following sub-sections, a few detailed designs can be discussed based on relevant proposals.

### 2.1.1 Assistance information of serving cell for UE to estimate when the serving cell stops providing coverage at the present UE location

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | Proposal 1: For NTN-NTN cell reselection with earth moving cell, to consider providing parameters of serving cell to UE for UE to estimate the stop time of serving cell. These parameters of the serving cell can be satellite orbital parameters, location coordinates of cell center and the radius of cell coverage. |
| [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx) | Proposal 1: UE performs individual estimation, considering satellite’s ephemeris, cell reference location and its own location to enable location-based reselections in Earth-moving scenario. |
| [R2-2210468](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210468-8.7.4-cell-reselection-enhancement.docx)  | Proposal 4: If the serving cell is an earth-moving cell, NW provides assistance information for UE to estimate the serving cell movement for location-based cell reselection measurement. |
| [R2-2210737](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210737-Discussion-on-idle-mode-aspects-for-NTN.docx) | Proposal 5 Multiple reference locations and its time information should be broadcasted to provide time-variant reference location of earth moving cell. |
| R2-2210090 | Proposal 1 RAN2 to discuss the following options on location-based measurement initiation for earth moving cell:- Option 1: A new distance threshold for the distance between UE and the serving satellite, i.e., service link distance.- Option 2: Rel-17 distance threshold with the cell reference location determination based on the sub-satellite point (derived by satellite ephemeris) and the broadcasted location offset between sub-satellite point and the cell reference location.  |

Based on above proposals, in Earth-moving cell UE is able to estimate the movement of cell coverage according to assistance information provided by network. As UE location is also known by UE, then UE can tell when serving cell stops providing coverage at the present UE location.

Regarding the assistance information provided by network,

1. satellite orbital parameters. Ephemeris data (one type is for satellite orbital parameters, the other type is for instantaneous position and velocity of satellite) is already included in SIB19. And for prediction of movement of cell coverage, satellite orbital parameters should be provided.

2. the location of cell center. Similarly, the reference location has been specified for Quasi-Earth-fixed cell, and it can also be provided in Earth-moving cell. Another alternative is to provide “Multiple reference locations and its time information”, instead of updating the value every time along with the cell movement.

3. the radius of cell coverage. Similarly, the distance threshold have been specified for Quasi-Earth-fixed cell, and it can also be provided in Earth-moving cell.

**Question 1: Regarding the assistance information of serving cell for UE to estimate when the serving cell stops providing coverage at the present UE location, whether the following parameters should be provided by network** **in Earth-moving cell:**

1. **satellite orbital parameters, not instantaneous position and velocity of satellite**
2. **location coordinates of cell center, or in other term, cell reference location**
3. **the radius of cell coverage, or in other term, a distance threshold**
4. **a distance threshold between UE and satellite**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2: Regarding how to provide the location coordinates of cell center by network (if it is agreed to be provided as discussed in Q1):**

**Option 1: only location coordinates of current cell center, and network is supposed to update the values every time when it is provided for Earth-moving cell.**

**Option 2:** **multiple reference locations and its time information of Earth-moving cell.**

**Option 3: based on the sub-satellite point derived by satellite ephemeris and the broadcasted location offset between sub-satellite point and the cell reference location**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1 or 2 or 3** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

As for how to provide this assistance information, the following proposal is made.

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx) | Proposal 3: System information is the basic means for providing necessary parameters to assist the NTN UE in intra-NTN cell reselection process. |

Considering the outcome of Q1 and Q2, the proposal is updated to be more specific as below:

Proposal: System information is the basic means for providing necessary parameters to assist UE to estimate when the serving cell stops providing coverage at the present UE location.

**Question 3: whether the following proposal is agreeable:**

**Proposal: System information is the basic means for providing necessary parameters to assist UE to estimate when the serving cell stops providing coverage at the present UE location.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.1.2 Assistance information of neighbour cell for UE to estimate when the neighbour cell starts providing coverage at the present UE location

According to the following proposal, if a UE is able to estimate when the serving cell stops providing coverage at the present UE location, it can also estimate when the neighbour cell starts providing coverage at the present UE location, then it can know which neighbour cells are the next upcoming cells.

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | Proposal 3: The parameters explained in Proposal 1 can also be for neighbour cells for UE to estimate which cells are the upcoming cells for cell reselection. I.e., these parameters of the neighbour cell can be satellite orbital parameters, location coordinates of cell center and the radius of cell coverage. |

**Question 4: whether the assistance information below of a neighbour cell can be used for UE to estimate when the neighbour cell starts providing coverage at the present UE location.**

1. **satellite orbital parameters, not instantaneous position and velocity of satellite**
2. **location coordinates of cell center, or in other term, cell reference location**
3. **the radius of cell coverage, or in other term, a distance threshold**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.1.3 Whether a UE can relax neighbour cell measurements before the serving cell stops providing coverage at the present UE location

According to the following proposal, in order to save UE power consumption, before the serving cell stops providing coverage at the present UE location, it’s beneficial to relax neighbour cell measurements.

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | Proposal 2: If proposal 1 is agreed, to define a new trigger for the measurement relaxation considering the estimated cell stop time. For example, after UE camps in a cell, or for certain time “x”, UE may be allowed to relax neighbour cell measurements until the estimated cell stop time or certain time “y” before the estimated stop time. |

**Question 5: whether a UE is allowed to relax neighbour cell measurements** **before the serving cell stops providing coverage at the present UE location.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.1.4 t-service in Earth-moving cell

In previous questions, the discussion point is whether UE can estimate the “t-service” itself for Earth-moving cell. According to the following proposals, it’s proposed to t-service is still provided in Earth-moving cell, e.g., only “valid for a particular location on Earth”. And the t-service update scheme should also be considered.

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx) | Proposal 2: To enable time-based reselections in Earth-moving scenario, the IDLE UE is capable of computing its own location to adjust t-Service provided in SIB19.  |
| [R2-2210589](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210589.docx) | Proposal 4: Introduce reference location and/or t-service update scheme for cell reselection enhancements for earth moving cell |
| R2-2210090 | Proposal 2 For time-based measurement initiation for earth moving cell, RAN2 consider introducing a new time threshold T1 according to the time when the moving serving cell comes across some neighbour cells’ coverage. FFS on whether T1 is configured per UE or per frequency. |

**Question 6: if RAN2 agrees that UE is able to estimate when the serving cell stops providing coverage at the present UE location, whether t-service still needs to be provided in system information by network in Earth-moving cell.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 NTN-TN cell reselection

During the online discussion in first week, the following agreement was achieved:

Agreements:

1. To enhance NTN-TN cell reselection, means are defined for a UE to differentiate when camping in an area only covered by NTN network (earth-moving or earth-fixed) vs an area where TN network(s) is/are also available.

### 2.2.1 Cell type (i.e. “TN” vs “NTN”)

Regarding the cell type (i.e. “TN” vs “NTN”), it is proposed that it should be indicated explicitly for a neighbour cell in some proposals below. And there is also one proposal to mention that “a UE can distinguish whether a neighbor cell or frequency belongs to a terrestrial or non-terrestrial network via existing specification”, e.g., “based on the ARFCN of the neighbouring carrier”.

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | Proposal 4.1. If proposal 4 is agreed,” cell type" (i.e. “TN” vs “NTN”) of a neighbour cell is indicated to UE (e.g. explicitly or implicitly). |
| [R2-2210217](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210217.docx) | Proposal 3: Serving cell’s system information include an indication that whether a neighbour cell is an NTN cell or not. |
| [R2-2210438](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210438--R18-NR-NTN-WI-AI-8.7.4--Idle-Inactive-enhancements.docx) | Proposal 7: RAN2 to confirm that a UE can distinguish whether a neighbor cell or frequency belongs to a terrestrial or non-terrestrial network via existing specification. |
| [R2-2210598](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210598.docx) | Proposal 3: We can introduce an indication to identify TN cells in the different neighbor lists. |

After further checking, Rapporteur thinks it’s not feasible to solely rely on ARFCN to distinguish TN cell from NTN cell, as there is an overlap between TN bands and NTN bands.

RAN4 has defined NTN specific band in TS 38.101-5 as below:

Table 5.2.2-1: NTN satellite bands in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NTN satellite operating band | Uplink (UL) operating bandSatellite Access Node receive / UE transmitFUL,low – FUL,high | Downlink (DL) operating bandSatellite Access Node transmit / UE receiveFDL,low – FDL,high  | Duplex mode |
| n256 | 1980MHz – 2010 MHz | 2170 MHz – 2200 MHz | FDD |
| n255 | 1626.5 MHz – 1660.5 MHz | 1525 MHz – 1559 MHz | FDD |
| NOTE: NTN satellite bands are numbered in descending order from n256. |

And the NTN frequency range is totally the same as (n255 and n24) or included in TN bands (n256 and n65).

Table 5.2-1: NR operating bands in FR1

|  |  |  |  |
| --- | --- | --- | --- |
| NR operating band | Uplink (UL) *operating band*BS receive / UE transmitFUL\_low  – FUL\_high | Downlink (DL) *operating band*BS transmit / UE receiveFDL\_low – FDL\_high | Duplex Mode |
| n1 | 1920 MHz – 1980 MHz | 2110 MHz – 2170 MHz | FDD |
| n2 | 1850 MHz – 1910 MHz | 1930 MHz – 1990 MHz | FDD |
| n3 | 1710 MHz – 1785 MHz | 1805 MHz – 1880 MHz | FDD |
| n5 | 824 MHz – 849 MHz | 869 MHz – 894 MHz | FDD |
| n7 | 2500 MHz – 2570 MHz | 2620 MHz – 2690 MHz | FDD |
| n8 | 880 MHz – 915 MHz | 925 MHz – 960 MHz | FDD |
| n12 | 699 MHz – 716 MHz | 729 MHz – 746 MHz | FDD |
| n13 | 777 MHz – 787 MHz | 746 MHz – 756 MHz | FDD |
| n14 | 788 MHz – 798 MHz | 758 MHz – 768 MHz | FDD |
| n18 | 815 MHz – 830 MHz | 860 MHz – 875 MHz | FDD |
| n20 | 832 MHz – 862 MHz | 791 MHz – 821 MHz | FDD |
| n2416 | 1626.5 MHz – 1660.5 MHz | 1525 MHz – 1559 MHz | FDD |
| n25 | 1850 MHz – 1915 MHz | 1930 MHz – 1995 MHz | FDD |
| n26 | 814 MHz – 849 MHz | 859 MHz – 894 MHz | FDD |
| n28 | 703 MHz – 748 MHz | 758 MHz – 803 MHz | FDD |
| n29 | N/A | 717 MHz – 728 MHz | SDL |
| n303 | 2305 MHz – 2315 MHz | 2350 MHz – 2360 MHz | FDD |
| n34 | 2010 MHz – 2025 MHz | 2010 MHz – 2025 MHz | TDD |
| n3810 | 2570 MHz – 2620 MHz | 2570 MHz – 2620 MHz | TDD |
| n39 | 1880 MHz – 1920 MHz | 1880 MHz – 1920 MHz | TDD |
| n40 | 2300 MHz – 2400 MHz | 2300 MHz – 2400 MHz | TDD |
| n41 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD |
| n46 | 5150 MHz – 5925 MHz | 5150 MHz – 5925 MHz | TDD13 |
| n4711 | 5855 MHz – 5925 MHz | 5855 MHz – 5925 MHz | TDD |
| n48 | 3550 MHz – 3700 MHz | 3550 MHz – 3700 MHz | TDD |
| n50 | 1432 MHz – 1517 MHz | 1432 MHz – 1517 MHz | TDD1 |
| n51 | 1427 MHz – 1432 MHz | 1427 MHz – 1432 MHz | TDD |
| n53 | 2483.5 MHz – 2495 MHz | 2483.5 MHz – 2495 MHz | TDD |
| n65 | 1920 MHz – 2010 MHz | 2110 MHz – 2200 MHz | FDD4 |
| n66 | 1710 MHz – 1780 MHz | 2110 MHz – 2200 MHz | FDD |
| n67 | N/A | 738 MHz – 758 MHz | SDL |
| n70 | 1695 MHz – 1710 MHz | 1995 MHz – 2020 MHz | FDD |
| n71 | 663 MHz – 698 MHz | 617 MHz – 652 MHz | FDD |
| n74 | 1427 MHz – 1470 MHz | 1475 MHz – 1518 MHz | FDD |
| n75 | N/A | 1432 MHz – 1517 MHz | SDL |
| n76 | N/A | 1427 MHz – 1432 MHz | SDL |
| n7712 | 3300 MHz – 4200 MHz | 3300 MHz – 4200 MHz | TDD |
| n78 | 3300 MHz – 3800 MHz | 3300 MHz – 3800 MHz | TDD |
| n7917 | 4400 MHz – 5000 MHz | 4400 MHz – 5000 MHz | TDD |
| n80 | 1710 MHz – 1785 MHz | N/A | SUL  |
| n81 | 880 MHz – 915 MHz | N/A | SUL  |
| n82 | 832 MHz – 862 MHz | N/A | SUL  |
| n83 | 703 MHz – 748 MHz | N/A | SUL |
| n84 | 1920 MHz – 1980 MHz | N/A | SUL |
| n85 | 698 MHz – 716 MHz  | 728 MHz – 746 MHz | FDD |
| n86 | 1710 MHz – 1780 MHz | N/A | SUL |
| n89 | 824 MHz – 849 MHz | N/A | SUL |
| n90 | 2496 MHz – 2690 MHz | 2496 MHz – 2690 MHz | TDD5 |
| n91 | 832 MHz – 862 MHz | 1427 MHz – 1432 MHz | FDD9 |
| n92 | 832 MHz – 862 MHz | 1432 MHz – 1517 MHz | FDD9 |
| n93 | 880 MHz – 915 MHz | 1427 MHz – 1432 MHz | FDD9 |
| n94 | 880 MHz – 915 MHz | 1432 MHz – 1517 MHz | FDD9 |
| n958 | 2010 MHz – 2025 MHz | N/A | SUL |
| n9614 | 5925 MHz – 7125 MHz | 5925 MHz – 7125 MHz | TDD13 |
| n9715 | 2300 MHz – 2400 MHz | N/A | SUL |
| n9815 | 1880 MHz – 1920 MHz | N/A | SUL |
| n9916 | 1626.5 MHz – 1660.5 MHz | N/A | SUL |
| n100 | 874.4 MHz – 880 MHz | 919.4 MHz – 925 MHz | FDD |
| n101 | 1900 MHz – 1910 MHz | 1900 MHz – 1910 MHz | TDD |
| n10214 | 5925 MHz – 6425 MHz | 5925 MHz – 6425 MHz | TDD13 |
| n10417,18 | 6425 MHz – 7125 MHz | 6425 MHz – 7125 MHz | TDD |
| NOTE 1: UE that complies with the NR Band n50 minimum requirements in this specification shall also comply with the NR Band n51 minimum requirements.NOTE 2: UE that complies with the NR Band n75 minimum requirements in this specification shall also comply with the NR Band n76 minimum requirements.NOTE 3: Uplink transmission is not allowed at this band for UE with external vehicle-mounted antennas.NOTE 4: A UE that complies with the NR Band n65 minimum requirements in this specification shall also comply with the NR Band n1 minimum requirements.NOTE 5: Unless otherwise stated, the applicability of requirements for Band n90 is in accordance with that for Band n41; a UE supporting Band n90 shall meet the requirements for Band n41. A UE supporting Band n90 shall also support band n41.NOTE 6: A UE that supports NR Band n66 shall receive in the entire DL operating band.NOTE 7: A UE that supports NR Band n66 and CA operation in any CA band shall also comply with the minimum requirements specified for the DL CA configurations CA\_n66B and CA\_n66(2A) in the current version of the specification.NOTE 8: This band is applicable in China only.NOTE 9: Variable duplex operation does not enable dynamic variable duplex configuration by the network, and is used such that DL and UL frequency ranges are supported independently in any valid frequency range for the band. NOTE 10: When this band is used for V2X SL service, the band is exclusively used for NR V2X in particular regions.NOTE 11: This band is unlicensed band used for V2X service. There is no expected network deployment in this band.NOTE 12: In the USA this band is restricted to 3450 – 3550 MHz and 3700 – 3980 MHz. In Canada this band is restricted to 3450 – 3650 MHz and 3650 – 3980 MHz.NOTE 13: This band is restricted to operation with shared spectrum channel access as defined in 37.213.NOTE 14: This band is applicable only in countries/regions designating this band for shared-spectrum access use subject to country-specific conditions.NOTE 15: The requirements for this band are applicable only where no other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area. For scenarios where other NR or E-UTRA TDD operating band(s) are used within the frequency range of this band in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.NOTE 16: DL operation in this band is restricted to 1526 – 1536 MHz and UL operation is restricted to 1627.5 – 1637.5 MHz and 1646.5 – 1656.5 MHz.NOTE 17: For this band, CORESET#0 values from Table 13-5 or Table 13-6 in [8, TS 38.213] are applied regardless of the minimum channel bandwidth.NOTE 18: [This band is applicable only to RCC countries in accordance with RCC Recommendation 1/21] |

**Question 7: whether the following proposal is agreeable:**

**Proposal: add an indication of the “cell type” (i.e. “TN” vs “NTN”) of a neighbour cell in system information.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2.2 Assistance information for UE to identify an area where TN network is available

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | Proposal 4.2. If proposal 4 is agreed, network provides assistance information of NTN-only area (e.g., cell center and cell radius of TN neighbour cells and NTN serving cell, or the boundary line between TN area and NTN area). |
| [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx) | Proposal 5: RAN2 is asked to consider the method where System Information provides a location-related indication where the search for TN coverage shall be initiated.  |
| R2-2209753 | Proposal 3 In NTN-TN cell reselection for high priority cells, RAN2 shall introduce a new distance threshold for measurement enhancement. |
| [R2-2210045](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210045_NTN_mobility.docx) | Proposal 1: Network provides reference location(s) of TN cells and a distance threshold for measurements of TN frequencies in SIB19 to assist RRC\_IDLE/RRC\_INACTIVE UE in determining whether to perform measurements of TN frequencies for cell reselection. |
| [R2-2210090](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210090-Discussion-on-mobility-enhancements-for-idle-and-inactive-UEs.doc) | Proposal 3 For quasi-earth fixed cells, TN coverage described by a distance range from the cell center and an angle range based on a reference direction can be broadcasted to UEs to assist the TN neighbour cell measurement initiation. Proposal 4 RAN2 to discuss the following options for the distance/angle range:- Option 1: Two thresholds, i.e., the minimum threshold and the maximum threshold.- Option 2: One minimum threshold and one range, i.e. the maximum threshold can be determined based on the minimum threshold and the range.  |
| [R2-2210159](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210159-Cell-reselection-enhancements.docx) | Proposal 6: It is proposed to provide reference location of TN neighbor cell, cell coverage radius of TN neighbor cell, relative position to the current NTN cell, etc. to help UE choose suitable TN neighbor cell. |
| [R2-2210217](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210217.docx) | Proposal 1: For RRC\_IDLE and RRC\_INACTIVE UEs, an indication could be included in system information to indicate NTN cell’s coverage overlaps with terrestrial TN cell’s coverage. With this indication, UE may ignore serving cell thresholds and perform TN cell measurements. |
| [R2-2210468](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210468-8.7.4-cell-reselection-enhancement.docx)  | Proposal 3: For cell reselection in NTN-NTN and NTN-TN mobility, NW provides TN cell information according to the location within a NTN cell. |
| [R2-2210737](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210737-Discussion-on-idle-mode-aspects-for-NTN.docx) | Proposal 2 Introduce assistance information about an area where TN cell is not deployed and TN frequency identifier to perform reduced measurement on TN frequencies. |

Regarding the Assistance information for UE to identify an area where TN network is available, the following options are proposed based on the proposals above:

1. The cell center and cell radius of TN neighbour cells, or in other terms, the reference location and a distance threshold of TN neighbour cells
2. the boundary line between TN area and NTN area
3. For quasi-earth fixed cells, TN coverage is described by a distance range from the cell center and an angle range based on a reference direction
4. an indication could be included in system information to indicate NTN cell’s coverage overlaps with terrestrial TN cell’s coverage

**Question 8: Regarding the Assistance information for UE to identify an area where TN network is available, which option(s) is agreeable:**

1. The cell center and cell radius of TN neighbour cells, or in other terms, the reference location and a distance threshold of TN neighbour cells
2. The boundary line between TN area and NTN area
3. For quasi-earth fixed cells, TN coverage is described by a distance range from the cell center and an angle range based on a reference direction
4. An indication could be included in system information to indicate NTN cell’s coverage overlaps with terrestrial TN cell’s coverage

|  |  |  |
| --- | --- | --- |
| **Company** | **option 1/2/3/4** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2.3 UE measurement related behaviour in an area where TN network is not available

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2209578](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2209578%20Discussion%20on%20NTN%20cell%20reselection%20enhancements.docx) | If proposal 4 is agreed, when a UE is in NTN only area, UE is not required to perform neighbour cell measurements for TN neighbour cells. |
| [R2-2210045](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210045_NTN_mobility.docx) | Proposal 2: If reference location(s) of TN cells and a distance threshold for measurements of TN frequencies are provided in SIB19, and if the distance between UE and any of the reference location(s) of TN cells is longer than the distance threshold, UE is not required to perform measurements of TN frequencies for inter-frequency cell reselection. |
| [R2-2210217](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210217.docx) | Proposal 2: The assistance information could be a distance threshold to a reference location. If UE moves beyond that threshold then it will start performing TN measurement. |
| [R2-2210737](file:///C%3A%5CRAN2%20work%5CRAN2-119bis%202210%5Ctdoc%5CR2-2210737-Discussion-on-idle-mode-aspects-for-NTN.docx) | Proposal 1 The UE performs measurement on TN frequencies where it can find available TN cells. |

According to the proposals above, UE is not required to perform neighbour cell measurements for TN neighbour cells, when there is no TN network coverage.

**Question 9: whether the following proposal is agreeable:**

**Proposal: UE is not required to perform neighbour cell measurements for TN neighbour cells in an area where there is no TN network coverage.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2.4 Detection of NTN coverage

|  |  |
| --- | --- |
| Tdoc | Proposals |
| [R2-2210353](file:///C%3A%5CData%5C3GPP%5CExtracts%5CR2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx) | **Proposal 4: RAN2 is asked to consider the method of detecting the transmission energy or SIB presence to determine the NTN coverage.** |

In R2-2210353, one enhancement is proposed that it would be beneficial to start searching for NTN cells only when needed, e.g., UE is about to move out from TN coverage. And the corresponding method could be detecting the transmission energy or SIB presence to determine the NTN coverage.

**Question 10: whether to consider the method of detecting the transmission energy or SIB presence to determine the NTN coverage when a UE currently camps on a TN cell?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y or N** | **Additional comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion