3GPP TSG-RAN WG2 Meeting #119bis Electronic draftR2-2210862

Elbonia, 10 – 19 October 2022

**Agenda item: 8.7.4**

**Source: Nokia, Nokia Shanghai Bell**

**Title: Report from [AT119bis-e][119][NR NTN Enh] HO enhancements (Nokia)**

**WID/SID: NR\_NTN\_enh – Rel-18**

**Document for: Discussion and Decision**

# 1 Introduction

This is to discuss the following:

* [AT119bis-e][119][NR NTN Enh] HO enhancements (Nokia)

Scope: Discuss possible CHO-based approach (p6 in [R2-2210353](file:///C:\Data\3GPP\Extracts\R2-2210353%20Further%20view%20on%20Idle-%20and%20Connected-mode%20NTN%20mobility%20in%20Rel-18.docx)) and “same PCI” approach (p5 in [R2-2210405](file:///C:\Data\3GPP\Extracts\R2-2210405%20Discussion%20on%20NTN%20mobility%20enhancements.doc)) for connected mode mobility enhancements in NTN

Initial intended outcome: Summary of the offline discussion with e.g.:

* List of proposals for agreement (if any)
* List of proposals that require online discussions
* List of proposals that should not be pursued (if any)

Initial deadline (for companies' feedback): Tuesday 2022-10-18 1600 UTC

Initial deadline (for rapporteur's summary in R2-2210862): Tuesday 2022-10-18 1800 UTC

In the next section we elaborate on CHO enhancements and on reusing the same PCI in quasi-Earth-fixed scenario.

# 2 Discussion

## 2.1 NTN-specific CHO enhancements

In [1] it is suggested to consider how to reduce the signalling overhead and allow the UE to keep the CHO commands even after HO execution. It is claimed that in NTN the sequence of next serving cells can be predicted with high probability (assuming the UE does not move significantly, compared to the satellite coverage, which should be the case in NTN). We would like to ask the companies if they agree with such statement.

|  |  |  |
| --- | --- | --- |
| **Question 1: Do you agree that in NTN the sequence of next serving cells can be predicted?** | | |
| **Company** | **Answer** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

*Summary for Q1:*

If the approximate sequence of cells can be known in advance and as Conditional Handover (CHO) is a supported solution, [1] suggests to combine these two and allow preparing the UE for multiple cell hops in advance (i.e. enhancement compared to contemporary CHO standard, where the UE can be prepared just for the nearest cell change). UE would be provided in advance with cell-specific resources and configurations for one or more of the next serving cells (i.e. not only for the single cell change operation).

|  |  |  |
| --- | --- | --- |
| **Question 2: Do you support allowing the UE to be configured with CHO commands for multiple cell changes in advance and store some of these commands after CHO execution?** | | |
| **Company** | **Answer** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

*Summary for Q2:*

## 2.2 Reusing PCI after satellite changes

Another connected mobility enhancement is considered in [2]. It is proposed to address the quasi-Earth fixed scenario using the same gNB serving a particular area, even after the satellite changes. The authors of [2] claim the clear gain is that the UE will not have to handover and can continue using the same configuration. However, the authors of [2] indicate that the UE will have to anyway perform UL synchronization due to the changed position of the satellites. While the idea seems to be simple and promising in terms of the gains on the UE side, it is not clarified what is the expected impact/additional complexity on the NW side. In addition, the rapporteur wonders how would that co-exist with Rel-17 NTN mobility. Thus, we would like to ask the following:

|  |  |  |
| --- | --- | --- |
| **Question 3: Do you support the mobility scheme where PCI remains the same after switching of the satellites? Please provide the details on:**   1. **expected impact on the NW side** 2. **co-existence with Rel-17 NTN mobility** | | |
| **Company** | **Answer** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

*Summary for Q3:*

# 3 Conclusion

This paper discussed selected mobility enhancements for Rel-18 NTN. The following proposals are made:

For agreement:

For further discussion:

# References

1. R2-2210353 Further view on Idle- and Connected-mode NTN mobility in Rel-18, 3GPP TSG RAN2 Meeting #119bis Electronic Meeting, Oct 10 - 19, 2022
2. R2-2210405 Discussion on NTN mobility enhancements, 3GPP TSG RAN2 Meeting #119bis Electronic Meeting, Oct 10 - 19, 2022