3GPP TSG-RAN WG2 Meeting #119bis-e R2-2210863

Electronic Meeting, 10 – 19 October, 2022

**Agenda item: 8.6.2.1**

**Source: CMCC**

**Title: Report for [AT119bis-e][120][IoT NTN Enh]** **HARQ enhancements (CMCC)**

**WID/SID: IoT\_NTN\_enh**

**Document for: Discussion and Decision**

# Introduction

This document aims at address the remaining open issues for HARQ enhancements for IoT NTN.

* [AT119bis-e][120][IoT NTN Enh] HARQ enhancements (CMCC)

Scope: Continue the discussion on p4, p5 from [R2-2210152](file:///C:\Data\3GPP\Extracts\R2-2210152%20Discussion%20on%20the%20HARQ%20enhancement%20for%20IoT-NTN.docx) as well as p6 and p8 from [R2-2210036](file:///C:\Data\3GPP\Extracts\R2-2210036%20Discussion%20on%20disabling%20of%20HARQ%20feedback.doc)

Initial intended outcome: Summary of the offline discussion with e.g.:

* List of proposals for agreement (if any)
* List of proposals that require online discussions
* List of proposals that should not be pursued (if any)

Initial deadline (for companies' feedback): Tuesday 2022-10-18 1000 UTC

Initial deadline (for rapporteur's summary in R2-2210863): Tuesday 2022-10-18 1200 UTC

2 Contact Information

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion

## 3.1 DRX impacts

### 3.1.1 For DL HARQ process

In Rel-17 NR NTN, RAN2 agreed the following agreements on enabling/disabling DL HARQ feedback.

|  |
| --- |
| * For HARQ process with DL HARQ feedback disabled, the UE will not start drx-HARQ-RTT-TimerDL. * For HARQ process with DL HARQ feedback enabled, the UE will extend the value of drx-HARQ-RTT-TimerDL by UE-gNB RTT and start the timer.   For HARQ process not configured with DL HARQ feedback enabled/disabled, drx-HARQ-RTT-TimerDL behaves as per legacy. |

And RAN2-119 meeting agreed to support HARQ feedback enabling/disabling for DL and two HARQ modes for UL in both NB-IoT and eMTC.

|  |
| --- |
| Agreements:   1. Disabling DL HARQ feedback is supported for NB-IoT and eMTC NTN. FFS on UE capability 2. For UL HARQ operation, introduce two HARQ modes, i.e., HARQ mode A and HARQ mode B in IoT NTN (both NB-IoT and eMTC NTN), similarly to NR NTN 3. From RAN2 perspective, at least for eMTC, enabling/disabling HARQ feedback can be configured per DL HARQ process at least via UE specific RRC signalling. FFS for NB-IoT (and especially for CP solution for NB-IOT). |

Meanwhile, for NB-IoT DL transmission, RAN1 is discussing the HARQ feedback enabling/disabling for DL transmission with below agreement:

|  |
| --- |
| Agreement :  For NB-IoT NTN, to configure/indicate enabling/disabling of HARQ feedback for downlink transmission, down select one or more from the following options:   * Option 1: per HARQ process via UE specific RRC signaling * Option 3: explicitly indicated by DCI (e.g., new field or reusing existing field) * Option 4: implicitly indicated by existing configured/indicated/combined parameter(s) in the DCI (e.g., repetition number, TBS) * Option 6: combinations of some options above |

As no data retransmission will be expected by UE based on HARQ feedback when the corresponding HARQ processes with DL HARQ feedback is disabled, the UE needn’t wait RTT timer to receive PDCCH for retransmission. Therefore, not start drx*-HARQ-RTT-TimerDL* can work for this purpose.

However, during online discussion, there is no consensus on the DRX impacts for HARQ process with DL HARQ feedback disabled, as there are concerns on whether there are some different behaviours are needed for NB-IoT with single HARQ process.

Since there is no new arrival data expected by the UE with single HARQ process when a last transmission grant has been just received, new transmission grant will not trigger the start of drx-InactivityTimer while the timer will be started if a HARQ RTT timer expires, and the timer is stopped when receiving the UL/DL assignment.

Then, as explained in [12], company thinks if we follow the NR NTN solution, the *HARQ RTT Timer* is not started upon the last PDSCH transmission in IoT NTN. This implies both the *drx-inactivityTimer* and the retransmission timer (when the transmission is not successful) will not be started for IoT NTN with single HARQ process. It forces the NW only schedule blind retransmissions and new data transmission relying on on-duration timer. Generally, the on-duration timer will be started periodically which means it is not always close to initial DL transmission in time domain. In this case, UE has to stay on RRC Connected state and wait for next on duration timer for blind retransmission and following new data transmission. Obviously, it will reduce the schedule opportunities and restrict the NW scheduling flexibility. In the end, the UE’s power consumption will be wasted since it has to stay in RRC Connected mode for quite long time for data transmission.

Therefore, how to specify the UE behaviour on the DRX timer when the corresponding HARQ processes with DL HARQ feedback disabled requires being determined:

**Q1: Do you agree to take R17 NR NTN DRX solution as baseline for IoT NTN, e.g. for HARQ process with DL HARQ feedback disabled, the UE will not start the corresponding DL HARQ RTT timer? Other enhancements (if any) can be further discussed.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2: Do you agree to enhance the DRX for NB-IoT NTN with single HARQ process when the HARQ feedback is disabled?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3: if Q2 is confirmed, which option is your preference?**

* **Option1: set HARQ RTT Timer=0;**
* **Option2: start/restart drx-inactivity timer in the subframe containing the last repetition of the corresponding PDSCH reception;**
* **Option3: others…**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 3.1.2 For UL HARQ process

For UL HARQ operation, RAN2#119-e agreed to introduce HARQ mode A and HARQ mode B in IoT NTN similarly to NR NTN.

In Rel-17 NR NTN, the following agreements are achieved:

* For HARQ mode A, the UE will extend the length of drx-HARQ-RTT-TimerUL by UE-gNB RTT.
* For HARQ mode B, the UE will not start drx-HARQ-RTT-TimerUL.
* Configuration of UL HARQ re-transmission mode is semi-static, signalled via RRC, and the decision and criteria to configure UL HARQ re-transmission mode is under network control.

During online discussion, company suggests to use HARQ mode A/B for further discussion.Similar issues to DL HARQ process, how to specify the UE behaviour on the DRX timer when the corresponding HARQ processes in HARQ mode B requires being determined:

**Q4: Do you agree to take R17 NR NTN DRX solution as baseline for IoT NTN, e.g. for HARQ process in HARQ mode B, the UE will not start the corresponding UL HARQ RTT timer? Other enhancements (if any) can be further discussed.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5: Do you agree to enhance the DRX for NB-IoT NTN with single HARQ process in HARQ mode B?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q6: If you are positive to the proposal in Question 2, companies are expected to provide your preference?**

* **Option1: set HARQ RTT Timer=0;**
* **Option2: start/restart drx-inactivity timer in the subframe containing the last repetition of the corresponding PUSCH reception;**
* **Option3: others…**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.2 LS to RAN1

R2-2210036 proposed to send LS to RAN1 that RAN2 has agreed to introduce new HARQ state for uplink transmission, and ask RAN1 to take it into consideration when deciding on DCI based enabling/disabling HARQ feedback for downlink transmission.

**Q3: Do you agree to send LS to RAN1 about the new introduced HARQ state for UL? Please provide your view in the table below.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**TBA**

## 3.3 LCP restriction

R2-2210036 proposed to introduce LCP restriction on allowed HARQ mode for IoT-NTN. Some companies are also interested in this issue. According to the contributions, [2,11] propose that the similar mechanism to NR NTN can be introduced for IoT NTN in order to avoid LCH mapping to unsuitable HARQ mode and allow different logical channels to be mapped to different HARQ types. However, [3] think that there is no strong motivation to introduce the LCP restriction for IoT NTN since most services for NB-IoT and eMTC are delay-tolerant, and LCP resriction is not supported in LTE. [R2-2210088](file:///C:\Data\3GPP\Extracts\R2-2210088%20-%20Discussion%20on%20HARQ%20enhancement%20for%20IoT%20NTN.doc) [10] also proposes there is no need to introduce LCP restriction for NB-IoT, because data and signaling are carried over the same radio bearer which means that LCP cannot perform prioritization between data and control signalling. Anyway, more discussion is needed.

**Q4: Do you agree the solutions of LCP restriction on allowed HARQ mode in NR NTN can be reused for IoT NTN? Companies are expected to provide your preferred design in the table below:**

**Option 1: only for eMTC over NTN;**

**Option 2: both eMTC and NB-IoT over NTN;**

**Option 3: None**

|  |  |  |
| --- | --- | --- |
| **Company** | **Options** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 4 Conclusion

TBA:

# 5 References

1. R2-2210152 Discussion on the HARQ enhancement for IoT-NTN CMCC
2. R2-2210036 Discussion on disabling of HARQ feedback Xiaomi
3. R2-2210702 On HARQ enhancements for IoT NTN Samsung R&D Institute UK
4. [R2-2209410](file:///C:\Data\3GPP\Extracts\R2-2209410.docx) Discussion on the HARQ disabling in IoT NTN CATT
5. [R2-2209442](file:///C:\Data\3GPP\Extracts\R2-2209442_Discussion%20on%20disabling%20HARQ%20feedback%20in%20IoT-NTN.docx) Discussion on disabling HARQ Feedback in IoT-NTN MediaTek Inc.
6. [R2-2209666](file:///C:\Data\3GPP\Extracts\R2-2209666%20Discussion%20on%20disabling%20DL%20HARQ%20feedback.docx) Discussion on disabling DL HARQ feedback Huawei, HiSilicon
7. [R2-2209717](file:///C:\Data\3GPP\Extracts\R2-2209717%20IoT%20HARQ%20process.doc) Enhancement for UL and DL HARQ processes Qualcomm Incorporated
8. [R2-2209750](file:///C:\Data\3GPP\Extracts\R2-2209750%20Discussion%20on%20performance%20enhancement%20for%20IoT%20NTN.docx) Discussion on performance enhancement for IoT NTN Transsion Holdings
9. [R2-2209834](file:///C:\Data\3GPP\Extracts\R2-2209834%20Further%20discussion%20on%20HARQ%20enhancements.docx) Further discussion on HARQ enhancements ZTE Corporation, Sanechips
10. [R2-2210088](file:///C:\Data\3GPP\Extracts\R2-2210088%20-%20Discussion%20on%20HARQ%20enhancement%20for%20IoT%20NTN.doc) Discussion on HARQ enhancement for IoT NTN OPPO
11. [R2-2210195](file:///C:\Data\3GPP\Extracts\R2-2210195%20(R18%20IoT-NTN%20WI%20AI%208.6.2.1)%20-%20disabling%20HARQ%20feedback.docx) Disabling HARQ feedback for IoT-NTN Interdigital, Inc.

1. [R2-2210643](file:///C:\\Data\\3GPP\\Extracts\\R2-2210643%20On%20HARQ%20enhancements%20for%20IoT%20NTN.docx" \o "C:Data3GPPExtractsR2-2210643 On HARQ enhancements for IoT NTN.docx) On HARQ enhancements for IoT NTN Nokia, Nokia Shanghai Bell
2. [R2-2210761](file:///C:\Data\3GPP\Extracts\R2-2210761%20-%20R18%20IoT%20NTN%20performance%20enhancement.docx) R18 IoT NTN performance enhancement Ericsson