**3GPP TSG- Meeting #bis-eR2-22xxxxx**

**Electronic,**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **3534** | **rev** | **2** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Miscellaneous correction for Positioning | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | | 2022-09-30 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | * To specify that the network always configures inactivePosSRS-TimeAlignmentTimer when SRS-PosRRC-InactiveConfig is configured in the configures inactivePosSRS-TimeAlignmentTimer field description. * To capture the agreement to cancel the triggered UL MAC CE for MG activation and deactivation for the condition “When an indication from upper layers that the gaps are not needed any more or a gap with a new id needs to be activated is received”. * A minor correction in the field description of cg-SDT-timeAlignmentTimer is needed to specifically say that the configuration is for this field description. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Field description of inactivePosSRS-TimeAlignmentTimer is updated and minor correction for cg-SDT-timeAlignmentTimer in section 6.2.2. * The clause to cancel the triggered UL MAC CE for MG activation and deactivation for the condition “When an indication from upper layers that the gaps are not needed any more or a gap with a new id needs to be activated is received” has been added to section 5.5.6.2   **Impact Analysis**  Impacted 5G architecture options: NR SA, (NG)EN-DC, NE-DC,NR-DC  Impacted functionality:  Cancellation of triggerred UL MAC CE for Preconfigured measurement gap, UL-SRS transmission for RRC Inactive mode Positioning  Inter-operability:  For Cancellation of triggerred UL MAC CE for Preconfigured measurement gap   * If UE implements as per the CR and NW does not,   + No inter-operability seen * If NW implements as per the CR and UE does not   + invalid UL MAC CE trigger may exist in UE   For UL-SRS transmission for RRC Inactive Mode positioning   * If UE implements as per the CR and NW does not   + NW may miss to configure the TA validity timer for UL-SRS for positioning during RRC Inactive mode * If NW implements as per the CR and UE does not   + No inter-operability seen | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | * Incomplete specification from RRC perspective * Invalid UL MAC CE trigger max exist in UE * Inefficient RRC Inactive mode positioning based upon UL-SRS | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5.6.2, 6.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR … CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | The CR is based upon R2-2209429, R2-2210480 | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*Beginning of Changes*

5.5.6.2 Initiation

The UE shall:

1> if and only if upper layers indicate to start performing location measurements towards E-UTRA or NR or start subframe and slot timing detection towards E-UTRA, and the UE requires measurement gaps for these operations while measurement gaps are either not configured or not sufficient:

2> if preconfigured measurement gaps for positioning are configured and the UE considers that at least one of the preconfigured measurement gaps for positioning is sufficient for the location measurement when activated:

3> trigger the lower layers to initiate the measurement gap activation request using UL MAC CE as specified in TS 38.321 [6];

2> else:

3> initiate the procedure to indicate start as specified in clause 5.5.6.3;

NOTE 1: The UE verifies the measurement gap situation only upon receiving the indication from upper layers. If at this point in time sufficient gaps are available, the UE does not initiate the procedure. Unless it receives a new indication from upper layers, the UE is only allowed to further repeat the procedure in the same PCell once per frequency of the target RAT if the provided measurement gaps are insufficient.

NOTE 1a: When indication is received from upper layers for performing location measurement and there is pre-configured measurement gap configured (not preconfigured measurement gap for positioning), the UE considers this preconfigured measurement gap to be not sufficient if the measurement gap is not considered to be always activated according to clause 9.1.7.2 of TS 38.133 [14].

1> if and only if upper layers indicate to stop performing location measurements towards E-UTRA or NR or stop subframe and slot timing detection towards E-UTRA:

2> if there is no activated preconfigured measurement gap for positioning:

3> if there is previously triggered UL MAC CE transmission for the measurement gap activation for positioning:

4> indicate to the lower layers to cancel the triggered UL MAC CE transmission for the measurement gap activation as specified in TS 38.321 [6];

3> else:

4> initiate the procedure to indicate stop as specified in 5.5.6.3.

2> else if there is activated preconfigured measurement gap for positioning:

3> trigger the lower layers to deactivate all the activated measurement gap(s) for positioning as specified in TS 38.321 [6].

NOTE 2: The UE may initiate the procedure to indicate stop even if it did not previously initiate the procedure to indicate start.

*Next Change*

6.2.2 Message definitions

– *CounterCheck*

#### *<Skip Unmodified Changes>*

#### – *RRCRelease*

The *RRCRelease* message is used to command the release of an RRC connection or the suspension of the RRC connection.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

*RRCRelease* message

-- ASN1START

-- TAG-RRCRELEASE-START

RRCRelease ::= SEQUENCE {

rrc-TransactionIdentifier RRC-TransactionIdentifier,

criticalExtensions CHOICE {

rrcRelease RRCRelease-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

RRCRelease-IEs ::= SEQUENCE {

redirectedCarrierInfo RedirectedCarrierInfo OPTIONAL, -- Need N

cellReselectionPriorities CellReselectionPriorities OPTIONAL, -- Need R

suspendConfig SuspendConfig OPTIONAL, -- Need R

deprioritisationReq SEQUENCE {

deprioritisationType ENUMERATED {frequency, nr},

deprioritisationTimer ENUMERATED {min5, min10, min15, min30}

} OPTIONAL, -- Need N

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension RRCRelease-v1540-IEs OPTIONAL

}

RRCRelease-v1540-IEs ::= SEQUENCE {

waitTime RejectWaitTime OPTIONAL, -- Need N

nonCriticalExtension RRCRelease-v1610-IEs OPTIONAL

}

RRCRelease-v1610-IEs ::= SEQUENCE {

voiceFallbackIndication-r16 ENUMERATED {true} OPTIONAL, -- Need N

measIdleConfig-r16 SetupRelease {MeasIdleConfigDedicated-r16} OPTIONAL, -- Need M

nonCriticalExtension RRCRelease-v1650-IEs OPTIONAL

}

RRCRelease-v1650-IEs ::= SEQUENCE {

mpsPriorityIndication-r16 ENUMERATED {true} OPTIONAL, -- Cond Redirection2

nonCriticalExtension RRCRelease-v1710-IEs OPTIONAL

}

RRCRelease-v1710-IEs ::= SEQUENCE {

noLastCellUpdate-r17 ENUMERATED {true} OPTIONAL, -- Need S

nonCriticalExtension SEQUENCE {} OPTIONAL

}

RedirectedCarrierInfo ::= CHOICE {

nr CarrierInfoNR,

eutra RedirectedCarrierInfo-EUTRA,

...

}

RedirectedCarrierInfo-EUTRA ::= SEQUENCE {

eutraFrequency ARFCN-ValueEUTRA,

cnType ENUMERATED {epc,fiveGC} OPTIONAL -- Need N

}

CarrierInfoNR ::= SEQUENCE {

carrierFreq ARFCN-ValueNR,

ssbSubcarrierSpacing SubcarrierSpacing,

smtc SSB-MTC OPTIONAL, -- Need S

...

}

SuspendConfig ::= SEQUENCE {

fullI-RNTI I-RNTI-Value,

shortI-RNTI ShortI-RNTI-Value,

ran-PagingCycle PagingCycle,

ran-NotificationAreaInfo RAN-NotificationAreaInfo OPTIONAL, -- Need M

t380 PeriodicRNAU-TimerValue OPTIONAL, -- Need R

nextHopChainingCount NextHopChainingCount,

...,

[[

sl-UEIdentityRemote-r17 RNTI-Value OPTIONAL, -- Cond L2RemoteUE

sdt-Config-r17 SetupRelease { SDT-Config-r17 } OPTIONAL, -- Need M

srs-PosRRC-Inactive-r17 SetupRelease { SRS-PosRRC-Inactive-r17 } OPTIONAL, -- Need M

ran-ExtendedPagingCycle-r17 ExtendedPagingCycle-r17 OPTIONAL -- Cond RANPaging

]]

}

PeriodicRNAU-TimerValue ::= ENUMERATED { min5, min10, min20, min30, min60, min120, min360, min720}

CellReselectionPriorities ::= SEQUENCE {

freqPriorityListEUTRA FreqPriorityListEUTRA OPTIONAL, -- Need M

freqPriorityListNR FreqPriorityListNR OPTIONAL, -- Need M

t320 ENUMERATED {min5, min10, min20, min30, min60, min120, min180, spare1} OPTIONAL, -- Need R

...,

[[

freqPriorityListDedicatedSlicing-r17 FreqPriorityListDedicatedSlicing-r17 OPTIONAL -- Need M

]]

}

PagingCycle ::= ENUMERATED {rf32, rf64, rf128, rf256}

ExtendedPagingCycle-r17 ::= ENUMERATED {rf256, rf512, rf1024, spare1}

FreqPriorityListEUTRA ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityEUTRA

FreqPriorityListNR ::= SEQUENCE (SIZE (1..maxFreq)) OF FreqPriorityNR

FreqPriorityEUTRA ::= SEQUENCE {

carrierFreq ARFCN-ValueEUTRA,

cellReselectionPriority CellReselectionPriority,

cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

FreqPriorityNR ::= SEQUENCE {

carrierFreq ARFCN-ValueNR,

cellReselectionPriority CellReselectionPriority,

cellReselectionSubPriority CellReselectionSubPriority OPTIONAL -- Need R

}

RAN-NotificationAreaInfo ::= CHOICE {

cellList PLMN-RAN-AreaCellList,

ran-AreaConfigList PLMN-RAN-AreaConfigList,

...

}

PLMN-RAN-AreaCellList ::= SEQUENCE (SIZE (1.. maxPLMNIdentities)) OF PLMN-RAN-AreaCell

PLMN-RAN-AreaCell ::= SEQUENCE {

plmn-Identity PLMN-Identity OPTIONAL, -- Need S

ran-AreaCells SEQUENCE (SIZE (1..32)) OF CellIdentity

}

PLMN-RAN-AreaConfigList ::= SEQUENCE (SIZE (1..maxPLMNIdentities)) OF PLMN-RAN-AreaConfig

PLMN-RAN-AreaConfig ::= SEQUENCE {

plmn-Identity PLMN-Identity OPTIONAL, -- Need S

ran-Area SEQUENCE (SIZE (1..16)) OF RAN-AreaConfig

}

RAN-AreaConfig ::= SEQUENCE {

trackingAreaCode TrackingAreaCode,

ran-AreaCodeList SEQUENCE (SIZE (1..32)) OF RAN-AreaCode OPTIONAL -- Need R

}

SDT-Config-r17 ::= SEQUENCE {

sdt-DRB-List-r17 SEQUENCE (SIZE (0..maxDRB)) OF DRB-Identity OPTIONAL, -- Need M

sdt-SRB2-Indication-r17 ENUMERATED {allowed} OPTIONAL, -- Need R

sdt-MAC-PHY-CG-Config-r17 SetupRelease {SDT-CG-Config-r17} OPTIONAL, -- Need M

sdt-DRB-ContinueROHC-r17 ENUMERATED { cell, rna } OPTIONAL -- Need S

}

SDT-CG-Config-r17 ::= OCTET STRING (CONTAINING SDT-MAC-PHY-CG-Config-r17)

SDT-MAC-PHY-CG-Config-r17 ::= SEQUENCE {

-- CG-SDT specific configuration

cg-SDT-ConfigLCH-RestrictionToAddModList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF CG-SDT-ConfigLCH-Restriction-r17 OPTIONAL, -- Need N

cg-SDT-ConfigLCH-RestrictionToReleaseList-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

cg-SDT-ConfigInitialBWP-NUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

cg-SDT-ConfigInitialBWP-SUL-r17 SetupRelease {BWP-UplinkDedicatedSDT-r17} OPTIONAL, -- Need M

cg-SDT-ConfigInitialBWP-DL-r17 BWP-DownlinkDedicatedSDT-r17 OPTIONAL, -- Need M

cg-SDT-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

cg-SDT-RSRP-ThresholdSSB-r17 RSRP-Range OPTIONAL, -- Need M

cg-SDT-TA-ValidationConfig-r17 SetupRelease { CG-SDT-TA-ValidationConfig-r17 } OPTIONAL, -- Need M

cg-SDT-CS-RNTI-r17 RNTI-Value OPTIONAL, -- Need M

...

}

CG-SDT-TA-ValidationConfig-r17 ::= SEQUENCE {

cg-SDT-RSRP-ChangeThreshold-r17 ENUMERATED { dB2, dB4, dB6, dB8, dB10, dB14, dB18, dB22,

dB26, dB30, dB34, spare5, spare4, spare3, spare2, spare1}

}

BWP-DownlinkDedicatedSDT-r17 ::= SEQUENCE {

pdcch-Config-r17 SetupRelease { PDCCH-Config } OPTIONAL, -- Need M

pdsch-Config-r17 SetupRelease { PDSCH-Config } OPTIONAL, -- Need M

...

}

BWP-UplinkDedicatedSDT-r17 ::= SEQUENCE {

pusch-Config-r17 SetupRelease { PUSCH-Config } OPTIONAL, -- Need M

configuredGrantConfigToAddModList-r17 ConfiguredGrantConfigToAddModList-r16 OPTIONAL, -- Need N

configuredGrantConfigToReleaseList-r17 ConfiguredGrantConfigToReleaseList-r16 OPTIONAL, -- Need N

...

}

CG-SDT-ConfigLCH-Restriction-r17 ::= SEQUENCE {

logicalChannelIdentity-r17 LogicalChannelIdentity,

configuredGrantType1Allowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

allowedCG-List-r17 SEQUENCE (SIZE (0.. maxNrofConfiguredGrantConfigMAC-1-r16)) OF ConfiguredGrantConfigIndexMAC-r16

OPTIONAL -- Need R

}

SRS-PosRRC-Inactive-r17 ::= OCTET STRING (CONTAINING SRS-PosRRC-InactiveConfig-r17)

SRS-PosRRC-InactiveConfig-r17 ::= SEQUENCE {

srs-PosConfigNUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

srs-PosConfigSUL-r17 SRS-PosConfig-r17 OPTIONAL, -- Need R

bwp-NUL-r17 BWP OPTIONAL, -- Need S

bwp-SUL-r17 BWP OPTIONAL, -- Need S

inactivePosSRS-TimeAlignmentTimer-r17 TimeAlignmentTimer OPTIONAL, -- Need M

inactivePosSRS-RSRP-changeThreshold-r17 RSRP-ChangeThreshold-r17 OPTIONAL -- Need M

}

RSRP-ChangeThreshold-r17 ::= ENUMERATED {dB4, dB6, dB8, dB10, dB14, dB18, dB22, dB26, dB30, dB34, spare6, spare5, spare4, spare3, spare2, spare1}

SRS-PosConfig-r17 ::= SEQUENCE {

srs-PosResourceSetToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSetId-r16 OPTIONAL,-- Need N

srs-PosResourceSetToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResourceSets-r16)) OF SRS-PosResourceSet-r16 OPTIONAL,-- Need N

srs-PosResourceToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResourceId-r16 OPTIONAL,-- Need N

srs-PosResourceToAddModList-r17 SEQUENCE (SIZE(1..maxNrofSRS-PosResources-r16)) OF SRS-PosResource-r16 OPTIONAL -- Need N

}

-- TAG-RRCRELEASE-STOP

-- ASN1STOP

|  |
| --- |
| *RRCRelease-IEs* field descriptions |
| ***cellReselectionPriorities***  Dedicated priorities to be used for cell reselection as specified in TS 38.304 [20]*.* The maximum number of NR carrier frequencies that the network can configure through *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing* together is eight. If the same frequency is configured in both *FreqPriorityListNR* and *FreqPriorityListDedicatedSlicing*, the frequency is only counted once. |
| ***cnType***  Indicate that the UE is redirected to EPC or 5GC. |
| ***deprioritisationReq***  Indicates whether the current frequency or RAT is to be de-prioritised. |
| ***deprioritisationTimer***  Indicates the period for which either the current carrier frequency or NR is deprioritised. Value *minN* corresponds to N minutes. |
| ***measIdleConfig***  Indicates measurement configuration to be stored and used by the UE while in RRC\_IDLE or RRC\_INACTIVE. |
| ***mpsPriorityIndication***  Indicates the UE can set the establishment cause to mps-PriorityAccess for a new connection following a redirect to NR. If the target RAT is E-UTRA, see TS 36.331 [10]. The gNB sets the indication only for UEs authorized to receive MPS treatment as indicated by ARP and/or QoS characteristics at the gNB, and it is applicable only for this instance of release with redirection to carrier/RAT included in the *redirectedCarrierInfo* field in the *RRCRelease* message. |
| ***noLastCellUpdate***  Presence of the field indicates that the last used cell for PEI shall not be updated. When the field is absent, the PEI-capable UE shall update its last used cell with the current cell. |
| ***srs-PosRRCInactiveConfig***  SRS for positioning confifuration during RRC\_INACTIVE State. |
| ***suspendConfig***  Indicates configuration for the RRC\_INACTIVE state. The network does not configure *suspendConfig* when the network redirect the UE to an inter-RAT carrier frequency or if the UE is configured with a DAPS bearer. |
| ***redirectedCarrierInfo***  Indicates a carrier frequency (downlink for FDD) and is used to redirect the UE to an NR or an inter-RAT carrier frequency, by means of cell selection at transition to RRC\_IDLE or RRC\_INACTIVE as specified in TS 38.304 [20]. Based on UE capability, the network may include *redirectedCarrierInfo* in *RRCRelease* message with *suspendConfig* if this message is sent in response to an *RRCResumeRequest* or an *RRCResumeRequest1* which is triggered by the NAS layer (see 5.3.1.4 in TS 24.501 [23]). |
| ***voiceFallbackIndication***  Indicates the RRC release is triggered by EPS fallback for IMS voice as specified in TS 23.502 [43]. |

|  |
| --- |
| *CarrierInfoNR* field descriptions |
| ***carrierFreq***  Indicates the redirected NR frequency. |
| ***ssbSubcarrierSpacing***  Subcarrier spacing of SSB in the redirected SSB frequency.  Only the following values are applicable depending on the used frequency:  FR1: 15 or 30 kHz  FR2-1: 120 or 240 kHz  FR2-2: 120, 480, or 960 kHz |
| ***smtc***  The SSB periodicity/offset/duration configuration for the redirected SSB frequency. It is based on timing reference of PCell. If the field is absent, the UE uses the SMTC configured in the measObjectNR having the same SSB frequency and subcarrier spacing. |

|  |
| --- |
| *RAN-NotificationAreaInfo* field descriptions |
| ***cellList***  A list of cells configured as RAN area. |
| ***ran-AreaConfigList***  A list of RAN area codes or RA code(s) as RAN area. |

|  |
| --- |
| *PLMN-RAN-AreaConfig* field descriptions |
| ***plmn-Identity***  PLMN Identity to which the cells in *ran-Area* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-Area* always belongs to the registered SNPN). |
| ***ran-AreaCodeList***  The total number of RAN-AreaCodes of all PLMNs does not exceed 32. |
| ***ran-Area***  Indicates whether TA code(s) or RAN area code(s) are used for the RAN notification area. The network uses only TA code(s) or both TA code(s) and RAN area code(s) to configure a UE. The total number of TACs across all PLMNs does not exceed 16. |

|  |
| --- |
| *PLMN-RAN-AreaCell* field descriptions |
| ***plmn-Identity***  PLMN Identity to which the cells in *ran-AreaCells* belong. If the field is absent the UE not in SNPN access mode uses the ID of the registered PLMN. This field is not included for UE in SNPN access mode (for UE in SNPN access mode the *ran-AreaCells* always belongs to the registered SNPN). |
| ***ran-AreaCells***  The total number of cells of all PLMNs does not exceed 32. |

|  |
| --- |
| *SDT-Config* field descriptions |
| ***sdt-DRB-ContinueROHC***  Indicates whether the PDCP entity of the radio bearers configured for SDT continues or resets the ROHC header compression protocol during PDCP re-establishment during SDT procedure, as specified in TS 38.323 [5]. Value *cell* indicates that ROHC header compression continues when the UE resumes for SDT in the same cell as the PCell when the RRCRelease message was received. Value *rna* indicates that ROHC header compression continues when the UE resumes for SDT in a cell belonging to the same RNA as the PCell where the RRCRelease message was received. If the field is absent, the UE releases any stored value for this field and the PDCP entity of the radio bearers configured for SDT always resets the ROHC header compression protocol during PDCP re-establishment when SDT procedure is initiated, as specified in TS 38.323 [5]. |
| ***sdt-DRB-List***  Indicates the ID(s) of the DRB(s) that are configured for SDT. If size of the sequence is zero, then the UE assumes that none of the DRBs are configured for SDT. The network only configures MN terminated MCG bearers for SDT. |
| ***sdt-SRB2-Indication***  Indiates whether SRB2 is configured for SDT or not. |

|  |
| --- |
| *SDT-MAC-PHY-CG-Config* field descriptions |
| ***cg-SDT-ConfigInitialBWP-DL***  Downlink BWP configuration for CG-SDT. If a UE is a RedCap UE and if the *initialDownlinkBWP-RedCap* is configured in *downlinkConfigCommon* in *SIB1*, this field is configured for *initialDownlinkBWP-RedCap*, otherwise it is configured for *initialDownlinkBWP*. |
| ***cg-SDT-ConfigInitialBWP-NUL***  UL BWP configuration for CG-SDT on NUL carrier. If a UE is a RedCap UE and if the *initialUplinkBWP-RedCap* is configured in *uplinkConfigCommon* in *SIB1*, this field is configured for *initialUplinkBWP-RedCap*, otherwise it is configured for *initialUplinkBWP* for NUL. |
| ***cg-SDT-ConfigInitialBWP-SUL***  UL BWP configuration for CG-SDT on SUL carrier configured for the *initialUplinkBWP* for SUL. |
| ***cg-SDT-CS-RNTI***  The CS-RNTI value for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-RSRP-ThresholdSSB***  An RSRP threshold configured for SSB selection for CG-SDT as specified in TS 38.321 [3]. |
| ***cg-SDT-TA-ValidationConfig***  Configuration for the RSRP based TA validation. If this field is not configured, then the UE does not perform RSRP based TA validation. |
| ***cg-SDT-timeAlignmentTimer***  TAT value for CG-SDT as specified in TS 38.321 [3]. The network always configures this field when *sdt-MAC-PHY-CG-Config* is configured. |

|  |
| --- |
| *CG-SDT-TA-ValidationConfig* field descriptions |
| ***cg-SDT-RSRP-ChangeThreshold***  The RSRP threshold for TA validation for CG-SDT as specified in TS 38.321 [3]. Value *dB2* corresponds to 2 dB, value *dB4* corresponds to 4 dB and so on. |

|  |
| --- |
| *SRS-PosRRC-InactiveConfig* field descriptions |
| ***bwp-NUL***  BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Normal Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***bwp-SUL***  BWP configuration for SRS for Positioning during the RRC\_INACTIVE state in Supplementary Uplink Carrier. If the field is absent UE is configured with an SRS for Positioning associated with the initial UL BWP and transmitted, during the RRC\_INACTIVE state, inside the initial UL BWP with the same CP and SCS as configured for initial UL BWP. |
| ***inactivePosSRS-RSRP-changeThreshold***  RSRP threshold for the increase/decrease of RSRP for time alignment validation as specified in TS 38.321 [3]. |
| ***inactivePosSRS-TimeAlignmentTimer***  TAT value for SRS for positioning transmission during RRC\_INACTIVE State as specified in TS 38.321 [3]. The network always configures this field when *SRS-PosRRC-InactiveConfig* is configured. |
| ***srs-PosConfigNUL***  SRS for Positioning configuration in RRC\_INACTIVE state in Normal Uplink Carrier. |
| ***srs-PosConfigSUL***  SRS for Positioning configuration in RRC\_INACTIVE state in Supplementary Uplink Carrier. |

|  |
| --- |
| *SuspendConfig* field descriptions |
| ***ran-ExtendedPagingCycle***  The extended DRX (eDRX) cycle for RAN-initiated paging to be applied by the UE. Value *rf256* corresponds to 256 radio frames, value *rf512* corresponds to 512 radio frames and so on. Value of the field indicates an eDRX cycle which is shorter or equal to the IDLE mode eDRX cycle configured for the UE. |
| ***ran-NotificationAreaInfo***  Network ensures that the UE in RRC\_INACTIVE always has a valid *ran-NotificationAreaInfo*. |
| ***ran-PagingCycle***  Refers to the UE specific cycle for RAN-initiated paging. Value *rf32* corresponds to 32 radio frames, value *rf64* corresponds to 64 radio frames and so on. |
| ***sl-UEIdentityRemote***  Indicates the C-RNTI to the L2 U2N Remote UE. |
| ***t380***  Refers to the timer that triggers the periodic RNAU procedure in UE. Value *min5* corresponds to 5 minutes, value *min10* corresponds to 10 minutes and so on. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *L2RemoteUE* | The field is mandatory present for L2 U2N Remote UE's RNAU; otherwise it is absent. |
| *RANPaging* | This field is optionally present, Need R, if the UE is configured with eDRX in IDLE mode, see TS 24.401 [23]; otherwise the field is not present. |
| *Redirection2* | The field is optionally present, Need R, if *redirectedCarrierInfo* is included; otherwise the field is not present. |

*End of Changes*