**3GPP TSG-RAN WG2 Meeting #119bis-e R2-22xxxxx**

**Online, 10-17 October 2022**

Source: Huawei, HiSilicon

Title: [Offline-418][POS] Positioning MAC CR (Huawei)

Agenda Item: 6.11.1

Document for: Discussion and Decision

# Introduction

This document provides a summary of the following contributions submitted to AI 6.11 for MAC corrections.

## Contacts

|  |  |  |
| --- | --- | --- |
| Name | Company | Email |
| Jianxiang Li | CATT | lijianxiang@catt.cn |
|  |  |  |

# Discussion

The following CR has been proposed to align with the agreement for CG-SDT on 2-step RACH.

[R2-2209427](file:///C%3A%5CUsers%5Cmtk16923%5CDocuments%5C3GPP%20Meetings%5C202210%20-%20RAN2_119bis-e%2C%20Online%5CExtracts%5CR2-2209427%20Correction%20to%20MAC%20spec%20for%20Positioning%20enhancement.docx) Correction to MAC spec for Positioning enhancement Huawei, HiSilicon CR Rel-17 38.321 17.2.0 1408 - F NR\_pos\_enh-Core

The following change has been proposed on the alignment

|  |
| --- |
| 1> when an Absolute Timing Advance Command is received in response to a MSGA transmission including C-RNTI MAC CE as specified in clause 5.1.4a:2> apply the Timing Advance Command for PTAG;2> if *inactivePosSRS-TimeAlignmentTimer* is configured and there is ongoing Positioning SRS Transmission in RRC\_INACTIVE as in clause 5.26:3> start or restart the *inactivePosSRS-TimeAlignmentTimer* associated with the indicated TAG.2> if CG-SDT procedure is ongoing:3> start or restart the *cg-SDT-TimeAlignmentTimer* associated with PTAG.2> else:3> start or restart the *timeAlignmentTimer* associated with PTAG. |

Rapp’s comment:

* In the discussion for R2-2209429, a general consensus has been reached that we can align with the field description for CG-SDT that when SRS transmission in RRC\_INACTIVE is configured, *inactivePosSRS-TimerAlignmentTimer* is always configured
* During the online discussion for R2-2209427
	+ Consensus has been made that we should align with CG-SDT’s agreement for 2-step RACH
	+ One concern is that if in RRC spec, we mention that “*inactivePosSRS-TimerAlignmentTimer* is always configured”, then in the MAC spec, is it still necessary to add “if inactivePosSRS-TimeAlignmentTimer is configured” as a condition.

Based on the above, the rapp thinks that it is reasonable to not to have the condition “if inactivePosSRS-TimeAlignmentTimer is configured” if inactive SRS TAT is always configured. We propose the following TP based on the above.

|  |
| --- |
| The MAC entity shall:1> when a Timing Advance Command MAC CE is received, and if an NTA (as defined in TS 38.211 [8]) has been maintained with the indicated TAG:2> apply the Timing Advance Command for the indicated TAG;2> ifthere is ongoing Positioning SRS Transmission in RRC\_INACTIVE as in clause 5.26:3> start or restart the *inactivePosSRS-TimeAlignmentTimer* associated with the indicated TAG.2> if CG-SDT procedure triggered as in clause 5.27 is ongoing:3> start or restart the *cg-SDT-TimeAlignmentTimer* associated with the indicated TAG.2> else:3> start or restart the *timeAlignmentTimer* associated with the indicated TAG.===TEXT OMITTED===1> when an Absolute Timing Advance Command is received in response to a MSGA transmission including C-RNTI MAC CE as specified in clause 5.1.4a:2> apply the Timing Advance Command for PTAG;2> if there is ongoing Positioning SRS Transmission in RRC\_INACTIVE as in clause 5.26:3> start or restart the *inactivePosSRS-TimeAlignmentTimer* associated with the indicated TAG.2> if CG-SDT procedure is ongoing:3> start or restart the *cg-SDT-TimeAlignmentTimer* associated with PTAG.2> else:3> start or restart the *timeAlignmentTimer* associated with PTAG. |

***Question1, Do companies agree with the change above considering change in CR R2-2209427 and that inactivePosSRS-TimeAlignmenTimer is always configured?***

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| CATT | Yes |  |

In the following CR, a change has been proposed for the description for PPW ID in the MAC spec

R[2-2210607](file:///E%3A%5C%5CWORK%5C%5C1%203GPP%5C%5CMeeting%5C%5CRAN2%20119bis-e%5C%5C2%20During%5C%5CDocs%5C%5CR2-2210607.zip) Clarification on the PPW index vivo draftCR Rel-17 38.321 17.2.0 D NR\_pos\_enh-Core

|  |
| --- |
| 6.1.3.42 PPW Activation/Deactivation Command MAC CEThe PPW Activation/Deactivation Command MAC CE is identified by MAC subheader with eLCID as specified in Table 6.2.1-1b.It has variable size defined as follows (Figure 6.1.3.42-1):- numEntry: This field indicates the number of entries N-1 in the MAC CE. 00 indicates that N equals to 2; 01 indicates that N equals to 3 and so on. The length of the field is 2 bits;- Serving Cell ID: This field indicates the identity of the Serving Cell for which the MAC CE applies. The length of the field is 5 bits;- PPW ID: This field indicates the index of the PPW configured on active DL BWP of the Serving Cell identified by the above Serving Cell ID. Index 0 corresponds to the first entry within the list of the PPW configuration which is maintained in the UE and is ordered by the addition time in this BWP, index 1 corresponds to the second entry in the list and so on. The length of the field is 2 bits;- A/D: This field indicates the activation or deactivation of the PPW. The field is set to 1 to indicate activation, otherwise it indicates deactivation. The length of the field is 1 bit;- R: Reserved bit, set to 0.**Figure 6.1.3.42-1: PPW Activation/Deactivation Command MAC CE** |

While in the RRC spec, the PPW configuration within a certain BWP is given as follows under *BWP-DownlinkDedicated*:

|  |
| --- |
| DL-PPW-PreConfigToAddModList-r17 ::= SEQUENCE (SIZE (1..maxNrofPPW-Config-r17)) OF DL-PPW-PreConfig-r17DL-PPW-PreConfigToReleaseList-r17 ::= SEQUENCE (SIZE (1..maxNrofPPW-Config-r17)) OF DL-PPW-ID-r17 |

With the maximum number of PPW that can be configured under a BWP equaling to 4

|  |
| --- |
| maxNrofPPW-Config-r17 INTEGER ::= 4 -- Maximum number of Preconfigured PRS processing windows per DL BWP |

**Rapp’s Comment:**

* The maximum number of PPW that can be configured is 4, which can be fully covered by the PPW ID field within the MAC CE, with 2 bits
* It seems better to directly map the PPW ID in the MAC spec to the *PPW-ID* field in the RRC spec:
	+ PPW ID with value 0 corresponds to the entry with *PPW-ID* set to 1 within the configured list of PPWs in TS 38.331; PPW ID with value 1 corresponds to the entry with *PPW-ID* set to 1 within the configured list of PPWs, and so on.

With the discussion above, we propose the following text proposal for the clarification of the PPW ID in the MAC spec:

|  |
| --- |
| 6.1.3.42 PPW Activation/Deactivation Command MAC CEThe PPW Activation/Deactivation Command MAC CE is identified by MAC subheader with eLCID as specified in Table 6.2.1-1b.It has variable size defined as follows (Figure 6.1.3.42-1):- numEntry: This field indicates the number of entries N-1 in the MAC CE. 00 indicates that N equals to 2; 01 indicates that N equals to 3 and so on. The length of the field is 2 bits;- Serving Cell ID: This field indicates the identity of the Serving Cell for which the MAC CE applies. The length of the field is 5 bits;- PPW ID: This field indicates the index of the PPW configured on active DL BWP of the Serving Cell identified by the above Serving Cell ID. Index 0 corresponds to the entry within the list of the PPW configuration(s) with the field *PPW-ID* in TS 38.331 [5] set to 1 in this BWP; index 1 corresponds to the entry in the list with the field *PPW-ID* in TS 38.331 [5] set to 2 in this BWP and so on. The length of the field is 2 bits;- A/D: This field indicates the activation or deactivation of the PPW. The field is set to 1 to indicate activation, otherwise it indicates deactivation. The length of the field is 1 bit;- R: Reserved bit, set to 0.**Figure 6.1.3.42-1: PPW Activation/Deactivation Command MAC CE** |

***Quesiton2: Do companies agree with the change above for the clarification of PPW ID field in the MAC CE?***

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| CATT | No | PPW configuration is a delta configuration to UE, so the list of the PPW configuration is maintained by UE which should be the same with gNB side. So we understood the motivation of vivo’s CR is that both UE and gNB should have the same understanding of the index of the PPW configured on active DL BWP of the Serving Cell identified by the above Serving Cell ID. However how to order the list can be clarified in TS38.331, instead of in MAC.So we prefer to delete the description of the order way as below, i.e. delete the second correction.- PPW ID: This field indicates the index of the PPW configured on active DL BWP of the Serving Cell identified by the above Serving Cell ID. Index 0 corresponds to the first entry within the list of the PPW configuration in this BWP, index 1 corresponds to the second entry in the list and so on. The length of the field is 2 bits;On the other hand, the TP proposed by rapporteur is not supported because the ‘first’ and ‘second’ in the original version indicate the relationship with the index. No need to change the original description. |

# Conclusion

Based on the summary as above, we propose the following for discussion:

***TBD***