**3GPP TSG-RAN WG2 Meeting #119bis R2-221xxxx**

**Electronic, 10th – 19th Oct, 2022**

**Source: CATT**

**Title:****[AT119bis-e][422][Relay] Remaining proposals on discovery and (re)selection (CATT)**

**Agenda Item:** **6.7.2.4**

**Document for:** **Discussion and Decision**

# Introduction

This is the trigger of the following email discussion:

* [AT119bis-e][422][Relay] Remaining proposals on discovery and (re)selection (CATT)

Scope: Discuss P3a/P3b/P5a/P5b of R2-2210777.

Intended outcome: Report to CB session

Deadline: Friday 2022-10-14 1000 UTC

Companies are invited to provide comments for Phase 1 of this email discussion by 2022-10-13, 1000 UTC.

# Discussion

### 2.1 SL CG for discovery message

|  |  |  |
| --- | --- | --- |
| R2-2210111[1] | Support of SL CG for discovery message | Huawei, HiSilicon, Nokia, Kyocera |

This issue (SL CG for discovery message) had been discussed in [AT119-e][418][Relay] but without conclusion. During the last RAN2 meeting, some companies expressed their concern that there is no traffic pattern defined for discovery message, so it is not suitable for UE to provide any assistance information for SL CG for discovery message to gNB. In this meeting, the proponent companies have shown that the discovery message transmissions for both Model A and Model B are indeed periodic from the very beginning of the Proximity-based services design and this is already captured in sections 5.3.1.2 and 5.4.4.1 of 23.303 [3], which is listed below with highlighted text:

|  |
| --- |
| **5.3.1.2 ProSe Direct Discovery Models**  The following models for ProSe Direct Discovery exist:  **Model A ("I am here")**  This model defines two roles for the ProSe-enabled UEs that are participating in ProSe Direct Discovery.  - Announcing UE: The UE announces certain information that could be used by UEs in proximity that have permission to discover.  - Monitoring UE: The UE that monitors certain information of interest in proximity of announcing UEs.  In this model the announcing UE broadcasts discovery messages at pre-defined discovery intervals and the monitoring UEs that are interested in these messages read them and process them.  NOTE: This model is equivalent to "I am here" since the announcing UE would broadcast information about itself e.g. its ProSe Application Code in the discovery message. |

|  |
| --- |
| 5.4.4 Direct communication via ProSe UE-to-Network Relay5.4.4.1 General A ProSe UE-to-Network Relay capable UE may attach to the network (if it is not already connected) and connect to a PDN connection enabling the necessary relay traffic, or it may need to connect to additional PDN connection(s) in order to provide relay traffic towards Remote UE(s). PDN connection(s) supporting UE-to-Network Relay shall only be used for Remote ProSe UE(s) relay traffic.  ….  After being connected to the ProSe UE-to-Network Relay, the Remote UE keeps performing the measurement of the signal strength of the discovery message sent by the ProSe UE-to-Network Relay (i.e. the UE-to-Network Relay Discovery Announcement message in Model A or a UE-to-Network Relay Discovery Response message in Model B) for relay reselection as defined in TS 36.300 [17]. For Model B, to measure the PC5 link quality, the Remote UE sends a UE-to-Network Relay Discovery Solicitation message periodically. The message may contain a ProSe Relay UE ID of its serving ProSe UE-to-Network Relay. If the ProSe Relay UE ID is included in the message, then only the ProSe UE-to-Network Relay, which owns this ProSe Relay UE ID, shall respond to the UE-to-Network Relay Discovery Solicitation message. |

**Question 1: Do companies agree that for NR sidelink discovery message, transmissions will be performed periodically (see highlighted text from 23.303 [3]** **above) and for such periodical PC5-S signalling/message transmission, it is beneficial to support discovery transmissions via SL CG ? If no, please provide the reason/comments.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Ericsson | No | CG is mainly designed to reduce the latency due to dynamic scheduling. Since discovery message has no QoS profile, we see no reason to couple discovery to CG. |
| Apple |  | We agree that PC5 Discovery messages are periodic. But the PC5-S signalling like “keepalive” messages are also periodic in NR SL Rel-16. So, I think this is not a completely new problem. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In rapporteur’s view, the framework for support of discovery transmissions via SL CG is already specified in Rel-17. The proponent companies propose to add the missing bit to this framework/procedure by introducing the new assistance information, which is very similar to SL-TrafficPatternInfo in UEAssistanceInformation message, to assist gNB to configure SL CG resources for discovery message transmission with minimal spec impacts. Otherwise, the whole effect of introducing SL CG for discovery transmissions in the specification will reduced.

**Question 2: Considering the framework for supporting of discovery transmissions via SL CG has already specified in Rel-17, do companies agree to add the missing bit to this framework/procedure by introducing the new assistance information, very similar to existing SL-TrafficPatternInfo in UEAssistanceInformation message to assist gNB to configure SL CG type 1 for discovery with minimal spec impacts? If no, please provide the reason/comments.**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Ericsson | No | See comments for Q1 |
| Apple | Prefer no | We have concern about ASN.1 impact in this late stage. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 3: If the answer to Question2 is yes, Can TP in** [**R2-2210111**](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208228.zip) **be agreed as baseline?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Ericsson | No |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2 Resource allocation scheme when sensing result is not available for NR sidelink discovery

|  |  |  |
| --- | --- | --- |
| R2-2210633[2] | Discussion on Resource Allocation for Sidelink Discovery | CATT |

When mode2 is selected for NR sidelink discovery transmission, the UE will perform resource pool selection and perform resource selection mechanism selection based on the sl-AllowedResourceSelectionConfig of the selected resource pool.

|  |  |
| --- | --- |
| **sl-AllowedResourceSelectionConfig** | **Allowed resource selection mechanism(s)** |
| c1 | only full sensing |
| c2 | only partial sensing |
| c3 | only random selection |
| c4 | full sensing + random selection |
| c5 | full sensing + partial sensing |
| c6 | partial sensing + random selection |
| c7 | full sensing + partial sensing + random selection |

According to the current RRC spec, UE will use exceptional pool in the following two cases:

* Case1: when discovery pool is configured, if partial/full sensing is selected and is allowed by sl-AllowedResourceSelectionConfig, and the sensing result is not available.
* Case2: when discovery pool is not configured, if partial/full sensing for common pool is selected and is allowed by sl-AllowedResourceSelectionConfig, and the sensing result is not available.

For the resource pool, if c1/c2/c5 is configured for sl-AllowedResourceSelectionConfig, the current spec procedure is clear. But if c4/c6/c7 is configured for  
sl-AllowedResourceSelectionConfig, when the sensing result is not available, besides limiting the UE to use exceptional pool, [2] raised that UE can also use random selection with the merit of reducing the pressure on the exceptional pool.

**Question 4: For the selected resource pool, if the configured value of sl-AllowedResourceSelectionConfig is c4/c6/c7, do companies agree that UE can use random selection on the selected resource pool instead of using exceptional pool when the sensing result is not available?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Ericsson | Yes |  |
| OPPO | No | currently, in R17 eSL, the selection of full/partial/random (if allowed by the pool) is fully up to UE implementation, so our view is it is OK for UE to select random in normal pool if it is allowed, yet we do not see the need to pursue spec impact for “**UE can use random selection on the selected resource pool instead of using exceptional pool when the sensing result is not available**” |
| Apple | No | Having no sensing results is a temporary situation. So, it is proper to deal with this behaviour in the exceptional pool, instead of normal TX pool. Adding more random transmissions in a normal TX pool has negative impact on other UEs selecting resources based on sensing schemes in the same pool.  Even in LTE V2X, the UE is configured to support random selection and partial sensing in a P2X TX pool is still allowed to use exceptional pool when partial sensing results are not available. If it works in LTE SL, it could work in NR SL.  So, we are not sure there is a need to support this additional enhancement. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 5: If the answer to Question4 is yes, Can TP in** [**R2-2210633**](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_119-e/Docs/R2-2208228.zip) **be agreed as baseline?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Ericsson | Yes |  |
| OPPO | No | The specification from R17 eSL is sufficient already. |
| Apple | No |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion

Based on the input from all companies, the rapporteur proposes that:

# Reference

1. R2-2210111 Support of SL CG for discovery message Huawei, HiSilicon, Nokia, Kyocera
2. R2-2210633 Discussion on Resource Allocation for Sidelink Discovery CATT
3. TS 23.303 Proximity-based services (ProSe); Stage 2 V17.0.0