3GPP TSG-RAN WG2 Meeting #119bis-e R2-22xxxxx

Online, October 10 – October 19, 2022

**Agenda item: 6.1.4**

**Source: Samsung**

**Title: Report of Offline 603: UP Correction for Rel-17 MBS**

**Document for: Report**

# Introduction

This document is a summary of the following offline discussion.

* [AT119bis-e][603][MBS-R17] UP corrections (Samsung)

Scope: Treat [R2-2210051](file:///C:\Users\Dwx974486\Documents\3GPP\Extracts\R2-2210051%20Miscellaneous%20corrections%20for%20MBS%2038.323.docx) and remaining issues from documents in 6.1.4.

Outcome: Report (Samsung) + CR(s) as needed:

* 38.323: Xiaomi
* 38.321: OPPO

Deadline: Report available: Tuesday 2022-10-18 1000 UTC, agreeable CR(s): EOM

This offline discussion covers remaining issues in user plane.

# Contact Information

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email** |
| Samsung | Sangkyu Baek | sangkyu.baek@samsung.com |
| LGE | Seong Kim | sj117.kim@lge.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

## Issue #1: PDCP Rapporteur CR

The PDCP rapporteur CR (R2-2210551) proposed to correct the RRC field name to align with the RRC spec, as follows:

|  |
| --- |
| For multicast MRBs, the initial value of RX\_DELIV is set by *initialRX-DELIV* in TS 38.331 [3]. |

**Q1. Do companies agree the change of R2-2210551?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #2: Clarification on CSI-Masking

For unicast DRX, consideration for running of *drx-onDurationTimer* of a DRX group includes “grants/assignments scheduled on Serving Cell(s)”. It is because of the case of transition between long DRX and short DRX due to the grant/assignment discussed during LTE Rel-11. Multicast DRX does not have short DRX, so Samsung (R2-2209438) proposed to remove this part for Multicast DRX, as follows:

|  |
| --- |
| 2> if CSI masking (*csi-Mask*) is setup by upper layers:  3> in current symbol n, if *drx-onDurationTimer* of a DRX group would not be running considering grants/assignments scheduled on Serving Cell(s) in this DRX group and DRX Command MAC CE/Long DRX Command MAC CE received until 4 ms prior to symbol n when evaluating all DRX Active Time conditions as specified in this clause; and  3> if *allowCSI-SRS-Tx-MulticastDRX-Active* is not configured or, in current symbol n, if *drx-onDurationTimerPTM(s)* of all multicast DRXes corresponding to the DRX group would not be running considering DRX Command MAC CE for MBS multicast received until 4 ms prior to symbol n when evaluating all DRX Active Time conditions as specified in Clause 5.7b and all multicast sessions corresponding to the DRX group are configured with multicast DRX:  4> not report CSI on PUCCH in this DRX group. |

**Q2. Do companies agree to remove “multicast assignments” as running condition of *drx-onDurationTimerPTM?***

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes | Agree to Samsung’s analysis. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #3: HARQ RTT Timer Start Condition

### Pre-condition of RTT timer start and retransmission timer stop

Huawei/CBN/HiSilicon (R2-2209656) pointed out that the pre-condition of the start of *drx-HARQ-RTT-TimerDL* and the stop of *drx-RetransmissionTimerDL* in multicast DRX, i.e. *“When multicast DRX is configured for a G-RNTI or G-CS-RNTI”* is incorrect. The problematic case is that the unicast DRX is not configured. For this case, the proponent companies proposed to add a condition and a note to clarify as follows:

|  |
| --- |
| 5.7b Discontinuous Reception (DRX) for MBS Multicast \*\*\*\*\*Text omitted\*\*\*\*\*  When multicast DRX is configured for a G-RNTI or G-CS-RNTI or when unicast DRX is configured, the MAC entity shall for this G-RNTI or G-CS-RNTI:  NOTE 0: The operations related to unicast DRX timers are performed only if unicast DRX is configured, and the operations related to multicast DRX timers are performed only if multicast DRX is configured.  1> if a MAC PDU is received in a configured downlink multicast assignment:  2> if HARQ feedback is enabled:  3> start the *drx-HARQ-RTT-TimerDL-PTM* for the corresponding HARQ process in the first symbol after the end of the corresponding transmission carrying the DL HARQ feedback;  3> start the *drx-HARQ-RTT-TimerDL* for the corresponding HARQ process in the first symbol after the end of the corresponding transmission carrying the DL HARQ feedback.  2> stop the *drx-RetransmissionTimerDL-PTM* for the corresponding HARQ process;  2> stop the *drx-RetransmissionTimerDL* for the corresponding HARQ process. |

**Q3-1a. Do companies agree to clarify that the behaviour of unicast DRX timers doesn’t depend on the configuration of multicast DRX, i.e. start of *drx-HARQ-RTT-TimerDL* and the stop of *drx-RetransmissionTimerDL?* (TP above is a baseline.)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | No | If unicast DRX is not configured, there is no unicast DRX timers. Then, UE does not start/stop the unicast DRX RTT timers. Therefore, such change is not needed.  But, if clarification is really required, we prefer a simple one as follows:  …  3> start the *drx-HARQ-RTT-TimerDL,* if configured, for the corresponding HARQ process in the first symbol after the end of the corresponding transmission carrying the DL HARQ feedback.  …  2> stop the *drx-RetransmissionTimerDL,* if configured, for the corresponding HARQ process.  … |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For unicast DRX, there is a same issue on the pre-condition for stop of *drx-RetransmissionTimerDL-PTM:* When DRX is configured. Similar to Multicast DRX, the proponent companies proposed to add a condition and a note to clarify as follows:

|  |
| --- |
| 5.7 Discontinuous Reception (DRX) \*\*\*\*\*Text omitted\*\*\*\*\*  When DRX is configured or when multicast DRX is configured, the MAC entity shall:  NOTE 0: The operations related to unicast DRX timers are performed only if unicast DRX is configured, and the operations related to multicast DRX timers are performed only if multicast DRX is configured.  1> if a MAC PDU is received in a configured downlink assignment for unicast:  \*\*\*\*\*Text omitted\*\*\*\*\*  2> stop the *drx-RetransmissionTimerDL* for the corresponding HARQ process;  2> stop the *drx-RetransmissionTimerDL-PTM* for the corresponding HARQ process.  \*\*\*\*\*Text omitted\*\*\*\*\* |

**Q3-1b. Do companies agree to clarify that the behaviour of multicast DRX timers doesn’t depend on the configuration of unicast DRX, i.e. the stop of *drx-RetransmissionTimerDL-PTM?* (TP above is a baseline.)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | No | If multicast DRX is not configured, there is no multicast DRX timers. Then, UE does not start/stop the multicast DRX RTT timers. Therefore, such change is not needed.  But, if clarification is really required, we prefer a simple one as follows:  2> stop the *drx-RetransmissionTimerDL-PTM,* if configured, for the corresponding HARQ process. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### *drx-HARQ-RTT-TimerDL* Start in case UE does not support PTP retransmission

In the current MAC specification, when a UE receives a PTM transmission, the unicast DRX timer *drx-HARQ-RTT-TimerDL* is always started. Even if the UE does not support PTP retransmission based on 33-2d (PTP retransmission for multicast dynamic scheduling) and 33-5-1d (PTP retransmission for SPS group-common PDSCH for multicast), *drx-HARQ-RTT-TimerDL* is started. Huawei/CBN/HiSilicon (R2-2209656) pointed out that *drx-HARQ-RTT-TimerDL* does not need to be started at least for UE not supporting PTP retransmission via C-RNTI for a PTM transmission. The proponent companies proposed to clarify this case.

**Q3-2. Do companies agree to clarify the UE doesn’t need to start *drx-HARQ-RTT-TimerDL* after receiving a PTM transmission if the UE does not support PTP retransmission via C-RNTI for the initial PTM transmission?**

**- Yes: Clarify this (FFS: Detail)**

**- No change: Always start *drx-HARQ-RTT-TimerDL*. It may waste UE power consumption but may be considered as an optimization.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | No | It seems an optimization. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #4: Correction on DRX Command MAC CE

In the MAC specification, “DCI scrambled with C-RNTI” and “DCI scrambled with a G-RNTI” are used to identify the DRX Command MAC CEs for Unicast DRX and Multicast DRX, respectively. LG (R2-2210592) and Google (R2-2210684) pointed out that it is a physical layer operation which has not been specified by MAC and even PHY specification doe not use this condition. The propoenent companies proposed to use “PDCCH addressed to C-RNTI/G-RNTI” to align with other texts in the MAC specification.

**Q4-1. Do companies agree to modify the text “DCI scrambled with C-RNTI/G-RNTI”?**

**- Option 1: Yes, LG’s TP is preferred (R2-2210592).**

|  |
| --- |
| if a DRX Command MAC CE is received by PDCCH addressed to C-RNTI for unicast transmission  if a DRX Command MAC CE is received by PDCCH addressed to a G-RNTI |

**- Option 2: Yes, Google’s TP is preferred (R2-2210684).**

|  |
| --- |
| if a DRX Command MAC CE with PDCCH addressed to the C-RNTI for unicast transmission is received  if a DRX Command MAC CE with PDCCH addressed to a G-RNTI is received |

**- Option 3: No change**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comment** |
| LGE | Option 1 |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

When ‘a DRX Command MAC CE with DCI scrambled with C-RNTI for unicast transmission’ is received, the intended behaviour is to apply the MAC CE to unicast DRX cycle only if the MAC PDU containing the MAC CE does not contain a MAC SDU intended for MTCH logical channel. However, there is no clear definition of unicast transmission. If unicast transmission is misinterpreted as a transmission only to the UE configured with the C-RNTI, the UE can apply the MAC CE to unicast DRX even if the MAC PDU containing the MAC CE contains a MAC SDU intended for MTCH logical channel. LG (R2-2210592) proposed to add a note to clarify this.

**Q4-2. Do companies agree to add the following note in TS 38.321?**

NOTE x : The unicast transmission does not contain a MAC SDU for MTCH logical channel.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #5: (De-)multiplexing block for MCCH in TS 38.300

The MAC specification clarified that (de-)multiplexing function is supported for MCCH. However, this has not been simultaneously captured in the Stage-2 specification. vivo (R2-2209416) proposed to incorporate (de-)multiplexing block for MCCH in TS 38.300 as follows:

|  |
| --- |
| **Figure 16.10.3-2: Downlink Layer 2 Architecture for Broadcast Session** |

**Q5. Do companies agree to modify Figure 16.10.3-2 in TS 38.300 to add the (de-)multiplexing block?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #6: HARQ Buffer Flush at MAC Reset

During the online session on Monday, RAN2 agreed to clarify MAC Reset operation not to treat broadcast bundle as a new transmission as follows:

* Do not remove the exception for MBS for flushing soft buffers.
* Clarify that the transmission after MAC reset should not (always) be treated as a new transmission for MBS broadcast soft buffer. E.g. add “except for MBS broadcast” for the relevant bullet.
* DL HARQ buffers (soft buffers) are not flushed due to TAT expiry. No change needed for HARQ buffers flushing due to TAT expiry.

The rapporteur would suggest to have the same condition with the case of buffer flushing.

**Q6. Do companies agree to add the following condition which excludes HP being used for broadcast?**

If a reset of the MAC entity is requested by upper layers or the reset of the MAC entity is triggered due to SCG deactivation as defined in clause 5.29, the MAC entity shall:

…

1> flush the soft buffers for all DL HARQ processes, except for the DL HARQ process being used for MBS broadcast;

1> for each DL HARQ process, except for the DL HARQ process being used for MBS broadcast, consider the next received transmission for a TB as the very first transmission;

**- Yes**

**- No (Please provide alternative wording)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes | We can accept it. It is aligned with the intention of ‘not flushing DL soft buffers for MBS broadcast’. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #7: MRB Type Determination by Target Configuration

During the online session on Monday, RAN2 made the following agreements on MRB type change.

* We keep the principle of UM MRB and AM MRB in PDCP specs (no change to PDCP specs).
* For PDCP procedures, MRB type is determined by the target/latest/received configuration when the RLC entity associated to the PDCP entity is changed between UM and AM. (capture as a NOTE at least in PDCP specs, the exact wording discussed as part of CR update, can consider adding a NOTE in RRC specs as well).

This offline discussion should focus on how to capture the agreement in the specification. As captured in the agreement, a note in PDCP will be added and the final wording will be discussed during the CR phase. The issue here is whether a similar note is needed in the RRC specification.

**Q7. Do companies agree to have a note in RRC specification?**

e.g. NOTE x: At PDCP re-establishment, the MRB type (i.e. UM MRB or AM MRB) is determined by the target configuration.‎

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Issue #8: PDCP State Variable Handling

During the online discussion on Monday, RAN2 made the following agreement on PDCP state variable handling:

* Do not reset RX\_NEXT and RX\_DELIV to the initial value when MRB PDCP is suspended unless a serious issue is found.
* Continue offline with other proposals

The agreements were based on Nokia’s contribution (R2-2209551) having the following proposals:

|  |
| --- |
| **Proposal 1:** Do not reset TX\_NEXT, RX\_NEXT and RX\_DELIV to the initial value when MRB PDCP is suspended.  **Proposal 2:** Continue PDCP COUNT when a deactivated MBS multicast session is activated.  **Proposal 3:** There is no need for configuration of initial value of RX\_DELIV when PDCP is re-established for AM MRB. |

For PDCP suspend, the issue seems to have been resolved by not resetting the variable. One thing to check is if there is any serious issue.

**Q8-1. Do companies have any serious issue that makes the procedure not work if RX\_NEXT and RX\_DELIV are not reset at PDCP Suspend?**

**- Yes (please explain the serious issue)**

**- No issue**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | No |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Now the remaining issue is for PDCP Re-establishment of AM MRB. During the online discussion, Proposal 3 of R2-2209551 was almost agreeable but not officially agreed due to the lack of time. The rapporteur would like to quickly check if we can directly agree it.

**Q8-2. Do companies agree the following proposal? (Note that P3 requires no specification change)**

Proposal 3: There is no need for configuration of initial value of RX\_DELIV when PDCP is re-established for AM MRB.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

For Proposal 2 of R2-2209551, many companies thought that it is up to NW configuration if P3 is agreed, since MRB release and add is already supported. Thus, the rapporteur would like to ask companies’ view on whether additional specification impact is expected.

**Q8-3. Do companies agree that the following proposal has no specification impact assuming that P3 of R2-2209551 is agreed?**

**Proposal 2:** NW may configure to continue PDCP COUNT when a deactivated MBS multicast session is activated. (no specification impact)

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comment (please explain the required spec change if your answer is “no”)** |
| LGE | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusion