3GPP TSG-RAN WG2 #119bis-e Tdoc R2-xxxxxxx

Electronic meeting, 10th - 19th Oct. 2022

Agenda Item: 8.13.4

Source: Ericsson (Rapporteur of the offline)

Title: [AT119bis-e][803][R18 SON/MDT] SON of NR-U (Ericsson)

Document for: Discussion, Decision

# 1 Introduction

This document is for the following offline discussion focusing on the proposal 3-8 of the summary document R2-2210799.

 **[AT119bis-e][803][R18 SON/MDT] SON of NR-U (Ericsson)**

Discussion on the proposals 3-8 in R2-2210799.

Intended outcome: Report

Deadline: 04:44 UTC, Friday October 14th

Deadline for comments: 18:00 UTC Thursday October 13th

# 2 Contact list

Contact person for each participating company:

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Ericsson | Ali Parichehreh | Ali.Parichehreh@ericsson.com |
| Samsung | Aby K Abraham | Aby.abraham@samsung.com |
| Xiaomi | xiaowei jiang | jiangxiaowei@xiaomi.com |
| Huawei, HiSilicon | Jun Chen | jun.chen@huawei.com |
| CATT | Jie Shi | shijie@catt.cn |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion for enhancing RA Report for NR-U

In this section, we focus on the proposals and summary of the proposals for the NRU related measurements and information to be collected as part of RA report.

Please note that proposals are reshuffled for the offline discussion from the ones which are easy to be agreed to the ones that require more discussion.

Based on the contributions, 6 companies including Lenovo, ZTE, Samsung, CATT, Ericsson and CMCC in [1, 3, 5, 7, 10] proposed to introduce an indication of consistent LBT failure in the RA report. 4 companies proposed to have the consistent LBT failure indication as a new *raPurpose*. Provided that the rapporteur proposes the following:

Proposal 7: Introduce a new *raPurpose* in the *RA-Report* to indicate that the RA was initiated following a “consistent LBT failures” in the SpCell.

* **Q1: Do you agree to introduce a new *raPurpose,* indicating “consistent LBT failure”, as proposed in Proposal 7?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Samsung | Yes |  |
| Xiaomi | Yes |  |
| Huawei, HiSilicon | No | We see that some new parameters are likely to be introduced in RA report and they are related to “consistent LBT failure”, so “consistent LBT failures” type can be implicitly indicated. |
| CATT | Yes | We think it is necessary to introduce a new *raPurpose* to convey which event triggers the RACH procedure. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

In addition, Xiaomi proposed that the value 0 should be introduced for the number of preambles sent over selected SSB and CSI-RS. Although this is provided by a single company, rapporteur thinks this is a valid and easily agreeable proposal, hence proposing the following.

**Proposal 8: RAN2 to introduce value 0 for the numberOfPreamblesSentOnSSB and numberOfPreamblesSentOnCSI-RS.**

* **Q2: Do you agree to Proposal 8?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Samsung | Yes |  |
| Xiaomi | Yes |  |
| Huawei, HiSilicon | Yes |  |
| CATT | Yes |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

Xiaomi in [6] proposed to clarify the definition of the RA attempt. The reasoning is that RA procedure tailored for the NR-U, works slightly different from legacy RA procedure and *PREAMBLE\_TRANSMISSION\_COUNTER* does not increase when UE experience LBT failure (and is configured with the LBT recovery) upon transmitting the preamble. This is shown in the following excerpt from TS 38.331.

1> if LBT failure indication is received from lower layers for this Random Access Preamble transmission:

2> if *lbt-FailureRecoveryConfig* is configured:

3> perform the Random Access Resource selection procedure (see clause 5.1.2).

2> else:

3> increment *PREAMBLE\_TRANSMISSION\_COUNTER* by 1;

In fact, instead of *PREAMBLE\_TRANSMISSION\_COUNTER* UE counts the number of LBT failures experienced along with the attempt to transmit the preambles and concludes the failure of RA procedure upon reaching the maximum number of LBT failure instances configured by the network.

Therefore, rapporteur proposes the following:

**Proposal 6-a: RAN2 clarify that in NR-U:**

1. **An RA attempt is an attempt to transmit a preamble as UE executes section 5.1.3 of TS 38.321**

**or**

1. **An RA attempt is only counted when the PREAMBLE\_TRANSMISSION\_COUNTER increased (i.e., when UE accesses the channel at the PHY layer, and transmits the preamble).**

Based on the above proposal rapporteur would like to ask companies the following question.

* **Q3: Which one of the options proposed in Proposal 6-a is acceptable?**

|  |  |  |
| --- | --- | --- |
| Company | a/b | Comments |
| Samsung | b |  |
| Xiaomi | b | Since preamble transmission with LBT failure will not be counted for PREAMBLE\_TRANSMISSION\_COUNTER, and the list size of RA attempt is equal to the maximum preamble transmission, if we record every preamble transmission with LBT failure, the records of RA attempts will easily reach the maximum value, and easily make UE buffer full. |
| CATT | b |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

In addition, Samsung and Ericsson in [3 and 8] proposed to include the LBT indication per RA attempt, while Huawei in [4] and CMCC in [7] proposed to include the number of LBT failures and Lenovo [5] proposed to include the time duration of the LBT issue in the RA report. Rapporteur judges that a middle-ground solution between camp (a) and (b) can be the number of LBT failures per selected reference signal e.g., number of LBT failures per SSB. Needless to mention that this solution would be beneficial for the network to configure the SSB beams for the UEs based on the LBT issues.

Therefore, the rapporteur of the offline discussion proposes the following:

**Proposal 6-b: RAN2 discuss which of the following measurement and information to be added to the RA-InformationCommon**

1. **Whether each RA attempt (i.e., preamble transmission) was blocked by LBT,**
2. **Total number of LBT failures during an RA procedure,**
3. **Number of LBT failures per selected beam,**
4. **Time duration of the LBT failures during the RA procedure.**

Based on the above proposal rapporteur would like to ask companies the following question.

* **Q4: Which options proposed in Proposal 6-b is acceptable?**

|  |  |  |
| --- | --- | --- |
| Company | a/b/c/d | Comments |
| Samsung | b | We think that b) provides sufficient granularity. |
| Xiaomi | b | In WI NR above 52.6GHz, directional LBT was discussed, but RAN2 at last do not introduce directional LBT, consistent LBT failure still based on omni-direction. Thus, there is no need to count LBT failure per SSB. |
| Huawei, HiSilicon | b | For a), it may bring significant overhead. For any impacts to the field PerRAAttemptInfo-r16, we should be careful as there are some iterations inside the RA report, e.g.  RA-InformationCommon-r16 ::= SEQUENCE {  perRAInfoList-r16 PerRAInfoList-r16,  }  PerRAInfoList-r16 ::= SEQUENCE (SIZE (1..200)) OF PerRAInfo-r16  PerRAInfo-r16 ::= CHOICE {  perRASSBInfoList-r16 PerRASSBInfo-r16,  perRACSI-RSInfoList-r16 PerRACSI-RSInfo-r16  }  PerRASSBInfo-r16 ::= SEQUENCE {  ssb-Index-r16 SSB-Index,  numberOfPreamblesSentOnSSB-r16 INTEGER (1..200),  perRAAttemptInfoList-r16 PerRAAttemptInfoList-r16  }  PerRAAttemptInfoList-r16 ::= SEQUENCE (SIZE (1..200)) OF PerRAAttemptInfo-r16  PerRAAttemptInfo-r16 ::= SEQUENCE {  contentionDetected-r16 BOOLEAN OPTIONAL,  dlRSRPAboveThreshold-r16 BOOLEAN OPTIONAL,  ...,  [[  fallbackToFourStepRA-r17 ENUMERATED {true} OPTIONAL  ]]  }  For c) and d), we are not clear about the value from network point of view. |
| CATT | b) | a. We think option a) only includes Preamble transmission which is not sufficient.  c. It is a bit of complex and we are wondering how to use the beam information since LBT is performed per BWP.  d. we are wondering how to do the statistic on the time duration of the LBT failures during the RA procedure since LBT is performed for each UL transmission. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

Companies (including Huawei, Ericsson [4, 8]) proposed to include the RSSI and EDT in the RA report. Huawei proposed to log the RSSI in the RA-InformationCommon and Ericsson proposed to include the RSSI measurements per RA attempt. Rapporture believes the granularity of the RSSI measurements value can be discussed as FFS, when companies agreed to include the RSSI measurements in the RA-InformationCommon.

**Proposal 3: UE logs RSSI measurement and the applied EDT value in the RA-InformationCommon. FFS on logging granularity.**

Based on the above proposal rapporteur would like to ask companies the following question.

* **Q5: Do you agree with Proposal 3?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| Samsung | Yes |  |
| Xiaomi | Yes |  |
| Huawei, HiSilicon | Yes | We are open to discuss the logging level/granularity, and the signalling overhead should be checked. |
| CATT | Yes for RSSI | We think RSSI can be included in the RA-InformationCommon. But we are wondering whether EDT value is included in RA-InformationCommon since EDT value is set to be less or equal to the maximum EDT threshold which is configured by the network or set by the UE based on some rules. This value is more about optimization of LBT configuration. And even this value is reported to NW, how the NW uses this value is still unclear. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

In addition, BWP specific lbt-FailureRecoveryConfig is proposed to be logged in the RA report and in particular in the RA-InformationCommon. However, it is proposed in [2] to consult RAN3 whether it is possible and evaluate the cost for the network nodes to know this information without UE reporting. Therefor rapporteur of the offline discussion proposed the following:

**Proposal 5: RAN2 to**

1. **Include BWP specific lbt-FailureRecoveryConfig in the RA report, or**
2. **Consult RAN3 to whether it is possible and evaluate the cost for the network to know the lbt-FailureRecoveryConfig without UE reporting.**

Based on the above proposal rapporteur would like to ask companies the following question.

* **Q6: Which of the options (a/b) in Proposal 5 is acceptable?**

|  |  |  |
| --- | --- | --- |
| Company | a/b | Comments |
| Samsung | Consult RAN3 |  |
| Xiaomi | b | We should understand whether there is need to report the whole lbt-FailureRecoveryConfig, perhaps in some scenario, network only needs to know whether lbt-FailureRecoveryConfig is configured or not. |
| Huawei, HiSilicon | b |  |
| CATT | b | We think we can consult RAN3 for decision. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Rapporteur´s summary: To be added later

# Conclusion

To be added later.

# References

1. [R2-2209573](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209573.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2209573)[NR-U enhancements for SON](file:///C:\R2-2209573.zip) **CATT**
2. [R2-2209765](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209765.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2209765)[SON enhancements for NR-U](file:///C:\R2-2209765.zip) **Apple**
3. [R2-2209824](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209824.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2209824)[SON/MDT enhancements for NR-U](file:///C:\R2-2209824.zip) **Samsung R&D Institute India**
4. [R2-2209897](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209897.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2209897)[Discussion on SON for NR-U](file:///C:\R2-2209897.zip) **Huawei, HiSilicon**
5. [R2-2209958](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2209958.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2209958)[Discussion on MRO for NR-U](file:///C:\R2-2209958.zip) **Lenovo**
6. [R2-2210039](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210039.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2210039)[Discussion on SON for NR-U](file:///C:\R2-2210039.zip) **Xiaomi**
7. [R2-2210148](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210148.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2210148)[SONMDT enhancement for NR-U](file:///C:\R2-2210148.zip) **CMCC**
8. [R2-2210180](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210180.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2210180)[Enhancements of SON reports for NR-U](file:///C:\R2-2210180.zip) **Ericsson**
9. [R2-2210270](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210270.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2210270)[MRO and MDT enhancements for NR-U](file:///C:\R2-2210270.zip) **Nokia, Nokia Shanghai Bell**
10. [R2-2210290](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_119bis-e/Docs/R2-2210290.zip)[M](http://mannerheim.nomadiclab.com/Mannerheim/tdoc/R2-2210290)[Consideration on NR-U related SON](file:///C:\R2-2210290.zip) **ZTE Corporation, Sanechips**