3GPP TS 38.463 V15.12.0 (2023-06)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

NG-RAN;

E1 Application Protocol (E1AP)

(Release 15)



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 8

1 Scope 9

2 References 9

3 Definitions and abbreviations 10

3.1 Definitions 10

3.2 Abbreviations 11

4 General 11

4.1 Procedure specification principles 11

4.2 Forwards and backwards compatibility 12

4.3 Specification notations 12

5 E1AP services 12

6 Services expected from signalling transport 12

7 Functions of E1AP 12

8 E1AP procedures 13

8.1 List of E1AP Elementary Procedures 13

8.2 Interface Management procedures 14

8.2.1 Reset 14

8.2.1.1 General 14

8.2.1.2 Successful Operation 14

8.2.1.2.1 Reset Procedure Initiated from the gNB-CU-CP 14

8.2.1.2.2 Reset Procedure Initiated from the gNB-CU-UP 15

8.2.1.3 Abnormal Conditions 16

8.2.2 Error Indication 16

8.2.2.1 General 16

8.2.2.2 Successful Operation 16

8.2.2.3 Abnormal Conditions 16

8.2.3 gNB-CU-UP E1 Setup 17

8.2.3.1 General 17

8.2.3.2 Successful Operation 17

8.2.3.3 Unsuccessful Operation 18

8.2.3.4 Abnormal Conditions 18

8.2.4 gNB-CU-CP E1 Setup 18

8.2.4.1 General 18

8.2.4.2 Successful Operation 19

8.2.4.3 Unsuccessful Operation 19

8.2.4.4 Abnormal Conditions 19

8.2.5 gNB-CU-UP Configuration Update 20

8.2.5.1 General 20

8.2.5.2 Successful Operation 20

8.2.5.3 Unsuccessful Operation 21

8.2.5.4 Abnormal Conditions 21

8.2.6 gNB-CU-CP Configuration Update 21

8.2.6.1 General 21

8.2.6.2 Successful Operation 22

8.2.6.3 Unsuccessful Operation 23

8.2.6.4 Abnormal Conditions 23

8.2.7 E1 Release 23

8.2.7.1 General 23

8.2.7.2 Successful Operation 23

8.2.7.2.1 E1 Release Procedure Initiated from the gNB-CU-CP 23

8.2.7.2.2 E1 Release Procedure Initiated from the gNB-CU-UP 24

8.2.7.3 Abnormal Conditions 24

8.2.8 gNB-CU-UP Status Indication 24

8.2.8.1 General 24

8.2.8.2 Successful Operation 24

8.2.8.3 Abnormal Conditions 25

8.3 Bearer Context Management procedures 25

8.3.1 Bearer Context Setup 25

8.3.1.1 General 25

8.3.1.2 Successful Operation 25

8.3.1.3 Unsuccessful Operation 28

8.3.1.4 Abnormal Conditions 28

8.3.2 Bearer Context Modification (gNB-CU-CP initiated) 28

8.3.2.1 General 28

8.3.2.2 Successful Operation 29

8.3.2.3 Unsuccessful Operation 32

8.3.2.4 Abnormal Conditions 33

8.3.3 Bearer Context Modification Required (gNB-CU-UP initiated) 33

8.3.3.1 General 33

8.3.3.2 Successful Operation 33

8.3.3.3 Abnormal Conditions 34

8.3.4 Bearer Context Release (gNB-CU-CP initiated) 34

8.3.4.1 General 34

8.3.4.2 Successful Operation 34

8.3.4.3 Abnormal Conditions 34

8.3.5 Bearer Context Release Request (gNB-CU-UP initiated) 34

8.3.5.1 General 34

8.3.5.2 Successful Operation 35

8.3.5.3 Abnormal Conditions 35

8.3.6 Bearer Context Inactivity Notification 35

8.3.6.1 General 35

8.3.6.2 Successful Operation 35

8.3.6.3 Abnormal Conditions 36

8.3.7 DL Data Notification 36

8.3.7.1 General 36

8.3.7.2 Successful Operation 36

8.3.7.3 Abnormal Conditions 36

8.3.8 Data Usage Report 36

8.3.8.1 General 36

8.3.8.2 Successful Operation 37

8.3.8.3 Abnormal Conditions 37

8.3.9 gNB-CU-UP Counter Check 37

8.3.9.1 General 37

8.3.9.2 Successful Operation 37

8.3.9.3 Unsuccessful Operation 37

8.3.9.4 Abnormal Conditions 37

8.3.10 UL Data Notification 38

8.3.10.1 General 38

8.3.10.2 Successful Operation 38

8.3.10.3 Abnormal Conditions 38

8.3.11 MR-DC Data Usage Report 38

8.3.11.1 General 38

8.3.11.2 Successful Operation 38

8.3.11.3 Abnormal Conditions 38

9 Elements for E1AP communication 39

9.1 General 39

9.2 Message Functional Definition and Content 39

9.2.1 Interface Management messages 39

9.2.1.1 RESET 39

9.2.1.2 RESET ACKNOWLEDGE 40

9.2.1.3 ERROR INDICATION 40

9.2.1.4 GNB-CU-UP E1 SETUP REQUEST 40

9.2.1.5 GNB-CU-UP E1 SETUP RESPONSE 41

9.2.1.6 GNB-CU-UP E1 SETUP FAILURE 41

9.2.1.7 GNB-CU-CP E1 SETUP REQUEST 42

9.2.1.8 GNB-CU-CP E1 SETUP RESPONSE 42

9.2.1.9 GNB-CU-CP E1 SETUP FAILURE 42

9.2.1.10 GNB-CU-UP CONFIGURATION UPDATE 43

9.2.1.11 GNB-CU-UP CONFIGURATION UPDATE ACKNOWLEDGE 43

9.2.1.12 GNB-CU-UP CONFIGURATION UPDATE FAILURE 44

9.2.1.13 GNB-CU-CP CONFIGURATION UPDATE 44

9.2.1.14 GNB-CU-CP CONFIGURATION UPDATE ACKNOWLEDGE 46

9.2.1.15 GNB-CU-CP CONFIGURATION UPDATE FAILURE 46

9.2.1.16 E1 RELEASE REQUEST 46

9.2.1.17 E1 RELEASE RESPONSE 47

9.2.1.18 GNB-CU-UP STATUS INDICATION 47

9.2.2 Bearer Context Management messages 47

9.2.2.1 BEARER CONTEXT SETUP REQUEST 47

9.2.2.2 BEARER CONTEXT SETUP RESPONSE 48

9.2.2.3 BEARER CONTEXT SETUP FAILURE 49

9.2.2.4 BEARER CONTEXT MODIFICATION REQUEST 49

9.2.2.5 BEARER CONTEXT MODIFICATION RESPONSE 51

9.2.2.6 BEARER CONTEXT MODIFICATION FAILURE 51

9.2.2.7 BEARER CONTEXT MODIFICATION REQUIRED 52

9.2.2.8 BEARER CONTEXT MODIFICATION CONFIRM 52

9.2.2.9 BEARER CONTEXT RELEASE COMMAND 53

9.2.2.10 BEARER CONTEXT RELEASE COMPLETE 53

9.2.2.11 BEARER CONTEXT RELEASE REQUEST 53

9.2.2.12 BEARER CONTEXT INACTIVITY NOTIFICATION 54

9.2.2.13 DL DATA NOTIFICATION 55

9.2.2.14 DATA USAGE REPORT 56

9.2.2.15 GNB-CU-UP COUNTER CHECK REQUEST 56

9.2.2.16 UL DATA NOTIFICATION 57

9.2.2.17 MR-DC DATA USAGE REPORT 58

9.3 Information Element Definitions 58

9.3.1 Radio Network Layer Related IEs 58

9.3.1.1 Message Type 58

9.3.1.2 Cause 58

9.3.1.3 Criticality Diagnostics 61

9.3.1.4 gNB-CU-CP UE E1AP ID 62

9.3.1.5 gNB-CU-UP UE E1AP ID 62

9.3.1.6 Time To wait 63

9.3.1.7 PLMN Identity 63

9.3.1.8 Slice Support List 63

9.3.1.9 S-NSSAI 63

9.3.1.10 Security Information 63

9.3.1.11 Cell Group Information 64

9.3.1.12 QoS Flow List 64

9.3.1.13 UP Parameters 65

9.3.1.14 NR CGI 65

9.3.1.15 gNB-CU-UP ID 65

9.3.1.16 DRB ID 65

9.3.1.17 E-UTRAN QoS 65

9.3.1.18 E-UTRAN Allocation and Retention Priority 66

9.3.1.19 GBR QoS Information 66

9.3.1.20 Bit Rate 67

9.3.1.21 PDU Session ID 67

9.3.1.22 PDU Session Type 67

9.3.1.23 Security Indication 68

9.3.1.24 QoS Flow Identifier 68

9.3.1.25 QoS Flow QoS Parameters List 68

9.3.1.26 QoS Flow Level QoS Parameters 68

9.3.1.27 Non Dynamic 5QI Descriptor 69

9.3.1.28 Dynamic 5QI Descriptor 69

9.3.1.29 NG-RAN Allocation and Retention Priority 70

9.3.1.30 GBR QoS Flow Information 71

9.3.1.31 Security Algorithm 72

9.3.1.32 User Plane Security Keys 72

9.3.1.33 UL Configuration 72

9.3.1.34 gNB-CU-UP Cell Group Related Configuration 73

9.3.1.35 PDCP Count 73

9.3.1.36 NR CGI Support List 74

9.3.1.37 QoS Parameters Support List 74

9.3.1.38 PDCP Configuration 74

9.3.1.39 SDAP Configuration 76

9.3.1.40 ROHC Parameters 76

9.3.1.41 T-Reordering Timer 76

9.3.1.42 Discard Timer 77

9.3.1.43 UL Data Split Threshold 77

9.3.1.44 Data Usage Report List 77

9.3.1.45 Flow Failed List 78

9.3.1.46 Packet Loss Rate 79

9.3.1.47 Packet Delay Budget 79

9.3.1.48 Packet Error Rate 79

9.3.1.49 Averaging Window 79

9.3.1.50 Maximum Data Burst Volume 79

9.3.1.51 Priority Level 79

9.3.1.52 Security Result 80

9.3.1.53 Transaction ID 80

9.3.1.54 Inactivity timer 80

9.3.1.55 Paging Priority Indicator (PPI) 80

9.3.1.56 gNB-CU-UP Capacity 80

9.3.1.58 PDCP SN Status Information 81

9.3.1.59 QoS Flow Mapping List 81

9.3.1.60 QoS Flow Mapping Indication 82

9.3.1.61 PDCP SN Size 82

9.3.1.62 Network Instance 82

9.3.1.63 MR-DC Usage Information 82

9.3.1.64 MR-DC Data Usage Report List 83

9.3.1.65 gNB-DU ID 84

9.3.1.66 Common Network Instance 84

9.3.1.67 Activity Notification Level 85

9.3.2 Transport Network Layer Related IEs 85

9.3.2.1 UP Transport Layer Information 85

9.3.2.2 CP Transport Layer Information 85

9.3.2.3 GTP-TEID 85

9.3.2.4 Transport Layer Address 85

9.3.2.5 Data Forwarding Information Request 86

9.3.2.6 Data Forwarding Information 86

9.3.3 Container and List IE definitions 86

9.3.3.1 DRB To Setup List E-UTRAN 86

9.3.3.2 PDU Session Resource To Setup List 87

9.3.3.3 DRB Setup List E-UTRAN 89

9.3.3.4 DRB Failed List E-UTRAN 89

9.3.3.5 PDU Session Resource Setup List 89

9.3.3.6 PDU Session Resource Failed List 90

9.3.3.7 DRB To Setup Modification List E-UTRAN 90

9.3.3.8 DRB To Modify List E-UTRAN 91

9.3.3.9 DRB To Remove List E-UTRAN 91

9.3.3.10 PDU Session Resource To Setup Modification List 92

9.3.3.11 PDU Session Resource To Modify List 94

9.3.3.12 PDU Session Resource To Remove List 97

9.3.3.13 DRB Setup Modification List E-UTRAN 97

9.3.3.14 DRB Failed Modification List E-UTRAN 97

9.3.3.15 DRB Modified List E-UTRAN 98

9.3.3.16 DRB Failed To Modify List E-UTRAN 98

9.3.3.17 PDU Session Resource Setup Modification List 98

9.3.3.18 PDU Session Resource Failed Modification List 99

9.3.3.19 PDU Session Resource Modified List 99

9.3.3.20 PDU Session Resource Failed To Modify List 101

9.3.3.21 DRB Required To Modify List E-UTRAN 101

9.3.3.22 DRB Required To Remove List E-UTRAN 101

9.3.3.23 PDU Session Resource Required To Modify List 101

9.3.3.24 DRB Confirm Modified List E-UTRAN 102

9.3.3.25 PDU Session Resource Confirm Modified List 102

9.4 Message and Information Element Abstract Syntax (with ASN.1) 103

9.4.1 General 103

9.4.2 Usage of private message mechanism for non-standard use 103

9.4.3 Elementary Procedure Definitions 104

9.4.4 PDU Definitions 110

9.4.5 Information Element Definitions 133

9.4.6 Common Definitions 170

9.4.7 Constant Definitions 171

9.4.8 Container Definitions 174

9.5 Message Transfer Syntax 178

9.6 Timers 178

10 Handling of unknown, unforeseen and erroneous protocol data 178

Annex A (informative): Change History 179

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the 5G radio network layer signalling protocol for the E1 interface. The E1 interface provides means for interconnecting a gNB-CU-CP and a gNB-CU-UP of a gNB within an NG-RAN, or for interconnecting a gNB-CU-CP and a gNB-CU-UP of an en-gNB within an E-UTRAN. The E1 Application Protocol (E1AP) supports the functions of E1 interface by signalling procedures defined in the present document. E1AP is developed in accordance to the general principles stated in TS 38.401 [2] and TS 38.460 [3].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.401: "NG-RAN; Architecture Description".

[3] 3GPP TS 38.460: "NG-RAN; E1 general aspects and principles".

[4] 3GPP TS 38.300: "NR; Overall description; Stage-2".

[5] 3GPP TR 25.921 (version.7.0.0): "Guidelines and principles for protocol description and error".

[6] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[7] ITU-T Recommendation X.691 (2002-07): "Information technology - ASN.1 encoding rules - Specification of Packed Encoding Rules (PER)".

[8] ITU-T Recommendation X.680 (07/2002): "Information technology – Abstract Syntax Notation One (ASN.1): Specification of basic notation".

[9] ITU-T Recommendation X.681 (07/2002): "Information technology – Abstract Syntax Notation One (ASN.1): Information object specification".

[10] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol Specificaiton”.

[11] 3GPP TS 23.401: “General Packet Radio Service (GPRS) Enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access”.

[12] 3GPP TS 23.203: “Policy and Charging Control Architecture”.

[13] 3GPP TS 33.501: “Security Architecture and Procedures for 5G System”.

[14] IETF RFC 5905: “Network Time Protocol Version 4: Protocol and Algorithms Specification”.

[15] 3GPP TS 29.281: “General Packet Radio System (GPRS) Tunnelling Protocol User Plane (GTPv1-U)”.

[16] 3GPP TS 38.414: “NG-RAN; NG Data Transport”.

[17] 3GPP TS 38.323: "NR; Packet Data Convergence Protocol (PDCP) specification".

[18] 3GPP TS 38.462: "NG-RAN; E1 Signalling Transport".

[19] 3GPP TS 37.340: "NR; Multi-connectivity; Overall description; Stage-2".

[20] 3GPP TS 23.501: "System Architecture for the 5G System".

[21] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC) protocol specification".

[22] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[23] 3GPP TS 23.003: "Numbering, addressing and identification".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

Elementary Procedure**:** E1AP consists of Elementary Procedures (EPs). An Elementary Procedure is a unit of interaction between gNB-CU-CP and gNB-CU-UP. These Elementary Procedures are defined separately and are intended to be used to build up complete sequences in a flexible manner. If the independence between some EPs is restricted, it is described under the relevant EP description. Unless otherwise stated by the restrictions, the EPs may be invoked independently of each other as standalone procedures, which can be active in parallel. The usage of several E1AP EPs together is specified in stage 2 specifications (e.g., TS 38.460 [3]).

An EP consists of an initiating message and possibly a response message. Two kinds of EPs are used:

- **Class 1:** Elementary Procedures with response (success and/or failure).

- **Class 2:** Elementary Procedures without response.

For Class 1 EPs, the types of responses can be as follows:

Successful:

- A signalling message explicitly indicates that the elementary procedure successfully completed with the receipt of the response.

Unsuccessful:

- A signalling message explicitly indicates that the EP failed.

- On time supervision expiry (i.e., absence of expected response).

Successful and Unsuccessful:

- One signalling message reports both successful and unsuccessful outcome for the different included requests. The response message used is the one defined for successful outcome.

Class 2 EPs are considered always successful.

gNB: as defined in TS 38.300 [4].

gNB-CU: as defined in TS 38.401 [2].

gNB-DU: as defined in TS 38.401 [2].

gNB-CU-CP: as defined in TS 38.401 [2].

gNB-CU-UP: as defined in TS 38.401 [2].

PDU Session Resource: as defined in TS 38.401 [2].

UE-associated signalling: When E1AP messages associated to one UE uses the UE-associated logical E1-connection for association of the message to the UE in gNB-CU-UP and gNB-CU-CP.

UE-associated logical E1-connection:The UE-associated logical E1-connection uses the identities *GNB-CU-CP UE E1AP ID* and *GNB-CU-UP UE E1AP ID* according to the definition in TS 38.401 [2]. For a received UE associated E1AP message thegNB-CU-CP identifies the associated UE based on the *GNB-CU-CP UE E1AP ID* IE and the gNB-CU-UP identifies the associated UE based on the *GNB-CU-UP UE E1AP ID* IE.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply.   
An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

5QI 5G QoS Identifier

CGI Cell Global Identifier

CN Core Network

CP Control Plane

DL Downlink

EN-DC E-UTRA-NR Dual Connectivity

EPC Evolved Packet Core

MCG Master Cell Group

NSSAI Network Slice Selection Assistance Information

RANAC RAN Area Code

SCG Secondary Cell Group

SDAP Service Data Adaptation Protocol

S-NSSAI Single Network Slice Selection Assistance Information

TNLA Transport Network Layer Association

# 4 General

## 4.1 Procedure specification principles

The principle for specifying the procedure logic is to specify the functional behaviour of the terminating node exactly and completely. Any rule that specifies the behaviour of the originating node shall be possible to be verified with information that is visible within the system.

The following specification principles have been applied for the procedure text in clause 8:

- The procedure text discriminates between:

1) Functionality which "shall" be executed.

The procedure text indicates that the receiving node "shall" perform a certain function Y under a certain condition. If the receiving node supports procedure X but cannot perform functionality Y requested in the REQUEST message of a Class 1 EP, the receiving node shall respond with the message used to report unsuccessful outcome for this procedure, containing an appropriate cause value.

2) Functionality which "shall, if supported" be executed.

The procedure text indicates that the receiving node "shall, if supported," perform a certain function Y under a certain condition. If the receiving node supports procedure X, but does not support functionality Y, the receiving node shall proceed with the execution of the EP, possibly informing the requesting node about the not supported functionality.

- Any required inclusion of an optional IE in a response message is explicitly indicated in the procedure text. If the procedure text does not explicitly indicate that an optional IE shall be included in a response message, the optional IE shall not be included. For requirements on including *Criticality Diagnostics* IE, see clause 10.

## 4.2 Forwards and backwards compatibility

The forwards and backwards compatibility of the protocol is assured by mechanism where all current and future messages, and IEs or groups of related IEs, include ID and criticality fields that are coded in a standard format that will not be changed in the future. These parts can always be decoded regardless of the standard version.

## 4.3 Specification notations

For the purposes of the present document, the following notations apply:

Procedure When referring to an elementary procedure in the specification the Procedure Name is written with the first letters in each word in upper case characters followed by the word "procedure", e.g. Handover Preparation procedure.

Message When referring to a message in the specification the MESSAGE NAME is written with all letters in upper case characters followed by the word "message", e.g. HANDOVER REQUEST message.

IE When referring to an information element (IE) in the specification the *Information Element Name* is written with the first letters in each word in upper case characters and all letters in Italic font followed by the abbreviation "IE", e.g. *E-RAB ID* IE.

Value of an IE When referring to the value of an information element (IE) in the specification the "Value" is written as it is specified in the specification enclosed by quotation marks, e.g. "Value".

# 5 E1AP services

E1AP provides the signalling service between the gNB-CU-CP and the gNB-CU-UP that is required to fulfil the E1AP functions described in clause 7. E1AP services are divided into two groups:

Non UE-associated services: They are related to the whole E1 interface instance between the gNB-CU-CP and gNB-CU-UP utilising a non UE-associated signalling connection.

UE-associated services: They are related to one UE. E1AP functions that provide these services are associated with a UE-associated signalling connection that is maintained for the UE in question.

Unless explicitly indicated in the procedure specification, at any instance in time one protocol endpoint shall have a maximum of one ongoing E1AP procedure related to a certain UE.

# 6 Services expected from signalling transport

The signalling connection shall provide in sequence delivery of E1AP messages. E1AP shall be notified if the signalling connection breaks.

# 7 Functions of E1AP

The functions of E1AP are described in TS 38.460 [3].

# 8 E1AP procedures

## 8.1 List of E1AP Elementary Procedures

In the following tables, all EPs are divided into Class 1 and Class 2 EPs (see subclause 3.1 for explanation of the different classes):

Table 1: Class 1 procedures

|  |  |  |  |
| --- | --- | --- | --- |
| **Elementary Procedure** | **Initiating Message** | **Successful Outcome** | **Unsuccessful Outcome** |
| **Response message** | **Response message** |
| Reset | RESET | RESET ACKNOWLEDGE |  |
| gNB-CU-UP E1 Setup | GNB-CU-UP E1 SETUP REQUEST | GNB-CU-UP E1 SETUP RESPONSE | GNB-CU-UP E1 SETUP FAILURE |
| gNB-CU-CP E1 Setup | GNB-CU-CP E1 SETUP REQUEST | GNB-CU-CP E1 SETUP RESPONSE | GNB-CU-CP E1 SETUP FAILURE |
| gNB-CU-UP Configuration Update | GNB-CU-UP CONFIGURATION UPDATE | GNB-CU-UP CONFIGURATION UPDATE ACKNOWLEDGE | GNB-CU-UP CONFIGURATION UPDATE FAILURE |
| gNB-CU-CP Configuration Update | GNB-CU-CP CONFIGURATION UPDATE | GNB-CU-CP CONFIGURATION UPDATE ACKNOWLEDGE | GNB-CU-CP CONFIGURATION UPDATE FAILURE |
| E1 Release | E1 RELEASE REQUEST | E1 RELEASE RESPONSE |  |
| Bearer Context Setup | BEARER CONTEXT SETUP REQUEST | BEARER CONTEXT SETUP RESPONSE | BEARER CONTEXT SETUP FAILURE |
| Bearer Context Modification (gNB-CU-CP initiated) | BEARER CONTEXT MODIFICATION REQUEST | BEARER CONTEXT MODIFICATION RESPONSE | BEARER CONTEXT MODIFICATION FAILURE |
| Bearer Context Modification Required (gNB-CU-UP initiated) | BEARER CONTEXT MODIFICATION REQUIRED | BEARER CONTEXT MODIFICATION CONFIRM |  |
| Bearer Context Release (gNB-CU-CP initiated) | BEARER CONTEXT RELEASE COMMAND | BEARER CONTEXT RELEASE COMPLETE |  |

Table 2: Class 2 procedures

|  |  |
| --- | --- |
| **Elementary Procedure** | **Message** |
| Error Indication | ERROR INDICATION |
| Bearer Context Release Request (gNB-CU-UP initiated) | BEARER CONTEXT RELEASE REQUEST |
| Bearer Context Inactivity Notification | BEARER CONTEXT INACTIVITY NOTIFICATION |
| DL Data Notification | DL DATA NOTIFICATION |
| UL Data Notification | UL DATA NOTIFICATION |
| Data Usage Report | DATA USAGE REPORT |
| gNB-CU-UP Counter Check | GNB-CU-UP COUNTER CHECK |
| gNB-CU-UP Status Indication | GNB-CU-UP STATUS INDICATION |
| MR-DC Data Usage Report | MR-DC DATA USAGE REPORT |

## 8.2 Interface Management procedures

### 8.2.1 Reset

#### 8.2.1.1 General

The purpose of the Reset procedure is to initialise or re-initialise the E1AP UE-related contexts, in the event of a failure in the gNB-CU-CP or gNB-CU-UP. This procedure does not affect the application level configuration data exchanged during, e.g., the E1 Setup procedure.

The procedure uses non-UE associated signalling.

#### 8.2.1.2 Successful Operation

##### 8.2.1.2.1 Reset Procedure Initiated from the gNB-CU-CP



Figure 8.2.1.2.1-1: Reset procedure initiated from the gNB-CU-CP. Successful operation.

In the event of a failure at the gNB-CU-CP, which has resulted in the loss of some or all transaction reference information, a RESET message shall be sent to the gNB-CU-UP.

At reception of the RESET message the gNB-CU-UP shall release all allocated resources on E1 related to the UE association(s) indicated explicitly or implicitly in the RESET message and remove the indicated bearer contexts including E1AP ID.

After the gNB-CU-UP has released all assigned E1 resources and the UE E1AP IDs for all indicated UE associations which can be used for new UE-associated logical E1-connections over the E1 interface, the gNB-CU-UP shall respond with the RESET ACKNOWLEDGE message. The gNB-CU-UP does not need to wait for the release of bearer resources to be completed before returning the RESET ACKNOWLEDGE message.

If the RESET message contains the *UE-associated logical E1-connection list* IE, then:

- The gNB-CU-UP shall use the *gNB-CU-CP UE E1AP ID* IE and/or the *gNB-CU-UP UE E1AP ID* IE to explicitly identify the UE association(s) to be reset.

- The gNB-CU-UP shall include in the RESET ACKNOWLEDGE message, for each UE association to be reset, the *UE-associated logical E1-connection Item* IE in the *UE-associated logical E1-connection list* IE. The *UE-associated logical E1-connection Item* IEs shall be in the same order as received in the RESET message and shall include also unknown UE-associated logical E1-connections. Empty *UE-associated logical E1-connection Item* IEs, received in the RESET message, may be omitted in the RESET ACKNOWLEDGE message.

- If the *gNB-CU-CP UE E1AP ID* IE is included in the *UE-associated logical E1-connection Item* IE for a UE association, the gNB-CU-UP shall include the *gNB-CU-CP UE E1AP ID* IE in the corresponding *UE-associated logical E1-connection Item* IE in the RESET ACKNOWLEDGE message.

- If the *gNB-CU-UP UE E1AP ID* IE is included in the *UE-associated logical E1-connection Item* IE for a UE association, the gNB-CU-UP shall include the *gNB-CU-UP UE E1AP ID* IE in the corresponding *UE-associated logical E1-connection Item* IE in the RESET ACKNOWLEDGE message.

**Interactions with other procedures:**

If the RESET message is received, any other ongoing procedure (except for another Reset procedure) on the same E1 interface related to a UE association, indicated explicitly or implicitly in the RESET message, shall be aborted.

##### 8.2.1.2.2 Reset Procedure Initiated from the gNB-CU-UP



Figure 8.2.1.2.2-1: Reset procedure initiated from the gNB-CU-UP. Successful operation.

In the event of a failure at the gNB-CU-UP, which has resulted in the loss of some or all transaction reference information, a RESET message shall be sent to the gNB-CU-CP.

At reception of the RESET message the gNB-CU-CP shall release all allocated resources on E1 related to the UE association(s) indicated explicitly or implicitly in the RESET message and remove the E1AP ID for the indicated UE associations.

After the gNB-CU-CP has released all assigned E1 resources and the UE E1AP IDs for all indicated UE associations which can be used for new UE-associated logical E1-connections over the E1 interface, the gNB-CU-CP shall respond with the RESET ACKNOWLEDGE message. The gNB-CU-CP does not need to wait for the release of bearer resources to be completed before returning the RESET ACKNOWLEDGE message.

If the RESET message contains the *UE-associated logical E1-connection list* IE, then:

- The gNB-CU-CP shall use the *gNB-CU-CP UE E1AP ID* IE and/or the *gNB-CU-UP UE E1AP ID* IE to explicitly identify the UE association(s) to be reset.

- The gNB-CU-CP shall in the RESET ACKNOWLEDGE message include, for each UE association to be reset, the *UE-associated logical E1-connection* Item IE in the *UE-associated logical E1-connection list* IE. The *UE-associated logical E1-connection Item* IEs shall be in the same order as received in the RESET message and shall include also unknown UE-associated logical E1-connections. Empty *UE-associated logical E1-connection Item* IEs, received in the RESET message, may be omitted in the RESET ACKNOWLEDGE message.

- If the *gNB-CU-CP UE E1AP ID* IE is included in the *UE-associated logical E1-connection Item* IE for a UE association, the gNB-CU-CP shall include the *gNB-CU-CP UE E1AP ID* IE in the corresponding *UE-associated logical E1-connection Item* IE in the RESET ACKNOWLEDGE message.

- If the *gNB-CU-UP UE E1AP ID* IE is included in a *UE-associated logical E1-connection Item* IE for a UE association, the gNB-CU-CP shall include the *gNB-CU-UP UE E1AP ID* IE in the corresponding *UE-associated logical E1-connection Item* IE in the RESET ACKNOWLEDGE message.

**Interactions with other procedures:**

If the RESET message is received, any other ongoing procedure (except for another Reset procedure) on the same E1 interface related to a UE association, indicated explicitly or implicitly in the RESET message, shall be aborted.

#### 8.2.1.3 Abnormal Conditions

Not applicable.

### 8.2.2 Error Indication

#### 8.2.2.1 General

The Error Indication procedure is initiated by a node in order to report detected errors in one incoming message, provided they cannot be reported by an appropriate failure message.

If the error situation arises due to reception of a message utilising UE associated signalling, then the Error Indication procedure uses UE associated signalling. Otherwise the procedure uses non-UE associated signalling.

#### 8.2.2.2 Successful Operation



Figure 8.2.2.2-1: Error Indication procedure, gNB-CU-CP originated. Successful operation.



Figure 8.2.2.2-2: Error Indication procedure, gNB-CU-UP originated. Successful operation.

When the conditions defined in clause 10 are fulfilled, the Error Indication procedure is initiated by an ERROR INDICATION message sent from the receiving node.

The ERROR INDICATION message shall contain at least either the *Cause* IE or the *Criticality Diagnostics* IE. In case the Error Indication procedure is triggered by utilising UE associated signalling the *gNB-CU-CP UE E1AP ID* IE and *gNB-CU-UP UE E1AP ID* IE shall be included in the ERROR INDICATION message. If one or both of the *gNB-CU-CP UE E1AP ID* IE and the *gNB-CU-UP UE E1AP ID* IE are not correct, the cause shall be set to appropriate value, e.g., "Unknown or already allocated gNB-CU-CP UE E1AP ID", "Unknown or already allocated gNB-CU-UP UE E1AP ID" or "Unknown or inconsistent pair of UE E1AP ID".

#### 8.2.2.3 Abnormal Conditions

Not applicable.

### 8.2.3 gNB-CU-UP E1 Setup

#### 8.2.3.1 General

The purpose of the gNB-CU-UP E1 Setup procedure is to exchange application level data needed for the gNB-CU-UP and the gNB-CU-CP to correctly interoperate on the E1 interface. If the gNB-CU-UP initiates the first TNL association, it shall also initiate the gNB-CU-UP E1 Setup procedure. The procedure uses non-UE associated signalling.

This procedure erases any existing application level configuration data in the two nodes and replaces it by the one received. This procedure also re-initialises the E1AP UE-related contexts (if any) and erases all related signalling connections in the two nodes like a Reset procedure would do.

#### 8.2.3.2 Successful Operation



Figure 8.2.3.2-1: gNB-CU-UP E1 Setup procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending a GNB-CU-UP E1 SETUP REQUEST message including the appropriate data to the gNB-CU-CP. The gNB-CU-CP responds with a GNB-CU-UP E1 SETUP RESPONSE message including the appropriate data.

If the GNB-CU-UP E1 SETUP REQUEST message contains the *gNB-CU-UP Name* IE the gNB-CU-CP may use this IE as a human readable name of the gNB-CU-UP.

If the *Slice Support List* IE is contained in the GNB-CU-UP E1 SETUP REQUEST message, the gNB-CU-CP shall store the corresponding information and it may take it into account for bearer context establishment.

If the *NR CGI Support List* IE is contained in the GNB-CU-UP E1 SETUP REQUEST message, the gNB-CU-CP shall store the corresponding information and it may take it into account for bearer context establishment.

If the *QoS Parameters Support List* IE is contained in the GNB-CU-UP E1 SETUP REQUEST message, the gNB-CU-CP shall store the corresponding information and it may take it into account for bearer context establishment.

The exchanged data shall be stored in respective node and used as long as there is an operational TNL association. When this procedure is finished, the E1 interface is operational and other E1 messages can be exchanged.

If the *gNB-CU-UP Capacity* IE is contained in the GNB-CU-UP E1 SETUP REQUEST message, the gNB-CU-CP shall take this IE into account.

#### 8.2.3.3 Unsuccessful Operation



Figure 8.2.3.3-1: gNB-CU-UP E1 Setup procedure: Unsuccessful Operation.

If the gNB-CU-CP cannot accept the setup, it shall respond with a GNB-CU-UP E1 SETUP FAILURE and appropriate cause value.

If the GNB-CU-UP E1 SETUP FAILURE message includes the *Time To Wait* IE, the gNB-CU-UP shall wait at least for the indicated time before reinitiating the E1 setup towards the same gNB-CU-CP.

#### 8.2.3.4 Abnormal Conditions

If the first message received for a specific TNL association is not a GNB-CU-CP E1 SETUP REQUEST, GNB-CU-UP E1 SETUP RESPONSE, or GNB-CU-UP E1 SETUP FAILURE message then this shall be treated as a logical error.

If the gNB-CU-UP does not receive either GNB-CU-UP E1 SETUP RESPONSE message or GNB-CU-UP E1 SETUP FAILURE message, the gNB-CU-UP may reinitiate the gNB-CU-UP E1 Setup procedure towards the same gNB-CU-CP, provided that the content of the new GNB-CU-UP E1 SETUP REQUEST message is identical to the content of the previously unacknowledged GNB-CU-UP E1 SETUP REQUEST message.

If the gNB-CU-UP receives a GNB-CU-CP E1 SETUP REQUEST message from the peer entity on the same E1 interface:

- In case the gNB-CU-UP answers with a GNB-CU-CP E1 SETUP RESPONSE message and receives a subsequent GNB-CU-UP E1 SETUP FAILURE message, the gNB-CU-UP shall consider the E1 interface as non operational and the procedure as unsuccessfully terminated according to sub clause 8.2.3.3.

- In case the gNB-CU-UP answers with a GNB-CU-CP E1 SETUP FAILURE message and receives a subsequent GNB-CU-UP E1 SETUP RESPONSE message, the gNB-CU-UP shall ignore the GNB-CU-UP E1 SETUP RESPONSE message and consider the E1 interface as non operational.

### 8.2.4 gNB-CU-CP E1 Setup

#### 8.2.4.1 General

The purpose of the gNB-CU-CP E1 Setup procedure is to exchange application level data needed for the gNB-CU-CP and the gNB-CU-UP to correctly interoperate on the E1 interface. If the gNB-CU-CP initiates the first TNL association, it shall also initiate the gNB-CU-CP E1 Setup procedure.The procedure uses non-UE associated signalling.

This procedure erases any existing application level configuration data in the two nodes and replaces it by the one received. This procedure also re-initialises the E1AP UE-related contexts (if any) and erases all related signalling connections in the two nodes like a Reset procedure would do.

#### 8.2.4.2 Successful Operation



Figure 8.2.4.2-1: gNB-CU-CP E1 Setup procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending a GNB-CU-CP E1 SETUP REQUEST message including the appropriate data to the gNB-CU-UP. The gNB-CU-UP responds with a GNB-CU-CP E1 SETUP RESPONSE message including the appropriate data.

If the GNB-CU-CP E1 SETUP REQUEST message contains the *gNB-CU-CP Name* IE the gNB-CU-UP may use this IE as a human readable name of the gNB-CU-CP.

The exchanged data shall be stored in respective node and used as long as there is an operational TNL association. When this procedure is finished, the E1 interface is operational and other E1 messages can be exchanged.

If the *gNB-CU-UP Capacity* IE is contained in the GNB-CU-CP E1 SETUP RESPONSE message, the gNB-CU-CP shall take this IE into account.

#### 8.2.4.3 Unsuccessful Operation



Figure 8.2.4.3-1: gNB-CU-CP E1 Setup procedure: Unsuccessful Operation.

If the gNB-CU-UP cannot accept the setup, it shall respond with a GNB-CU-CP E1 SETUP FAILURE and appropriate cause value.

If the GNB-CU-CP E1 SETUP FAILURE message includes the *Time To Wait* IE, the gNB-CU-CP shall wait at least for the indicated time before reinitiating the E1 setup towards the same gNB-CU-UP.

#### 8.2.4.4 Abnormal Conditions

If the first message received for a specific TNL association is not a GNB-CU-UP E1 SETUP REQUEST, GNB-CU-CP E1 SETUP RESPONSE, or GNB-CU-CP E1 SETUP FAILURE message then this shall be treated as a logical error.

If the gNB-CU-CP does not receive either GNB-CU-CP E1 SETUP RESPONSE message or GNB-CU-CP E1 SETUP FAILURE message, the gNB-CU-CP may reinitiate the gNB-CU-CP E1 Setup procedure towards the same gNB-CU-UP, provided that the content of the new GNB-CU-CP E1 SETUP REQUEST message is identical to the content of the previously unacknowledged GNB-CU-CP E1 SETUP REQUEST message.

If the gNB-CU-CP receives a GNB-CU-UP E1 SETUP REQUEST message from the peer entity on the same E1 interface:

- In case the gNB-CU-CP answers with a GNB-CU-UP E1 SETUP RESPONSE message and receives a subsequent GNB-CU-CP E1 SETUP FAILURE message, the gNB-CU-CP shall consider the E1 interface as non operational and the procedure as unsuccessfully terminated according to sub clause 8.2.4.3.

- In case the gNB-CU-CP answers with a GNB-CU-UP E1 SETUP FAILURE message and receives a subsequent GNB-CU-CP E1 SETUP RESPONSE message, the gNB-CU-CP shall ignore the GNB-CU-CP E1 SETUP RESPONSE message and consider the E1 interface as non operational.

### 8.2.5 gNB-CU-UP Configuration Update

#### 8.2.5.1 General

The purpose of the gNB-CU-UP Configuration Update procedure is to update application level configuration data needed for the gNB-CU-UP and the gNB-CU-CP to interoperate correctly on the E1 interface. This procedure does not affect existing UE-related contexts, if any. The procedure uses non-UE associated signalling.

#### 8.2.5.2 Successful Operation



Figure 8.2.5.2-1: gNB-CU-UP Configuration Update procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending a GNB-CU-UP CONFIGURATION UPDATE message to the gNB-CU-CP including an appropriate set of updated configuration data that it has just taken into operational use. The gNB-CU-CP responds with GNB-CU-UP CONFIGURATION UPDATE ACKNOWLEDGE message to acknowledge that it successfully updated the configuration data. If an information element is not included in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall interpret that the corresponding configuration data is not changed and shall continue to operate with the existing related configuration data.

If the *Supported PLMNs* IE is included in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall overwrite the whole list of information and store the corresponding information.

- If the *Slice Support List* IE is contained in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall store the corresponding information and replace any existing information.

- If the *NR CGI Support List* IE is contained in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall store the corresponding information and replace any existing information.

- If the *QoS Parameters Support List* IE is contained in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall store the corresponding information and replace any existing information.

The updated configuration data shall be stored in both nodes and used as long as there is an operational TNL association or until any further update is performed.

If the *gNB-CU-UP Capacity* IE is contained in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall take this IE into account.

If the *gNB-CU-UP ID* IE is included in the GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall associate the TNLA to the E1 interface instance using the gNB-CU-UP ID.

If the GNB-CU-UP CONFIGURATION UPDATE message includes *gNB-CU-UP TNLA To Remove List* IE, and the *Endpoint IP address* IE and the *Port Number* IE for both TNL endpoints of the TNL association(s) are included in the *gNB-CU-UP TNLA To Remove List* IE, the gNB-CU-CP shall, if supported, consider that the TNL association(s) indicated by both received TNL endpoints will be removed by the gNB-CU-UP. If the *Endpoint IP address* IE, or the *Endpoint IP address* IE and the *Port Number* IE for one or both of the TNL endpoints is included in the *gNB-CU-UP TNLA To Remove List* IE in GNB-CU-UP CONFIGURATION UPDATE message, the gNB-CU-CP shall, if supported, consider that the TNL association(s) indicated by the received endpoint IP address(es) will be removed by the gNB-CU-UP.

#### 8.2.5.3 Unsuccessful Operation



Figure 8.2.5.3-1: gNB-CU-UP Configuration Update procedure: Unsuccessful Operation.

If the gNB-CU-CP cannot accept the update, it shall respond with a GNB-CU-UP CONFIGURATION UPDATE FAILURE message and appropriate cause value.

If the GNB-CU-UP CONFIGURATION UPDATE FAILURE message includes the *Time To Wait* IE, the gNB-CU-CP shall wait at least for the indicated time before reinitiating the GNB-CU-UP CONFIGURATION UPDATE message towards the same gNB-CU-CP.

#### 8.2.5.4 Abnormal Conditions

Not applicable.

### 8.2.6 gNB-CU-CP Configuration Update

#### 8.2.6.1 General

The purpose of the gNB-CU-CP Configuration Update procedure is to update application level configuration data needed for the gNB-CU-CP and the gNB-CU-UP to interoperate correctly on the E1 interface. This procedure does not affect existing UE-related contexts, if any. The procedure uses non-UE associated signalling.

#### 8.2.6.2 Successful Operation



Figure 8.2.6.2-1: gNB-CU-CP Configuration Update procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending a GNB-CU-CP CONFIGURATION UPDATE message to the gNB-CU-UP including an appropriate set of updated configuration data that it has just taken into operational use. The gNB-CU-UP responds with GNB-CU-CP CONFIGURATION UPDATE ACKNOWLEDGE message to acknowledge that it successfully updated the configuration data. If an information element is not included in the GNB-CU-CP CONFIGURATION UPDATE message, the gNB-CU-UP shall interpret that the corresponding configuration data is not changed and shall continue to operate with the existing related configuration data.

The updated configuration data shall be stored in both nodes and used as long as there is an operational TNL association or until any further update is performed.

If the *gNB-CU-CP TNLA To Add List* IE is contained in the gNB-CU-CP CONFIGURATION UPDATE message, the gNB-CU-UP shall, if supported, use it to establish the TNL association(s) with the gNB-CU-CP. The gNB-CU-UP shall report to the gNB-CU-CP, in the gNB-CU-CP CONFIGURATION UPDATE ACKNOWLEDGE message, the successful establishment of the TNL association(s) with the gNB-CU-CP as follows:

- A list of TNL address(es) with which the gNB-CU-UP successfully established the TNL association shall be included in the *gNB-CU-CP TNLA Setup List* IE;

- A list of TNL address(es) with which the gNB-CU-UP failed to establish the TNL association shall be included in the *gNB-CU-CP TNLA Failed To Setup List* IE.

If the GNB-CU-CP CONFIGURATION UPDATE message includes *gNB-CU-CP TNLA To Remove List* IE, and the *Endpoint IP address* IE and the *Port Number* IE for both TNL endpoints of the TNL association(s) are included in the *gNB-CU-CP TNLA To Remove List* IE, the gNB-CU-UP shall, if supported, initiate removal of the TNL association(s) indicated by both received TNL endpoints towards the gNB-CU-CP. If the *Endpoint IP address* IE, or the *Endpoint IP address* IE and the *Port Number* IE for one or both of the TNL endpoints is included in the *gNB-CU-CP TNLA To Remove List* IE, the gNB-CU-UP shall, if supported, initiate removal of the TNL association(s) indicated by the received endpoint IP address(es).

If the *gNB-CU-CP TNLA To Update List* IE is contained in the gNB-CU-CP CONFIGURATION UPDATE message the gNB-CU-UP shall, if supported, overwrite the previously stored information for the related TNL association.

If the *TNLA* *Usage* IE is included in the *gNB-CU-CP TNLA To Add List* IE or the *gNB-CU-CP TNLA To Update List* IE in the gNB-CU-CP CONFIGURATION UPDATE message, the gNB-CU-UP shall, if supported, use it as described in TS 38.462 [18].

#### 8.2.6.3 Unsuccessful Operation



Figure 8.2.6.3-1: gNB-CU-CP Configuration Update procedure: Unsuccessful Operation.

If the gNB-CU-UP cannot accept the update, it shall respond with a GNB-CU-CP CONFIGURATION UPDATE FAILURE message and appropriate cause value.

If the GNB-CU-CP CONFIGURATION UPDATE FAILURE message includes the *Time To Wait* IE, the gNB-CU-CP shall wait at least for the indicated time before reinitiating the GNB-CU-CP CONFIGURATION UPDATE message towards the same gNB-CU-UP.

#### 8.2.6.4 Abnormal Conditions

Not applicable.

### 8.2.7 E1 Release

#### 8.2.7.1 General

The purpose of the E1 Release procedure is to release all existing signalling connections and related application level data. This procedure does not affect existing UE-related contexts, if any. The procedure uses non-UE associated signalling.

#### 8.2.7.2 Successful Operation

##### 8.2.7.2.1 E1 Release Procedure Initiated from the gNB-CU-CP



Figure 8.2.7.2.1-1: E1 Release procedure initiated from the gNB-CU-CP. Successful operation.

The gNB-CU-CP initiates the procedure by sending the E1 RELEASE REQUEST message to the gNB-CU-UP.

Upon reception of the E1 RELEASE REQUEST message, the gNB-CU-UP shall release any existing resources related to the E1 interface. The gNB-CU-UP shall respond with a E1 RELEASE RESPONSE message to confirm that it has initiated the release of the resources, if existing, and that the signalling connection for the E1AP application protocol is released.

##### 8.2.7.2.2 E1 Release Procedure Initiated from the gNB-CU-UP



Figure 8.2.7.2.2-1: E1 Release procedure initiated from the gNB-CU-UP. Successful operation.

The gNB-CU-UP initiates the procedure by sending the E1 RELEASE REQUEST message to the gNB-CU-CP.

Upon reception of the E1 RELEASE REQUEST message, the gNB-CU-CP shall release any existing resources related to the E1 interface. The gNB-CU-CP shall respond with a E1 RELEASE RESPONSE message to confirm that it has initiated the release of the resources, if existing, and that the signalling connection for the E1AP application protocol is released.

#### 8.2.7.3 Abnormal Conditions

Not applicable.

### 8.2.8 gNB-CU-UP Status Indication

#### 8.2.8.1 General

The purpose of the gNB-CU-UP Status Indication procedure is to inform the gNB-CU-CP that the gNB-CU-UP is overloaded so that overload reduction actions can be applied. The procedure uses non-UE associated signalling.

#### 8.2.8.2 Successful Operation



**Figure 8.3.7.2-1: DL Data Notification procedure: Successful Operation.**

The gNB-CU-UP initiates the procedure by sending the GNB-CU-UP STATUS INDICATION message to the gNB-CU-CP.

If the *gNB-CU-UP* *Overload Information* IE in the GNB-CU-UP STATUS INDICATION message indicates that the gNB-CU-UP is overloaded, the gNB-CU-CP shall apply overload reduction actions until informed, with a new GNB-CU-UP STATUS INDICATION message, that the overload situation has ceased.

The detailed overload reduction policy is up to gNB-CU-CP implementation.

#### 8.2.8.3 Abnormal Conditions

Not applicable.

## 8.3 Bearer Context Management procedures

### 8.3.1 Bearer Context Setup

#### 8.3.1.1 General

The purpose of the Bearer Context Setup procedure is to allow the gNB-CU-CP to establish a bearer context in the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.1.2 Successful Operation



Figure 8.3.1.2-1: Bearer Context Setup procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending the BEARER CONTEXT SETUP REQUEST message to the gNB-CU-UP. If the gNB-CU-UP succeeds to establish the requested resources, it replies to the gNB-CU-CP with the BEARER CONTEXT SETUP RESPONSE message.

The gNB-CU-UP shall report to the gNB-CU-CP, in the BEARER CONTEXT SETUP RESPONSE message, the result for all the requested resources in the following way:

For E-UTRAN:

- A list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- A list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

For NG-RAN:

- A list of PDU Session Resources which are successfully established shall be included in the *PDU Session Resource Setup List* IE;

- A list of PDU Session Resources which failed to be established shall be included in the *PDU Session Resource Failed List* IE;

- For each established PDU Session Resource, a list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- For each established PDU Session Resource, a list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

- For each established DRB, a list of QoS Flows which are successfully established shall be included in the *Flow Setup List* IE;

- For each established DRB, a list of QoS Flows which failed to be established shall be included in the *Flow Failed List* IE;

When the gNB-CU-UP reports the unsuccessful establishment of a PDU Session Resource, DRB or QoS Flow the cause value should be precise enough to enable the gNB-CU-CP to know the reason for the unsuccessful establishment.

If the *Existing Allocated NG DL UP Transport Layer Information* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP may re-use the indicated resources already allocated for this bearer context. If the gNB-CU-UP decides to re-use the indicated resources, it shall include the *NG DL UP Unchanged* IE in the BEARER CONTEXT SETUP RESPONSE message.

If the *PDU Session Resource DL Aggregate Maximum Bit Rate* IE is contained in the *PDU Session Resource To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall store and use the information for the down link traffic policing for the Non-GBR QoS flows for the concerned UE as specified in TS 23.501 [20].

If the *Data Forwarding Information Request* IE, *PDU Session Data Forwarding Information Request* IE or the *DRB Data Forwarding Information Request* IE are included in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall include the requested forwarding information in the *Data Forwarding Information Response* IE, *PDU Session Data Forwarding Information Response* IE or the *DRB Data Forwarding Information Response* IE in the BEARER CONTEXT SETUP RESPONSE message.

If the *DL UP Parameters* IE is contained in the *DRB To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall configure the corresponding information.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE of the BEARER CONTEXT SETUP REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "preferred", then the gNB-CU-UP should, if supported, perform user plane integrity protection or ciphering, respectively, for the concerned PDU session and shall notify whether it performed the user plane integrity protection or ciphering by including the *Integrity Protection Result* IE or *Confidentiality Protection Result* IE, respectively, in the *PDU Session Resource Setup List* IE of the BEARER CONTEXT SETUP RESPONSE message.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE of the BEARER CONTEXT SETUP REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "required", then the gNB-CU-UP shall perform user plane integrity protection or ciphering, respectively, for the concerned PDU Session. If the gNB-CU-UP cannot perform the user plane integrity protection or ciphering, it shall reject the setup of the PDU Session Resources with an appropriate cause value.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE of the BEARER CONTEXT SETUP REQUEST message:

- if the *Integrity Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane integrity protection for the concerned PDU session;

-if the *Confidentiality Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane ciphering for the concerned PDU session.

If the *UE DL Maximum Integrity Protected Data Rate* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall use this value when enforcing the maximum integrity protected data rate for the UE.

If the *Bearer Context Status Change* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall consider the UE RRC state and act as specified in TS 38.401 [2].

For each requested DRB, if the *PDCP Duplication* IE is included in the *PDCP Configuration* IE contained in the BEARER CONTEXT SETUP REQUEST message, and one cell group is included in *Cell Group Information* IE, then the gNB-CU-UP shall include two *UP Transport Layer Information* IEs in the BEARER CONTEXT SETUP RESPONSE message to support packet duplication for intra-gNB-DU CA. The first *UP Transport Layer Information* IE of the two *UP Transport Layer Information* IEs is for the primary path.

If the *PDCP SN Status Information* IE is contained within the *DRB To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall take it into account and act as specified in TS 38.401 [2].

If the *QoS Flow Mapping Indication* IE is contained in the *QoS Flows Information To Be Setup* IE within the *DRB To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP may take it into account that only the uplink or downlink QoS flow is mapped to the DRB.

For each PDU Session Resource, if the *Network Instance* IE is included in the *PDU Session Resource To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message and the *Common Network Instance* IE is not included, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

For each PDU session, if the *Common Network Instance* IE is included in the *PDU Session Resource To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

If *UE Inactivity Timer* IE or *PDU session Inactivity Timer* IE or *DRB Inactivity Timer* IE is contained in BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall take it into account when perform inactivity monitoring.

If the *DRB QoS* IE is contained within the *DRB To Setup List* IE in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall, if supported, take it into account as specified in TS 28.552 [22].

If the *gNB-DU-ID* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall store the information received.

If the *RAN UE ID* IE is contained in the BEARER CONTEXT SETUP REQUEST message, the gNB-CU-UP shall store the information received.

For each successfully established DRB, the gNB-CU-UP shall provide, in the respective *UL UP Parameters* IE of the BEARER CONTEXT SETUP RESPONSE, one UL UP Transport Layer Information Item per cell group entry contained in the respective *Cell Group Information* IE of the BEARER CONTEXT SETUP REQUEST message.

#### 8.3.1.3 Unsuccessful Operation



Figure 8.3.1.3-1: Bearer Context Setup procedure: Unsuccessful Operation.

If the gNB-CU-UP cannot establish the requested bearer context, or cannot even establish one bearer it shall consider the procedure as failed and respond with a BEARER CONTEXT SETUP FAILURE message and appropriate cause value.

#### 8.3.1.4 Abnormal Conditions

If the gNB-CU-UP receives a BEARER CONTEXT SETUP REQUEST message containing a *E-UTRAN QoS* IE in the *DRB To Setup List* IE for a GBR QoS DRB but where the *GBR QoS Information* IE is not present, the gNB-CU-UP shall report the establishment of the corresponding DRB as failed in the *DRB Failed List* IE of the BEARER CONTEXT SETUP RESPONSE message with an appropriate cause value.

If the gNB-CU-UP receives a BEARER CONTEXT SETUP REQUEST message containing a *QoS Flow Level QoS Parameters* IE in the *PDU Session Resource To Setup List* IE for a GBR QoS Flow but where the *GBR QoS Flow Information* IE is not present, the gNB-CU-UP shall report the establishment of the corresponding QoS Flow as failed in the corresponding *Flow Failed List* IE of the BEARER CONTEXT SETUP RESPONSE message with an appropriate cause value.

### 8.3.2 Bearer Context Modification (gNB-CU-CP initiated)

#### 8.3.2.1 General

The purpose of the Bearer Context Modification procedure is to allow the gNB-CU-CP to modify a bearer context in the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.2.2 Successful Operation



Figure 8.3.2.2-1: Bearer Context Modification procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending the BEARER CONTEXT MODIFICATION REQUEST message to the gNB-CU-UP. If the gNB-CU-UP succeeds to modify the bearer context, it replies to the gNB-CU-CP with the BEARER CONTEXT MODIFICATION RESPONSE message.

The gNB-CU-UP shall report to the gNB-CU-CP, in the BEARER CONTEXT MODIFICATION RESPONSE message, the result for all the requested resources in the following way:

For E-UTRAN:

- A list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- A list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

- A list of DRBs which are successfully modified shall be included in the *DRB Modified List* IE;

- A list of DRBs which failed to be modified shall be included in the *DRB Failed To Modify List* IE;

For NG-RAN:

- A list of PDU Session Resources which are successfully established shall be included in the *PDU Session Resource Setup List* IE;

- A list of PDU Session Resources which failed to be established shall be included in the *PDU Session Resource Failed List* IE;

- A list of PDU Session Resources which are successfully modified shall be included in the *PDU Session Resource Modified List* IE;

- A list of PDU Session Resources which failed to be modified shall be included in the *PDU Session Resource Failed To Modify List* IE;

- For each successfully established or modified PDU Session Resource, a list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- For each successfully established or modified PDU Session Resource, a list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

- For each successfully modified PDU Session Resource, a list of DRBs which are successfully modified shall be included in the *DRB Modified List* IE;

- For each successfully modified PDU Session Resource, a list of DRBs which failed to be modified shall be included in the *DRB Failed To Modify List* IE;

- For each successfully established or modified DRB, a list of QoS Flows which are successfully established shall be included in the *Flow Setup List* IE;

- For each successfully established or modified DRB, a list of QoS Flows which failed to be established shall be included in the *Flow Failed List* IE;

When the gNB-CU-UP reports the unsuccessful establishment of a PDU Session Resource, DRB or QoS Flow the cause value should be precise enough to enable the gNB-CU-CP to know the reason for the unsuccessful establishment.

If the *Security Information* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *UE DL Aggregate Maximum Bit Rate* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *UE DL Maximum Integrity Protected Data Rate* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Bearer Context Status Change* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall consider the UE RRC state and act as specified in TS 38.401 [2].

If the *Data Forwarding Information Request* IE, *PDU Session Data Forwarding Information Request* IE or the *DRB Data Forwarding Information Request* IE are included in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall include the requested forwarding information in the *Data Forwarding Information Response* IE, *PDU Session Data Forwarding Information Response* IE or the *DRB Data Forwarding Information Response* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *PDU Session Data Forwarding Information* IE is included in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, consider that data forwarding is applicable for the indicated QoS flows for the concerned PDU session.

If the *PDCP Configuration* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information, except for the *PDCP SN UL Size* IE, the *PDCP SN DL Size* IE and the *RLC mode* IE which shall be ignored.

If the *E-UTRAN QoS* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *PDCP SN Status Request* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall include the *UL COUNT Value* IE and the *DL COUNT Value* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *PDCP SN Status Information* IE is contained in the *DRB To Setup List* IE or the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall take it into account and act as specified in TS 38.401 [2].

If the *DL UP Parameters* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Cell Group To Add* IE or the *Cell Group To Modify* IE or the *Cell Group To Remove* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall add or modify or remove the corresponding cell group.

If the *PDU Session Resource DL Aggregate Maximum Bit Rate* IE is contained in the *PDU Session Resource To Setup List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall replace the information in the UE context and use it when enforcing downlink traffic policing for the non GBR QoS flows for the concerned UE, as specified in TS 23.501 [20].

If the *PDU Session Resource DL Aggregate Maximum Bit Rate* IE is contained in the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *SDAP Configuration* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Flow Mapping Information* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

For each requested DRB, if the *PDCP Duplication* IE is included in the *PDCP Configuration* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, and one cell group is included in *Cell Group Information* IE, then the gNB-CU-CP shall include two *UP Transport Layer Information* IEs in the BEARER CONTEXT MODIFICATION REQUEST message, and the gNB-CU-UP shall also include two *UP Transport Layer Information* IEs in the BEARER CONTEXT MODIFICATION RESPONSE message to support packet duplication for intra-gNB-DU CA. The first *UP Transport Layer Information* IE of the two *UP Transport Layer Information* IEs is for the primary path.

For a certain DRB which was allocated with two GTP-U tunnels, if such DRB is modified and given one GTP-U tunnel via the Bearer Context Modification (gNB-CU-CP initiated) procedure, i.e. only one UP Transport Layer Information per Cell Group ID is present in *DL UP Parameters* IE for the concerned DRB, then the gNB-CU-UP shall consider that PDCP duplication is deconfigured for this DRB. If such Bearer Context Modification (gNB-CU-CP initiated) procedure occurs, the *Duplication Activation* IE shall not be included for the concerned DRB.

If the *New UL TNL Information Required* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall include the new UP Transport Layer Information in the BEARER CONTEXT MODIFICATION RESPONSE message.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "preferred", then the gNB-CU-UP should, if supported, perform user plane integrity protection or ciphering, respectively, for the concerned PDU session and shall notify whether it performed the user plane integrity protection or ciphering by including the *Integrity Protection Result* IE or *Confidentiality Protection Result* IE, respectively, in the *PDU Session Resource Setup List* IE or the *PDU Session Resource Modified List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "required", then the gNB-CU-UP shall perform user plane integrity protection or ciphering, respectively, for the concerned PDU Session. If the gNB-CU-UP cannot perform the user plane integrity protection or ciphering, it shall reject the setup of the PDU Session Resources with an appropriate cause value.

For each PDU session for which the Security Indication IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message:

- if the *Integrity Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane integrity protection for the concerned PDU session;

-if the *Confidentiality Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane ciphering for the concerned PDU session.

For each PDU Session Resource, if the *Network Instance* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message and the *Common Network Instance* IE is not included, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

For each PDU session, if the *Common Network Instance* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

If the *QoS Flow Mapping Indication* IE is contained in the *QoS Flow QoS Parameters List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, replace any previously received value and take it into account that only the uplink or downlink QoS flow is mapped to the DRB.

If the *Data Discard Required* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message and the value is set to “Required”, the gNB-CU-UP shall consider that a RAN Paging Failure occurred for that UE. The gNB-CU-UP shall discard the user plane data for that UE and consider that the bearer context is still suspended.

If *UE Inactivity Timer* IE or *PDU session Inactivity Timer* IE or *DRB Inactivity Timer* IE is contained in BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall take it into account when perform inactivity monitoring.

If the *S-NSSAI* IE is contained in the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store the corresponding information and replace any existing information.

If the *DRB QoS* IE is contained within the *DRB To Setup List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, take it into account for each DRB, as specified in TS 28.552 [22].

If the *DRB QoS* IE is contained within the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, replace any previously received value and take it into account for each DRB, as specifed in TS 28.552 [22].

If the *gNB-DU-ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the *RAN UE ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message including *Activity Notification Level* IE and its value does not match the current bearer context, the gNB-CU-UP shall ignore the *Activity Notification Level* IE and also the requested modification of inactivity timer.

For each successfully established DRB, the gNB-CU-UP shall provide, in the respective *UL UP Parameters* IE of the BEARER CONTEXT MODIFICATION RESPONSE, one UL UP Transport Layer Information Item per cell group entry contained in the respective *Cell Group Information* IE of the BEARER CONTEXT MODIFICATION REQUEST message.

If the *Old QoS Flow List - UL End Marker expected* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message for a DRB to be modified, the gNB-CU-UP shall consider that the source NG-RAN node has initiated QoS flow re-mapping and has not yet received SDAP end markers, as described in TS 38.300 [8]. The gNB-CU-UP shall consider that the *Old QoS Flow List - UL End Marker expected* IE only contains UL QoS flow information for QoS flows for which no SDAP end marker has been yet received on the source side.

**Interaction with the Bearer Context Modification (gNB-CU-CP initiated)**

If the BEARER CONTEXT MODIFICATION REQUEST message includes for a DRB in the *DRB To Modify List* IE the *PDCP SN Status Request IE* set to “requested” and if the gNB-CU-UP has not yet received a SDAP end marker packet for a QoS flow which has been previously re-configured to another DRB by means of a gNB-CU-CP initiated Bearer Context Modification procedure, the gNB-CU-UP shall includes the QoS Flow Identifier of that QoS flow in the *Old QoS Flow List - UL End Marker expected* IE in the *PDU Session Resource Modified List* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

#### 8.3.2.3 Unsuccessful Operation



Figure 8.3.2.3-1: Bearer Context Modification procedure: Unsuccessful Operation.

If the gNB-CU-UP cannot successfully perform any of the requested bearer context modifications, it shall respond with a BEARER CONTEXT MODIFICATION FAILURE message and appropriate cause value.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing the *Security Indication Modify* IE in the *PDU Session Resource To Modify List* IE for a PDU session that may result in the change of security status that has been applied but the DRBs that have been established for that PDU session are not requested to be released via the *DRB To Remove List* IEs as specified in TS 38.331 [10], then the gNB-CU-UP shall respond with a BEARER CONTEXT MODIFICATION FAILURE message and appropriate cause value.

#### 8.3.2.4 Abnormal Conditions

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing a *E-UTRAN QoS* IE in the *DRB To Setup List* or the *DRB To Modify List* IE for a GBR QoS DRB but where the *GBR QoS Information* IE is not present, the gNB-CU-UP shall report the addition or the modification of the corresponding DRB as failed in the *DRB Failed List* IE or the *DRB Failed To Modify List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message with an appropriate cause value.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing a *QoS Flow Level QoS Parameters* IE in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE for a GBR QoS Flow but where the *GBR QoS Flow Information* IE is not present, the gNB-CU-UP shall report the addition or the modification of the corresponding QoS Flow as failed in the corresponding *Flow Failed List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message with an appropriate cause value.

### 8.3.3 Bearer Context Modification Required (gNB-CU-UP initiated)

#### 8.3.3.1 General

The purpose of the Bearer Context Modification Required procedure is to allow the gNB-CU-UP to modify a bearer context (e.g., due to local problems) and inform the gNB-CU-CP. The procedure uses UE-associated signalling.

#### 8.3.3.2 Successful Operation



Figure 8.3.3.2-1: Bearer Context Modification Required procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the BEARER CONTEXT MODIFICATION REQUIRED message to the gNB-CU-CP. The gNB-CU-CP replies with the BEARER CONTEXT MODIFICATION CONFIRM message.

If the *S1 DL UP Transport Layer Information* IE or the *NG DL UP Transport Layer Information* IE is contained in the BEARER CONTEXT MODIFICATION REQUIRED message, the gNB-CU-CP shall update the corresponding information.

If the *gNB-CU-UP Cell Group Related Configuration* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUIRED message, the gNB-CU-CP shall try to change the cell group related configuration accordingly. If the gNB-CU-CP is not able to update the requested cell group related configuration, it shall include the *Cell Group Information* IE with the current cell group configuration in the *DRB Modified List* IE in the BEARER CONTEXT MODIFICATION CONFIRM message.

#### 8.3.3.3 Abnormal Conditions

Not applicable.

### 8.3.4 Bearer Context Release (gNB-CU-CP initiated)

#### 8.3.4.1 General

The purpose of the Bearer Context Release procedure is to allow the gNB-CU-CP to command the release of an UE-associated logical E1 connection. The procedure uses UE-associated signalling.

#### 8.3.4.2 Successful Operation



Figure 8.3.4.2-1: Bearer Context Release procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending the BEARER CONTEXT RELEASE COMMAND message to the gNB-CU-UP. The gNB-CU-UP replies with the BEARER CONTEXT RELEASE COMPLETE message.

Upon reception of the BEARER CONTEXT RELEASE COMMAND message, the gNB-CU-UP shall release all related signalling and user data transport resources and reply with the BEARER CONTEXT RELEASE COMPLETE message.

#### 8.3.4.3 Abnormal Conditions

Not applicable.

### 8.3.5 Bearer Context Release Request (gNB-CU-UP initiated)

#### 8.3.5.1 General

The purpose of the Bearer Context Release Request procedure is to allow the gNB-CU-UP to request the gNB-CU-CP to release an UE-associated logical E1 connection. The procedure uses UE-associated signalling.

#### 8.3.5.2 Successful Operation



Figure 8.3.5.2-1: Bearer Context Release Requset procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the BEARER CONTEXT RELEASE REQUEST message to the gNB-CU-CP.

If the *DRB Status List* IE is included in the BEARER CONTEXT RELEASE REQUEST message, the gNB-CU-CP shall act as specified in TS 38.401 [2].

**Interactions with Bearer Context Release procedure:**

The Bearer Context Release (gNB-CU-CP initiated) procedure may be initiated upon reception of a BEARER CONTEXT RELEASE REQUEST message.

**Interaction with Bearer Context Modification (gNB-CU-CP initiated) procedure:**

If applicable, as specified in TS 38.401 [2], the gNB-CU-UP may receive, after having performed the Bearer Context Release Request (gNB-CU-UP initiated) procedure, the BEARER CONTEXT MODIFICATION REQUEST message including the *Data Forwarding Information Request* IE within the *DRBs To Modify List* IE.

#### 8.3.5.3 Abnormal Conditions

Not applicable.

### 8.3.6 Bearer Context Inactivity Notification

#### 8.3.6.1 General

This procedure is initiated by the gNB-CU-UP to indicate the inactivity/resumption of activity related to the UE. The procedure uses UE-associated signalling.

#### 8.3.6.2 Successful Operation



Figure 8.3.6.2-1: Bearer Context Inactivity Notification procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the BEARER CONTEXT INACTIVITY NOTIFICATION message to the gNB-CU-CP.

If the Activity Notification Level was set to “DRB” during the Bearer Context establishment, the gNB-CU-UP shall include the *DRB Activity List* IE in the BEARER CONTEXT INACTIVITY NOTIFICATION message.

If the Activity Notification Level was set to “PDU Session” during the Bearer Context establishment, the gNB-CU-UP shall include the *PDU Session Resource Activity List* IE in the BEARER CONTEXT INACTIVITY NOTIFICATION message.

If the Activity Notification Level was set to “UE” during the Bearer Context establishment, the gNB-CU-UP shall include the *UE Activity* IE in the BEARER CONTEXT INACTIVITY NOTIFICATION message.

#### 8.3.6.3 Abnormal Conditions

Not applicable.

### 8.3.7 DL Data Notification

#### 8.3.7.1 General

This procedure is initiated by the gNB-CU-UP to indicate the detection of DL data arrival for the UE. The procedure uses UE-associated signalling.

#### 8.3.7.2 Successful Operation



Figure 8.3.7.2-1: DL Data Notification procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the DL DATA NOTIFICATION message to the gNB-CU-CP.

If the *PPI* IE is included in the DL DATA NOTIFICATION message, the gNB-CU-CP shall use it for paging policy differentiation.

#### 8.3.7.3 Abnormal Conditions

Not applicable.

### 8.3.8 Data Usage Report

#### 8.3.8.1 General

This procedure is initiated by the gNB-CU-UP to report data volume served at the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.8.2 Successful Operation



Figure 8.3.8.2-1: Data Usage Report procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the DATA USAGE REPORT message to the gNB-CU-CP.

#### 8.3.8.3 Abnormal Conditions

Not applicable.

### 8.3.9 gNB-CU-UP Counter Check

#### 8.3.9.1 General

This procedure is initiated by the gNB-CU-UP to request the gNB-CU-CP to execute a counter check procedure to verify the value of the PDCP COUNTs associated with DRBs established in the gNB-CU-UP.

The procedure uses UE-associated signalling.

#### 8.3.9.2 Successful Operation



Figure 8.3.9.2-1: gNB-CU-UP Counter Check procedure, successful operation.

The gNB-CU-UP initiates the procedure by sending the gNB-CU-UP COUNTER CHECK REQUEST message to the gNB-CU-CP.

Upon reception of the gNB-CU-UP COUNTER CHECK REQUEST message, the gNB-CU-CP may perform the RRC counter check procedure as defined in TS 33.501 [13].

#### 8.3.9.3 Unsuccessful Operation

Not applicable.

#### 8.3.9.4 Abnormal Conditions

Not applicable.

### 8.3.10 UL Data Notification

#### 8.3.10.1 General

This procedure is initiated by the gNB-CU-UP to notify the gNB-CU-CP that an UL packet including a QFI value in the SDAP header not configured by the *Flow Mapping Information* IE is received for the first time at the default DRB. The procedure uses UE-associated signalling.

#### 8.3.10.2 Successful Operation



Figure 8.3.10.2-1: UL Data Notification procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the UL DATA NOTIFICATION message to the gNB-CU-CP.

#### 8.3.10.3 Abnormal Conditions

Not applicable.

### 8.3.11 MR-DC Data Usage Report

#### 8.3.11.1 General

This procedure is initiated by the gNB-CU-UP to report data volume served at the gNB-CU-UP, where the UE is connected to the 5GC. The procedure uses UE-associated signalling.

#### 8.3.11.2 Successful Operation



Figure 8.3.11.2-1: MR-DC Data Usage Report procedure: Successful Operation.

The gNB-CU-UP initiates the procedure by sending the MR-DC DATA USAGE REPORT message to the gNB-CU-CP.

#### 8.3.11.3 Abnormal Conditions

Not applicable.

# 9 Elements for E1AP communication

## 9.1 General

Subclauses 9.2 and 9.3 present the E1AP message and IE definitions in tabular format. The corresponding ASN.1 definition is presented in subclause 9.4. In case there is contradiction between the tabular format and the ASN.1 definition, the ASN.1 shall take precedence, except for the definition of conditions for the presence of conditional IEs, where the tabular format shall take precedence.

The messages have been defined in accordance to the guidelines specified in TR 25.921 [5].

When specifying IEs which are to be represented by bitstrings, if not otherwise specifically stated in the semantics description of the concerned IE or elsewhere, the following principle applies with regards to the ordering of bits:

- The first bit (leftmost bit) contains the most significant bit (MSB);

- The last bit (rightmost bit) contains the least significant bit (LSB);

- When importing bitstrings from other specifications, the first bit of the bitstring contains the first bit of the concerned information;

The following attributes are used for the tabular description of the messages and information elements: Presence, Range Criticality and Assigned Criticality. Their definition and use can be found in TS 38.413 [6].

## 9.2 Message Functional Definition and Content

### 9.2.1 Interface Management messages

#### 9.2.1.1 RESET

This message is sent by both the gNB-CU-CP and the gNB-CU-UP and is used to request that the E1 interface, or parts of the E1 interface, to be reset.

Direction: gNB-CU-CP → gNB-CU-UP and gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| CHOICE *Reset Type* | M |  |  |  | YES | reject |
| >*E1 interface* |  |  |  |  |  |  |
| >>Reset All | M |  | ENUMERATED (Reset all,…) |  | - |  |
| >*Part of E1 interface* |  |  |  |  |  |  |
| **>>UE-associated logical E1-connection list** |  | *1* |  |  | - |  |
| **>>>UE-associated logical E1-connection Item** |  | *1 .. <maxnoofIndividualE1ConnectionsToReset>* |  |  | EACH | reject |
| >>>>gNB-CU-CP UE E1AP ID | O |  | 9.3.1.4 |  | - |  |
| >>>>gNB-CU-UP UE E1AP ID | O |  | 9.3.1.5 |  | - |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofIndividualE1ConnectionsToReset | Maximum no. of UE-associated logical E1-connections allowed to reset in one message. Value is 65536. |

#### 9.2.1.2 RESET ACKNOWLEDGE

This message is sent by both the gNB-CU-CP and the gNB-CU-UP as a response to a RESET message.

Direction: gNB-CU-UP → gNB-CU-CP and gNB-CU-CP → gNB-CU-UP.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| **UE-associated logical E1-connection list** |  | *0..1* |  |  | YES | ignore |
| **>UE-associated logical E1-connection Item** |  | *1 .. <maxnoofIndividualE1ConnectionsToReset>* |  |  | EACH | ignore |
| >>gNB-CU-CP UE E1AP ID | O |  | 9.3.1.4 |  | - |  |
| >>gNB-CU-UP UE E1AP ID | O |  | 9.3.1.5 |  | - |  |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofIndividualE1ConnectionsToReset | Maximum no. of UE-associated logical E1-connections allowed to reset in one message. Value is 65536. |

#### 9.2.1.3 ERROR INDICATION

This message is sent by both the gNB-CU-CP and the gNB-CU-UP and is used to indicate that some error has been detected in the node.

Direction: gNB-CU-CP → gNB-CU-UP and gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | ignore |
| Transaction ID | M |  | 9.3.1.53 | This IE is ignored if received in UE associated signalling message. | YES | reject |
| gNB-CU-CP UE E1AP ID | O |  | 9.3.1.4 |  | YES | ignore |
| gNB-CU-UP UE E1AP ID | O |  | 9.3.1.5 |  | YES | ignore |
| Cause | O |  | 9.3.1.2 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.4 GNB-CU-UP E1 SETUP REQUEST

This message is sent by the gNB-CU-UP to transfer information for a TNL association.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-UP ID | M |  | 9.3.1.15 |  | YES | reject |
| gNB-CU-UP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-UP. | YES | ignore |
| CN Support | M |  | ENUMERATED (EPC. 5GC, both, …) |  | YES | reject |
| **Supported PLMNs** |  | *1..<maxnoofSPLMNs>* |  | Supported PLMNs | YES | reject |
| >PLMN Identity | M |  | 9.3.1.7 |  | - | - |
| >Slice Support List | O |  | 9.3.1.8 | Supported S-NSSAIs per PLMN. | - | - |
| >NR CGI Support List | O |  | 9.3.1.36 | Supported cells. | - | - |
| >QoS Parameters Support List | O |  | 9.3.1.37 | Supported QoS parameters per PLMN. | - | - |
| gNB-CU-UP Capacity | O |  | 9.3.1.56 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofSPLMNs | Maximum no. of Supported PLMN Ids. Value is 12. |

#### 9.2.1.5 GNB-CU-UP E1 SETUP RESPONSE

This message is sent by the gNB-CU-CP to transfer information for a TNL association.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-CP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-CP. | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.6 GNB-CU-UP E1 SETUP FAILURE

This message is sent by the gNB-CU-CP to indicate E1 Setup failure.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Time To wait | O |  | 9.3.1.6 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.7 GNB-CU-CP E1 SETUP REQUEST

This message is sent by the gNB-CU-CP to transfer information for a TNL association.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-CP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-CP. | YES | ignore |

#### 9.2.1.8 GNB-CU-CP E1 SETUP RESPONSE

This message is sent by the gNB-CU-UP to transfer information for a TNL association.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-UP ID | M |  | 9.3.1.15 |  | YES | reject |
| gNB-CU-UP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-UP. | YES | ignore |
| CN Support | M |  | ENUMERATED (EPC. 5GC, both, …) |  | YES | reject |
| **Supported PLMNs** |  | *1..<maxnoofSPLMNs>* |  | Supported PLMNs | YES | reject |
| >PLMN Identity | M |  | 9.3.1.7 |  | - | - |
| >Slice Support List | O |  | 9.3.1.8 | Supported S-NSSAIs per PLMN. | - | - |
| >NR CGI Support List | O |  | 9.3.1.36 | Supported cells. | - | - |
| >QoS Parameters Support List | O |  | 9.3.1.37 | Supported QoS parameters per PLMN. | - | - |
| gNB-CU-UP Capacity | O |  | 9.3.1.56 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofSPLMNs | Maximum no. of Supported PLMN Ids. Value is 12. |

#### 9.2.1.9 GNB-CU-CP E1 SETUP FAILURE

This message is sent by the gNB-CU-UP to indicate E1 Setup failure.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Time To wait | O |  | 9.3.1.6 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.10 GNB-CU-UP CONFIGURATION UPDATE

This message is sent by the gNB-CU-UP to transfer updated information for a TNL association.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-UP ID | O |  | 9.3.1.15 |  | YES | reject |
| gNB-CU-UP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-UP. | YES | ignore |
| **Supported PLMNs** |  | *0..<maxnoofSPLMNs>* |  | Supported PLMNs | YES | reject |
| >PLMN Identity | M |  | 9.3.1.7 |  | - | - |
| >Slice Support List | O |  | 9.3.1.8 | Supported S-NSSAIs per PLMN. | - | - |
| >NR CGI Support List | O |  | 9.3.1.36 | Supported cells. | - | - |
| >QoS Parameters Support List | O |  | 9.3.1.37 | Supported QoS parameters per PLMN. | - | - |
| gNB-CU-UP Capacity | O |  | 9.3.1.56 |  | YES | ignore |
| gNB-CU-UP TNLA To Remove List |  | *0..1* |  |  | YES | reject |
| >gNB-CU-UP TNLA To Remove Item IEs |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Address | M |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-UP. | - | - |
| >>TNLA Transport Layer Address gNB-CU-CP | O |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-CP. | - | - |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofSPLMNs | Maximum no. of Supported PLMN Ids. Value is 12. |
| maxnoofTNLAssociations | Maximum numbers of TNL Associations between the gNB-CU-UP and the gNB-CU-CP. Value is 32. |

#### 9.2.1.11 GNB-CU-UP CONFIGURATION UPDATE ACKNOWLEDGE

This message is sent by a gNB-CU-CP to a gNB-CU-UP to acknowledge update of information for a TNL association.

Direction: gNB-CU-CP → gNB-CU-UP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.12 GNB-CU-UP CONFIGURATION UPDATE FAILURE

This message is sent by the gNB-CU-CP to indicate gNB-CU-UP Configuration Update failure.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Time To wait | O |  | 9.3.1.6 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.13 GNB-CU-CP CONFIGURATION UPDATE

This message is sent by the gNB-CU-CP to transfer updated information for a TNL association.

Direction: gNB-CU-CP → gNB-CU-UP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-CP Name | O |  | PrintableString(SIZE(1..150,…)) | Human readable name of the gNB-CU-CP | YES | ignore |
| **gNB-CU-CP TNLA To Add List** |  | *0..1* |  |  | YES | ignore |
| **>gNB-CU-CP TNLA To Add Item IEs** |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Information | M |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-CP. | - | - |
| >>TNLA Usage | M |  | ENUMERATED (ue, non-ue, both, …) | Indicates whether the TNLA is only used for UE-associated signalling, or non-UE-associated signalling, or both. For usage of this IE, refer to TS 38.462 [18]. | - | - |
| **gNB-CU-CP TNLA To Remove List** |  | *0..1* |  |  | YES | ignore |
| **>gNB-CU-CP TNLA To Remove Item IEs** |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Address | M |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-CP. | - | - |
| >>TNLA Transport Layer Address gNB-CU-UP | O |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-UP. | YES | reject |
| **gNB-CU-CP TNLA To Update List** |  | *0..1* |  |  | YES | ignore |
| **>gNB-CU-CP TNLA To Update Item IEs** |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Address | M |  | CP Transport Layer Address  9.3.2.2 | Transport Layer Address of the gNB-CU-CP. | - | - |
| >>TNLA Usage | O |  | ENUMERATED (ue, non-ue, both, …) | Indicates whether the TNLA is only used for UE-associated signalling, or non-UE-associated signalling, or both. For usage of this IE, refer to TS 38.462 [18]. | - | - |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofTNLAssociations | Maximum numbers of TNL Associations between the gNB-CU-CP and the gNB-CU-UP. Value is 32. |

#### 9.2.1.14 GNB-CU-CP CONFIGURATION UPDATE ACKNOWLEDGE

This message is sent by a gNB-CU-UP to a gNB-CU-CP to acknowledge update of information for a TNL association.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| **gNB-CU-CP TNLA Setup List** |  | *0..1* |  |  | YES | ignore |
| **>gNB-CU-CP TNLA Setup Item IEs** |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Address | M |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-CP | - | - |
| **gNB-CU-CP TNLA Failed to Setup List** |  | *0..1* |  |  | YES | ignore |
| **>gNB-CU-CP TNLA Failed To Setup Item IEs** |  | *1..<maxnoofTNLAssociations>* |  |  | - | - |
| >>TNLA Transport Layer Address | M |  | CP Transport Layer Information  9.3.2.2 | Transport Layer Address of the gNB-CU-CP | - | - |
| >>Cause | M |  | 9.3.1.2 |  |  |  |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofTNLAssociations | Maximum numbers of TNL Associations between the gNB-CU-CP and the gNB-CU-UP. Value is 32. |

#### 9.2.1.15 GNB-CU-CP CONFIGURATION UPDATE FAILURE

This message is sent by the gNB-CU-UP to indicate gNB-CU-CP Configuration Update failure.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Time To wait | O |  | 9.3.1.6 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.16 E1 RELEASE REQUEST

This message is sent by both the gNB-CU-CP and the gNB-CU-UP and is used to request the release of the E1 interface.

Direction: gNB-CU-CP → gNB-CU-UP and gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |

#### 9.2.1.17 E1 RELEASE RESPONSE

This message is sent by both the gNB-CU-CP and the gNB-CU-UP as a response to an E1 RELEASE REQUEST message.

Direction: gNB-CU-UP → gNB-CU-CP and gNB-CU-CP → gNB-CU-UP.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.1.18 GNB-CU-UP STATUS INDICATION

This message is sent by the gNB-CU-UP to indicate to the gNB-CU-CP its status of overload.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| Transaction ID | M |  | 9.3.1.53 |  | YES | reject |
| gNB-CU-UP Overload Information | M |  | ENUMERATED (overloaded, not-overloaded) |  | YES | reject |

### 9.2.2 Bearer Context Management messages

#### 9.2.2.1 BEARER CONTEXT SETUP REQUEST

This message is sent by the gNB-CU-CP to request the gNB-CU-UP to setup a bearer context.

Direction: gNB-CU-CP → gNB-CU-UP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| Security Information | M |  | 9.3.1.10 |  | YES | reject |
| UE DL Aggregate Maximum Bit Rate | M |  | Bit Rate 9.3.1.20 |  | YES | reject |
| UE DL Maximum Integrity Protected Data Rate | O |  | Bit Rate 9.3.1.20 | The Bit Rate is a portion of the UE’s Maximum Integrity Protected Data Rate, and is enforced by the gNB-CU-UP node. | YES | reject |
| Serving PLMN | M |  | PLMN Identity  9.3.1.7 |  | YES | ignore |
| Activity Notification Level | M |  | 9.3.1.67 |  | YES | reject |
| UE Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to UE. | - | - |
| Bearer Context Status Change | O |  | ENUMERATED (Suspend, Resume, …) | Indicates the status of the Bearer Context | YES | reject |
| CHOICE *System* | M |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB To Setup List | M |  | DRB To Setup List E-UTRAN  9.3.3.1 |  | YES | reject |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource To Setup List | M |  | 9.3.3.2 |  | YES | reject |
| RAN UE ID | O |  | OCTET STRING (SIZE(8)) |  | YES | ignore |
| gNB-DU ID | O |  | 9.3.1.65 | Included whenever it is known by the gNB-CU-CP | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.2 BEARER CONTEXT SETUP RESPONSE

This message is sent by the gNB-CU-UP to confirm the setup of the requested bearer context.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE *System* | M |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB Setup List | M |  | DRB Setup List E-UTRAN  9.3.3.3 |  | YES | reject |
| >>DRB Failed List | O |  | DRB Failed List E-UTRAN  9.3.3.4 |  | YES | reject |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource Setup List | M |  | 9.3.3.5 |  | YES | reject |
| >>PDU Session Resource Failed List | O |  | 9.3.3.6 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.3 BEARER CONTEXT SETUP FAILURE

This message is sent by the gNB-CU-UP to indicate that the setup of the bearer context was unsuccessful.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | O |  | 9.3.1.5 |  | YES | ignore |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.2.4 BEARER CONTEXT MODIFICATION REQUEST

This message is sent by the gNB-CU-CP to request the gNB-CU-UP to modify a bearer context.

Direction: gNB-CU-CP → gNB-CU-UP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Security Information | O |  | 9.3.1.10 |  | YES | reject |
| UE DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 |  | YES | reject |
| UE DL Maximum Integrity Protected Data Rate | O |  | Bit Rate 9.3.1.20 | The Bit Rate is a portion of the UE’s Maximum Integrity Protected Data Rate, and is enforced by the gNB-CU-UP node. | YES | reject |
| Bearer Context Status Change | O |  | ENUMERATED (Suspend, Resume, …) | Indicates the status of the Bearer Context | YES | reject |
| New UL TNL Information Required | O |  | ENUMERATED (required, …) | Indicates that new UL TNL information has been requested to be provided. | YES | reject |
| UE Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to UE. | - | - |
| Data Discard Required | O |  | ENUMERATED (required, …) | Indicate to discard the DL user data in case of RAN paging failure. | YES | ignore |
| CHOICE *System* | O |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB To Setup List | O |  | DRB To Setup Modification List E-UTRAN  9.3.3.7 |  | YES | reject |
| >>DRB To Modify List | O |  | DRB To Modify List E-UTRAN  9.3.3.8 |  | YES | reject |
| >>DRB To Remove List | O |  | DRB To Remove List E-UTRAN  9.3.3.9 |  | YES | reject |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource To Setup List | O |  | PDU Session Resource To Setup Modification List  9.3.3.10 |  | YES | reject |
| >>PDU Session Resource To Modify List | O |  | 9.3.3.11 |  | YES | reject |
| >>PDU Session Resource To Remove List | O |  | 9.3.3.12 |  | YES | reject |
| RAN UE ID | O |  | OCTET STRING (SIZE(8)) |  | YES | ignore |
| gNB-DU ID | O |  | 9.3.1.65 |  | YES | ignore |
| Activity Notification Level | O |  | 9.3.1.67 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.5 BEARER CONTEXT MODIFICATION RESPONSE

This message is sent by the gNB-CU-UP to confirm the modification of the requested bearer context.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE *System* | O |  |  |  | YES | ignore |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB Setup List | O |  | DRB Setup Modification List E-UTRAN  9.3.3.13 |  | YES | ignore |
| >>DRB Failed List | O |  | DRB Failed Modification List E-UTRAN  9.3.3.14 |  | YES | ignore |
| >>DRB Modified List | O |  | DRB Modified List E-UTRAN  9.3.3.15 |  | YES | ignore |
| >>DRB Failed To Modify List | O |  | DRB Failed To Modify List E-UTRAN  9.3.3.16 |  | YES | ignore |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource Setup List | O |  | PDU Session Resource Setup Modification List  9.3.3.17 |  | YES | ignore |
| >>PDU Session Resource Failed List | O |  | PDU Session Resource Failed Modification List  9.3.3.18 |  | YES | ignore |
| >>PDU Session Resource Modified List | O |  | 9.3.3.19 |  | YES | ignore |
| >>PDU Session Resource Failed To Modify List | O |  | 9.3.3.20 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.6 BEARER CONTEXT MODIFICATION FAILURE

This message is sent by the gNB-CU-UP to indicate that the modification of the bearer context was unsuccessful.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.2.7 BEARER CONTEXT MODIFICATION REQUIRED

This message is sent by the gNB-CU-UP to inform the gNB-CU-CP that a modification of a bearer context is required (e.g., due to local problems at the gNB-CU-UP).

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE *System* | M |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB To Modify List | O |  | DRB Required To Modify List E-UTRAN  9.3.3.21 |  | YES | reject |
| >>DRB To Remove List | O |  | DRB Required To Remove List  9.3.3.22 |  | YES | reject |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource To Modify List | O |  | PDU Session Resource Required To Modify List  9.3.3.23 |  | YES | reject |
| >>PDU Session Resource To Remove List | O |  | 9.3.3.12 |  | YES | reject |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.8 BEARER CONTEXT MODIFICATION CONFIRM

This message is sent by the gNB-CU-CP to confirm the modification of the requested bearer context.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE *System* | O |  |  |  | YES | ignore |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB Modified List | O |  | DRB Confirm Modified List E-UTRAN  9.3.3.24 |  | YES | ignore |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource Modified List | O |  | PDU Session Resource Confirm Modified List  9.3.3.25 |  | YES | Ignore |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.9 BEARER CONTEXT RELEASE COMMAND

This message is sent by the gNB-CU-CP to command the gNB-CU-UP to release an UE-associated logical E1 connection.

Direction: gNB-CU-CP → gNB-CU-UP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |

#### 9.2.2.10 BEARER CONTEXT RELEASE COMPLETE

This message is sent by the gNB-CU-UP to confirm the release of the UE-associated logical E1 connection.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Criticality Diagnostics | O |  | 9.3.1.3 |  | YES | ignore |

#### 9.2.2.11 BEARER CONTEXT RELEASE REQUEST

This message is sent by the gNB-CU-UP to request the release of an UE-associated logical E1 connection.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| **DRB Status List** |  | *0.. 1* |  |  | YES | ignore |
| **>DRB Status Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>PDCP DL Count | O |  | PDCP Count  9.3.1.35 | PDCP count for next DL packet to be assigned. | - | - |
| >>PDCP UL Count | O |  | PDCP Count  9.3.1.35 | PDCP count for first un-acknowledged UL packet. | - | - |
| Cause | M |  | 9.3.1.2 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.2.2.12 BEARER CONTEXT INACTIVITY NOTIFICATION

This message is sent by the gNB-CU-UP to provide information about the UE activity to the gNB-CU-CP.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE Activity Information | M |  |  |  | YES | reject |
| **>DRB Activity List** |  | *1* |  | Used if the *Activity Notification Level* IE is set as “DRB” in BEARER CONTEXT SETUP Request message | YES | reject |
| **>>DRB Activity Item** |  | *1 .. <maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>DRB Activity | M |  | ENUMERATED (Active, Not active, …) |  | - | - |
| **>PDU Session Resource Activity List** |  | *1* |  | Used if the *Activity Notification Level* IE is set as “PDU Session” in the BEARER CONTEXT SETUP Request message | YES | reject |
| **>>PDU Session Resource Activity Item** |  | *1 .. <maxnoofPDUSessionResource>* |  |  | - | - |
| >>>PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >>>PDU Session Resource Activity | M |  | ENUMERATED (Active, Not active, …) |  | - | - |
| >UE Activity | M |  | ENUMERATED (Active, Not active, …) | Used if the *Activity Notification Level* IE is set as “UE” in the BEARER CONTEXT SETUP Request message | YES | reject |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRB for a UE, the maximum value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.2.2.13 DL DATA NOTIFICATION

This message is sent by the gNB-CU-UP to provide information about the DL data detection to the gNB-CU-CP.

Direction: gNB-CU-UP → gNB-CU-CP

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Paging Priority Indicator (PPI) | O |  | 9.3.1.55 |  | YES | ignore |

#### 9.2.2.14 DATA USAGE REPORT

This message is sent by the gNB-CU-UP to report data volumes.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Data Usage Report List | M |  | 9.3.1.44 |  | YES | ignore |

#### 9.2.2.15 GNB-CU-UP COUNTER CHECK REQUEST

This message is sent by the gNB-CU-UP to request the verification of the value of the PDCP COUNTs associated with the DRBs established in the gNB-CU-UP.

Direction: gNB-CU-UP → gNB-CU-CP.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| CHOICE *System* | M |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| **>>DRBs Subject to**  **Counter Check List** |  | *1* |  |  | YES | ignore |
| **>>>DRBs Subject to Counter Check Item** |  | *1 .. <maxnoof DRBs>* |  |  | - | - |
| >>>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>>PDCP UL Count | M |  | PDCP Count 9.3.1.35 | Indicates the value of uplink COUNT associated to this DRB, as specified in TS 38.331 [8]. | - | - |
| >>>>PDCP DL Count | M |  | PDCP Count 9.3.1.35 | Indicates the value of downlink COUNT associated to this DRB, as specified in TS 38.331 [8]. | - | - |
| *>NG-RAN* |  |  |  |  |  |  |
| **>>DRBs Subject to Counter Check List** |  | *1* |  |  | YES | ignore |
| **>>>DRBs Subject to Counter Check Item** |  | *1 .. <maxnoof DRBs>* |  |  | - | - |
| >>>>PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >>>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>>PDCP UL Count | M |  | PDCP Count 9.3.1.35 | Indicates the value of uplink COUNT associated to this DRB, as specified in TS 38.331 [8]. | - | - |
| >>>>PDCP DL Count | M |  | PDCP Count 9.3.1.35 | Indicates the value of downlink COUNT associated to this DRB, as specified in TS 38.331 [8]. | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.2.2.16 UL DATA NOTIFICATION

This message is sent by the gNB-CU-UP to provide information about the UL data detection to the gNB-CU-CP.

Direction: gNB-CU-UP → gNB-CU-CP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| **PDU Session To Notify List** |  | *1* |  |  | YES | reject |
| **>PDU Session To Notify Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >>PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >>QoS Flow List | M |  | 9.3.1.12 |  | - | - |

#### 9.2.2.17 MR-DC DATA USAGE REPORT

This message is sent by the gNB-CU-UP to report data volumes when the UE is connected to the 5GC.

Direction: gNB-CU-UP → gNB-CU-CP.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| **PDU Session Resource Data Usage List** |  | *1* |  |  | YES | ignore |
| **>PDU Session Resource Data Usage Item** |  | *1 .. <maxnoof PDUsessions>* |  |  | – |  |
| >>PDU Session ID | M |  | 9.3.1.21 |  | – |  |
| >>MR-DC Usage Information | M |  | 9.3.1.63 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUsessions | Maximum no. of PDU sessions. Value is 256 |

## 9.3 Information Element Definitions

### 9.3.1Radio Network Layer Related IEs

#### 9.3.1.1 Message Type

The *Message Type* IE uniquely identifies the message being sent. It is mandatory for all messages.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **Message Type** |  |  |  |  |
| >Procedure Code | M |  | INTEGER (0..255) |  |
| >Type of Message | M |  | CHOICE (Initiating Message, Successful Outcome, Unsuccessful Outcome, …) |  |

#### 9.3.1.2 Cause

The purpose of the *Cause* IE is to indicate the reason for a particular event for the E1AP protocol.

| **IE/Group Name** | **Presence** | **Range** | **IE Type and Reference** | **Semantics Description** |
| --- | --- | --- | --- | --- |
| CHOICE *Cause Group* | M |  |  |  |
| >*Radio Network Layer* |  |  |  |  |
| >>Radio Network Layer Cause | M |  | ENUMERATED (Unspecified,  Unknown or already allocated gNB-CU-CP UE E1AP ID,  Unknown or already allocated gNB-CU-UP UE E1AP ID,  Unknown or inconsistent pair of UE E1AP ID,  Interaction with other procedure,  PDCP Count Wrap Around,  Not supported QCI value,  Not supported 5QI value,  Encryption algorithms not supported,  Integrity protection algorithms not supported,  UP integrity protection not possible,  UP confidentiality protection not possible,  Multiple PDU Session ID Instances,  Unknown PDU Session ID,  Multiple QoS Flow ID Instances,  Unknown QoS Flow ID,  Multiple DRB ID Instances,  Unknown DRB ID,  Invalid QoS combination,  Procedure cancelled,  Normal release,  No radio resources available,  Action desirable for radio reasons,  Resources not available for the slice,  PDCP configuration not supported,  …,  UE DL maximum integrity protected data rate reason,  UP integrity protection failure, Release due to Pre-Emption) |  |
| *>Transport Layer* |  |  |  |  |
| >>Transport Layer Cause | M |  | ENUMERATED (Unspecified,  Transport Resource Unavailable, …) |  |
| *>Protocol* |  |  |  |  |
| >>Protocol Cause | M |  | ENUMERATED (Transfer Syntax Error, Abstract Syntax Error (Reject), Abstract Syntax Error (Ignore and Notify), Message not Compatible with Receiver State,  Semantic Error,  Abstract Syntax Error (Falsely Constructed Message), Unspecified, …) |  |
| *>Misc* |  |  |  |  |
| >>Miscellaneous Cause | M |  | ENUMERATED (Control Processing Overload, Not enough User Plane Processing Resources, Hardware Failure, O&M Intervention, Unspecified, …) |  |

The meaning of the different cause values is described in the following table. In general, "not supported" cause values indicate that the related capability is missing. On the other hand, "not available" cause values indicate that the related capability is present, but insufficient resources were available to perform the requested action.

| **Radio Network Layer cause** | **Meaning** |
| --- | --- |
| Unspecified | Sent for radio network layer cause when none of the specified cause values applies. |
| Unknown or already allocated gNB-CU-CP UE E1AP ID | The action failed because the gNB-CU-CP UE E1AP ID is either unknown, or (for a first message received at the gNB-CU) is known and already allocated to an existing context. |
| Unknown or already allocated gNB-CU-UP UE E1AP ID | The action failed because the gNB-CU-UP UE E1AP ID is either unknown, or (for a first message received at the gNB-CU-UP) is known and already allocated to an existing context. |
| Unknown or inconsistent pair of UE E1AP ID | The action failed because both UE E1AP IDs are unknown, or are known but do not define a single UE context. |
| Interaction with other procedure | The action is due to an ongoing interaction with another procedure. |
| PDCP COUNT wrap around | PDCP COUNT approaches the maximum value. |
| Not supported QCI value | The action failed because the requested QCI is not supported. |
| Not supported 5QI value | The action failed because the requested 5QI is not supported. |
| Encryption algorithms not supported | The gNB-CU-UP is unable to support the selected encryption algorithm for the UE. |
| Integrity protection algorithms not supported | The gNB-CU-UP is unable to support the selected integrity protection algorithm for the UE. |
| UP integrity protection not possible | The PDU Session cannot be accepted according to the required user plane integrity protection policy. |
| UP confidentiality protection not possible | The PDU Session cannot be accepted according to the required user plane confidentiality protection policy |
| Multiple PDU Session ID Instances | The action failed because multiple instances of the same PDU Session had been provided. |
| Unknown PDU Session ID | The action failed because the PDU Session ID is unknown. |
| Multiple QoS Flow ID Instances | The action failed because multiple instances of the same QoS flow had been provided. |
| Unknown QoS Flow ID | The action failed because the QoS Flow ID is unknow. |
| Multiple DRB ID Instances | The action failed because multiple instances of the same DRB had been provided. |
| Unknown DRB ID | The action failed because the DRB ID is unknow. |
| Invalid QoS combination | The action was failed because of invalid QoS combination |
| Procedure cancelled | The sending node cancelled the procedure due to other urgent actions to be performed. |
| Normal release | The action is due to a normal release of the UE (e.g. because of mobility) and does not indicate an error. |
| No radio resources available | The requested node doesn’t have sufficient radio resources available. |
| Action desirable for radio reasons | The reason for requesting the action is radio related. |
| Resources not available for the slice | The requested resources are not available for the slice. |
| PDCP configuration not supported, | The gNB-CU-UP is unable to support the selected PDCP configuration for the UE. |
| UE DL maximum integrity protected data rate reason | The request is not accepted in order to comply with the maximum downlink data rate for integrity protection supported by the UE. |
| UP integrity protection failure | The gNB-CU-UP detects an integrity protection failure in the UL PDU. |
| Release due to Pre-Emption | Release is initiated due to pre-emption. |

|  |  |
| --- | --- |
| **Transport Layer cause** | **Meaning** |
| Unspecified | Sent when none of the above cause values applies but still the cause is Transport Network Layer related. |
| Transport Resource Unavailable | The required transport resources are not available. |

|  |  |
| --- | --- |
| **Protocol cause** | **Meaning** |
| Transfer Syntax Error | The received message included a transfer syntax error. |
| Abstract Syntax Error (Reject) | The received message included an abstract syntax error and the concerning criticality indicated "reject". |
| Abstract Syntax Error (Ignore And Notify) | The received message included an abstract syntax error and the concerning criticality indicated "ignore and notify". |
| Message Not Compatible With Receiver State | The received message was not compatible with the receiver state. |
| Semantic Error | The received message included a semantic error. |
| Abstract Syntax Error (Falsely Constructed Message) | The received message contained IEs or IE groups in wrong order or with too many occurrences. |
| Unspecified | Sent when none of the above cause values applies but still the cause is Protocol related. |

| **Miscellaneous cause** | **Meaning** |
| --- | --- |
| Control Processing Overload | Control processing overload. |
| Not EnoughUser Plane Processing Resources Available | No enough resources are available related to user plane processing. |
| Hardware Failure | Action related to hardware failure. |
| O&M Intervention | The action is due to O&M intervention. |
| Unspecified Failure | Sent when none of the above cause values applies and the cause is not related to any of the categories Radio Network Layer, Transport Network Layer, NAS or Protocol. |

#### 9.3.1.3 Criticality Diagnostics

The *Criticality Diagnostics* IE is sent by the gNB-CU-UP or the gNB-CU-CP when parts of a received message have not been comprehended or were missing, or if the message contained logical errors. When applicable, it contains information about which IEs were not comprehended or were missing. The conditions for inclusion of the *Transaction ID* IE are described in clause 10.

For further details on how to use the *Criticality Diagnostics* IE, (see clause 10).

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| Procedure Code | O |  | INTEGER (0..255) | Procedure Code is to be used if Criticality Diagnostics is part of Error Indication procedure, and not within the response message of the same procedure that caused the error. |
| Triggering Message | O |  | ENUMERATED(initiating message, successful outcome, unsuccessful outcome) | The Triggering Message is used only if the Criticality Diagnostics is part of Error Indication procedure. |
| Procedure Criticality | O |  | ENUMERATED(reject, ignore, notify) | This Procedure Criticality is used for reporting the Criticality of the Triggering message (Procedure). |
| Transaction ID | O |  | 9.3.1.53 |  |
| **Information Element Criticality Diagnostics** |  | *0 .. <maxnoof Errors>* |  |  |
| >IE Criticality | M |  | ENUMERATED(reject, ignore, notify) | The IE Criticality is used for reporting the criticality of the triggering IE. The value 'ignore' is not applicable. |
| >IE ID | M |  | INTEGER (0..65535) | The IE ID of the not understood or missing IE. |
| >Type of Error | M |  | ENUMERATED(not understood, missing, …) |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofErrors | Maximum no. of IE errors allowed to be reported with a single message. The value for maxnoofErrors is 256. |

#### 9.3.1.4 gNB-CU-CP UE E1AP ID

The gNB-CU-CP UE E1AP ID uniquely identifies the UE association over the E1 interface within the gNB-CU-CP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| gNB-CU-CP UE E1AP ID | M |  | INTEGER (0 .. 232 -1) |  |

#### 9.3.1.5 gNB-CU-UP UE E1AP ID

The gNB-CU-UP UE E1AP ID uniquely identifies the UE association over the E1 interface within the gNB-CU-UP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| gNB-CU-UP UE E1AP ID | M |  | INTEGER (0 .. 232 -1) |  |

#### 9.3.1.6 Time To wait

This IE defines the minimum allowed waiting times.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Time To wait | M |  | ENUMERATED(1s, 2s, 5s, 10s, 20s, 60s) |  |

#### 9.3.1.7 PLMN Identity

This information element indicates the PLMN Identity.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| PLMN Identity | M |  | OCTET STRING (3) | - digits 0 to 9, encoded 0000 to 1001,  - 1111 used as filler digit,  two digits per octet,  - bits 4 to 1 of octet n encoding digit 2n-1  - bits 8 to 5 of octet n encoding digit 2n  -The PLMN identity consists of 3 digits from MCC followed by either  -a filler digit plus 2 digits from MNC (in case of 2 digit MNC) or  -3 digits from MNC (in case of a 3 digit MNC). |

#### 9.3.1.8 Slice Support List

This IE indicates the list of supported slices.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| **Slice Support Item IEs** |  | *1..<maxnoofSliceItems>* |  |  | - | - |
| >S-NSSAI | M |  | 9.3.1.9 |  | - |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofSliceItems | Maximum no. of signalled slice support items. Value is 1024. |

#### 9.3.1.9 S-NSSAI

This IE indicates the S-NSSAI as defined in TS 23.003 [23].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| SST | M |  | OCTET STRING (SIZE(1)) |  |
| SD | O |  | OCTET STRING (SIZE(3)) |  |

#### 9.3.1.10 Security Information

This IE provides the information for configuring UP ciphering and/or integrity protection.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Security Algorithm | M |  | 9.3.1.31 |  |
| User Plane Security Keys | M |  | 9.3.1.32 |  |

#### 9.3.1.11 Cell Group Information

This IE provides information about the cell group(s) (i.e., radio leg(s)) that are part of the DRB.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **Cell Group List** |  | *1* |  |  |
| **>Cell Group Item** |  | *1..<maxnoofCellGroups>* |  |  |
| >>Cell Group ID | M |  | INTEGER  (0..3, …) | Cell group ID as defined in TS 38.331 [10] (0=MCG, 1=SCG). In this version of the specification, values “2” and “3” are not used.  For E-UTRA Cell Groups, the same encoding is used as for NR Cell Groups.  NOTE: There is no corresponding IE defined in TS 36.331 [21]. |
| >>UL Configuration | O |  | 9.3.1.33 | Indicates whether the Cell Group is used for UL traffic. |
| >>DL TX Stop | O |  | ENUMERATED (stop, resume, …) |  |
| >>RAT Type | O |  | ENUMERATED (E-UTRA, NR, …) | Indicates the RAT. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofCellGroups | Maximum no. of cell groups for a DRB. Value is 4. |

#### 9.3.1.12 QoS Flow List

This IE includes a list of QoS Flows that are identified by the QoS Flow Identifier.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **QoS Flow List** |  | *1* |  |  | - | - |
| **>QoS Flow Item** |  | *1..<maxnoofQoSflows>* |  |  | - | - |
| >>QoS Flow Identifier | M |  | 9.3.1.24 |  | - | - |
| >>QoS Flow Mapping Indication | O |  | 9.3.1.60 | Indicates that only the uplink or downlink QoS flow is mapped to the DRB | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofQoSFlows | Maximum no. of QoS flows in a PDU Session. Value is 64. |

#### 9.3.1.13 UP Parameters

This IE provides information related to a DRB configured in the gNB-CU-UP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **UP Parameters List** |  | *1* |  |  |
| **>UP Parameters Item** |  | *1..<maxnoofUPParameters>* |  |  |
| >>UP Transport Layer Information | M |  | 9.3.2.1 |  |
| >>Cell Group ID | M |  | INTEGER (0..3, …) | Cell group ID as defined in TS 38.331 [10] (0=MCG, 1=SCG). In this version of the specification, values “2” and “3” are not used. |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofUPParameters | Maximum no. of UP parameters (e.g., GTP tunnels) for a DRB. Value is 8 |

#### 9.3.1.14 NR CGI

The NR Cell Global Identifier (NR CGI) is used to globally identify a cell.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| PLMN Identity | M |  | 9.3.1.7 |  |
| NR Cell Identity | M |  | BIT STRING (36) |  |

#### 9.3.1.15 gNB-CU-UP ID

The gNB-CU-UP ID uniquely identifies the gNB-CU-UP at least within a gNB-CU-CP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| gNB-CU-UP ID | M |  | INTEGER (0 .. 236-1) |  |

#### 9.3.1.16 DRB ID

This IE uniquely identifies a DRB for a UE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| DRB ID | M |  | INTEGER (1.. 32, ...) | Corresponds to the *DRB-Identity* defined in TS 38.331 [10]. |

#### 9.3.1.17 E-UTRAN QoS

This IE defines the QoS to be applied to a DRB for EN-DC case.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| QCI | M |  | INTEGER (0..255) | QoS Class Identifier defined in TS 23.401 [11].  Logical range and coding specified in TS 23.203 [12]. | – | – |
| E-UTRAN Allocation and Retention Priority | M |  | 9.3.1.18 | E-UTRAN Allocation and Retention Priority | – | – |
| GBR QoS Information | O |  | 9.3.1.19 | This IE applies to GBR bearers only and is ignored otherwise. | – | – |

#### 9.3.1.18 E-UTRAN Allocation and Retention Priority

This IE specifies the relative importance compared to other E-RABs for allocation and retention of the E-UTRAN Radio Access Bearer.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| Priority Level | M |  | INTEGER (0..15) | **Desc.:** This IE should be understood as "priority of allocation and retention" (see TS 23.401 [11]).  **Usage:**  Value 15 means "no priority".  Values between 1 and 14 are ordered in decreasing order of priority, i.e. 1 is the highest and 14 the lowest.  Value 0 shall be treated as a logical error if received. |
| Pre-emption Capability | M |  | ENUMERATED(shall not trigger pre-emption, may trigger pre-emption) | **Desc.:** This IE indicates the pre-emption capability of the request on other E-RABs  **Usage:**  The E-RAB shall not pre-empt other E-RABs or, the E-RAB may pre-empt other E-RABs  The Pre-emption Capability indicator applies to the allocation of resources for an E-RAB and as such it provides the trigger to the pre-emption procedures/processes of the eNB. |
| Pre-emption Vulnerability | M |  | ENUMERATED(not pre-emptable, pre-emptable) | **Desc.:** This IE indicates the vulnerability of the E-RAB to pre-emption of other E-RABs.  **Usage**:  The E-RAB shall not be pre-empted by other E-RABs or the E-RAB may be pre-empted by other RABs.  Pre-emption Vulnerability indicator applies for the entire duration of the E-RAB, unless modified, and as such indicates whether the E-RAB is a target of the pre-emption procedures/processes of the eNB. |

#### 9.3.1.19 GBR QoS Information

This IE indicates the maximum and guaranteed bit rates of a GBR E-RAB for downlink and uplink.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| E-RAB Maximum Bit Rate Downlink | M |  | Bit Rate  9.3.1.20 | Maximum Bit Rate in DL (i.e. from EPC to E-UTRAN) for the bearer.  Details in TS 23.401 [11]. | – | – |
| E-RAB Maximum Bit Rate Uplink | M |  | Bit Rate  9.3.1.20 | Maximum Bit Rate in UL (i.e. from E-UTRAN to EPC) for the bearer.  Details in TS 23.401 [11]. | – | – |
| E-RAB Guaranteed Bit Rate Downlink | M |  | Bit Rate  9.3.1.20 | Guaranteed Bit Rate (provided that there is data to deliver) in DL (i.e. from EPC to E-UTRAN) for the bearer.  Details in TS 23.401 [11]. | – | – |
| E-RAB Guaranteed Bit Rate Uplink | M |  | Bit Rate  9.3.1.20 | Guaranteed Bit Rate (provided that there is data to deliver) in UL (i.e. from E-UTRAN to EPC) for the bearer.  Details in TS 23.401 [11]. | – | – |

#### 9.3.1.20 Bit Rate

This IE indicates the number of bits delivered by NG-RAN in UL or to NG-RAN in DL within a period of time, divided by the duration of the period. It is used, for example, to indicate the maximum or guaranteed bit rate for a GBR QoS flow, or an aggregated maximum bit rate.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Bit Rate | M |  | INTEGER (0.. 4,000,000,000,000,…) | The unit is: bit/s |

#### 9.3.1.21 PDU Session ID

This IE identifies a PDU Session for a UE. The definition and use of the PDU Session ID is specified in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PDU Session ID | M |  | INTEGER (0 ..255) |  |

#### 9.3.1.22 PDU Session Type

This IE indicates the PDU Session Type as specified in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PDU Session Type | M |  | ENUMERATED (IPv4, IPv6, IPv4v6, ethernet, unstructured, ...) |  |

#### 9.3.1.23 Security Indication

This IE contains the user plane integrity protection indication and confidentiality protection indication which indicates the requirements on UP integrity protection and ciphering for corresponding PDU Session Resources, respectively.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Integrity Protection Indication | M |  | ENUMERATED (required, preferred, not needed, …) | Indicates whether UP integrity protection shall apply, should apply or shall not apply for the concerned PDU Session Resource. |
| Confidentiality Protection Indication | M |  | ENUMERATED (required, preferred, not needed, …) | Indicates whether UP ciphering shall apply, should apply or shall not apply for the concerned PDU Session Resource. |
| Maximum Integrity Protected Data Rate | C-ifIntegrityProtectionrequiredorpreferred |  | 9.3.1.57 | If present, this is the value received from the CN for the overall UE capability. This IE is ignored when enforcing the maximum IP data rate. |

|  |  |
| --- | --- |
| **Condition** | **Explanation** |
| ifIntegrityProtectionrequiredorpreferred | This IE shall be present if the *Integrity Protection Indication* IE within the *Security Indication* IE is set to “required” or “preferred”. |

#### 9.3.1.24 QoS Flow Identifier

This IE identifies a QoS Flow within a PDU Session. Definition and use of the QoS Flow Identifier is specified in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| QoS Flow Identifier | M |  | INTEGER (0 ..63) |  |

#### 9.3.1.25 QoS Flow QoS Parameters List

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **QoS Flow List** |  | *1* |  |  | - | - |
| **>QoS Flow Item** |  | *1..<maxnoofflows>* |  |  | - | - |
| >>QoS Flow Identifier | M |  | 9.3.1.24 |  | - | - |
| >>QoS Flow Level QoS Parameters | M |  | 9.3.1.26 |  | - | - |
| >>QoS Flow Mapping Indication | O |  | 9.3.1.60 | Indicates that only the uplink or downlink QoS flow is mapped to the DRB | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofQoSFlows | Maximum no. of QoS flows in a PDU Session. Value is 64. |

#### 9.3.1.26 QoS Flow Level QoS Parameters

This IE defines the QoS parameters to be applied to a QoS Flow.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| CHOICE *QoS Characteristics* | M |  |  |  |
| >*Non-dynamic 5QI* |  |  |  |  |
| >>Non Dynamic 5QI Descriptor | M |  | 9.3.1.27 |  |
| >*Dynamic 5QI* |  |  |  |  |
| >>Dynamic 5QI Descriptor | M |  | 9.3.1.28 |  |
| NG-RAN Allocation and Retention Priority | M |  | 9.3.1.29 |  |
| GBR QoS Flow Information | O |  | 9.3.1.30 | This IE shall be present for GBR QoS Flows and is ignored otherwise. |
| Reflective QoS Attribute | O |  | ENUMERATED (subject to, …) | Details in TS 23.501 [20]. This IE applies to Non-GBR flows only and is ignored otherwise. |
| Additional QoS Flow Information | O |  | ENUMERATED (more likely, …) | This IE indicates that traffic for this QoS flow is likely to appear more often than traffic for other flows established for the PDU Session. |
| Paging Priority Index | O |  | INTEGER  (1.. 8, …) | This IE is not used in this version of the specification. |
| RDI | O |  | ENUMERATED (enabled, …) | Indicates whether Reflective QoS flow to DRB mapping should be applied. |

#### 9.3.1.27 Non Dynamic 5QI Descriptor

This IE indicates the QoS Characteristics for a standardized or pre-configured 5QI for downlink and uplink.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| 5QI | M |  | INTEGER (0..255, …) | This IE contains the standardized or pre-configured 5QI as specified in TS 23.501 [20]. |
| Priority Level | O |  | 9.3.1.51 | For details see TS 23.501 [20]. When included overrides standardized or pre-configured value. |
| Averaging Window | O |  | 9.3.1.49 | This IE applies to GBR QoS Flows only. For details see TS 23.501 [20]. When included overrides standardized or pre-configured value. |
| Maximum Data Burst Volume | O |  | 9.3.1.50 | For details see TS 23.501 [20]. When included overrides standardized or pre-configured value. |

#### 9.3.1.28 Dynamic 5QI Descriptor

This IE indicates the QoS Characteristics for a Non-standardised or not pre-configured 5QI for downlink and uplink.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Priority Level | M |  | 9.3.1.51 | For details see TS 23.501 [20]. |
| Packet Delay Budget | M |  | 9.3.1.47 | For details see TS 23.501 [20]. |
| Packet Error Rate | M |  | 9.3.1.48 | For details see TS 23.501 [20]. |
| 5QI | O |  | INTEGER (0..255,…) | This IE contains the dynamically assigned 5QI as specified in TS 23.501 [20]. |
| Delay Critical | C-ifGBRflow |  | ENUMERATED (delay critical, non-delay critical) | For details see TS 23.501 [20]. |
| Averaging Window | C-ifGBRflow |  | 9.3.1.49 | For details see TS 23.501 [20]. |
| Maximum Data Burst Volume | O |  | 9.3.1.50 | For details see TS 23.501 [20]. This IE shall be included if the *Delay Critical* IE is set to “delay critical” and is ignored otherwise. |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifGBRflow | This IE shall be present if the *GBR QoS Flow Information* IE is present in the *QoS Flow Level QoS Parameters* IE. |

#### 9.3.1.29 NG-RAN Allocation and Retention Priority

This IE specifies the relative importance of a QoS flow compared to other QoS flows for allocation and retention of NG-RAN resources.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| Priority Level | M |  | INTEGER (1..15) | **Desc**.: This IE defines the relative importance of a resource request (see TS 23.501 [20]).  **Usage**: Values are ordered in decreasing order of priority, i.e., with 1 as the highest priority and 15 as the lowest priority. Further usage is defined in TS 23.501 [20]. |
| Pre-emption Capability | M |  | ENUMERATED (shall not trigger pre-emption, may trigger pre-emption) | **Desc.:** This IE indicates the pre-emption capability of the request on other QoS flows.  **Usage**: The QoS flow shall not pre-empt other QoS flows or, the QoS flow may pre-empt other QoS flows.  Specified in TS 23.501 [20]  NOTE: The Pre-emption Capability indicator applies to the allocation of resources for a QoS flow and as such it provides the trigger to the pre-emption procedures/processes of the NG-RAN node. |
| Pre-emption Vulnerability | M |  | ENUMERATED (not pre-emptable, pre-emptable) | **Desc.**: This IE indicates the vulnerability of the QoS flow to pre-emption of other QoS flows.  **Usage**: The QoS flow shall not be pre-empted by other QoS flows or the QoS flow may be pre-empted by other QoS flows. Specified in TS 23.501 [20]  NOTE: The Pre-emption Vulnerability indicator applies for the entire duration of the QoS flow, unless modified and as such indicates whether the QoS flow is a target of the pre-emption procedures/processes of the NG-RAN node. |

#### 9.3.1.30 GBR QoS Flow Information

This IE indicates QoS parameters for a GBR QoS flow for downlink and uplink.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| Maximum Flow Bit Rate Downlink | M |  | Bit Rate  9.3.1.20 | Maximum Bit Rate in DL. Details in TS 23.501 [20]. |
| Maximum Flow Bit Rate Uplink | M |  | Bit Rate  9.3.1.20 | Maximum Bit Rate in UL. Details in TS 23.501 [20]. |
| Guaranteed Flow Bit Rate Downlink | M |  | Bit Rate  9.3.1.20 | Guaranteed Bit Rate (provided there is data to deliver) in DL. Details in TS 23.501 [20]. |
| Guaranteed Flow Bit Rate Uplink | M |  | Bit Rate  9.3.1.20 | Guaranteed Bit Rate (provided there is data to deliver). Details in TS 23.501 [20]. |
| Maximum Packet Loss Rate Downlink | O |  | Packet Loass Rate  9.3.1.46 | Indicates the maximum rate for lost packets that can be tolerated in the downlink direction. Details in TS 23.501 [20]. |
| Maximum Packet Loss Rate Uplink | O |  | Packet Loss Rate  9.3.1.46 | Indicates the maximum rate for lost packets that can be tolerated in the uplink direction. Details in TS 23.501 [20]. |

#### 9.3.1.31 Security Algorithm

This IE defines the type of ciphering algorithm and/or integrity protection used for the DRBs.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Ciphering Algorithm | M |  | ENUMERATED (NEA0, 128-NEA1, 128-NEA2, 128-NEA3) | As defined in TS 33.501 [13]. |
| Integrity Protection Algorithm | O |  | ENUMERATED (NIA0, 128-NIA1, 128-NIA2, 128-NIA3) | As defined in TS 33.501 [13] for NG-RAN. |

#### 9.3.1.32 User Plane Security Keys

This IE contains the ciphering and/or integrity protection keys generated by the gNB-CU-CP.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Encryption Key | M |  | OCTET STRING | As defined in TS 33.501 [13]. |
| Integrity Protection Key | O |  | OCTET STRING | As defined in TS 33.501 [13] for NG-RAN. |

#### 9.3.1.33 UL Configuration

This IE includes the UL configuration for the DRB and the corresponding Cell Groups.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| UL Configuration | M |  | ENUMERATED (no-data, shared, only, ..) | Indicates the UL configuration for a Cell Group that is part of a DRB. “no data” means that the Cell Group is not used for UL data. “shared” means that the Cell Group is used for UL data together with at least another Cell Group. “only” means that only this Cellg Group is used for UL data. |

#### 9.3.1.34 gNB-CU-UP Cell Group Related Configuration

This IE provides information related to a cell group that the gNB-CU-UP is allowed to change.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **UP Parameters List** |  | *1* |  |  | - | - |
| **>UP Parameters Item** |  | *1..<maxnoofUPParameters>* |  |  | - | - |
| >>Cell Group ID | M |  | INTEGER (0..3, …) | Cell group ID as defined in TS 38.331 [10] (0=MCG, 1=SCG). Used to identify the Cell Group to modify. In this version of the specification, values “2” and “3” are not used. | - | - |
| >>UP Transport Layer Information | M |  | 9.3.2.1 |  | - | - |
| >>UL Configuration | O |  | 9.3.1.33 | Indicates whether the Cell Group is used for UL traffic. | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofUPParameters | Maximum no. of UP parameters (e.g., GTP tunnels) for a DRB. Value is 8. |

#### 9.3.1.35 PDCP Count

This IE include the PDCP Count information.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| >PDCP SN | M |  | INTEGER (0 .. ..2PDCP\_SN\_Size-1) | The PDCP SN Size is provided in the *PDCP Configuration* IE. |
| >HFN | M |  | INTEGER (0 .. 232-PDCP\_SN\_Size-1) | The PDCP SN Size is provided in the *PDCP Configuration* IE. |

#### 9.3.1.36 NR CGI Support List

This IE indicates the list of supported NR CGIs.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **NR CGI Support Item IEs** |  | *1..<maxnoofNRCGI>* |  |  |
| >NR CGI | M |  | 9.3.1.14 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofNRCGI | Maximum no. of supported NR CGIs. Value is 512. This range may be redefined. |

#### 9.3.1.37 QoS Parameters Support List

This IE indicates the list of supported QoS parameters.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| **E-UTRAN QoS Support List** | O |  |  |  |
| **>E-UTRAN QoS Support Item** |  | *1..<maxnoofEUTRNQOSParameters>* |  |  |
| >>E-UTRAN QoS | M |  | 9.3.1.17 |  |
| **NG-RAN QoS Support List** | O |  |  |  |
| **>NG-RAN QoS Support Item** |  | *1..<maxnoofNGRANQOSParameters>* |  |  |
| >>Non Dynamic 5QI Descriptor | M |  | 9.3.1.27 |  |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofEUTRANQOSParameters | Maximum no. of supported E-UTRAN QoS parameters. Value is 256. This range may be redefined. |
| maxnoofNGRANQOSParameters | Maximum no. of supported NG-RAN QoS parameters. Value is 256. This range may be redefined. |

#### 9.3.1.38 PDCP Configuration

This IE carries the PDCP configuration.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| --- | --- | --- | --- | --- | --- | --- |
| PDCP SN UL Size | M |  | PDCP SN Size  9.3.1.61 | Indicates the PDCP SN UL size in bits. For more information see *PDCP-Config IE* in TS 38.331 [10].  Is ignored if received through *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message. | - |  |
| PDCP SN DL Size | M |  | PDCP SN Size  9.3.1.61 | Indicates the PDCP SN DL size in bits. For more information see *PDCP-Config IE* in TS 38.331 [10].  Is ignored if received through *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message. | - |  |
| RLC mode | M |  | ENUMERATED (RLC-TM, RLC-AM, RLC-UM-Bidirectional, RLC-UM-Unidirectional-UL, RLC-UM-Unidirectional-DL, …) | Indicates the RLC mode for the DRB. For more information see *PDCP-Config IE* in TS 38.331 [10].  Is ignored if received through *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message. | - |  |
| ROHC Parameters | O |  | 9.3.1.40 |  | - |  |
| T-Reordering Timer | O |  | 9.3.1.41 |  | - |  |
| Discard Timer | O |  | 9.3.1.42 |  | - |  |
| UL Data Split Threshold | O |  | 9.3.1.43 |  | - |  |
| PDCP Duplication | O |  | ENUMERATED (True, …) | Indicates whether PDCP duplication is to be configured for the DRB. | - |  |
| PDCP Re-establishment | O |  | ENUMERATED (true,…) | Indicates PDCP entity re-establishment to be triggered as defined in TS 38.323 [17] | - |  |
| PDCP Data Recovery | O |  | ENUMERATED (true,…) | Indicates PDCP data recovery to be triggered as defined in TS 38.323 [17] | - |  |
| Duplication Activation | O |  | ENUMERATED (  Active, Inactive, …) | Information on the initial state of DL PDCP duplication | - |  |
| Out Of Order Delivery | O |  | ENUMERATED (true,…) | Indicates whether or not outOfOrderDelivery specified in TS 38.323 [17] is configured. Out of order delivery is configured only when the radio bearer is established. | - |  |
| PDCP Status Report Indication | O |  | ENUMERATED (downlink, uplink, both, …) | For AM DRB, “downlink” indicates that the PDCP entity is configured to send PDCP status report(s) to the UE, and “uplink” indicates that the UE is configured to send PDCP status report(s), as specified in TS 38.323 [17]. “both” indicates that both “downlink” and “uplink” should be applied. | YES | ignore |

#### 9.3.1.39 SDAP Configuration

This IE carries the SDAP configuration.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| Default DRB | M |  | ENUMERATED (True, False, …) | Indicates whether or not this is the default DRB for the PDU Session Resource. For more information see *SDAP-Config IE* in TS 38.331 [10]. |
| SDAP Header UL | M |  | ENUMERATED (Present, Absent, …) | Indicates whether or not a SDAP header is present for UL data on this DRB. For more information see *SDAP-Config IE* in TS 38.331 [10]. |
| SDAP Header DL | M |  | ENUMERATED (Present, Absent, …) | Indicates whether or not a SDAP header is present for DL data on this DRB. For more information see *SDAP-Config IE* in TS 38.331 [10]. |

#### 9.3.1.40 ROHC Parameters

This IE carries the ROCH parameters for header compressions.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| **Choice ROHC Parameters** | M |  |  | For more information see *PDCP-Config IE* in TS 38.331 [10]. |
| >ROHC |  |  |  |  |
| >>max CID | M |  | INTEGER (0..16383) | See description of maxCID inTS 38.331 [10] |
| >>ROHC Profiles | M |  | INTEGER (0..511) | Bitmap with supported UE profiles, bit 0 (LSB 0) = profile0x0001, bit 1 = profile0x0002, bit 2 = profile0x0003, bit 3 = profile0x0004, bit 4 = profile0x0006, bit 5 = profile0x0101, bit 6 = profile0x0102, bit 7 = profile0x0103, bit 8 = profile0x0104. See description of supportedROHC-Profiles in PDCP-Parameters in TS 38.331 [10]. |
| >>Continue ROHC | O |  | ENUMERATED (true, …) | See description of drb-ContinueROHC inTS 38.331 [10] |
| >uplinkOnlyROHC |  |  |  |  |
| >>max CID | M |  | INTEGER (0..16383) | See description of maxCID inTS 38.331 [10] |
| >>ROHC Profiles | M |  | INTEGER (0..511) | Bitmap with supported UE profiles, bit 4 = profile0x0006. See description of supportedROHC-Profiles in PDCP-Parameters in TS 38.331 [10]. |
| >>Continue ROHC | O |  | ENUMERATED (true, …) | See description of drb-ContinueROHC inTS 38.331 [10] |

#### 9.3.1.41 T-Reordering Timer

This IE indicates the t-Reordering timer.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| T-Reordering Timer | M |  | ENUMERATED (0, 1, 2, 4, 5, 8, 10, 15, 20, 30, 40, 50, 60, 80, 100, 120, 140, 160, 180, 200, 220, 240, 260, 280, 300, 500, 750, 1000, 1250, 1500, 1750, 2000, 2250, 2500, 2750, 3000, …) | Indicates the t-Reordering UL timer. The values are expressed in *ms*. For more information see *PDCP-Config IE* in TS 38.331 [10]. |

#### 9.3.1.42 Discard Timer

This IE indicates PDCP discard timer.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Discard Timer |  |  | ENUMERATED (10, 20, 30, 40, 50, 60, 75, 100, 150, 200, 250, 300, 500, 750, 1500, Infinity) | Indicates the PDCP discard timer. The values are expressed in *ms*. For more information see *PDCP-Config IE* in TS 38.331 [10]. |

#### 9.3.1.43 UL Data Split Threshold

This IE indicates UL data split threshold.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| UL Data Split Threshold |  |  | ENUMERATED (0, 100, 200, 400, 800, 1600, 3200, 6400, 12800, 25600, 51200, 102400, 204800, 409600, 819200, 1228800, 1638400, 2457600, 3276800, 4096000, 4915200, 5734400, 6553600, Infinity, …) | Indicates the UL data split threshold. The values are expressed in bytes. For more information see *PDCP-Config IE* in TS 38.331 [10]. |

#### 9.3.1.44 Data Usage Report List

This IE provides information on the data usage for the UE, e.g., secondary NR RAT in EN-DC as specified in TS 37.340 [19].

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Data usage report Item |  | 1 .. <maxnoofDRBs> |  |  | - | - |
| >DRB ID | M |  | 9.3.1.16 |  | - | - |
| > RAT Type | M |  | ENUMERATED (E-UTRA, NR, …) | The value E-UTRA is not used in this version of the specification. | - | - |
| >DRB Usage Report List |  | 1 |  |  | - | - |
| >>DRB Usage Report Item |  | 1.. <maxnooftimeperiods> |  |  | - | - |
| >>>Start timestamp | M |  | OCTET STRING (SIZE(4)) | Encoded in the same format as the first four octets of the 64-bit timestamp format as defined in section 6 of IETF RFC 5905 [14]. It indicates the UTC time when the recording of the Data Volume was started. | - | - |
| >>>End timestamp | M |  | OCTET STRING (SIZE(4)) | Encoded in the same format as the first four octets of the 64-bit timestamp format as defined in section 6 of IETF RFC 5905 [14]. It indicates the UTC time when the recording of the Data Volume was ended. | - | - |
| >>>Usage count UL | M |  | INTEGER (0..264-1) | The unit is: octets. | - | - |
| >>>Usage count DL | M |  | INTEGER (0..264-1) | The unit is: octets. | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs. Value is 32. |
| maxnooftimeperiods | Maximum no. of time reporting periods. Value is 2. |

#### 9.3.1.45 Flow Failed List

This IE contains a list of QoS flows with a cause value. It is used for example to indicate failed QoS flow(s) or QoS flow(s) to be released.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **QoS Flow Item IEs** |  | *1..<maxnoofQoSFlows>* |  |  | - | - |
| >QoS Flow Identifier | M |  | 9.3.1.24 |  | - | - |
| >Cause | M |  | 9.3.1.2 |  | - | - |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofQoSFlows | Maximum no. of QoS flows in a PDU Session. Value is 64. |

#### 9.3.1.46 Packet Loss Rate

This IE indicates the Packet Loss Rate for a QoS Flow.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Packet Loss Rate | M |  | INTEGER (0..1000, …) | Ratio of lost packets per number of packets sent, expressed in tenth of percent. |

#### 9.3.1.47 Packet Delay Budget

This IE indicates the Packet Delay Budget for a QoS Flow.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Packet Delay Budget | M |  | INTEGER (0..1023, …) | Upper bound value for the delay that a packet may experience expressed in unit of 0.5ms. |

#### 9.3.1.48 Packet Error Rate

This IE indicates the Packet Error Rate for a QoS Flow.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Scalar | M |  | INTEGER (0..9, …) | The packet error rate is expressed as Scalar x 10-k where k is the Exponent. |
| Exponent | M |  | INTEGER (0..9, …) |  |

#### 9.3.1.49 Averaging Window

This IE indicates the Averaging Window for a QoS Flow.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Averaging Window | M |  | INTEGER (0..4095, …) | Unit: ms.  The default value is 2000ms. |

#### 9.3.1.50 Maximum Data Burst Volume

This IE indicates the Maximum Data Burst Volume for a QoS Flow and applies to delay critical GBR QoS flows only.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Maximum Data Burst Volume | M |  | INTEGER (0..4095, ...) | Unit: byte. |

#### 9.3.1.51 Priority Level

This IE indicates the Priority Level for a QoS Flow.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Priority Level | M |  | INTEGER (1..127, …) | Values ordered in decreasing order of priority i.e. with 1 as the highest priority and 127 as the lowest priority. |

#### 9.3.1.52 Security Result

This IE indicates whether the security policy indicated as "preferred" in the *Security Indication* IE is performed or not.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| Integrity Protection Result | M |  | ENUMERATED (performed, not performed, …) | Indicates whether UP integrity protection is performed or not for the concerned PDU Session Resource. |
| Confidentiality Protection Result | M |  | ENUMERATED (performed, not performed, …) | Indicates whether UP ciphering is performed or not for the concerned PDU Session Resource. |

#### 9.3.1.53 Transaction ID

The *Transaction ID* IE uniquely identifies a procedure among all ongoing parallel procedures of the same type initiated by the same protocol peer. Messages belonging to the same procedure shall use the same Transaction ID. The Transaction ID is determined by the initiating peer of a procedure.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Transaction ID | M |  | INTEGER (0..255, …) |  |

#### 9.3.1.54 Inactivity timer

This IE indicates the inactivity timer.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Inactivity Timer | M |  | INTEGER  (1.. 7200, …) | Indicates the inactivity timer. The values are expressed in *seconds*. |

#### 9.3.1.55 Paging Priority Indicator (PPI)

The Paging Policy Indicator is used for paging policy differentiation (see details in TS 23.501 [20]).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PPI | M |  | INTEGER  (0.. 7, …) |  |

#### 9.3.1.56 gNB-CU-UP Capacity

This IE indicates the relative processing capacity of an gNB-CU-UP with respect to other gNB-CU-UPs in order to load-balance among different gNB-CU-UPs.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| gNB-CU-UP Capacity | M |  | INTEGER(0..255) |  | - | - |

9.3.1.57 Maximum Integrity Protected Data Rate

ThisIE indicates the maximum aggregate data rate for integrity protected DRBs for a UE as defined in TS 38.300 [8].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Maximum IP rate | M |  | ENUMERATED (64kbps, max-UErate, …) | Defines the upper bound of the aggregated data rate of user plane integrity protected data. This limit applies to both UL and DL independently. |

#### 9.3.1.58 PDCP SN Status Information

This IE contains information about PDCP PDU transfer status of a DRB.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **PDCP Status Transfer UL** |  | *1* |  |  | – |  |
| >Receive Status Of PDCP SDU | O |  | BIT STRING (1.. 131072) | The first bit indicates the status of the SDU after the First Missing UL PDCP SDU.  The Nth bit indicates the status of the UL PDCP SDU in position (N + First Missing SDU Number) modulo (1 + the maximum value of the PDCP-SN).  0: PDCP SDU has not been received.  1: PDCP SDU has been received correctly. | – |  |
| >UL COUNT Value | M |  | PDCP Count  9.3.1.35 | PDCP-SN and Hyper Frame Number of the first missing UL SDU | – |  |
| **PDCP Status Transfer DL** |  | *1* |  |  | – |  |
| >DL COUNT Value | M |  | PDCP Count  9.3.1.35 | PDCP-SN and Hyper Frame Number that the target NG-RAN node (handover) or the NG-RAN node to which the DRB context is transferred (dual connectivity) should assign for the next DL SDU not having an SN yet. | – |  |

#### 9.3.1.59 QoS Flow Mapping List

This IE contains a list of DRBs containing information about the mapped QoS flows.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| **QoS Flow Mapping Item** |  | *1..<maxnoofQoSFlows>* |  |  | – |  |
| >QoS Flow Identifier | M |  | 9.3.1.24 |  | – |  |
| >QoS Flow Mapping Indication | O |  | 9.3.1.60 |  | – |  |

| Range bound | Explanation |
| --- | --- |
| maxnoofQoSFlows | Maximum no. of QoS flows allowed within one PDU Session. Value is 64. |

#### 9.3.1.60 QoS Flow Mapping Indication

This IE is used to indicate whether only the uplink or only the downlink of a QoS flow is mapped to a DRB.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| QoS Flow Mapping Indication | M |  | ENUMERATED (ul, dl, ...) | Indicates that only the uplink or downlink QoS flow is mapped to the DRB |

#### 9.3.1.61 PDCP SN Size

This IE carries the PDCP SN Size.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| PDCP SN Size | M |  | ENUMERATED (s-12, s-18, …) | Indicates the PDCP SN size in bits. For more information see *PDCP-Config IE* in TS 38.331 [10]. |

#### 9.3.1.62 Network Instance

This IE provides the network instance to be used by the NG-RAN node when selecting a particular transport network resource as described in TS 23.501 [20].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Network Instance | M |  | INTEGER (1..256, …) |  |

#### 9.3.1.63 MR-DC Usage Information

This IE provides information on the data usage for the UE connected to 5GC, e.g., secondary RAT in MR-DC as specified in TS 37.340 [19].

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Data Usage per PDU Session Report | O |  |  |  | - |  |
| >Secondary RAT Type | M |  | ENUMERATED (nR, e-UTRA…) |  |  |  |
| >PDU session Timed Report List | M |  | MR-DC Data Usage Report List  9.3.1.64 |  |  |  |
| **Data Usage per QoS Flow List** | O |  |  |  |  |  |
| **>Data Usage per QoS Flow Item** |  | *1..<maxnoofQoSFlows>* |  |  | – |  |
| >>QoS Flow Indicator | M |  | 9.3.1.24 |  | – |  |
| >>Secondary RAT Type | M |  | ENUMERATED (nR, e-UTRA…) |  | – |  |
| >>QoS Flow Timed Report List | M |  | MR-DC Data Usage Report List  9.3.1.64 |  | – |  |

| Range bound | Explanation |
| --- | --- |
| maxnoofQoSFlows | Maximum no. of QoS flows allowed within one PDU session. Value is 64. |

#### 9.3.1.64 MR-DC Data Usage Report List

This IE provides information on the data usage.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MR-DC Data Usage Report Item** |  | *1.. <maxnooftimeperiods>* |  |  |
| >Start timestamp | M |  | OCTET STRING (SIZE(4)) | UTC time encoded in the same format as the first four octets of the 64-bit timestamp format as defined in section 6 of IETF RFC 5905 [14]. It indicates the start time of the collecting period of the included *Usage Count UL* IE and *Usage Count DL* IE. |
| >End timestamp | M |  | OCTET STRING (SIZE(4)) | UTC time encoded in the same format as the first four octets of the 64-bit timestamp format as defined in section 6 of IETF RFC 5905 [14]. It indicates the end time of the collecting period of the included *Usage Count UL* IE and *Usage Count DL* IE. |
| >Usage count UL | M |  | INTEGER (0..264-1) | The unit is: octets. |
| >Usage count DL | M |  | INTEGER (0..264-1) | The unit is: octets. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnooftimeperiods | Maximum no. of time reporting periods. Value is 2. |

#### 9.3.1.65 gNB-DU ID

The gNB-DU ID uniquely identifies a gNB-DU at least within a gNB-CU.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| gNB-DU ID | M |  | INTEGER (0 .. 236-1) | The gNB-DU ID is independently configured from cell identifiers, i.e. no connection between gNB-DU ID and cell identifiers. |

#### 9.3.1.66 Common Network Instance

This IE provides the common network instance to be used by the NG-RAN node when selecting a particular transport network resource as described in TS 23.501 [9] in a format common with 5GC.

| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| --- | --- | --- | --- | --- |
| Common Network Instance | M |  | OCTET STRING |  |

#### 9.3.1.67 Activity Notification Level

This IE contains information on which level activity notification shall be performed..

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Activity Notification Level | M |  | ENUMERATED (DRB, PDU Session, UE, …) |  |

### 9.3.2 Transport Network Layer Related IEs

#### 9.3.2.1 UP Transport Layer Information

The *UP Transport Layer Information* IE identifies an transport bearer associated to a DRB. It contains a Transport Layer Address and a GTP Tunnel Endpoint Identifier. The Transport Layer Address is an IP address to be used for the user plane transport.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| CHOICE *Transport Layer Information* | M |  |  |  |
| >*GTP Tunnel* |  |  |  |  |
| >>Transport Layer Address | M |  | 9.3.2.4 |  |
| >>GTP-TEID | M |  | 9.3.2.3 |  |

#### 9.3.2.2 CP Transport Layer Information

This IE is used to provide the E1 control plane transport layer information associated with an gNB-CU-CP and gNB-CU-UP pair.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| CHOICE *CP Transport Layer Information* |  |  |  |  |  |  |
| >*Endpoint-IP-address* |  |  |  |  | - | - |
| >> Endpoint IP address | M |  | Transport Layer Address  9.3.2.4 |  | - | - |
| >Endpoint-IP-address-and-port |  |  |  |  | YES | reject |
| >>Endpoint IP address | M |  | Transport Layer Address  9.3.2.4 |  | - | - |
| >>Port Number | M |  | BIT STRING (16) |  | - | - |

#### 9.3.2.3 GTP-TEID

The *GTP-TEID* IE is the GTP Tunnel Endpoint Identifier to be used for the user plane transport.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| GTP-TEID | M |  | OCTET STRING (SIZE(4)) | For details and range, see TS 29.281 [15]. |

#### 9.3.2.4 Transport Layer Address

This *Transport Layer Address* IE is an IP address.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Transport Layer Address | M |  | BIT STRING (SIZE(1..160, …)) | The Radio Network Layer is not supposed to interpret the address information. It should pass it to the Transport Layer for interpretation.  For details, see TS 38.414 [16]. |

#### 9.3.2.5 Data Forwarding Information Request

This IE offers the possibility for the gNB-CU-CP to request data forwarding addresses to the gNB-CU-UP. It also offers the possibility for the gNB-CU-CP to provide a list of QoS flows subject to PDU Session level or DRB level data forwarding to the gNB to which DRBs or QoS flows have been offloaded.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| Data Forwarding Request | M |  | ENUMERATED (UL, DL, both, …) |  |
| QoS Flows forwarded on the forwarding tunnel(s) | O |  | QoS Flow Mapping List  9.3.1.59 | This IE contains information for which QoS flows forwarded data packets are sent on:  - either the PDU Session forwarding tunnel (UL and DL)  - or the DRB forwarding tunnel (UL and DL). |

#### 9.3.2.6 Data Forwarding Information

This IE provides the data forwarding information when performing handover or data offloading.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| UL Data Forwarding | O |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| DL Data Forwarding | O |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| Data Forwarding to NG-RAN QoS Flow Information List |  | *0..1* |  | Providing QoS flows accepted for data forwarding to the source gNB-CU-UP. | YES | ignore |
| >Data Forwarding to NG-RAN QoS Flow Information List Item |  | *1..<maxnoofQoSflows>* |  |  | - | - |
| >>QoS Flow Identifier | M |  | QoS Flow Identifier  9.3.1.24 |  | - | - |

### 9.3.3Container and List IE definitions

#### 9.3.3.1 DRB To Setup List E-UTRAN

This IE contains DRB related information used at Bearer Context Setup Request in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB To Setup Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >PDCP Configuration | M |  | 9.3.1.38 |  |
| >E-UTRAN QoS | M |  | 9.3.1.17 |  |
| >S1 UL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >Data Forwarding Information Request | O |  | 9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. |
| >Cell Group Information | M |  | 9.3.1.11 |  |
| >DL UP Parameters | O |  | UP Parameters  9.3.1.13 |  |
| >DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. |
| >Existing Allocated S1 DL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 | This IE is not used in this version of the specification. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.2 PDU Session Resource To Setup List

This IE contains PDU session resource related information used at Bearer Context Setup Request

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **PDU Session Resource To Setup Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >PDU Session Type | M |  | 9.3.1.22 |  | - | - |
| >S-NSSAI | M |  | 9.3.1.9 |  | - | - |
| >Security Indication | M |  | 9.3.1.23 |  | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate  9.3.1.20 | This IE shall be present when at least one Non-GBR QoS Flows is being setup. | - | - |
| >NG UL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request  9.3.2.5 |  | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Existing Allocated NG DL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| >Network Instance | O |  | 9.3.1.62 | This IE is ignored if the *Common Network Instance* IE is included. | YES | ignore |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *1* |  |  | - | - |
| **>>DRB To Setup Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flows Information To Be Setup | M |  | QoS Flow QoS Parameters List  9.3.1.25 |  | - | - |
| >>>DRB Data forwarding information Request | O |  | Data Forwarding Information Request  9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Contains the PDCP SN Status at setup after Resume. | - | - |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.3 DRB Setup List E-UTRAN

This IE contains setup DRB related information at Bearer Context Setup Response in E-UTRAN

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **DRB Setup Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >S1 DL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >Data Forwarding Information Response | O |  | Data Forwarding Information  9.3.2.6 | Providing forwarding info from the target gNB-CU-UP. |
| >UL UP Parameters | M |  | UP Parameters  9.3.1.13 |  |
| >S1 DL UP Unchanged | O |  | ENUMERATED (True, …) | This IE is not used in this version of the specification. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.4 DRB Failed List E-UTRAN

This IE contains failed to setup DRB related information at Bearer Context Setup Response in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Failed Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.5 PDU Session Resource Setup List

This IE contains setup PDU session resource related information used at Bearer Context Setup Response

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **PDU Session Resource Setup Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >Security Result | O |  | 9.3.1.52 |  |
| >NG DL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >PDU Session Data Forwarding Information Response | O |  | Data Forwarding Information  9.3.2.6 | Providing forwarding info from the target gNB-CU-UP. |
| >NG DL UP Unchanged | O |  | ENUMERATED (True, …) |  |
| **>DRB Setup List** |  | *1* |  |  |
| **>>DRB Setup Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>DRB Data forwarding information Response | O |  | Data Forwarding Information  9.3.2.6 | Providing forwarding info from the target gNB-CU-UP. |
| >>>UL UP Parameters | M |  | UP Parameters 9.3.1.13 |  |
| >>>Flow Setup List | M |  | QoS Flow List  9.3.1.12 |  |
| >>>Flow Failed List | O |  | Flow Failed List  9.3.1.45 |  |
| **>DRB Failed List** |  | *0.. 1* |  |  |
| **>>DRB Failed Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.6 PDU Session Resource Failed List

This IE contains failed PDU session resource related information used at Bearer Context Setup Response

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **PDU Session Resource Failed Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.7 DRB To Setup Modification List E-UTRAN

This IE contains DRB to setup related information used at Bearer Context Modification Request in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB To Setup Modification Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >PDCP Configuration | M |  | 9.3.1.38 |  |
| >E-UTRAN QoS | M |  | 9.3.1.17 |  |
| >S1 UL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >Data Forwarding Information Request | O |  | 9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. |
| >Cell Group Information | M |  | 9.3.1.11 |  |
| >DL UP Parameters | O |  | UP Parameters  9.3.1.13 |  |
| >DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.8 DRB To Modify List E-UTRAN

This IE contains DRB to modify related information used at Bearer Context Modification Request in E-UTRAN

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **DRB To Modify Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >PDCP Configuration | O |  | 9.3.1.38 |  |
| >E-UTRAN QoS | O |  | 9.3.1.17 |  |
| >S1 UL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 |  |
| >Data Forwarding Information | O |  | 9.3.2.6 | Providing forwarding info to the source gNB-CU-UP. |
| >PDCP SN Status Request | O |  | ENUMERATED (requested, …) | The gNB-CU-CP requests the gNB-CU-UP to provide the PDCP SN Status in the response message. |
| >PDCP SN Status Information | O |  | 9.3.1.58 | Providing SN Status information to the target gNB-CU-UP. |
| >DL UP Parameters | O |  | UP Parameters  9.3.1.13 |  |
| >Cell Group To Add | O |  | Cell Group Information 9.3.1.11 |  |
| >Cell Group To Modify | O |  | Cell Group Information 9.3.1.11 |  |
| >Cell Group To Remove | O |  | Cell Group Information 9.3.1.11 |  |
| >DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.9 DRB To Remove List E-UTRAN

This IE contains DRB to remove related information used at Bearer Context Modification Request in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB To Remove Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.10 PDU Session Resource To Setup Modification List

This IE contains PDU session resource to setup related information used at Bearer Context Modification Request

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **PDU Session Resource To Setup Modification Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >PDU Session Type | M |  | 9.3.1.22 |  | - | - |
| >S-NSSAI | M |  | 9.3.1.9 |  | - | - |
| >Security Indication | M |  | 9.3.1.23 |  | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 | This IE shall be present when Non-GBR QoS Flows are setting up. | - | - |
| >NG UL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request  9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Network Instance | O |  | 9.3.1.62 |  | - | - |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *1* |  |  | - | - |
| **>>DRB To Setup Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flows Information To Be Setup | M |  | QoS Flow QoS Parameters List  9.3.1.25 |  | - | - |
| >>>DRB Data forwarding information Request | O |  | Data Forwarding Information Request  9.3.2.5 | Requesting forwarding info from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status at setup after Resume to the target gNB-CU-UP. | - | - |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.11 PDU Session Resource To Modify List

This IE contains PDU session resource to modify related information used at Bearer Context Modification Request

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **PDU Session Resource To Modify Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >Security Indication | O |  | 9.3.1.23 | This IE is not used in this release. | - | - |
| >PDU Session Resource DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 |  | - | - |
| >NG UL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 |  | - | - |
| >PDU Session Data Forwarding Information Request | O |  | Data Forwarding Information Request  9.3.2.5 | Requesting forwarding information from the target gNB-CU-UP. | - | - |
| >PDU Session Data Forwarding Information | O |  | Data Forwarding Information  9.3.2.6 | Providing forwarding information to the source gNB-CU-UP. | - | - |
| >PDU Session Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to PDU Session. | - | - |
| >Network Instance | O |  | 9.3.1.62 | This IE is ignored if the *Common Network Instance* IE is included. | YES | ignore |
| >Common Network Instance | O |  | 9.3.1.66 |  | YES | ignore |
| **>DRB To Setup List** |  | *0..1* |  |  | - | - |
| **>>DRB To Setup Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | M |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | M |  | 9.3.1.38 |  | - | - |
| >>>Cell Group Information | M |  | 9.3.1.11 |  | - | - |
| >>>QoS Flow Information To Be Setup | M |  | QoS Flow QoS Parameters List  9.3.1.25 |  | - | - |
| >>>DRB Data Forwarding Information Request | O |  | Data Forwarding Information Request  9.3.2.5 | Requesting forwarding information from the target gNB-CU-UP. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status at setup after Resume to the target gNB-CU-UP. | - | - |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB | YES | ignore |
| **>DRB To Modify List** |  | *0.. 1* |  |  | - | - |
| **>>DRB To Modify Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >>>SDAP Configuration | O |  | 9.3.1.39 |  | - | - |
| >>>PDCP Configuration | O |  | 9.3.1.38 |  | - | - |
| >>>DRB Data forwarding information | O |  | Data Forwarding Information  9.3.2.6 | Providing forwarding information to the source gNB-CU-UP. | - | - |
| >>>PDCP SN Status Request | O |  | ENUMERATED (requested, …) | The gNB-CU-CP requests the gNB-CU-UP to provide the PDCP SN Status in the response message. | - | - |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status to the target gNB-CU-UP. | - | - |
| >>>DL UP Parameters | O |  | UP Parameters  9.3.1.13 |  | - | - |
| >>>Cell Group To Add | O |  | Cell Group Information  9.3.1.11 |  | - | - |
| >>>Cell Group To Modify | O |  | Cell Group Information  9.3.1.11 |  | - | - |
| >>>Cell Group To Remove | O |  | Cell Group Information  9.3.1.11 |  | - | - |
| >>>Flow Mapping Information | O |  | QoS Flow QoS Parameters List  9.3.1.25 | Overrides previous mapping information. | - | - |
| >>>DRB Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to DRB. | - | - |
| >>>Old QoS Flow List - UL End Marker expected | O |  | QoS Flow List 9.3.1.12 | Indicates that the source NG-RAN node has initiated QoS flow re-mapping and has not yet received SDAP end markers, as described in TS 38.300 [8]. | YES | reject |
| >>>DRB QoS | O |  | 9.3.1.26 | Indicates the DRB QoS when more than one QoS Flow is mapped to the DRB | YES | ignore |
| **>DRB To Remove List** |  | *0.. 1* |  |  | - | - |
| **>>DRB To Remove Item** |  | *1..<maxnoofDRBs>* |  |  | - | - |
| >>>DRB ID | M |  | 9.3.1.16 |  | - | - |
| >S-NSSAI | O |  | 9.3.1.9 |  | YES | reject |
| >Security Indication Modify | O |  | Security Indication  9.3.1.23 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.12 PDU Session Resource To Remove List

This IE contains PDU session resource to remove related information

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **PDU Session Resource To Remove Item** |  | *1..<maxnoofPDUSessionResource>* |  |  | - | - |
| >PDU Session ID | M |  | 9.3.1.21 |  | - | - |
| >Cause | O |  | 9.3.1.2 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.13 DRB Setup Modification List E-UTRAN

This IE contains setup DRB related information at Bearer Context Modification Response in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Setup Modification Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >S1 DL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >Data Forwarding Information Response | O |  | 9.3.2.6 | Provides forwarding information from the target gNB-CU-UP. |
| >UL UP Parameters | M |  | UP Parameters  9.3.1.13 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.14 DRB Failed Modification List E-UTRAN

This IE contains failed to setup DRB related information at Bearer Context Modification Response in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Failed Modification Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.15 DRB Modified List E-UTRAN

This IE contains modified DRB related information at Bearer Context Modification Response in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Modified Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >S1 DL UP Transport Layer Information | O |  | UP Transport Layer Information 9.3.2.1 |  |
| >PDCP SN Status Information | O |  | 9.3.1.58 | Provides the PDCP SN Status from the source gNB-CU-UP. |
| >UL UP Parameters | O |  | UP Parameters  9.3.1.13 | Carries the UL UP parameters. |

| Range bound | Explanation |
| --- | --- |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.16 DRB Failed To Modify List E-UTRAN

This IE contains failed to modify DRB related information at Bearer Context Modification Response in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Failed To Modify Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.17 PDU Session Resource Setup Modification List

This IE contains setup PDU session resource related information used at Bearer Context Modification Response

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **PDU Session Resource Setup Modification Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >Security Result | O |  | 9.3.1.52 |  |
| >NG DL UP Transport Layer Information | M |  | UP Transport Layer Information  9.3.2.1 |  |
| >PDU Session Data Forwarding Information Response | O |  | Data Forwarding Information  9.3.2.6 | Provides forwarding information from the target gNB-CU-UP. |
| **>DRB Setup List** |  | *1* |  |  |
| **>>DRB Setup Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>DRB Data forwarding information Response | O |  | Data Forwarding Information  9.3.2.6 | Provides forwarding information from the target gNB-CU-UP. |
| >>>UL UP Parameters | M |  | UP Parameters  9.3.1.13 |  |
| >>>Flow Setup List | M |  | QoS Flow List  9.3.1.12 |  |
| >>>Flow Failed List | O |  | Flow Failed List  9.3.1.45 |  |
| **>DRB Failed List** |  | *0.. 1* |  |  |
| **>>DRB Failed Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.18 PDU Session Resource Failed Modification List

This IE contains failed to setup PDU session resource related information used at Bearer Context Modification Response

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **PDU Session Resource Failed Modification Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.19 PDU Session Resource Modified List

This IE contains modified PDU session resource related information used at Bearer Context Modification Response

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **PDU Session Resource Modified Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |  |  |
| >NG DL UP Transport Layer Information | O |  | UP Transport Layer Information 9.3.2.1 |  |  |  |
| >Security Result | O |  | 9.3.1.52 |  |  |  |
| >PDU Session Data Forwarding Information Response | O |  | Data Forwarding Information  9.3.2.6 |  |  |  |
| **>DRB Setup List** |  | *0.. 1* |  |  |  |  |
| **>>DRB Setup Item** |  | *1..<maxnoofDRBs>* |  |  |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |  |  |
| >>>DRB Data forwarding information Response | O |  | Data Forwarding Information  9.3.2.6 |  |  |  |
| >>>UL UP Parameters | M |  | UP Parameters  9.3.1.13 |  |  |  |
| >>>Flow Setup List | M |  | QoS Flow List  9.3.1.12 |  |  |  |
| >>>Flow Failed List | O |  | Flow Failed List  9.3.1.45 |  |  |  |
| **>DRB Failed List** |  | *0.. 1* |  |  |  |  |
| **>>DRB Failed Item** |  | *1..<maxnoofDRBs>* |  |  |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |  |  |
| >>>Cause | M |  | 9.3.1.2 |  |  |  |
| **>DRB Modified List** |  | *0.. 1* |  |  |  |  |
| **>>DRB Modified Item** |  | *1..<maxnoofDRBs>* |  |  |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |  |  |
| >>>UL UP Parameters | O |  | UP Parameters  9.3.1.13 | Carries the UL UP parameters. |  |  |
| >>>PDCP SN Status Information | O |  | 9.3.1.58 | Provides PDCP SN Status to the target gNB-CU-UP. |  |  |
| >>>Flow Setup List | O |  | QoS Flow List  9.3.1.12 |  |  |  |
| >>>Flow Failed List | O |  | Flow Failed List  9.3.1.45 |  |  |  |
| >>> Old QoS Flow List - UL End Marker expected | O |  | QoS Flow List  9.3.1.12 | Indicates the QoS flow(s) for which the gNB-CU-UP has not yet received SDAP end markers after the gNB-CU-CP reconfigured those QoS flow(s) to another DRB. | Yes | ignore |
| **>DRB Failed To Modify List** |  | *0.. 1* |  |  |  |  |
| **>>DRB Failed To Modify Item** |  | *1..<maxnoofDRBs>* |  |  |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |  |  |
| >>>Cause | M |  | 9.3.1.2 |  |  |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.20 PDU Session Resource Failed To Modify List

This IE contains failed to modify PDU session resource related information used at Bearer Context Modification Response

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **PDU Session Resource Failed To Modify Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >Cause | M |  | 9.3.1.2 |  |

| Range bound | Explanation |
| --- | --- |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.21 DRB Required To Modify List E-UTRAN

This IE contains DRB to modify related information used at Bearer Context Modification Required in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Required To Modify Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >S1 DL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 |  |
| >gNB-CU-UP Cell Group Related Configuration | O |  | 9.3.1.34 |  |
| >Cause | O |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.22 DRB Required To Remove List E-UTRAN

This IE contains DRB to remove related information used at Bearer Context Modification Required in E-UTRAN

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **DRB Required To Remove Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.23 PDU Session Resource Required To Modify List

This IE contains PDU session resource to modify related information used at Bearer Context Modification Required

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| **PDU Session Resource Required To Modify Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| >NG DL UP Transport Layer Information | O |  | UP Transport Layer Information  9.3.2.1 |  |
| **>DRB To Modify List** |  | *0.. 1* |  |  |
| **>>DRB To Modify Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>gNB-CU-UP Cell Group Related Configuration | O |  | 9.3.1.34 |  |
| >>>Flow To Remove | O |  | QoS Flow List  9.3.1.12 |  |
| >>>Cause | O |  | 9.3.1.2 |  |
| **>DRB To Remove List** |  | *0.. 1* |  |  |
| **>>DRB To Remove Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>Cause | M |  | 9.3.1.2 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

#### 9.3.3.24 DRB Confirm Modified List E-UTRAN

This IE contains modified DRB related information at Bearer Context Modification Confirm in E-UTRAN

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **DRB Confirm Modified Item E-UTRAN** |  | *1..<maxnoofDRBs>* |  |  |
| >DRB ID | M |  | 9.3.1.16 |  |
| >Cell Group Information | O |  | 9.3.1.11 | Included if the gNB-CU-CP was unable to change cell group related information as requested in the *gNB-CU-UP Cell Group Related Configuration* IE (e.g., UL Configuration). |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |

#### 9.3.3.25 PDU Session Resource Confirm Modified List

This IE contains modified PDU session resource related information used at Bearer Context Modification Confirm

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **PDU Session Resource Modified Item** |  | *1..<maxnoofPDUSessionResource>* |  |  |
| >PDU Session ID | M |  | 9.3.1.21 |  |
| **>DRB Modified List** |  | *0.. 1* |  |  |
| **>>DRB Modified Item** |  | *1..<maxnoofDRBs>* |  |  |
| >>>DRB ID | M |  | 9.3.1.16 |  |
| >>>Cell Group Information | O |  | 9.3.1.11 | Included if the gNB-CU-CP was unable to change cell group related information as requested in the *gNB-CU-UP Cell Group Related Configuration* IE (e.g., UL Configuration). |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

## 9.4 Message and Information Element Abstract Syntax (with ASN.1)

### 9.4.1 General

E1AP ASN.1 definition conforms to ITU-T Rec. X.691 [7], ITU-T Rec. X.680 [8] and ITU-T Rec. X.681 [9].

The ASN.1 definition specifies the structure and content of E1AP messages. E1AP messages can contain any IEs specified in the object set definitions for that message without the order or number of occurrence being restricted by ASN.1. However, for this version of the standard, a sending entity shall construct an E1AP message according to the PDU definitions module and with the following additional rules:

- IEs shall be ordered (in an IE container) in the order they appear in object set definitions.

- Object set definitions specify how many times IEs may appear. An IE shall appear exactly once if the presence field in an object has value "mandatory". An IE may appear at most once if the presence field in an object has value "optional" or "conditional". If in a tabular format there is multiplicity specified for an IE (i.e., an IE list) then in the corresponding ASN.1 definition the list definition is separated into two parts. The first part defines an IE container list where the list elements reside. The second part defines list elements. The IE container list appears as an IE of its own. For this version of the standard an IE container list may contain only one kind of list elements.

NOTE: In the above “IE” means an IE in the object set with an explicit ID. If one IE needs to appear more than once in one object set, then the different occurrences will have different IE IDs.

If an E1AP message that is not constructed as defined above is received, this shall be considered as Abstract Syntax Error, and the message shall be handled as defined for Abstract Syntax Error in clause 10.

### 9.4.2 Usage of private message mechanism for non-standard use

The private message mechanism for non-standard use may be used:

- for special operator- (and/or vendor) specific features considered not to be part of the basic functionality, i.e., the functionality required for a complete and high-quality specification in order to guarantee multivendor interoperability;

- by vendors for research purposes, e.g., to implement and evaluate new algorithms/features before such features are proposed for standardisation.

The private message mechanism shall not be used for basic functionality. Such functionality shall be standardised.

### 9.4.3 Elementary Procedure Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedure definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PDU-Descriptions {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-PDU-Descriptions (0) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Criticality,

ProcedureCode

FROM E1AP-CommonDataTypes

Reset,

ResetAcknowledge,

ErrorIndication,

GNB-CU-UP-E1SetupRequest,

GNB-CU-UP-E1SetupResponse,

GNB-CU-UP-E1SetupFailure,

GNB-CU-CP-E1SetupRequest,

GNB-CU-CP-E1SetupResponse,

GNB-CU-CP-E1SetupFailure,

GNB-CU-UP-ConfigurationUpdate,

GNB-CU-UP-ConfigurationUpdateAcknowledge,

GNB-CU-UP-ConfigurationUpdateFailure,

GNB-CU-CP-ConfigurationUpdate,

GNB-CU-CP-ConfigurationUpdateAcknowledge,

GNB-CU-CP-ConfigurationUpdateFailure,

BearerContextSetupRequest,

BearerContextSetupResponse,

BearerContextSetupFailure,

BearerContextModificationRequest,

BearerContextModificationResponse,

BearerContextModificationFailure,

BearerContextModificationRequired,

BearerContextModificationConfirm,

BearerContextReleaseCommand,

BearerContextReleaseComplete,

BearerContextReleaseRequest,

BearerContextInactivityNotification,

DLDataNotification,

ULDataNotification,

DataUsageReport,

E1ReleaseRequest,

E1ReleaseResponse,

GNB-CU-UP-CounterCheckRequest,

GNB-CU-UP-StatusIndication,

MRDC-DataUsageReport,

PrivateMessage

FROM E1AP-PDU-Contents

id-reset,

id-errorIndication,

id-gNB-CU-UP-E1Setup,

id-gNB-CU-CP-E1Setup,

id-gNB-CU-UP-ConfigurationUpdate,

id-gNB-CU-CP-ConfigurationUpdate,

id-e1Release,

id-bearerContextSetup,

id-bearerContextModification,

id-bearerContextModificationRequired,

id-bearerContextRelease,

id-bearerContextReleaseRequest,

id-bearerContextInactivityNotification,

id-dLDataNotification,

id-uLDataNotification,

id-dataUsageReport,

id-gNB-CU-UP-CounterCheck,

id-gNB-CU-UP-StatusIndication,

id-mRDC-DataUsageReport,

id-privateMessage

FROM E1AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure Class

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-ELEMENTARY-PROCEDURE ::= CLASS {

&InitiatingMessage ,

&SuccessfulOutcome OPTIONAL,

&UnsuccessfulOutcome OPTIONAL,

&procedureCode ProcedureCode UNIQUE,

&criticality Criticality DEFAULT ignore

}

WITH SYNTAX {

INITIATING MESSAGE &InitiatingMessage

[SUCCESSFUL OUTCOME &SuccessfulOutcome]

[UNSUCCESSFUL OUTCOME &UnsuccessfulOutcome]

PROCEDURE CODE &procedureCode

[CRITICALITY &criticality]

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface PDU Definition

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PDU ::= CHOICE {

initiatingMessage InitiatingMessage,

successfulOutcome SuccessfulOutcome,

unsuccessfulOutcome UnsuccessfulOutcome,

...

}

InitiatingMessage ::= SEQUENCE {

procedureCode E1AP-ELEMENTARY-PROCEDURE.&procedureCode ({E1AP-ELEMENTARY-PROCEDURES}),

criticality E1AP-ELEMENTARY-PROCEDURE.&criticality ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value E1AP-ELEMENTARY-PROCEDURE.&InitiatingMessage ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

SuccessfulOutcome ::= SEQUENCE {

procedureCode E1AP-ELEMENTARY-PROCEDURE.&procedureCode ({E1AP-ELEMENTARY-PROCEDURES}),

criticality E1AP-ELEMENTARY-PROCEDURE.&criticality ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value E1AP-ELEMENTARY-PROCEDURE.&SuccessfulOutcome ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

UnsuccessfulOutcome ::= SEQUENCE {

procedureCode E1AP-ELEMENTARY-PROCEDURE.&procedureCode ({E1AP-ELEMENTARY-PROCEDURES}),

criticality E1AP-ELEMENTARY-PROCEDURE.&criticality ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode}),

value E1AP-ELEMENTARY-PROCEDURE.&UnsuccessfulOutcome ({E1AP-ELEMENTARY-PROCEDURES}{@procedureCode})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedure List

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-ELEMENTARY-PROCEDURES E1AP-ELEMENTARY-PROCEDURE ::= {

E1AP-ELEMENTARY-PROCEDURES-CLASS-1 |

E1AP-ELEMENTARY-PROCEDURES-CLASS-2 ,

...

}

E1AP-ELEMENTARY-PROCEDURES-CLASS-1 E1AP-ELEMENTARY-PROCEDURE ::= {

reset |

gNB-CU-UP-E1Setup |

gNB-CU-CP-E1Setup |

gNB-CU-UP-ConfigurationUpdate |

gNB-CU-CP-ConfigurationUpdate |

e1Release |

bearerContextSetup |

bearerContextModification |

bearerContextModificationRequired |

bearerContextRelease ,

...

}

E1AP-ELEMENTARY-PROCEDURES-CLASS-2 E1AP-ELEMENTARY-PROCEDURE ::= {

errorIndication |

bearerContextReleaseRequest |

bearerContextInactivityNotification |

dLDataNotification |

uLDataNotification |

dataUsageReport |

gNB-CU-UP-CounterCheck |

gNB-CU-UP-StatusIndication |

mRDC-DataUsageReport |

privateMessage ,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Interface Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

reset E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE Reset

SUCCESSFUL OUTCOME ResetAcknowledge

PROCEDURE CODE id-reset

CRITICALITY reject

}

errorIndication E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ErrorIndication

PROCEDURE CODE id-errorIndication

CRITICALITY ignore

}

gNB-CU-UP-E1Setup E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-UP-E1SetupRequest

SUCCESSFUL OUTCOME GNB-CU-UP-E1SetupResponse

UNSUCCESSFUL OUTCOME GNB-CU-UP-E1SetupFailure

PROCEDURE CODE id-gNB-CU-UP-E1Setup

CRITICALITY reject

}

gNB-CU-CP-E1Setup E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-CP-E1SetupRequest

SUCCESSFUL OUTCOME GNB-CU-CP-E1SetupResponse

UNSUCCESSFUL OUTCOME GNB-CU-CP-E1SetupFailure

PROCEDURE CODE id-gNB-CU-CP-E1Setup

CRITICALITY reject

}

gNB-CU-UP-ConfigurationUpdate E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-UP-ConfigurationUpdate

SUCCESSFUL OUTCOME GNB-CU-UP-ConfigurationUpdateAcknowledge

UNSUCCESSFUL OUTCOME GNB-CU-UP-ConfigurationUpdateFailure

PROCEDURE CODE id-gNB-CU-UP-ConfigurationUpdate

CRITICALITY reject

}

gNB-CU-CP-ConfigurationUpdate E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-CP-ConfigurationUpdate

SUCCESSFUL OUTCOME GNB-CU-CP-ConfigurationUpdateAcknowledge

UNSUCCESSFUL OUTCOME GNB-CU-CP-ConfigurationUpdateFailure

PROCEDURE CODE id-gNB-CU-CP-ConfigurationUpdate

CRITICALITY reject

}

e1Release E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE E1ReleaseRequest

SUCCESSFUL OUTCOME E1ReleaseResponse

PROCEDURE CODE id-e1Release

CRITICALITY reject

}

bearerContextSetup E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextSetupRequest

SUCCESSFUL OUTCOME BearerContextSetupResponse

UNSUCCESSFUL OUTCOME BearerContextSetupFailure

PROCEDURE CODE id-bearerContextSetup

CRITICALITY reject

}

bearerContextModification E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextModificationRequest

SUCCESSFUL OUTCOME BearerContextModificationResponse

UNSUCCESSFUL OUTCOME BearerContextModificationFailure

PROCEDURE CODE id-bearerContextModification

CRITICALITY reject

}

bearerContextModificationRequired E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextModificationRequired

SUCCESSFUL OUTCOME BearerContextModificationConfirm

PROCEDURE CODE id-bearerContextModificationRequired

CRITICALITY reject

}

bearerContextRelease E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextReleaseCommand

SUCCESSFUL OUTCOME BearerContextReleaseComplete

PROCEDURE CODE id-bearerContextRelease

CRITICALITY reject

}

bearerContextReleaseRequest E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextReleaseRequest

PROCEDURE CODE id-bearerContextReleaseRequest

CRITICALITY ignore

}

bearerContextInactivityNotification E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE BearerContextInactivityNotification

PROCEDURE CODE id-bearerContextInactivityNotification

CRITICALITY ignore

}

dLDataNotification E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE DLDataNotification

PROCEDURE CODE id-dLDataNotification

CRITICALITY ignore

}

uLDataNotification E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE ULDataNotification

PROCEDURE CODE id-uLDataNotification

CRITICALITY ignore

}

dataUsageReport E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE DataUsageReport

PROCEDURE CODE id-dataUsageReport

CRITICALITY ignore

}

gNB-CU-UP-CounterCheck E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-UP-CounterCheckRequest

PROCEDURE CODE id-gNB-CU-UP-CounterCheck

CRITICALITY ignore

}

gNB-CU-UP-StatusIndication E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE GNB-CU-UP-StatusIndication

PROCEDURE CODE id-gNB-CU-UP-StatusIndication

CRITICALITY ignore

}

privateMessage E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE PrivateMessage

PROCEDURE CODE id-privateMessage

CRITICALITY ignore

}

mRDC-DataUsageReport E1AP-ELEMENTARY-PROCEDURE ::= {

INITIATING MESSAGE MRDC-DataUsageReport

PROCEDURE CODE id-mRDC-DataUsageReport

CRITICALITY ignore

}

END

-- ASN1STOP

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for E1AP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Cause,

CriticalityDiagnostics,

GNB-CU-CP-UE-E1AP-ID,

GNB-CU-UP-UE-E1AP-ID,

UE-associatedLogicalE1-ConnectionItem,

GNB-CU-UP-ID,

GNB-CU-UP-Name,

GNB-CU-CP-Name,

CNSupport,

PLMN-Identity,

Slice-Support-List,

NR-CGI-Support-List,

QoS-Parameters-Support-List,

SecurityInformation,

BitRate,

BearerContextStatusChange,

DRB-To-Setup-List-EUTRAN,

DRB-Setup-List-EUTRAN,

DRB-Failed-List-EUTRAN,

DRB-To-Modify-List-EUTRAN,

DRB-Modified-List-EUTRAN,

DRB-Failed-To-Modify-List-EUTRAN,

DRB-To-Remove-List-EUTRAN,

DRB-Required-To-Remove-List-EUTRAN,

DRB-Required-To-Modify-List-EUTRAN,

DRB-Confirm-Modified-List-EUTRAN,

DRB-To-Setup-Mod-List-EUTRAN,

DRB-Setup-Mod-List-EUTRAN,

DRB-Failed-Mod-List-EUTRAN,

PDU-Session-Resource-To-Setup-List,

PDU-Session-Resource-Setup-List,

PDU-Session-Resource-Failed-List,

PDU-Session-Resource-To-Modify-List,

PDU-Session-Resource-Modified-List,

PDU-Session-Resource-Failed-To-Modify-List,

PDU-Session-Resource-To-Remove-List,

PDU-Session-Resource-Required-To-Modify-List,

PDU-Session-Resource-Confirm-Modified-List,

PDU-Session-Resource-To-Setup-Mod-List,

PDU-Session-Resource-Setup-Mod-List,

PDU-Session-Resource-Failed-Mod-List,

PDU-Session-To-Notify-List,

DRB-Status-Item,

DRB-Activity-Item,

Data-Usage-Report-List,

TimeToWait,

ActivityNotificationLevel,

ActivityInformation,

New-UL-TNL-Information-Required,

GNB-CU-CP-TNLA-Setup-Item,

GNB-CU-CP-TNLA-Failed-To-Setup-Item,

GNB-CU-CP-TNLA-To-Add-Item,

GNB-CU-CP-TNLA-To-Remove-Item,

GNB-CU-CP-TNLA-To-Update-Item,

GNB-CU-UP-TNLA-To-Remove-Item,

TransactionID,

Inactivity-Timer,

DRBs-Subject-To-Counter-Check-List-EUTRAN,

DRBs-Subject-To-Counter-Check-List-NG-RAN,

PPI,

GNB-CU-UP-Capacity,

GNB-CU-UP-OverloadInformation,

DataDiscardRequired,

PDU-Session-Resource-Data-Usage-List,

RANUEID,

GNB-DU-ID

FROM E1AP-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerList{},

ProtocolIE-SingleContainer{},

E1AP-PRIVATE-IES,

E1AP-PROTOCOL-EXTENSION,

E1AP-PROTOCOL-IES

FROM E1AP-Containers

id-Cause,

id-CriticalityDiagnostics,

id-gNB-CU-CP-UE-E1AP-ID,

id-gNB-CU-UP-UE-E1AP-ID,

id-ResetType,

id-UE-associatedLogicalE1-ConnectionItem,

id-UE-associatedLogicalE1-ConnectionListResAck,

id-gNB-CU-UP-ID,

id-gNB-CU-UP-Name,

id-gNB-CU-CP-Name,

id-CNSupport,

id-SupportedPLMNs,

id-SecurityInformation,

id-UEDLAggregateMaximumBitRate,

id-BearerContextStatusChange,

id-System-BearerContextSetupRequest,

id-System-BearerContextSetupResponse,

id-System-BearerContextModificationRequest,

id-System-BearerContextModificationResponse,

id-System-BearerContextModificationConfirm,

id-System-BearerContextModificationRequired,

id-DRB-Status-List,

id-Data-Usage-Report-List,

id-TimeToWait,

id-ActivityNotificationLevel,

id-ActivityInformation,

id-New-UL-TNL-Information-Required,

id-GNB-CU-CP-TNLA-Setup-List,

id-GNB-CU-CP-TNLA-Failed-To-Setup-List,

id-GNB-CU-CP-TNLA-To-Add-List,

id-GNB-CU-CP-TNLA-To-Remove-List,

id-GNB-CU-CP-TNLA-To-Update-List,

id-GNB-CU-UP-TNLA-To-Remove-List,

id-DRB-To-Setup-List-EUTRAN,

id-DRB-To-Modify-List-EUTRAN,

id-DRB-To-Remove-List-EUTRAN,

id-DRB-Required-To-Modify-List-EUTRAN,

id-DRB-Required-To-Remove-List-EUTRAN,

id-DRB-Setup-List-EUTRAN,

id-DRB-Failed-List-EUTRAN,

id-DRB-Modified-List-EUTRAN,

id-DRB-Failed-To-Modify-List-EUTRAN,

id-DRB-Confirm-Modified-List-EUTRAN,

id-DRB-To-Setup-Mod-List-EUTRAN,

id-DRB-Setup-Mod-List-EUTRAN,

id-DRB-Failed-Mod-List-EUTRAN,

id-PDU-Session-Resource-To-Setup-List,

id-PDU-Session-Resource-To-Modify-List,

id-PDU-Session-Resource-To-Remove-List,

id-PDU-Session-Resource-Required-To-Modify-List,

id-PDU-Session-Resource-Setup-List,

id-PDU-Session-Resource-Failed-List,

id-PDU-Session-Resource-Modified-List,

id-PDU-Session-Resource-Failed-To-Modify-List,

id-PDU-Session-Resource-Confirm-Modified-List,

id-PDU-Session-Resource-Setup-Mod-List,

id-PDU-Session-Resource-Failed-Mod-List,

id-PDU-Session-Resource-To-Setup-Mod-List,

id-PDU-Session-To-Notify-List,

id-TransactionID,

id-Serving-PLMN,

id-UE-Inactivity-Timer,

id-System-GNB-CU-UP-CounterCheckRequest,

id-DRBs-Subject-To-Counter-Check-List-EUTRAN,

id-DRBs-Subject-To-Counter-Check-List-NG-RAN,

id-PPI,

id-gNB-CU-UP-Capacity,

id-GNB-CU-UP-OverloadInformation,

id-UEDLMaximumIntegrityProtectedDataRate,

id-DataDiscardRequired,

id-PDU-Session-Resource-Data-Usage-List,

id-RANUEID,

id-GNB-DU-ID,

maxnoofErrors,

maxnoofSPLMNs,

maxnoofDRBs,

maxnoofTNLAssociations,

maxnoofIndividualE1ConnectionsToReset

FROM E1AP-Constants;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- RESET

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Reset

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Reset ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {ResetIEs} },

...

}

ResetIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-ResetType CRITICALITY reject TYPE ResetType PRESENCE mandatory },

...

}

ResetType ::= CHOICE {

e1-Interface ResetAll,

partOfE1-Interface UE-associatedLogicalE1-ConnectionListRes,

choice-extension ProtocolIE-SingleContainer {{ResetType-ExtIEs}}

}

ResetType-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

ResetAll ::= ENUMERATED {

reset-all,

...

}

UE-associatedLogicalE1-ConnectionListRes ::= SEQUENCE (SIZE(1.. maxnoofIndividualE1ConnectionsToReset)) OF ProtocolIE-SingleContainer { { UE-associatedLogicalE1-ConnectionItemRes } }

UE-associatedLogicalE1-ConnectionItemRes E1AP-PROTOCOL-IES ::= {

{ ID id-UE-associatedLogicalE1-ConnectionItem CRITICALITY reject TYPE UE-associatedLogicalE1-ConnectionItem PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Reset Acknowledge

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ResetAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {ResetAcknowledgeIEs} },

...

}

ResetAcknowledgeIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-UE-associatedLogicalE1-ConnectionListResAck CRITICALITY ignore TYPE UE-associatedLogicalE1-ConnectionListResAck PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

UE-associatedLogicalE1-ConnectionListResAck ::= SEQUENCE (SIZE(1.. maxnoofIndividualE1ConnectionsToReset)) OF ProtocolIE-SingleContainer { { UE-associatedLogicalE1-ConnectionItemResAck } }

UE-associatedLogicalE1-ConnectionItemResAck E1AP-PROTOCOL-IES ::= {

{ ID id-UE-associatedLogicalE1-ConnectionItem CRITICALITY ignore TYPE UE-associatedLogicalE1-ConnectionItem PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- ERROR INDICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ErrorIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{ErrorIndication-IEs}},

...

}

ErrorIndication-IEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY ignore TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE optional}|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY ignore TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE optional}|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE optional}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP E1 SETUP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP E1 Setup Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-E1SetupRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-E1SetupRequestIEs} },

...

}

GNB-CU-UP-E1SetupRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-ID CRITICALITY reject TYPE GNB-CU-UP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-Name CRITICALITY ignore TYPE GNB-CU-UP-Name PRESENCE optional }|

{ ID id-CNSupport CRITICALITY reject TYPE CNSupport PRESENCE mandatory }|

{ ID id-SupportedPLMNs CRITICALITY reject TYPE SupportedPLMNs-List PRESENCE mandatory }|

{ ID id-gNB-CU-UP-Capacity CRITICALITY ignore TYPE GNB-CU-UP-Capacity PRESENCE optional },

...

}

SupportedPLMNs-List ::= SEQUENCE (SIZE (1..maxnoofSPLMNs)) OF SupportedPLMNs-Item

SupportedPLMNs-Item ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

slice-Support-List Slice-Support-List OPTIONAL,

nR-CGI-Support-List NR-CGI-Support-List OPTIONAL,

qoS-Parameters-Support-List QoS-Parameters-Support-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SupportedPLMNs-ExtIEs } } OPTIONAL,

...

}

SupportedPLMNs-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP E1 Setup Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-E1SetupResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-E1SetupResponseIEs} },

...

}

GNB-CU-UP-E1SetupResponseIEs

E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-CP-Name CRITICALITY ignore TYPE GNB-CU-CP-Name PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP E1 Setup Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-E1SetupFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-E1SetupFailureIEs} },

...

}

GNB-CU-UP-E1SetupFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP E1 SETUP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP E1 Setup Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-E1SetupRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-E1SetupRequestIEs} },

...

}

GNB-CU-CP-E1SetupRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-CP-Name CRITICALITY ignore TYPE GNB-CU-CP-Name PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP E1 Setup Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-E1SetupResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-E1SetupResponseIEs} },

...

}

GNB-CU-CP-E1SetupResponseIEs

E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-ID CRITICALITY reject TYPE GNB-CU-UP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-Name CRITICALITY ignore TYPE GNB-CU-UP-Name PRESENCE optional }|

{ ID id-CNSupport CRITICALITY reject TYPE CNSupport PRESENCE mandatory }|

{ ID id-SupportedPLMNs CRITICALITY reject TYPE SupportedPLMNs-List PRESENCE mandatory }|

{ ID id-gNB-CU-UP-Capacity CRITICALITY ignore TYPE GNB-CU-UP-Capacity PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP E1 Setup Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-E1SetupFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-E1SetupFailureIEs} },

...

}

GNB-CU-CP-E1SetupFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP CONFIGURATION UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP Configuration Update

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-ConfigurationUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-ConfigurationUpdateIEs} },

...

}

GNB-CU-UP-ConfigurationUpdateIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-ID CRITICALITY reject TYPE GNB-CU-UP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-Name CRITICALITY ignore TYPE GNB-CU-UP-Name PRESENCE optional }|

{ ID id-SupportedPLMNs CRITICALITY reject TYPE SupportedPLMNs-List PRESENCE optional }|

{ ID id-gNB-CU-UP-Capacity CRITICALITY ignore TYPE GNB-CU-UP-Capacity PRESENCE optional }|

{ ID id-GNB-CU-UP-TNLA-To-Remove-List CRITICALITY reject TYPE GNB-CU-UP-TNLA-To-Remove-List PRESENCE optional },

...

}

GNB-CU-UP-TNLA-To-Remove-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-UP-TNLA-To-Remove-Item

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP Configuration Update Acknowledge

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-ConfigurationUpdateAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-ConfigurationUpdateAcknowledgeIEs} },

...

}

GNB-CU-UP-ConfigurationUpdateAcknowledgeIEs

E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP Configuration Update Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-ConfigurationUpdateFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-UP-ConfigurationUpdateFailureIEs} },

...

}

GNB-CU-UP-ConfigurationUpdateFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP CONFIGURATION UPDATE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP Configuration Update

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-ConfigurationUpdate ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-ConfigurationUpdateIEs} },

...

}

GNB-CU-CP-ConfigurationUpdateIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-gNB-CU-CP-Name CRITICALITY ignore TYPE GNB-CU-UP-Name PRESENCE optional }|

{ ID id-GNB-CU-CP-TNLA-To-Add-List CRITICALITY ignore TYPE GNB-CU-CP-TNLA-To-Add-List PRESENCE optional }|

{ ID id-GNB-CU-CP-TNLA-To-Remove-List CRITICALITY ignore TYPE GNB-CU-CP-TNLA-To-Remove-List PRESENCE optional }|

{ ID id-GNB-CU-CP-TNLA-To-Update-List CRITICALITY ignore TYPE GNB-CU-CP-TNLA-To-Update-List PRESENCE optional },

...

}

GNB-CU-CP-TNLA-To-Add-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-CP-TNLA-To-Add-Item

GNB-CU-CP-TNLA-To-Remove-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-CP-TNLA-To-Remove-Item

GNB-CU-CP-TNLA-To-Update-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-CP-TNLA-To-Update-Item

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP Configuration Update Acknowledge

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-ConfigurationUpdateAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-ConfigurationUpdateAcknowledgeIEs} },

...

}

GNB-CU-CP-ConfigurationUpdateAcknowledgeIEs

E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional }|

{ ID id-GNB-CU-CP-TNLA-Setup-List CRITICALITY ignore TYPE GNB-CU-CP-TNLA-Setup-List PRESENCE optional }|

{ ID id-GNB-CU-CP-TNLA-Failed-To-Setup-List CRITICALITY ignore TYPE GNB-CU-CP-TNLA-Failed-To-Setup-List PRESENCE optional },

...

}

GNB-CU-CP-TNLA-Setup-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-CP-TNLA-Setup-Item

GNB-CU-CP-TNLA-Failed-To-Setup-List ::= SEQUENCE (SIZE(1.. maxnoofTNLAssociations)) OF GNB-CU-CP-TNLA-Failed-To-Setup-Item

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-CP Configuration Update Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-ConfigurationUpdateFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {GNB-CU-CP-ConfigurationUpdateFailureIEs} },

...

}

GNB-CU-CP-ConfigurationUpdateFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-TimeToWait CRITICALITY ignore TYPE TimeToWait PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E1 RELEASE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E1 Release Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1ReleaseRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {E1ReleaseRequestIEs} },

...

}

E1ReleaseRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- E1 Release Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1ReleaseResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { {E1ReleaseResponseIEs} },

...

}

E1ReleaseResponseIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT SETUP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Setup Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextSetupRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextSetupRequestIEs} },

...

}

BearerContextSetupRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-SecurityInformation CRITICALITY reject TYPE SecurityInformation PRESENCE mandatory }|

{ ID id-UEDLAggregateMaximumBitRate CRITICALITY reject TYPE BitRate PRESENCE mandatory }|

{ ID id-UEDLMaximumIntegrityProtectedDataRate CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-Serving-PLMN CRITICALITY ignore TYPE PLMN-Identity PRESENCE mandatory }|

{ ID id-ActivityNotificationLevel CRITICALITY reject TYPE ActivityNotificationLevel PRESENCE mandatory }|

{ ID id-UE-Inactivity-Timer CRITICALITY reject TYPE Inactivity-Timer PRESENCE optional }|

{ ID id-BearerContextStatusChange CRITICALITY reject TYPE BearerContextStatusChange PRESENCE optional }|

{ ID id-System-BearerContextSetupRequest CRITICALITY reject TYPE System-BearerContextSetupRequest PRESENCE mandatory }|

{ ID id-RANUEID CRITICALITY ignore TYPE RANUEID PRESENCE optional }|

{ ID id-GNB-DU-ID CRITICALITY ignore TYPE GNB-DU-ID PRESENCE optional },

...

}

System-BearerContextSetupRequest ::= CHOICE {

e-UTRAN-BearerContextSetupRequest ProtocolIE-Container {{EUTRAN-BearerContextSetupRequest}},

nG-RAN-BearerContextSetupRequest ProtocolIE-Container {{NG-RAN-BearerContextSetupRequest}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextSetupRequest-ExtIEs}}

}

System-BearerContextSetupRequest-ExtIEs E1AP-PROTOCOL-IES::= {

...

}

EUTRAN-BearerContextSetupRequest E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-To-Setup-List-EUTRAN CRITICALITY reject TYPE DRB-To-Setup-List-EUTRAN PRESENCE mandatory },

...

}

NG-RAN-BearerContextSetupRequest E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-To-Setup-List CRITICALITY reject TYPE PDU-Session-Resource-To-Setup-List PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Setup Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextSetupResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextSetupResponseIEs} },

...

}

BearerContextSetupResponseIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-System-BearerContextSetupResponse CRITICALITY ignore TYPE System-BearerContextSetupResponse PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

System-BearerContextSetupResponse::= CHOICE {

e-UTRAN-BearerContextSetupResponse ProtocolIE-Container {{EUTRAN-BearerContextSetupResponse}},

nG-RAN-BearerContextSetupResponse ProtocolIE-Container {{NG-RAN-BearerContextSetupResponse}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextSetupResponse-ExtIEs}}

}

System-BearerContextSetupResponse-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

EUTRAN-BearerContextSetupResponse E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-Setup-List-EUTRAN CRITICALITY ignore TYPE DRB-Setup-List-EUTRAN PRESENCE mandatory }|

{ ID id-DRB-Failed-List-EUTRAN CRITICALITY ignore TYPE DRB-Failed-List-EUTRAN PRESENCE optional },

...

}

NG-RAN-BearerContextSetupResponse E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-Setup-List CRITICALITY ignore TYPE PDU-Session-Resource-Setup-List PRESENCE mandatory }|

{ ID id-PDU-Session-Resource-Failed-List CRITICALITY ignore TYPE PDU-Session-Resource-Failed-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Setup Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextSetupFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextSetupFailureIEs} },

...

}

BearerContextSetupFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY ignore TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT MODIFICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextModificationRequestIEs} },

...

}

BearerContextModificationRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-SecurityInformation CRITICALITY reject TYPE SecurityInformation PRESENCE optional }|

{ ID id-UEDLAggregateMaximumBitRate CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-UEDLMaximumIntegrityProtectedDataRate CRITICALITY reject TYPE BitRate PRESENCE optional }|

{ ID id-BearerContextStatusChange CRITICALITY reject TYPE BearerContextStatusChange PRESENCE optional }|

{ ID id-New-UL-TNL-Information-Required CRITICALITY reject TYPE New-UL-TNL-Information-Required PRESENCE optional }|

{ ID id-UE-Inactivity-Timer CRITICALITY reject TYPE Inactivity-Timer PRESENCE optional }|

{ ID id-DataDiscardRequired CRITICALITY ignore TYPE DataDiscardRequired PRESENCE optional }|

{ ID id-System-BearerContextModificationRequest CRITICALITY reject TYPE System-BearerContextModificationRequest PRESENCE optional }|

{ ID id-RANUEID CRITICALITY ignore TYPE RANUEID PRESENCE optional }|

{ ID id-GNB-DU-ID CRITICALITY ignore TYPE GNB-DU-ID PRESENCE optional }|

{ ID id-ActivityNotificationLevel CRITICALITY ignore TYPE ActivityNotificationLevel PRESENCE optional },

...

}

System-BearerContextModificationRequest ::= CHOICE {

e-UTRAN-BearerContextModificationRequest ProtocolIE-Container {{EUTRAN-BearerContextModificationRequest}},

nG-RAN-BearerContextModificationRequest ProtocolIE-Container {{NG-RAN-BearerContextModificationRequest}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextModificationRequest-ExtIEs}}

}

System-BearerContextModificationRequest-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

EUTRAN-BearerContextModificationRequest E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-To-Setup-Mod-List-EUTRAN CRITICALITY reject TYPE DRB-To-Setup-Mod-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-To-Modify-List-EUTRAN CRITICALITY reject TYPE DRB-To-Modify-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-To-Remove-List-EUTRAN CRITICALITY reject TYPE DRB-To-Remove-List-EUTRAN PRESENCE optional },

...

}

NG-RAN-BearerContextModificationRequest E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-To-Setup-Mod-List CRITICALITY reject TYPE PDU-Session-Resource-To-Setup-Mod-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-To-Modify-List CRITICALITY reject TYPE PDU-Session-Resource-To-Modify-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-To-Remove-List CRITICALITY reject TYPE PDU-Session-Resource-To-Remove-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Response

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextModificationResponseIEs} },

...

}

BearerContextModificationResponseIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-System-BearerContextModificationResponse CRITICALITY ignore TYPE System-BearerContextModificationResponse PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

System-BearerContextModificationResponse ::= CHOICE {

e-UTRAN-BearerContextModificationResponse ProtocolIE-Container {{EUTRAN-BearerContextModificationResponse}},

nG-RAN-BearerContextModificationResponse ProtocolIE-Container {{NG-RAN-BearerContextModificationResponse}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextModificationResponse-ExtIEs}}

}

System-BearerContextModificationResponse-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

EUTRAN-BearerContextModificationResponse E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-Setup-Mod-List-EUTRAN CRITICALITY ignore TYPE DRB-Setup-Mod-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-Failed-Mod-List-EUTRAN CRITICALITY ignore TYPE DRB-Failed-Mod-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-Modified-List-EUTRAN CRITICALITY ignore TYPE DRB-Modified-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-Failed-To-Modify-List-EUTRAN CRITICALITY ignore TYPE DRB-Failed-To-Modify-List-EUTRAN PRESENCE optional },

...

}

NG-RAN-BearerContextModificationResponse E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-Setup-Mod-List CRITICALITY reject TYPE PDU-Session-Resource-Setup-Mod-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-Failed-Mod-List CRITICALITY reject TYPE PDU-Session-Resource-Failed-Mod-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-Modified-List CRITICALITY reject TYPE PDU-Session-Resource-Modified-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-Failed-To-Modify-List CRITICALITY reject TYPE PDU-Session-Resource-Failed-To-Modify-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Failure

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationFailure ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextModificationFailureIEs} },

...

}

BearerContextModificationFailureIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT MODIFICATION REQUIRED

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Required

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationRequired ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextModificationRequiredIEs} },

...

}

BearerContextModificationRequiredIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-System-BearerContextModificationRequired CRITICALITY reject TYPE System-BearerContextModificationRequired PRESENCE mandatory },

...

}

System-BearerContextModificationRequired ::= CHOICE {

e-UTRAN-BearerContextModificationRequired ProtocolIE-Container {{EUTRAN-BearerContextModificationRequired}},

nG-RAN-BearerContextModificationRequired ProtocolIE-Container {{NG-RAN-BearerContextModificationRequired}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextModificationRequired-ExtIEs}}

}

System-BearerContextModificationRequired-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

EUTRAN-BearerContextModificationRequired E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-Required-To-Modify-List-EUTRAN CRITICALITY reject TYPE DRB-Required-To-Modify-List-EUTRAN PRESENCE optional }|

{ ID id-DRB-Required-To-Remove-List-EUTRAN CRITICALITY reject TYPE DRB-Required-To-Remove-List-EUTRAN PRESENCE optional },

...

}

NG-RAN-BearerContextModificationRequired E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-Required-To-Modify-List CRITICALITY reject TYPE PDU-Session-Resource-Required-To-Modify-List PRESENCE optional }|

{ ID id-PDU-Session-Resource-To-Remove-List CRITICALITY reject TYPE PDU-Session-Resource-To-Remove-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Confirm

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationConfirm ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextModificationConfirmIEs} },

...

}

BearerContextModificationConfirmIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-System-BearerContextModificationConfirm CRITICALITY ignore TYPE System-BearerContextModificationConfirm PRESENCE optional }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

System-BearerContextModificationConfirm ::= CHOICE {

e-UTRAN-BearerContextModificationConfirm ProtocolIE-Container {{EUTRAN-BearerContextModificationConfirm}},

nG-RAN-BearerContextModificationConfirm ProtocolIE-Container {{NG-RAN-BearerContextModificationConfirm}},

choice-extension ProtocolIE-SingleContainer {{System-BearerContextModificationConfirm-ExtIEs}}

}

System-BearerContextModificationConfirm-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

EUTRAN-BearerContextModificationConfirm E1AP-PROTOCOL-IES ::= {

{ ID id-DRB-Confirm-Modified-List-EUTRAN CRITICALITY ignore TYPE DRB-Confirm-Modified-List-EUTRAN PRESENCE optional },

...

}

NG-RAN-BearerContextModificationConfirm E1AP-PROTOCOL-IES ::= {

{ ID id-PDU-Session-Resource-Confirm-Modified-List CRITICALITY ignore TYPE PDU-Session-Resource-Confirm-Modified-List PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT RELEASE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Release Command

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextReleaseCommand ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextReleaseCommandIEs} },

...

}

BearerContextReleaseCommandIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Release Complete

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextReleaseComplete ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextReleaseCompleteIEs} },

...

}

BearerContextReleaseCompleteIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT RELEASE REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Release Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextReleaseRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextReleaseRequestIEs} },

...

}

BearerContextReleaseRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-DRB-Status-List CRITICALITY ignore TYPE DRB-Status-List PRESENCE optional }|

{ ID id-Cause CRITICALITY ignore TYPE Cause PRESENCE mandatory },

...

}

DRB-Status-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRB-Status-Item

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT INACTIVITY NOTIFICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Inactivity Notification

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextInactivityNotification ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { BearerContextInactivityNotificationIEs } },

...

}

BearerContextInactivityNotificationIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-ActivityInformation CRITICALITY reject TYPE ActivityInformation PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- DL DATA NOTIFICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- DL Data Notification

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

DLDataNotification ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { DLDataNotificationIEs } },

...

}

DLDataNotificationIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-PPI CRITICALITY ignore TYPE PPI PRESENCE optional },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UL Data Notification

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ULDataNotification ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { ULDataNotificationIEs } },

...

}

ULDataNotificationIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-PDU-Session-To-Notify-List CRITICALITY reject TYPE PDU-Session-To-Notify-List PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- DATA USAGE REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Data Usage Report

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

DataUsageReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { DataUsageReportIEs } },

...

}

DataUsageReportIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-Data-Usage-Report-List CRITICALITY ignore TYPE Data-Usage-Report-List PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- GNB-CU-UP COUNTER CHECK

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- gNB-CU-UP Counter Check Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-CounterCheckRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { GNB-CU-UP-CounterCheckRequestIEs } },

...

}

GNB-CU-UP-CounterCheckRequestIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

{ ID id-System-GNB-CU-UP-CounterCheckRequest CRITICALITY reject TYPE System-GNB-CU-UP-CounterCheckRequest PRESENCE mandatory },

...

}

System-GNB-CU-UP-CounterCheckRequest ::= CHOICE {

e-UTRAN-GNB-CU-UP-CounterCheckRequest ProtocolIE-Container {{EUTRAN-GNB-CU-UP-CounterCheckRequest}},

nG-RAN-GNB-CU-UP-CounterCheckRequest ProtocolIE-Container {{NG-RAN-GNB-CU-UP-CounterCheckRequest}},

choice-extension ProtocolIE-SingleContainer {{System-GNB-CU-UP-CounterCheckRequest-ExtIEs}}

}

System-GNB-CU-UP-CounterCheckRequest-ExtIEs E1AP-PROTOCOL-IES::= {

...

}

EUTRAN-GNB-CU-UP-CounterCheckRequest E1AP-PROTOCOL-IES ::= {

{ ID id-DRBs-Subject-To-Counter-Check-List-EUTRAN CRITICALITY ignore TYPE DRBs-Subject-To-Counter-Check-List-EUTRAN PRESENCE mandatory },

...

}

NG-RAN-GNB-CU-UP-CounterCheckRequest E1AP-PROTOCOL-IES ::= {

{ ID id-DRBs-Subject-To-Counter-Check-List-NG-RAN CRITICALITY ignore TYPE DRBs-Subject-To-Counter-Check-List-NG-RAN PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- gNB-CU-UP STATUS INDICATION ELEMENTARY PROCEDURE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- gNB-CU-UP Status Indication

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-UP-StatusIndication ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { GNB-CU-UP-StatusIndicationIEs} },

...

}

GNB-CU-UP-StatusIndicationIEs E1AP-PROTOCOL-IES ::= {

{ ID id-TransactionID CRITICALITY reject TYPE TransactionID PRESENCE mandatory }|

{ ID id-GNB-CU-UP-OverloadInformation CRITICALITY reject TYPE GNB-CU-UP-OverloadInformation PRESENCE mandatory },

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- MR-DC DATA USAGE REPORT

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

MRDC-DataUsageReport ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { MRDC-DataUsageReportIEs } },

...

}

MRDC-DataUsageReportIEs E1AP-PROTOCOL-IES ::= {

{ ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory}|

{ ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory}|

{ ID id-PDU-Session-Resource-Data-Usage-List CRITICALITY ignore TYPE PDU-Session-Resource-Data-Usage-List PRESENCE mandatory},

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PRIVATE MESSAGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateMessage ::= SEQUENCE {

privateIEs PrivateIE-Container {{PrivateMessage-IEs}},

...

}

PrivateMessage-IEs E1AP-PRIVATE-IES ::= {

...

}

END

-- ASN1STOP

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

id-CommonNetworkInstance,

id-SNSSAI,

id-OldQoSFlowMap-ULendmarkerexpected,

id-DRB-QoS,

id-endpoint-IP-Address-and-Port,

id-NetworkInstance,

id-QoSFlowMappingIndication,

id-TNLAssociationTransportLayerAddressgNBCUUP,

id-Cause,

id-PDCP-StatusReportIndication,

id-DataForwardingtoNG-RANQoSFlowInformationList,

id-SecurityIndicationModify,

maxnoofErrors,

maxnoofSliceItems,

maxnoofEUTRANQOSParameters,

maxnoofNGRANQOSParameters,

maxnoofDRBs,

maxnoofPDUSessionResource,

maxnoofQoSFlows,

maxnoofUPParameters,

maxnoofCellGroups,

maxnooftimeperiods,

maxnoofNRCGI

FROM E1AP-Constants

Criticality,

ProcedureCode,

ProtocolIE-ID,

TriggeringMessage

FROM E1AP-CommonDataTypes

ProtocolExtensionContainer{},

ProtocolIE-SingleContainer{},

E1AP-PROTOCOL-EXTENSION,

E1AP-PROTOCOL-IES

FROM E1AP-Containers;

-- A

ActivityInformation ::= CHOICE {

dRB-Activity-List DRB-Activity-List,

pDU-Session-Resource-Activity-List PDU-Session-Resource-Activity-List,

uE-Activity UE-Activity,

choice-extension ProtocolIE-SingleContainer {{ActivityInformation-ExtIEs}}

}

ActivityInformation-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

ActivityNotificationLevel ::= ENUMERATED {

drb,

pdu-session,

ue,

...

}

AveragingWindow ::= INTEGER (0..4095, ...)

-- B

BearerContextStatusChange ::= ENUMERATED {

suspend,

resume,

...

}

BitRate ::= INTEGER (0..4000000000000,...)

-- C

Cause ::= CHOICE {

radioNetwork CauseRadioNetwork,

transport CauseTransport,

protocol CauseProtocol,

misc CauseMisc,

choice-extension ProtocolIE-SingleContainer {{Cause-ExtIEs}}

}

Cause-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

CauseMisc ::= ENUMERATED {

control-processing-overload,

not-enough-user-plane-processing-resources,

hardware-failure,

om-intervention,

unspecified,

...

}

CauseProtocol ::= ENUMERATED {

transfer-syntax-error,

abstract-syntax-error-reject,

abstract-syntax-error-ignore-and-notify,

message-not-compatible-with-receiver-state,

semantic-error,

abstract-syntax-error-falsely-constructed-message,

unspecified,

...

}

CauseRadioNetwork ::= ENUMERATED {

unspecified,

unknown-or-already-allocated-gnb-cu-cp-ue-e1ap-id,

unknown-or-already-allocated-gnb-cu-up-ue-e1ap-id,

unknown-or-inconsistent-pair-of-ue-e1ap-id,

interaction-with-other-procedure,

pPDCP-Count-wrap-around,

not-supported-QCI-value,

not-supported-5QI-value,

encryption-algorithms-not-supported,

integrity-protection-algorithms-not-supported,

uP-integrity-protection-not-possible,

uP-confidentiality-protection-not-possible,

multiple-PDU-Session-ID-Instances,

unknown-PDU-Session-ID,

multiple-QoS-Flow-ID-Instances,

unknown-QoS-Flow-ID,

multiple-DRB-ID-Instances,

unknown-DRB-ID,

invalid-QoS-combination,

procedure-cancelled,

normal-release,

no-radio-resources-available,

action-desirable-for-radio-reasons,

resources-not-available-for-the-slice,

pDCP-configuration-not-supported,

...,

ue-dl-max-IP-data-rate-reason,

uP-integrity-protection-failure,

release-due-to-pre-emption

}

CauseTransport ::= ENUMERATED {

unspecified,

transport-resource-unavailable,

...

}

Cell-Group-Information ::= SEQUENCE (SIZE(1.. maxnoofCellGroups)) OF Cell-Group-Information-Item

Cell-Group-Information-Item ::= SEQUENCE {

cell-Group-ID Cell-Group-ID,

uL-Configuration UL-Configuration OPTIONAL,

dL-TX-Stop DL-TX-Stop OPTIONAL,

rAT-Type RAT-Type OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { Cell-Group-Information-Item-ExtIEs } } OPTIONAL,

...

}

Cell-Group-Information-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Cell-Group-ID ::= INTEGER (0..3, ...)

CipheringAlgorithm ::= ENUMERATED {

nEA0,

c-128-NEA1,

c-128-NEA2,

c-128-NEA3,

...

}

CNSupport ::= ENUMERATED {

c-epc,

c-5gc,

both,

...

}

CommonNetworkInstance ::= OCTET STRING

ConfidentialityProtectionIndication ::= ENUMERATED {

required,

preferred,

not-needed,

...

}

ConfidentialityProtectionResult ::= ENUMERATED {

performed,

not-performed,

...

}

CP-TNL-Information ::= CHOICE {

endpoint-IP-Address TransportLayerAddress,

choice-extension ProtocolIE-SingleContainer {{CP-TNL-Information-ExtIEs}}

}

CP-TNL-Information-ExtIEs E1AP-PROTOCOL-IES ::= {

{ ID id-endpoint-IP-Address-and-Port CRITICALITY reject TYPE Endpoint-IP-address-and-port PRESENCE mandatory},

...

}

CriticalityDiagnostics ::= SEQUENCE {

procedureCode ProcedureCode OPTIONAL,

triggeringMessage TriggeringMessage OPTIONAL,

procedureCriticality Criticality OPTIONAL,

transactionID TransactionID OPTIONAL,

iEsCriticalityDiagnostics CriticalityDiagnostics-IE-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

CriticalityDiagnostics-IE-List ::= SEQUENCE (SIZE (1..maxnoofErrors)) OF

SEQUENCE {

iECriticality Criticality,

iE-ID ProtocolIE-ID,

typeOfError TypeOfError,

iE-Extensions ProtocolExtensionContainer { {CriticalityDiagnostics-IE-List-ExtIEs} } OPTIONAL,

...

}

CriticalityDiagnostics-IE-List-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- D

Data-Forwarding-Information-Request ::= SEQUENCE {

data-Forwarding-Request Data-Forwarding-Request,

qoS-Flows-Forwarded-On-Fwd-Tunnels QoS-Flow-Mapping-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { Data-Forwarding-Information-Request-ExtIEs } } OPTIONAL,

...

}

Data-Forwarding-Information-Request-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Data-Forwarding-Information ::= SEQUENCE {

uL-Data-Forwarding UP-TNL-Information OPTIONAL,

dL-Data-Forwarding UP-TNL-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { Data-Forwarding-Information-ExtIEs } } OPTIONAL,

...

}

Data-Forwarding-Information-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-DataForwardingtoNG-RANQoSFlowInformationList CRITICALITY ignore EXTENSION DataForwardingtoNG-RANQoSFlowInformationList PRESENCE optional},

...

}

Data-Forwarding-Request ::= ENUMERATED {

uL,

dL,

both,

...

}

Data-Usage-per-PDU-Session-Report ::= SEQUENCE {

secondaryRATType ENUMERATED {nR, e-UTRA, ...},

pDU-session-Timed-Report-List SEQUENCE (SIZE(1..maxnooftimeperiods)) OF MRDC-Data-Usage-Report-Item,

iE-Extensions ProtocolExtensionContainer { { Data-Usage-per-PDU-Session-Report-ExtIEs} } OPTIONAL,

...

}

Data-Usage-per-PDU-Session-Report-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Data-Usage-per-QoS-Flow-List ::= SEQUENCE (SIZE(1..maxnoofQoSFlows)) OF Data-Usage-per-QoS-Flow-Item

Data-Usage-per-QoS-Flow-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

secondaryRATType ENUMERATED {nR, e-UTRA, ...},

qoS-Flow-Timed-Report-List SEQUENCE (SIZE(1..maxnooftimeperiods)) OF MRDC-Data-Usage-Report-Item,

iE-Extensions ProtocolExtensionContainer { { Data-Usage-per-QoS-Flow-Item-ExtIEs} } OPTIONAL,

...

}

Data-Usage-per-QoS-Flow-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Data-Usage-Report-List ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF Data-Usage-Report-Item

Data-Usage-Report-Item ::= SEQUENCE {

dRB-ID DRB-ID,

rAT-Type RAT-Type,

dRB-Usage-Report-List DRB-Usage-Report-List,

iE-Extensions ProtocolExtensionContainer { { Data-Usage-Report-ItemExtIEs } } OPTIONAL,

...

}

Data-Usage-Report-ItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DefaultDRB ::= ENUMERATED {

true,

false,

...

}

DiscardTimer ::= ENUMERATED {ms10, ms20, ms30, ms40, ms50, ms60, ms75, ms100, ms150, ms200, ms250, ms300, ms500, ms750, ms1500, infinity}

DL-TX-Stop ::= ENUMERATED {

stop,

resume,

...

}

DRB-Activity ::= ENUMERATED {

active,

not-active,

...

}

DRB-Activity-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRB-Activity-Item

DRB-Activity-Item ::= SEQUENCE {

dRB-ID DRB-ID,

dRB-Activity DRB-Activity,

iE-Extensions ProtocolExtensionContainer { { DRB-Activity-ItemExtIEs } } OPTIONAL,

...

}

DRB-Activity-ItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Confirm-Modified-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Confirm-Modified-Item-EUTRAN

DRB-Confirm-Modified-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

cell-Group-Information Cell-Group-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Confirm-Modified-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Confirm-Modified-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Confirm-Modified-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Confirm-Modified-Item-NG-RAN

DRB-Confirm-Modified-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

cell-Group-Information Cell-Group-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Confirm-Modified-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Confirm-Modified-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-Item-EUTRAN

DRB-Failed-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-Mod-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-Mod-Item-EUTRAN

DRB-Failed-Mod-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-Mod-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-Mod-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-Item-NG-RAN

DRB-Failed-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-Mod-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-Mod-Item-NG-RAN

DRB-Failed-Mod-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-Mod-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-Mod-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-To-Modify-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-To-Modify-Item-EUTRAN

DRB-Failed-To-Modify-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-To-Modify-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-To-Modify-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Failed-To-Modify-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Failed-To-Modify-Item-NG-RAN

DRB-Failed-To-Modify-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Failed-To-Modify-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Failed-To-Modify-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-ID ::= INTEGER (1..32, ...)

DRB-Modified-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Modified-Item-EUTRAN

DRB-Modified-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

s1-DL-UP-TNL-Information UP-TNL-Information OPTIONAL,

pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

uL-UP-Transport-Parameters UP-Parameters OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Modified-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Modified-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Modified-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Modified-Item-NG-RAN

DRB-Modified-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

uL-UP-Transport-Parameters UP-Parameters OPTIONAL,

pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

flow-Setup-List QoS-Flow-List OPTIONAL,

flow-Failed-List QoS-Flow-Failed-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Modified-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Modified-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-OldQoSFlowMap-ULendmarkerexpected CRITICALITY ignore EXTENSION QoS-Flow-List PRESENCE optional},

...

}

DRB-Required-To-Modify-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Required-To-Modify-Item-EUTRAN

DRB-Required-To-Modify-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

s1-DL-UP-TNL-Information UP-TNL-Information OPTIONAL,

gNB-CU-UP-CellGroupRelatedConfiguration GNB-CU-UP-CellGroupRelatedConfiguration OPTIONAL,

cause Cause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Required-To-Modify-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Required-To-Modify-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Required-To-Modify-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Required-To-Modify-Item-NG-RAN

DRB-Required-To-Modify-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

gNB-CU-UP-CellGroupRelatedConfiguration GNB-CU-UP-CellGroupRelatedConfiguration OPTIONAL,

flow-To-Remove QoS-Flow-List OPTIONAL,

cause Cause OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Required-To-Modify-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Required-To-Modify-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Setup-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Setup-Item-EUTRAN

DRB-Setup-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

s1-DL-UP-TNL-Information UP-TNL-Information,

data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

uL-UP-Transport-Parameters UP-Parameters,

s1-DL-UP-Unchanged ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Setup-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Setup-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Setup-Mod-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Setup-Mod-Item-EUTRAN

DRB-Setup-Mod-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

s1-DL-UP-TNL-Information UP-TNL-Information,

data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

uL-UP-Transport-Parameters UP-Parameters,

iE-Extensions ProtocolExtensionContainer { { DRB-Setup-Mod-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Setup-Mod-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Setup-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Setup-Item-NG-RAN

DRB-Setup-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

dRB-data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

uL-UP-Transport-Parameters UP-Parameters,

flow-Setup-List QoS-Flow-List,

flow-Failed-List QoS-Flow-Failed-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Setup-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Setup-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Setup-Mod-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Setup-Mod-Item-NG-RAN

DRB-Setup-Mod-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

dRB-data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

uL-UP-Transport-Parameters UP-Parameters,

flow-Setup-List QoS-Flow-List,

flow-Failed-List QoS-Flow-Failed-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Setup-Mod-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Setup-Mod-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Status-Item ::= SEQUENCE {

dRB-ID DRB-ID,

pDCP-DL-Count PDCP-Count OPTIONAL,

pDCP-UL-Count PDCP-Count OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-Status-ItemExtIEs } } OPTIONAL,

...

}

DRB-Status-ItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRBs-Subject-To-Counter-Check-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRBs-Subject-To-Counter-Check-Item-EUTRAN

DRBs-Subject-To-Counter-Check-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

pDCP-UL-Count PDCP-Count,

pDCP-DL-Count PDCP-Count,

iE-Extensions ProtocolExtensionContainer { { DRBs-Subject-To-Counter-Check-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRBs-Subject-To-Counter-Check-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRBs-Subject-To-Counter-Check-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRBs-Subject-To-Counter-Check-Item-NG-RAN

DRBs-Subject-To-Counter-Check-Item-NG-RAN ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

dRB-ID DRB-ID,

pDCP-UL-Count PDCP-Count,

pDCP-DL-Count PDCP-Count,

iE-Extensions ProtocolExtensionContainer { { DRBs-Subject-To-Counter-Check-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRBs-Subject-To-Counter-Check-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Modify-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Modify-Item-EUTRAN

DRB-To-Modify-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

pDCP-Configuration PDCP-Configuration OPTIONAL,

eUTRAN-QoS EUTRAN-QoS OPTIONAL,

s1-UL-UP-TNL-Information UP-TNL-Information OPTIONAL,

data-Forwarding-Information Data-Forwarding-Information OPTIONAL,

pDCP-SN-Status-Request PDCP-SN-Status-Request OPTIONAL,

pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

dL-UP-Parameters UP-Parameters OPTIONAL,

cell-Group-To-Add Cell-Group-Information OPTIONAL,

cell-Group-To-Modify Cell-Group-Information OPTIONAL,

cell-Group-To-Remove Cell-Group-Information OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Modify-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Modify-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Modify-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Modify-Item-NG-RAN

DRB-To-Modify-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

sDAP-Configuration SDAP-Configuration OPTIONAL,

pDCP-Configuration PDCP-Configuration OPTIONAL,

dRB-Data-Forwarding-Information Data-Forwarding-Information OPTIONAL,

pDCP-SN-Status-Request PDCP-SN-Status-Request OPTIONAL,

pdcp-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

dL-UP-Parameters UP-Parameters OPTIONAL,

cell-Group-To-Add Cell-Group-Information OPTIONAL,

cell-Group-To-Modify Cell-Group-Information OPTIONAL,

cell-Group-To-Remove Cell-Group-Information OPTIONAL,

flow-Mapping-Information QoS-Flow-QoS-Parameter-List OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Modify-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Modify-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-OldQoSFlowMap-ULendmarkerexpected CRITICALITY reject EXTENSION QoS-Flow-List PRESENCE optional}|

{ID id-DRB-QoS CRITICALITY ignore EXTENSION QoSFlowLevelQoSParameters PRESENCE optional},

...

}

DRB-To-Remove-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Remove-Item-EUTRAN

DRB-To-Remove-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Remove-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Remove-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Required-To-Remove-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Required-To-Remove-Item-EUTRAN

DRB-Required-To-Remove-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Required-To-Remove-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-Required-To-Remove-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Remove-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Remove-Item-NG-RAN

DRB-To-Remove-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Remove-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Remove-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-Required-To-Remove-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-Required-To-Remove-Item-NG-RAN

DRB-Required-To-Remove-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { DRB-Required-To-Remove-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-Required-To-Remove-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Setup-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Item-EUTRAN

DRB-To-Setup-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

pDCP-Configuration PDCP-Configuration,

eUTRAN-QoS EUTRAN-QoS,

s1-UL-UP-TNL-Information UP-TNL-Information,

data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

cell-Group-Information Cell-Group-Information,

dL-UP-Parameters UP-Parameters OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

existing-Allocated-S1-DL-UP-TNL-Info UP-TNL-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Setup-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Setup-Mod-List-EUTRAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Mod-Item-EUTRAN

DRB-To-Setup-Mod-Item-EUTRAN ::= SEQUENCE {

dRB-ID DRB-ID,

pDCP-Configuration PDCP-Configuration,

eUTRAN-QoS EUTRAN-QoS,

s1-UL-UP-TNL-Information UP-TNL-Information,

data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

cell-Group-Information Cell-Group-Information,

dL-UP-Parameters UP-Parameters OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Mod-Item-EUTRAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Setup-Mod-Item-EUTRAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRB-To-Setup-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Item-NG-RAN

DRB-To-Setup-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

sDAP-Configuration SDAP-Configuration,

pDCP-Configuration PDCP-Configuration,

cell-Group-Information Cell-Group-Information,

qos-flow-Information-To-Be-Setup QoS-Flow-QoS-Parameter-List,

dRB-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Setup-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-DRB-QoS CRITICALITY ignore EXTENSION QoSFlowLevelQoSParameters PRESENCE optional},

...

}

DRB-To-Setup-Mod-List-NG-RAN ::= SEQUENCE (SIZE(1.. maxnoofDRBs)) OF DRB-To-Setup-Mod-Item-NG-RAN

DRB-To-Setup-Mod-Item-NG-RAN ::= SEQUENCE {

dRB-ID DRB-ID,

sDAP-Configuration SDAP-Configuration,

pDCP-Configuration PDCP-Configuration,

cell-Group-Information Cell-Group-Information,

flow-Mapping-Information QoS-Flow-QoS-Parameter-List,

dRB-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

dRB-Inactivity-Timer Inactivity-Timer OPTIONAL,

pDCP-SN-Status-Information PDCP-SN-Status-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { DRB-To-Setup-Mod-Item-NG-RAN-ExtIEs } } OPTIONAL,

...

}

DRB-To-Setup-Mod-Item-NG-RAN-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-DRB-QoS CRITICALITY ignore EXTENSION QoSFlowLevelQoSParameters PRESENCE optional},

...

}

DRB-Usage-Report-List ::= SEQUENCE (SIZE(1..maxnooftimeperiods)) OF DRB-Usage-Report-Item

DRB-Usage-Report-Item ::= SEQUENCE {

startTimeStamp OCTET STRING (SIZE(4)),

endTimeStamp OCTET STRING (SIZE(4)),

usageCountUL INTEGER (0..18446744073709551615),

usageCountDL INTEGER (0..18446744073709551615),

iE-Extensions ProtocolExtensionContainer { { DRB-Usage-Report-Item-ExtIEs} } OPTIONAL,

...

}

DRB-Usage-Report-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Duplication-Activation ::= ENUMERATED {

active,

inactive,

...

}

Dynamic5QIDescriptor ::= SEQUENCE {

qoSPriorityLevel QoSPriorityLevel,

packetDelayBudget PacketDelayBudget,

packetErrorRate PacketErrorRate,

fiveQI INTEGER (0..255, ...) OPTIONAL,

delayCritical ENUMERATED {delay-critical, non-delay-critical} OPTIONAL,

averagingWindow AveragingWindow OPTIONAL,

maxDataBurstVolume MaxDataBurstVolume OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { Dynamic5QIDescriptor-ExtIEs } } OPTIONAL

}

Dynamic5QIDescriptor-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DataDiscardRequired ::= ENUMERATED {

required,

...

}

-- E

EncryptionKey ::= OCTET STRING

Endpoint-IP-address-and-port::= SEQUENCE {

endpoint-IP-Address TransportLayerAddress,

portNumber PortNumber,

iE-Extensions ProtocolExtensionContainer { { Endpoint-IP-address-and-port-ExtIEs} } OPTIONAL

}

Endpoint-IP-address-and-port-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

EUTRANAllocationAndRetentionPriority ::= SEQUENCE {

priorityLevel PriorityLevel,

pre-emptionCapability Pre-emptionCapability,

pre-emptionVulnerability Pre-emptionVulnerability,

iE-Extensions ProtocolExtensionContainer { {EUTRANAllocationAndRetentionPriority-ExtIEs} } OPTIONAL,

...

}

EUTRANAllocationAndRetentionPriority-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

EUTRAN-QoS-Support-List ::= SEQUENCE (SIZE(1.. maxnoofEUTRANQOSParameters)) OF EUTRAN-QoS-Support-Item

EUTRAN-QoS-Support-Item ::= SEQUENCE {

eUTRAN-QoS EUTRAN-QoS,

iE-Extensions ProtocolExtensionContainer { { EUTRAN-QoS-Support-Item-ExtIEs } } OPTIONAL

}

EUTRAN-QoS-Support-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

EUTRAN-QoS ::= SEQUENCE {

qCI QCI,

eUTRANallocationAndRetentionPriority EUTRANAllocationAndRetentionPriority,

gbrQosInformation GBR-QosInformation OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { EUTRAN-QoS-ExtIEs } } OPTIONAL,

...

}

EUTRAN-QoS-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- F

-- G

GNB-CU-CP-Name ::= PrintableString(SIZE(1..150,...))

GNB-CU-CP-UE-E1AP-ID ::= INTEGER (0..4294967295)

GNB-CU-UP-Capacity ::= INTEGER (0..255)

GNB-CU-UP-CellGroupRelatedConfiguration ::= SEQUENCE (SIZE(1.. maxnoofUPParameters)) OF GNB-CU-UP-CellGroupRelatedConfiguration-Item

GNB-CU-UP-CellGroupRelatedConfiguration-Item ::= SEQUENCE {

cell-Group-ID Cell-Group-ID,

uP-TNL-Information UP-TNL-Information,

uL-Configuration UL-Configuration OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {GNB-CU-UP-CellGroupRelatedConfiguration-Item-ExtIEs } } OPTIONAL

}

GNB-CU-UP-CellGroupRelatedConfiguration-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-UP-ID ::= INTEGER (0..68719476735)

GNB-CU-UP-Name ::= PrintableString(SIZE(1..150,...))

GNB-CU-UP-UE-E1AP-ID ::= INTEGER (0..4294967295)

GNB-CU-CP-TNLA-Setup-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-CP-TNLA-Setup-Item-ExtIEs} } OPTIONAL,

...

}

GNB-CU-CP-TNLA-Setup-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-CP-TNLA-Failed-To-Setup-Item ::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-CP-TNLA-Failed-To-Setup-Item-ExtIEs} } OPTIONAL

}

GNB-CU-CP-TNLA-Failed-To-Setup-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-CP-TNLA-To-Add-Item ::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

tNLAssociationUsage TNLAssociationUsage,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-CP-TNLA-To-Add-Item-ExtIEs} } OPTIONAL

}

GNB-CU-CP-TNLA-To-Add-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-CP-TNLA-To-Remove-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-CP-TNLA-To-Remove-Item-ExtIEs} } OPTIONAL

}

GNB-CU-CP-TNLA-To-Remove-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-TNLAssociationTransportLayerAddressgNBCUUP CRITICALITY reject EXTENSION CP-TNL-Information PRESENCE optional},

...

}

GNB-CU-CP-TNLA-To-Update-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

tNLAssociationUsage TNLAssociationUsage OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-CP-TNLA-To-Update-Item-ExtIEs} } OPTIONAL

}

GNB-CU-CP-TNLA-To-Update-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-UP-TNLA-To-Remove-Item::= SEQUENCE {

tNLAssociationTransportLayerAddress CP-TNL-Information,

tNLAssociationTransportLayerAddressgNBCUCP CP-TNL-Information OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GNB-CU-UP-TNLA-To-Remove-Item-ExtIEs} } OPTIONAL

}

GNB-CU-UP-TNLA-To-Remove-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GBR-QosInformation ::= SEQUENCE {

e-RAB-MaximumBitrateDL BitRate,

e-RAB-MaximumBitrateUL BitRate,

e-RAB-GuaranteedBitrateDL BitRate,

e-RAB-GuaranteedBitrateUL BitRate,

iE-Extensions ProtocolExtensionContainer { { GBR-QosInformation-ExtIEs} } OPTIONAL,

...

}

GBR-QosInformation-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GBR-QoSFlowInformation::= SEQUENCE {

maxFlowBitRateDownlink BitRate,

maxFlowBitRateUplink BitRate,

guaranteedFlowBitRateDownlink BitRate,

guaranteedFlowBitRateUplink BitRate,

maxPacketLossRateDownlink MaxPacketLossRate OPTIONAL,

maxPacketLossRateUplink MaxPacketLossRate OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { GBR-QosFlowInformation-ExtIEs} } OPTIONAL,

...

}

GBR-QosFlowInformation-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GTP-TEID ::= OCTET STRING (SIZE (4))

GTPTunnel ::= SEQUENCE {

transportLayerAddress TransportLayerAddress,

gTP-TEID GTP-TEID,

iE-Extensions ProtocolExtensionContainer { { GTPTunnel-ExtIEs} } OPTIONAL,

...

}

GTPTunnel-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

GNB-CU-UP-OverloadInformation ::= ENUMERATED {overloaded, not-overloaded}

GNB-DU-ID ::= INTEGER (0..68719476735)

-- H

HFN ::= INTEGER (0..4294967295)

-- I

IntegrityProtectionIndication ::= ENUMERATED {

required,

preferred,

not-needed,

...

}

IntegrityProtectionAlgorithm ::= ENUMERATED {

nIA0,

i-128-NIA1,

i-128-NIA2,

i-128-NIA3,

...

}

IntegrityProtectionKey ::= OCTET STRING

IntegrityProtectionResult ::= ENUMERATED {

performed,

not-performed,

...

}

Inactivity-Timer ::= INTEGER (1..7200, ...)

-- J

-- K

-- L

-- M

MaxDataBurstVolume ::= INTEGER (0..4095, ...)

MaximumIPdatarate ::= SEQUENCE {

maxIPrate MaxIPrate,

iE-Extensions ProtocolExtensionContainer { {MaximumIPdatarate-ExtIEs} } OPTIONAL,

...

}

MaximumIPdatarate-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

MaxIPrate ::= ENUMERATED {

bitrate64kbs,

max-UErate,

...

}

MaxPacketLossRate ::= INTEGER (0..1000, ...)

MRDC-Data-Usage-Report-Item ::= SEQUENCE {

startTimeStamp OCTET STRING (SIZE(4)),

endTimeStamp OCTET STRING (SIZE(4)),

usageCountUL INTEGER (0..18446744073709551615),

usageCountDL INTEGER (0..18446744073709551615),

iE-Extensions ProtocolExtensionContainer { { MRDC-Data-Usage-Report-Item-ExtIEs} } OPTIONAL,

...

}

MRDC-Data-Usage-Report-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

MRDC-Usage-Information ::= SEQUENCE {

data-Usage-per-PDU-Session-Report Data-Usage-per-PDU-Session-Report OPTIONAL,

data-Usage-per-QoS-Flow-List Data-Usage-per-QoS-Flow-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { MRDC-Usage-Information-ExtIEs} } OPTIONAL,

...

}

MRDC-Usage-Information-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- N

NetworkInstance ::= INTEGER (1..256, ...)

New-UL-TNL-Information-Required::= ENUMERATED {

required,

...

}

NGRANAllocationAndRetentionPriority ::= SEQUENCE {

priorityLevel PriorityLevel,

pre-emptionCapability Pre-emptionCapability,

pre-emptionVulnerability Pre-emptionVulnerability,

iE-Extensions ProtocolExtensionContainer { {NGRANAllocationAndRetentionPriority-ExtIEs} } OPTIONAL

}

NGRANAllocationAndRetentionPriority-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

NG-RAN-QoS-Support-List ::= SEQUENCE (SIZE(1.. maxnoofNGRANQOSParameters)) OF NG-RAN-QoS-Support-Item

NG-RAN-QoS-Support-Item ::= SEQUENCE {

non-Dynamic5QIDescriptor Non-Dynamic5QIDescriptor,

iE-Extensions ProtocolExtensionContainer { { NG-RAN-QoS-Support-Item-ExtIEs } } OPTIONAL

}

NG-RAN-QoS-Support-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Non-Dynamic5QIDescriptor ::= SEQUENCE {

fiveQI INTEGER (0..255, ...),

qoSPriorityLevel QoSPriorityLevel OPTIONAL,

averagingWindow AveragingWindow OPTIONAL,

maxDataBurstVolume MaxDataBurstVolume OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { Non-Dynamic5QIDescriptor-ExtIEs } } OPTIONAL

}

Non-Dynamic5QIDescriptor-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

NR-Cell-Identity ::= BIT STRING (SIZE(36))

NR-CGI ::= SEQUENCE {

pLMN-Identity PLMN-Identity,

nR-Cell-Identity NR-Cell-Identity,

iE-Extensions ProtocolExtensionContainer { { NR-CGI-ExtIEs } } OPTIONAL

}

NR-CGI-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

NR-CGI-Support-List ::= SEQUENCE (SIZE(1.. maxnoofNRCGI)) OF NR-CGI-Support-Item

NR-CGI-Support-Item ::= SEQUENCE {

nR-CGI NR-CGI,

iE-Extensions ProtocolExtensionContainer { { NR-CGI-Support-Item-ExtIEs } } OPTIONAL

}

NR-CGI-Support-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- O

OutOfOrderDelivery ::= ENUMERATED {

true,

...

}

-- P

PacketDelayBudget ::= INTEGER (0..1023, ...)

PacketErrorRate ::= SEQUENCE {

pER-Scalar PER-Scalar,

pER-Exponent PER-Exponent,

iE-Extensions ProtocolExtensionContainer { {PacketErrorRate-ExtIEs} } OPTIONAL,

...

}

PacketErrorRate-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PER-Scalar ::= INTEGER (0..9, ...)

PER-Exponent ::= INTEGER (0..9, ...)

PDCP-Configuration ::= SEQUENCE {

pDCP-SN-Size-UL PDCP-SN-Size,

pDCP-SN-Size-DL PDCP-SN-Size,

rLC-Mode RLC-Mode,

rOHC-Parameters ROHC-Parameters OPTIONAL,

t-ReorderingTimer T-ReorderingTimer OPTIONAL,

discardTimer DiscardTimer OPTIONAL,

uLDataSplitThreshold ULDataSplitThreshold OPTIONAL,

pDCP-Duplication PDCP-Duplication OPTIONAL,

pDCP-Reestablishment PDCP-Reestablishment OPTIONAL,

pDCP-DataRecovery PDCP-DataRecovery OPTIONAL,

duplication-Activation Duplication-Activation OPTIONAL,

outOfOrderDelivery OutOfOrderDelivery OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDCP-Configuration-ExtIEs } } OPTIONAL,

...

}

PDCP-Configuration-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-PDCP-StatusReportIndication CRITICALITY ignore EXTENSION PDCP-StatusReportIndication PRESENCE optional},

...

}

PDCP-Count ::= SEQUENCE {

pDCP-SN PDCP-SN,

hFN HFN,

iE-Extensions ProtocolExtensionContainer { { PDCP-Count-ExtIEs } } OPTIONAL,

...

}

PDCP-Count-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDCP-SN-Status-Request ::= ENUMERATED {

requested,

...

}

PDCP-DataRecovery ::= ENUMERATED {

true,

...

}

PDCP-Duplication ::= ENUMERATED {

true,

...

}

PDCP-Reestablishment ::= ENUMERATED {

true,

...

}

PDU-Session-Resource-Data-Usage-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Data-Usage-Item

PDU-Session-Resource-Data-Usage-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

mRDC-Usage-Information MRDC-Usage-Information,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Data-Usage-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Data-Usage-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDCP-SN ::= INTEGER (0..262143)

PDCP-SN-Size ::= ENUMERATED {

s-12,

s-18,

...

}

PDCP-SN-Status-Information ::= SEQUENCE {

pdcpStatusTransfer-UL DRBBStatusTransfer,

pdcpStatusTransfer-DL PDCP-Count,

iE-Extension ProtocolExtensionContainer { {DRBsSubjectToStatusTransfer-Item-ExtIEs} } OPTIONAL,

...

}

PDCP-StatusReportIndication ::= ENUMERATED {

downlink,

uplink,

both,

...

}

DRBsSubjectToStatusTransfer-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DRBBStatusTransfer ::= SEQUENCE {

receiveStatusofPDCPSDU BIT STRING (SIZE(1..131072)) OPTIONAL,

countValue PDCP-Count,

iE-Extension ProtocolExtensionContainer { {DRBBStatusTransfer-ExtIEs} } OPTIONAL,

...

}

DRBBStatusTransfer-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-ID ::= INTEGER (0..255)

PDU-Session-Resource-Activity ::= ENUMERATED {

active,

not-active,

...

}

PDU-Session-Resource-Activity-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Activity-Item

PDU-Session-Resource-Activity-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

pDU-Session-Resource-Activity PDU-Session-Resource-Activity,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Activity-ItemExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Activity-ItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Confirm-Modified-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Confirm-Modified-Item

PDU-Session-Resource-Confirm-Modified-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

dRB-Confirm-Modified-List-NG-RAN DRB-Confirm-Modified-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Confirm-Modified-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Confirm-Modified-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Failed-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Failed-Item

PDU-Session-Resource-Failed-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Failed-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Failed-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Failed-Mod-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Failed-Mod-Item

PDU-Session-Resource-Failed-Mod-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Failed-Mod-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Failed-Mod-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Failed-To-Modify-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Failed-To-Modify-Item

PDU-Session-Resource-Failed-To-Modify-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Failed-To-Modify-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Failed-To-Modify-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Modified-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Modified-Item

PDU-Session-Resource-Modified-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

nG-DL-UP-TNL-Information UP-TNL-Information OPTIONAL,

securityResult SecurityResult OPTIONAL,

pDU-Session-Data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

dRB-Setup-List-NG-RAN DRB-Setup-List-NG-RAN OPTIONAL,

dRB-Failed-List-NG-RAN DRB-Failed-List-NG-RAN OPTIONAL,

dRB-Modified-List-NG-RAN DRB-Modified-List-NG-RAN OPTIONAL,

dRB-Failed-To-Modify-List-NG-RAN DRB-Failed-To-Modify-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Modified-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Modified-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Required-To-Modify-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Required-To-Modify-Item

PDU-Session-Resource-Required-To-Modify-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

nG-DL-UP-TNL-Information UP-TNL-Information OPTIONAL,

dRB-Required-To-Modify-List-NG-RAN DRB-Required-To-Modify-List-NG-RAN OPTIONAL,

dRB-Required-To-Remove-List-NG-RAN DRB-Required-To-Remove-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Required-To-Modify-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Required-To-Modify-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Setup-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Setup-Item

PDU-Session-Resource-Setup-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

securityResult SecurityResult OPTIONAL,

nG-DL-UP-TNL-Information UP-TNL-Information,

pDU-Session-Data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

nG-DL-UP-Unchanged ENUMERATED {true, ...} OPTIONAL,

dRB-Setup-List-NG-RAN DRB-Setup-List-NG-RAN,

dRB-Failed-List-NG-RAN DRB-Failed-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Setup-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Setup-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-Setup-Mod-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-Setup-Mod-Item

PDU-Session-Resource-Setup-Mod-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

securityResult SecurityResult OPTIONAL,

nG-DL-UP-TNL-Information UP-TNL-Information,

pDU-Session-Data-Forwarding-Information-Response Data-Forwarding-Information OPTIONAL,

dRB-Setup-Mod-List-NG-RAN DRB-Setup-Mod-List-NG-RAN,

dRB-Failed-Mod-List-NG-RAN DRB-Failed-Mod-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-Setup-Mod-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-Setup-Mod-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Resource-To-Modify-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-To-Modify-Item

PDU-Session-Resource-To-Modify-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

securityIndication SecurityIndication OPTIONAL,

pDU-Session-Resource-DL-AMBR BitRate OPTIONAL,

nG-UL-UP-TNL-Information UP-TNL-Information OPTIONAL,

pDU-Session-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

pDU-Session-Data-Forwarding-Information Data-Forwarding-Information OPTIONAL,

pDU-Session-Inactivity-Timer Inactivity-Timer OPTIONAL,

networkInstance NetworkInstance OPTIONAL,

dRB-To-Setup-List-NG-RAN DRB-To-Setup-List-NG-RAN OPTIONAL,

dRB-To-Modify-List-NG-RAN DRB-To-Modify-List-NG-RAN OPTIONAL,

dRB-To-Remove-List-NG-RAN DRB-To-Remove-List-NG-RAN OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-To-Modify-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-To-Modify-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-SNSSAI CRITICALITY reject EXTENSION SNSSAI PRESENCE optional }|

{ID id-CommonNetworkInstance CRITICALITY ignore EXTENSION CommonNetworkInstance PRESENCE optional }|

{ID id-SecurityIndicationModify CRITICALITY ignore EXTENSION SecurityIndication PRESENCE optional },

...

}

PDU-Session-Resource-To-Remove-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-To-Remove-Item

PDU-Session-Resource-To-Remove-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-To-Remove-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-To-Remove-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-Cause CRITICALITY ignore EXTENSION Cause PRESENCE optional},

...

}

PDU-Session-Resource-To-Setup-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-To-Setup-Item

PDU-Session-Resource-To-Setup-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

pDU-Session-Type PDU-Session-Type,

sNSSAI SNSSAI,

securityIndication SecurityIndication,

pDU-Session-Resource-DL-AMBR BitRate OPTIONAL,

nG-UL-UP-TNL-Information UP-TNL-Information,

pDU-Session-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

pDU-Session-Inactivity-Timer Inactivity-Timer OPTIONAL,

existing-Allocated-NG-DL-UP-TNL-Info UP-TNL-Information OPTIONAL,

networkInstance NetworkInstance OPTIONAL,

dRB-To-Setup-List-NG-RAN DRB-To-Setup-List-NG-RAN,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-To-Setup-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-To-Setup-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ ID id-CommonNetworkInstance CRITICALITY ignore EXTENSION CommonNetworkInstance PRESENCE optional },

...

}

PDU-Session-Resource-To-Setup-Mod-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-Resource-To-Setup-Mod-Item

PDU-Session-Resource-To-Setup-Mod-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

pDU-Session-Type PDU-Session-Type,

sNSSAI SNSSAI,

securityIndication SecurityIndication,

pDU-Session-Resource-AMBR BitRate OPTIONAL,

nG-UL-UP-TNL-Information UP-TNL-Information,

pDU-Session-Data-Forwarding-Information-Request Data-Forwarding-Information-Request OPTIONAL,

pDU-Session-Inactivity-Timer Inactivity-Timer OPTIONAL,

dRB-To-Setup-Mod-List-NG-RAN DRB-To-Setup-Mod-List-NG-RAN,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-Resource-To-Setup-Mod-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-Resource-To-Setup-Mod-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-NetworkInstance CRITICALITY ignore EXTENSION NetworkInstance PRESENCE optional}|

{ID id-CommonNetworkInstance CRITICALITY ignore EXTENSION CommonNetworkInstance PRESENCE optional},

...

}

PDU-Session-To-Notify-List ::= SEQUENCE (SIZE(1.. maxnoofPDUSessionResource)) OF PDU-Session-To-Notify-Item

PDU-Session-To-Notify-Item ::= SEQUENCE {

pDU-Session-ID PDU-Session-ID,

qoS-Flow-List QoS-Flow-List,

iE-Extensions ProtocolExtensionContainer { { PDU-Session-To-Notify-Item-ExtIEs } } OPTIONAL,

...

}

PDU-Session-To-Notify-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

PDU-Session-Type ::= ENUMERATED {

ipv4,

ipv6,

ipv4v6,

ethernet,

unstructured,

...

}

PLMN-Identity ::= OCTET STRING (SIZE(3))

PortNumber ::= BIT STRING (SIZE(16))

PPI ::= INTEGER (0..7, ...)

PriorityLevel ::= INTEGER { spare (0), highest (1), lowest (14), no-priority (15) } (0..15)

Pre-emptionCapability ::= ENUMERATED {

shall-not-trigger-pre-emption,

may-trigger-pre-emption

}

Pre-emptionVulnerability ::= ENUMERATED {

not-pre-emptable,

pre-emptable

}

-- Q

QCI ::= INTEGER (0..255)

QoS-Characteristics ::= CHOICE {

non-Dynamic-5QI Non-Dynamic5QIDescriptor,

dynamic-5QI Dynamic5QIDescriptor,

choice-extension ProtocolIE-SingleContainer {{QoS-Characteristics-ExtIEs}}

}

QoS-Characteristics-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

QoS-Flow-Identifier ::= INTEGER (0..63)

QoS-Flow-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoS-Flow-Item

QoS-Flow-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

iE-Extensions ProtocolExtensionContainer { { QoS-Flow-Item-ExtIEs } } OPTIONAL,

...

}

QoS-Flow-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

{ID id-QoSFlowMappingIndication CRITICALITY ignore EXTENSION QoS-Flow-Mapping-Indication PRESENCE optional},

...

}

QoS-Flow-Failed-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoS-Flow-Failed-Item

QoS-Flow-Failed-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

cause Cause,

iE-Extensions ProtocolExtensionContainer { { QoS-Flow-Failed-Item-ExtIEs } } OPTIONAL,

...

}

QoS-Flow-Failed-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

QoS-Flow-Mapping-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoS-Flow-Mapping-Item

QoS-Flow-Mapping-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

qoSFlowMappingIndication QoS-Flow-Mapping-Indication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { QoS-Flow-Mapping-Item-ExtIEs } } OPTIONAL,

...

}

QoS-Flow-Mapping-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

QoS-Flow-Mapping-Indication ::= ENUMERATED {ul, dl, ...}

QoS-Parameters-Support-List ::= SEQUENCE {

eUTRAN-QoS-Support-List EUTRAN-QoS-Support-List OPTIONAL,

nG-RAN-QoS-Support-List NG-RAN-QoS-Support-List OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { QoS-Parameters-Support-List-ItemExtIEs} } OPTIONAL,

...

}

QoS-Parameters-Support-List-ItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

QoSPriorityLevel ::= INTEGER (0..127, ...)

QoS-Flow-QoS-Parameter-List ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF QoS-Flow-QoS-Parameter-Item

QoS-Flow-QoS-Parameter-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

qoSFlowLevelQoSParameters QoSFlowLevelQoSParameters,

qoSFlowMappingIndication QoS-Flow-Mapping-Indication OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { QoS-Flow-QoS-Parameter-Item-ExtIEs } } OPTIONAL,

...

}

QoS-Flow-QoS-Parameter-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

QoSFlowLevelQoSParameters ::= SEQUENCE {

qoS-Characteristics QoS-Characteristics,

nGRANallocationRetentionPriority NGRANAllocationAndRetentionPriority,

gBR-QoS-Flow-Information GBR-QoSFlowInformation OPTIONAL,

reflective-QoS-Attribute ENUMERATED {subject-to, ...} OPTIONAL,

additional-QoS-Information ENUMERATED {more-likely, ...} OPTIONAL,

paging-Policy-Index INTEGER (1..8, ...) OPTIONAL,

-- The paging-Policy-Index IE is not used in this version of the specification.

reflective-QoS-Indicator ENUMERATED {enabled, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { QoSFlowLevelQoSParameters-ExtIEs } } OPTIONAL

}

QoSFlowLevelQoSParameters-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

DataForwardingtoNG-RANQoSFlowInformationList ::= SEQUENCE (SIZE(1.. maxnoofQoSFlows)) OF DataForwardingtoNG-RANQoSFlowInformationList-Item

DataForwardingtoNG-RANQoSFlowInformationList-Item ::= SEQUENCE {

qoS-Flow-Identifier QoS-Flow-Identifier,

iE-Extensions ProtocolExtensionContainer { { DataForwardingtoNG-RANQoSFlowInformationList-Item-ExtIEs } } OPTIONAL,

...

}

DataForwardingtoNG-RANQoSFlowInformationList-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- R

RANUEID ::= OCTET STRING (SIZE (8))

RAT-Type ::= ENUMERATED {

e-UTRA,

nR,

...

}

RLC-Mode ::= ENUMERATED {

rlc-tm,

rlc-am,

rlc-um-bidirectional,

rlc-um-unidirectional-ul,

rlc-um-unidirectional-dl,

...

}

ROHC-Parameters ::= CHOICE {

rOHC ROHC,

uPlinkOnlyROHC UplinkOnlyROHC,

choice-Extension ProtocolIE-SingleContainer { { ROHC-Parameters-ExtIEs} }

}

ROHC-Parameters-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

ROHC ::= SEQUENCE {

maxCID INTEGER (0..16383, ...),

rOHC-Profiles INTEGER (0..511, ...),

continueROHC ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { ROHC-ExtIEs } } OPTIONAL

}

ROHC-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- S

SecurityAlgorithm ::= SEQUENCE {

cipheringAlgorithm CipheringAlgorithm,

integrityProtectionAlgorithm IntegrityProtectionAlgorithm OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SecurityAlgorithm-ExtIEs } } OPTIONAL,

...

}

SecurityAlgorithm-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SecurityIndication ::= SEQUENCE {

integrityProtectionIndication IntegrityProtectionIndication,

confidentialityProtectionIndication ConfidentialityProtectionIndication,

maximumIPdatarate MaximumIPdatarate OPTIONAL,

iE-Extensions ProtocolExtensionContainer { {SecurityIndication-ExtIEs} } OPTIONAL,

...

}

SecurityIndication-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SecurityInformation ::= SEQUENCE {

securityAlgorithm SecurityAlgorithm,

uPSecuritykey UPSecuritykey,

iE-Extensions ProtocolExtensionContainer { { SecurityInformation-ExtIEs } } OPTIONAL,

...

}

SecurityInformation-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SecurityResult ::= SEQUENCE {

integrityProtectionResult IntegrityProtectionResult,

confidentialityProtectionResult ConfidentialityProtectionResult,

iE-Extensions ProtocolExtensionContainer { {SecurityResult-ExtIEs} } OPTIONAL,

...

}

SecurityResult-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

Slice-Support-List ::= SEQUENCE (SIZE(1.. maxnoofSliceItems)) OF Slice-Support-Item

Slice-Support-Item ::= SEQUENCE {

sNSSAI SNSSAI,

iE-Extensions ProtocolExtensionContainer { { Slice-Support-Item-ExtIEs } } OPTIONAL

}

Slice-Support-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SNSSAI ::= SEQUENCE {

sST OCTET STRING (SIZE(1)),

sD OCTET STRING (SIZE(3)) OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { SNSSAI-ExtIEs } } OPTIONAL,

...

}

SNSSAI-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SDAP-Configuration ::= SEQUENCE {

defaultDRB DefaultDRB,

sDAP-Header-UL SDAP-Header-UL,

sDAP-Header-DL SDAP-Header-DL,

iE-Extensions ProtocolExtensionContainer { { SDAP-Configuration-ExtIEs } } OPTIONAL,

...

}

SDAP-Configuration-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

SDAP-Header-DL ::= ENUMERATED {

present,

absent,

...

}

SDAP-Header-UL ::= ENUMERATED {

present,

absent,

...

}

-- T

TimeToWait ::= ENUMERATED {v1s, v2s, v5s, v10s, v20s, v60s, ...}

TNLAssociationUsage ::= ENUMERATED {

ue,

non-ue,

both,

...

}

TransportLayerAddress ::= BIT STRING (SIZE(1..160, ...))

TransactionID ::= INTEGER (0..255, ...)

T-Reordering ::= ENUMERATED {ms0, ms1, ms2, ms4, ms5, ms8, ms10, ms15, ms20, ms30, ms40, ms50, ms60, ms80, ms100, ms120, ms140, ms160, ms180, ms200, ms220, ms240, ms260, ms280, ms300, ms500, ms750, ms1000, ms1250, ms1500, ms1750, ms2000, ms2250, ms2500, ms2750, ms3000, ...}

T-ReorderingTimer ::= SEQUENCE {

t-Reordering T-Reordering,

iE-Extensions ProtocolExtensionContainer { { T-ReorderingTimer-ExtIEs } } OPTIONAL,

...

}

T-ReorderingTimer-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

TypeOfError ::= ENUMERATED {

not-understood,

missing,

...

}

-- U

UE-Activity ::= ENUMERATED {

active,

not-active,

...

}

UE-associatedLogicalE1-ConnectionItem ::= SEQUENCE {

gNB-CU-CP-UE-E1AP-ID GNB-CU-CP-UE-E1AP-ID OPTIONAL,

gNB-CU-UP-UE-E1AP-ID GNB-CU-UP-UE-E1AP-ID OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { UE-associatedLogicalE1-ConnectionItemExtIEs} } OPTIONAL,

...

}

UE-associatedLogicalE1-ConnectionItemExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

UL-Configuration ::= ENUMERATED {

no-data,

shared,

only,

...

}

ULDataSplitThreshold ::= ENUMERATED {b0, b100, b200, b400, b800, b1600, b3200, b6400, b12800, b25600, b51200, b102400, b204800, b409600, b819200, b1228800, b1638400, b2457600, b3276800, b4096000, b4915200, b5734400, b6553600, infinity, ...}

UP-Parameters ::= SEQUENCE (SIZE(1.. maxnoofUPParameters)) OF UP-Parameters-Item

UP-Parameters-Item ::= SEQUENCE {

uP-TNL-Information UP-TNL-Information,

cell-Group-ID Cell-Group-ID,

iE-Extensions ProtocolExtensionContainer { { UP-Parameters-Item-ExtIEs } } OPTIONAL,

...

}

UP-Parameters-Item-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

UPSecuritykey ::= SEQUENCE {

encryptionKey EncryptionKey,

integrityProtectionKey IntegrityProtectionKey OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { UPSecuritykey-ExtIEs } } OPTIONAL,

...

}

UPSecuritykey-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

UP-TNL-Information ::= CHOICE {

gTPTunnel GTPTunnel,

choice-extension ProtocolIE-SingleContainer {{UP-TNL-Information-ExtIEs}}

}

UP-TNL-Information-ExtIEs E1AP-PROTOCOL-IES ::= {

...

}

UplinkOnlyROHC ::= SEQUENCE {

maxCID INTEGER (0..16383, ...),

rOHC-Profiles INTEGER (0..511, ...),

continueROHC ENUMERATED {true, ...} OPTIONAL,

iE-Extensions ProtocolExtensionContainer { { UplinkOnlyROHC-ExtIEs } } OPTIONAL

}

UplinkOnlyROHC-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

...

}

-- V

-- W

-- X

-- Y

-- Z

END

-- ASN1STOP

### 9.4.6 Common Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-CommonDataTypes {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-CommonDataTypes (3)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Common Data Types

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Criticality ::= ENUMERATED { reject, ignore, notify }

Presence ::= ENUMERATED { optional, conditional, mandatory }

PrivateIE-ID ::= CHOICE {

local INTEGER (0.. maxPrivateIEs),

global OBJECT IDENTIFIER

}

ProcedureCode ::= INTEGER (0..255)

ProtocolExtensionID ::= INTEGER (0..maxProtocolExtensions)

ProtocolIE-ID ::= INTEGER (0..maxProtocolIEs)

TriggeringMessage ::= ENUMERATED { initiating-message, successful-outcome, unsuccessful-outcome}

END

-- ASN1STOP

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

ProcedureCode,

ProtocolIE-ID

FROM E1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-reset ProcedureCode ::= 0

id-errorIndication ProcedureCode ::= 1

id-privateMessage ProcedureCode ::= 2

id-gNB-CU-UP-E1Setup ProcedureCode ::= 3

id-gNB-CU-CP-E1Setup ProcedureCode ::= 4

id-gNB-CU-UP-ConfigurationUpdate ProcedureCode ::= 5

id-gNB-CU-CP-ConfigurationUpdate ProcedureCode ::= 6

id-e1Release ProcedureCode ::= 7

id-bearerContextSetup ProcedureCode ::= 8

id-bearerContextModification ProcedureCode ::= 9

id-bearerContextModificationRequired ProcedureCode ::= 10

id-bearerContextRelease ProcedureCode ::= 11

id-bearerContextReleaseRequest ProcedureCode ::= 12

id-bearerContextInactivityNotification ProcedureCode ::= 13

id-dLDataNotification ProcedureCode ::= 14

id-dataUsageReport ProcedureCode ::= 15

id-gNB-CU-UP-CounterCheck ProcedureCode ::= 16

id-gNB-CU-UP-StatusIndication ProcedureCode ::= 17

id-uLDataNotification ProcedureCode ::= 18

id-mRDC-DataUsageReport ProcedureCode ::= 19

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxnoofErrors INTEGER ::= 256

maxnoofSPLMNs INTEGER ::= 12

maxnoofSliceItems INTEGER ::= 1024

maxnoofIndividualE1ConnectionsToReset INTEGER ::= 65536

maxnoofEUTRANQOSParameters INTEGER ::= 256

maxnoofNGRANQOSParameters INTEGER ::= 256

maxnoofDRBs INTEGER ::= 32

maxnoofNRCGI INTEGER ::= 512

maxnoofPDUSessionResource INTEGER ::= 256

maxnoofQoSFlows INTEGER ::= 64

maxnoofUPParameters INTEGER ::= 8

maxnoofCellGroups INTEGER ::= 4

maxnooftimeperiods INTEGER ::= 2

maxnoofTNLAssociations INTEGER ::= 32

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Cause ProtocolIE-ID ::= 0

id-CriticalityDiagnostics ProtocolIE-ID ::= 1

id-gNB-CU-CP-UE-E1AP-ID ProtocolIE-ID ::= 2

id-gNB-CU-UP-UE-E1AP-ID ProtocolIE-ID ::= 3

id-ResetType ProtocolIE-ID ::= 4

id-UE-associatedLogicalE1-ConnectionItem ProtocolIE-ID ::= 5

id-UE-associatedLogicalE1-ConnectionListResAck ProtocolIE-ID ::= 6

id-gNB-CU-UP-ID ProtocolIE-ID ::= 7

id-gNB-CU-UP-Name ProtocolIE-ID ::= 8

id-gNB-CU-CP-Name ProtocolIE-ID ::= 9

id-CNSupport ProtocolIE-ID ::= 10

id-SupportedPLMNs ProtocolIE-ID ::= 11

id-TimeToWait ProtocolIE-ID ::= 12

id-SecurityInformation ProtocolIE-ID ::= 13

id-UEDLAggregateMaximumBitRate ProtocolIE-ID ::= 14

id-System-BearerContextSetupRequest ProtocolIE-ID ::= 15

id-System-BearerContextSetupResponse ProtocolIE-ID ::= 16

id-BearerContextStatusChange ProtocolIE-ID ::= 17

id-System-BearerContextModificationRequest ProtocolIE-ID ::= 18

id-System-BearerContextModificationResponse ProtocolIE-ID ::= 19

id-System-BearerContextModificationConfirm ProtocolIE-ID ::= 20

id-System-BearerContextModificationRequired ProtocolIE-ID ::= 21

id-DRB-Status-List ProtocolIE-ID ::= 22

id-ActivityNotificationLevel ProtocolIE-ID ::= 23

id-ActivityInformation ProtocolIE-ID ::= 24

id-Data-Usage-Report-List ProtocolIE-ID ::= 25

id-New-UL-TNL-Information-Required ProtocolIE-ID ::= 26

id-GNB-CU-CP-TNLA-To-Add-List ProtocolIE-ID ::= 27

id-GNB-CU-CP-TNLA-To-Remove-List ProtocolIE-ID ::= 28

id-GNB-CU-CP-TNLA-To-Update-List ProtocolIE-ID ::= 29

id-GNB-CU-CP-TNLA-Setup-List ProtocolIE-ID ::= 30

id-GNB-CU-CP-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 31

id-DRB-To-Setup-List-EUTRAN ProtocolIE-ID ::= 32

id-DRB-To-Modify-List-EUTRAN ProtocolIE-ID ::= 33

id-DRB-To-Remove-List-EUTRAN ProtocolIE-ID ::= 34

id-DRB-Required-To-Modify-List-EUTRAN ProtocolIE-ID ::= 35

id-DRB-Required-To-Remove-List-EUTRAN ProtocolIE-ID ::= 36

id-DRB-Setup-List-EUTRAN ProtocolIE-ID ::= 37

id-DRB-Failed-List-EUTRAN ProtocolIE-ID ::= 38

id-DRB-Modified-List-EUTRAN ProtocolIE-ID ::= 39

id-DRB-Failed-To-Modify-List-EUTRAN ProtocolIE-ID ::= 40

id-DRB-Confirm-Modified-List-EUTRAN ProtocolIE-ID ::= 41

id-PDU-Session-Resource-To-Setup-List ProtocolIE-ID ::= 42

id-PDU-Session-Resource-To-Modify-List ProtocolIE-ID ::= 43

id-PDU-Session-Resource-To-Remove-List ProtocolIE-ID ::= 44

id-PDU-Session-Resource-Required-To-Modify-List ProtocolIE-ID ::= 45

id-PDU-Session-Resource-Setup-List ProtocolIE-ID ::= 46

id-PDU-Session-Resource-Failed-List ProtocolIE-ID ::= 47

id-PDU-Session-Resource-Modified-List ProtocolIE-ID ::= 48

id-PDU-Session-Resource-Failed-To-Modify-List ProtocolIE-ID ::= 49

id-PDU-Session-Resource-Confirm-Modified-List ProtocolIE-ID ::= 50

id-DRB-To-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 51

id-DRB-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 52

id-DRB-Failed-Mod-List-EUTRAN ProtocolIE-ID ::= 53

id-PDU-Session-Resource-Setup-Mod-List ProtocolIE-ID ::= 54

id-PDU-Session-Resource-Failed-Mod-List ProtocolIE-ID ::= 55

id-PDU-Session-Resource-To-Setup-Mod-List ProtocolIE-ID ::= 56

id-TransactionID ProtocolIE-ID ::= 57

id-Serving-PLMN ProtocolIE-ID ::= 58

id-UE-Inactivity-Timer ProtocolIE-ID ::= 59

id-System-GNB-CU-UP-CounterCheckRequest ProtocolIE-ID ::= 60

id-DRBs-Subject-To-Counter-Check-List-EUTRAN ProtocolIE-ID ::= 61

id-DRBs-Subject-To-Counter-Check-List-NG-RAN ProtocolIE-ID ::= 62

id-PPI ProtocolIE-ID ::= 63

id-gNB-CU-UP-Capacity ProtocolIE-ID ::= 64

id-GNB-CU-UP-OverloadInformation ProtocolIE-ID ::= 65

id-UEDLMaximumIntegrityProtectedDataRate ProtocolIE-ID ::= 66

id-PDU-Session-To-Notify-List ProtocolIE-ID ::= 67

id-PDU-Session-Resource-Data-Usage-List ProtocolIE-ID ::= 68

id-SNSSAI ProtocolIE-ID ::= 69

id-DataDiscardRequired ProtocolIE-ID ::= 70

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 71

id-DRB-QoS ProtocolIE-ID ::= 72

id-GNB-CU-UP-TNLA-To-Remove-List ProtocolIE-ID ::= 73

id-endpoint-IP-Address-and-Port ProtocolIE-ID ::= 74

id-TNLAssociationTransportLayerAddressgNBCUUP ProtocolIE-ID ::= 75

id-RANUEID ProtocolIE-ID ::= 76

id-GNB-DU-ID ProtocolIE-ID ::= 77

id-CommonNetworkInstance ProtocolIE-ID ::= 78

id-NetworkInstance ProtocolIE-ID ::= 79

id-QoSFlowMappingIndication ProtocolIE-ID ::= 80

id-PDCP-StatusReportIndication ProtocolIE-ID ::= 81

id-DataForwardingtoNG-RANQoSFlowInformationList ProtocolIE-ID ::= 136

id-SecurityIndicationModify ProtocolIE-ID ::= 143

END

-- ASN1STOP

### 9.4.8 Container Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-Containers {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-Containers (5) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

maxPrivateIEs,

maxProtocolExtensions,

maxProtocolIEs,

Criticality,

Presence,

PrivateIE-ID,

ProtocolIE-ID

FROM E1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PROTOCOL-IES ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PROTOCOL-EXTENSION ::= CLASS {

&id ProtocolIE-ID UNIQUE,

&criticality Criticality,

&Extension,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

EXTENSION &Extension

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Class Definition for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PRIVATE-IES ::= CLASS {

&id PrivateIE-ID,

&criticality Criticality,

&Value,

&presence Presence

}

WITH SYNTAX {

ID &id

CRITICALITY &criticality

TYPE &Value

PRESENCE &presence

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-Container { E1AP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (0..maxProtocolIEs)) OF

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-SingleContainer { E1AP-PROTOCOL-IES : IEsSetParam} ::=

ProtocolIE-Field {{IEsSetParam}}

ProtocolIE-Field { E1AP-PROTOCOL-IES : IEsSetParam} ::= SEQUENCE {

id E1AP-PROTOCOL-IES.&id ({IEsSetParam}),

criticality E1AP-PROTOCOL-IES.&criticality ({IEsSetParam}{@id}),

value E1AP-PROTOCOL-IES.&Value ({IEsSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container Lists for Protocol IE Containers

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolIE-ContainerList {INTEGER : lowerBound, INTEGER : upperBound, E1AP-PROTOCOL-IES : IEsSetParam} ::=

SEQUENCE (SIZE (lowerBound..upperBound)) OF

ProtocolIE-Container {{IEsSetParam}}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Protocol Extensions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ProtocolExtensionContainer { E1AP-PROTOCOL-EXTENSION : ExtensionSetParam} ::=

SEQUENCE (SIZE (1..maxProtocolExtensions)) OF

ProtocolExtensionField {{ExtensionSetParam}}

ProtocolExtensionField { E1AP-PROTOCOL-EXTENSION : ExtensionSetParam} ::= SEQUENCE {

id E1AP-PROTOCOL-EXTENSION.&id ({ExtensionSetParam}),

criticality E1AP-PROTOCOL-EXTENSION.&criticality ({ExtensionSetParam}{@id}),

extensionValue E1AP-PROTOCOL-EXTENSION.&Extension ({ExtensionSetParam}{@id})

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Container for Private IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

PrivateIE-Container { E1AP-PRIVATE-IES : IEsSetParam} ::=

SEQUENCE (SIZE (1..maxPrivateIEs)) OF

PrivateIE-Field {{IEsSetParam}}

PrivateIE-Field { E1AP-PRIVATE-IES : IEsSetParam} ::= SEQUENCE {

id E1AP-PRIVATE-IES.&id ({IEsSetParam}),

criticality E1AP-PRIVATE-IES.&criticality ({IEsSetParam}{@id}),

value E1AP-PRIVATE-IES.&Value ({IEsSetParam}{@id})

}

END

-- ASN1STOP

## 9.5 Message Transfer Syntax

E1AP shall use the ASN.1 Basic Packed Encoding Rules (BASIC-PER) Aligned Variant as transfer syntax, as specified in ITU-T Recommendation X.691 [7].

## 9.6 Timers

# 10 Handling of unknown, unforeseen and erroneous protocol data

Section 10 of TS 38.413 [6] is applicable for the purposes of the present document, with the following additions for non-UE-associated procedures:

- In case of Abstract Syntax Error, when reporting the *Criticality Diagnostics* IE for not comprehended IE/IEgroups or missing IE/IE groups, the *Transaction ID* IE shall also be included;

- In case of Logical Error, when reporting the *Criticality Diagnostics* IE, the *Transaction ID* IE shall also be included;

- In case of Logical Error in a response message of a Class 1 procedure, or failure to comprehend *Transaction ID* IE from a received message, the procedure shall be considered as unsuccessfully terminated or not terminated (e.g., transaction ID unknown in response message), and local error handling shall be initiated.

Annex A (informative):  
Change History

| **Change history** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Date | Meeting | TDoc | CR | Rev | Cat | Subject/Comment | New version |
| 2018-02 | R3 #99 | R3-181309 | - | - | - | Endorsed skeleton | 0.0.0 |
| 2018-03 | R3 #99 | R3-181597 | - | - | - | New version capturing agreements from RAN3#99 | 0.1.0 |
| 2018-04 | R3 #99b | R3-182531 | - | - | - | New version capturing agreements from RAN3#99b | 0.2.0 |
| 2018-05 | R3 #100 | R3-183601 | - | - | - | New version capturing agreements from RAN3#100 | 0.3.0 |
| 2018-06 | RAN#80 | RP-181154 |  |  |  | Submitted to RAN for approval. | 1.0.0 |
| 2018-06 | RAN#80 | - | - | - | - | Specification approved at TSG-RAN and placed under change control | 15.0.0 |
| 2018-09 | RAN#81 | RP-181925 | 0001 | 3 | F | BL CR for TS 38.463 covering agreements from RAN3-AH-1807 and R3-101  Note: CR not based on latest version of the spec. Changes to clause 8.3.2.2 in the CR were implemented in clause 8.3.2.3 in the spec. | 15.1.0 |
| 2018-12 | RAN#82 | RP-182451 | 0002 | 2 | F | NR Corrections (TS 38.463 Baseline CR covering RAN3-101Bis and RAN3-102 agreements) | 15.2.0 |
| 2019-03 | RAN#83 | RP-190560 | 0004 | 2 | F | Correction to Data Forwarding Information IE | 15.3.0 |
| 2019-03 | RAN#83 | RP-190555 | 0005 | 1 | F | Corrections related to Integrity Protection handling at the gNB-CU-UP | 15.3.0 |
| 2019-03 | RAN#83 | RP-190554 | 0007 | 2 | F | Corrections on gNB-CU-UP/gNB-DU-CP Configuration Update | 15.3.0 |
| 2019-03 | RAN#83 | RP-190556 | 0008 | 2 | F | Correction of QoS Flow Mapping Indication | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0009 | 1 | F | Paging Failure | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0011 | 1 | F | Release due to pre-emption | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0013 | - | F | Transaction ID in Error Indication procedure | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0017 | 1 | F | CR to TS 38.463 on inactivity timer over E1 | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0020 | 1 | F | Data volume reporting for MR-DC with 5GC | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0029 | 1 | F | TS 38.463 ASN.1 corrections | 15.3.0 |
| 2019-03 | RAN#83 | RP-190560 | 0030 | - | F | Rapporteur corrections for TS 38.463 | 15.3.0 |
| 2019-03 | RAN#83 | RP-190611 | 0035 | 3 | F | S-NSSAI update during EPS to 5GS handover | 15.3.0 |
| 2019-07 | RP#84 | RP-191399 | 0023 | 2 | F | Support of ongoing re-mapping on source side during SDAP mobility | 15.4.0 |
| 2019-07 | RP#84 | RP-191399 | 0028 | 1 | F | TS 38.463 Tabular clean up for Bearer Context messages | 15.4.0 |
| 2019-07 | RP-84 | RP-191396 | 0044 | 2 | F | Correction to DRB 5QI on E1 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0049 | 2 | F | Multiple SCTP associations over E1 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0050 | 2 | F | Rapporteur’s editorial corrections for TS 38.463 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0051 | - | F | E1AP failure messages correction | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0052 | 1 | F | New UL TNL Information clarification | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0053 | 4 | F | UE Identification over E1 | 15.4.0 |
| 2019-07 | RP-84 | RP-191394 | 0057 | 2 | F | CR to 38.463 on deconfiguring PDCP duplication | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0062 | 2 | F | Clarification on security indication in the modification procedure over E1 interface | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0064 | 2 | F | Clarification on counter check procedure | 15.4.0 |
| 2019-07 | RP-84 | RP-191397 | 0065 |  | F | Correction of Network Instance | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0073 | 1 | F | Activity Notification Level in Bearer Context Modification Request E1AP | 15.4.0 |
| 2019-07 | RP-84 | RP-191394 | 0075 | 1 | F | PDCP SN length and RLC mode related clean-up over To Be Modified structure in Bearer Context Modification procedure | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0084 | - | F | Bearer Context Release Request Cause | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0085 | - | F | Clarification on Bearer Context Setup and Bearer Context Modification failures | 15.4.0 |
| 2019-07 | RP-84 | RP-191396 | 0086 | 1 | F | PDU session split for E1 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0091 | - | F | Rapporteur’s editorial corrections for TS 38.463 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0092 | 1 | F | Rapporteur’s ASN.1 corrections for TS 38.463 | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0095 | 1 | F | CR to 38.463 on adding Cause when remove DRB and PDU Session | 15.4.0 |
| 2019-07 | RP-84 | RP-191399 | 0097 | - | F | Rapporteur’s ASN.1 corrections for TS 38.463 | 15.4.0 |
| 2019-09 | RP-85 | RP-192168 | 0094 | 2 | F | CR to 38.463 on Security Indication | 15.5.0 |
| 2019-09 | RP-85 | RP-192166 | 0098 | 1 | F | Correction of security indication | 15.5.0 |
| 2019-09 | RP-85 | RP-192166 | 0111 | 1 | F | Clarification for TNLA removal | 15.5.0 |
| 2019-09 | RP-85 | RP-192168 | 0122 | 2 | F | Correction of semantic descriptions in TS 38.463 (rapporteur) | 15.5.0 |
| 2019-12 | RP-86 | RP-192915 | 0158 | 1 | F | Correction of S-NSSAI coding | 15.6.0 |
| 2019-12 | RP-86 | RP-192915 | 0174 | 2 | F | UL Data Split Threshold correction | 15.6.0 |
| 2019-12 | RP-86 | RP-192915 | 0476 | 1 | F | Correction to DRB to Setup | 15.6.0 |
| 2020-07 | RP-88-e | RP-201091 | 0499 | 1 | F | Correction of the Old QoS Flow List update during HO | 15.7.0 |
| 2020-07 | RP-88-e | RP-201092 | 0501 | 2 | F | PDCP Status Report indication in PDCP-Configuration | 15.7.0 |
| 2020-09 | RP-89-e | RP-201953 | 0524 | 1 | F | Correction on reusing Source TEID at Handover | 15.8.0 |
| 2021-09 | RP-93-e | RP-211877 | 0611 | 1 | F | Correction of PDU Session level Data Forwarding Information and QoS Flow list | 15.9.0 |
| 2022-03 | RP-95-e | RP-220279 | 0674 | 2 | F | Security indication in the modification procedure over E1 interface | 15.10.0 |
| 2022-09 | RP-97-e | RP-222201 | 0704 | - | F | Correction on Missing Criticality Diagnostics over E1AP | 15.11.0 |
| 2023-06 | RAN#100 | RP-231070 | 0715 | 2 | F | Correction of RAT type in Data Usage Report List | 15.12.0 |
| 2023-06 | RAN#100 | RP-231070 | 0718 | 2 | F | Correction of Paging Priority Indicator in QoS Flow Level QoS Parameters | 15.12.0 |