**3GPP TSG-RAN4 Meeting #99-e *xxxxx***

**, May 19th – 27th, 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **1** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for TS 38.101-1: introduction of MSD test configurations related to IMD for inter-band combination CA\_n41C-n66A |
|  |  |
| ***Source to WG:*** | MediaTek Inc. |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_CADC\_R17\_2BDL\_xBUL-Core |  | ***Date:*** | 2021-08-23 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Inter-band combinations have been introduced in release 17 with intra-band UL CA as UL configuration without considering potential interfrence from the IMDs of the two CC allocation  |
|  |  |
| ***Summary of change:*** | Introduction of the related test points and CA\_n41C-n66A MSD in section 7.3A.5 |
|  |  |
| ***Consequences if not approved:*** | The UE may fail conformance test for these UL configurations if exceptions are not specified |
|  |  |
| ***Clauses affected:*** | 7.3A.5 Table 7.3A.5-1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-1  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<< Start of changed sections >>>

### 7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA

For inter-band carrier aggregation with uplink assigned to two NR bands given in Table 7.3A.5-1, Table 7.3A.5-1a and Table 7.3A.5-2 the reference sensitivity is defined only for the specific uplink and downlink test points specified in Table 7.3A.5-1, Table 7.3A.5-1a and Table 7.3A.5-2. For these test points the reference sensitivity requirement specified in Table 7.3.2-1 and Table 7.3.2-2 are relaxed by the amount of the corresponding parameter MSD given in Table 7.3A.5-1, Table 7.3A.5-1a and Table 7.3A.5-2.

Table 7.3A.5-1: 2DL/2UL interband Reference sensitivity QPSK PREFSENS and uplink/downlink configurations for PC3 CA

|  |  |
| --- | --- |
| Band / Channel bandwidth / NRB / Duplex mode | Source of IMD |
| NR CA band combination | NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL CLRB | DL Fc (MHz) | MSD (dB) | Duplex mode |  |
| CA\_n1-n3 | n1 | 1950 | 5 | 25 | 2140 | 23 | FDD | IMD3 |
|  | n3 | 1760 | 5 | 25 | 1855 | N/A | TDD | N/A |
| CA\_n1-n8 | n1 | 1965 | 5 | 25 | 2155 | 6.0 | FDD | IMD4 |
|  | n8 | 887.5 | 5 | 25 | 932.5 | N/A | FDD | N/A |
| CA\_n1-n77 | 1 | 1950 | 5 | 25 | 2140 | 29.8 | FDD | IMD24 |
|  |  |  |  |  |  | 32.5 5 |  |  |
|  | n77 | 4090 | 10 | 50 | 4090 | N/A | TDD | N/A |
|  | 1 | 1950 | 5 | 25 | 2140 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  | 10.75 |  |  |
|  | n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| CA\_n1-n78 | n1 | 1950 | 5 | 25 | 2140 | 8.0 | FDD | IMD4 |
|  |  |  |  |  |  | 10.75 |  |  |
|  | n78 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| CA\_n2-n48 | n2 | 1852.5 | 5 | 25 | 1932.5 | 12 | FDD | IMD4 |
|  | n48 | 3625 | 20 | 100 | 3625 | N/A | TDD | N/A |
| CA\_n2-n66 | n2 | 1855 | 5 | 25 | 1935 | 20 | FDD | IMD3 |
|  | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n2 | 1883.3 | 5 | 25 | 1963.3 | N/A | FDD | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 4 | FDD | IMD5 |
| CA\_n2-n77 | n2 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD2 |
|  |  |  |  |  |  | 28.75 |  |  |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n2 | 1885 | 5 | 25 | 1965 | 8.0 | FDD | IMD4 |
|  |  |  |  |  |  | 10.75 |  |  |
|  | n77 | 3690 | 10 | 50 | 3690 | N/A | TDD | N/A |
|  | n2 | 1885 | 5 | 25 | 1965 | 5 | FDD | IMD5 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n2 | N/A | 5 | N/A | 1987.5 | 2.7 | FDD | IMD7 |
|  | n77 | 3455 | 10 | 1 RBSTART=10 | 3455 | N/A | TDD | N/A |
| CA\_n2-n78 | n2 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD24 |
|  |  |  |  |  |  | 28.75 |  |  |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n3-n7 | n3 | 1730 | 5 | 25 | 1825 | N/A | FDD | N/A |
|  | n7 | 2535 | 10 | 50 | 2655 | 10.2 | FDD | IMD4 |
| CA\_n3-n8 | n3 | 1755 | 10 | 50 | 1850 | N/A | FDD | N/A |
|  | n8 | 900 | 5 | 25 | 945 | 8 | FDD | IMD44 |
|  | n3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | FDD | IMD5 |
|  | n8 | 897.5 | 5 | 25 | 942.5 | N/A | FDD | N/A |
| CA\_n3-n18 | n18 | 818 | 5 | 25 | 863 | N/A | FDD | N/A |
|  | n3 | 1731 | 5 | 25 | 1826 | 4 | FDD | IMD4 |
| CA\_n3-n38 | n3 | 1713 | 5 | 25 | 1808 | 8.2 | FDD | IMD4 |
| n38 | 2617 | 5 | 25 | 2617 | N/A | TDD | N/A |
| CA\_n3-n41 | n3 | 1740 | 5 | 25 | 1835 | 8.2 | FDD | IMD4 |
|  | n41 | 2657.5 | 10 | 50 | 2657.5 | N/A | TDD | N/A |
| CA\_n3-n77 | n3 | 1740 | 5 | 25 | 1835 | 26 | FDD | IMD24 |
|  |  |  |  |  |  | 28.74 |  |  |
|  | n77 | 3575 | 10 | 50 | 3575 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  | 10.74 |  |  |
|  | n77 | 3435 | 10 | 50 | 3435 | N/A | TDD | N/A |
|  | n3 | N/A | N/A | N/A | N/A | N/A6 | FDD | IMD5 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
|  | n3 | N/A | 5 | N/A | 1877.5 | [2.2] | FDD | IMD7 |
|  | n77 | 3455 | 10 | 1 (RBstart=10) | 3455 | N/A | TDD | N/A |
|  |  | 3945 | 10 | 1 (RBstart=0) | 3945 |  |  |  |
| CA\_n3-n78 | n3 | 1740 | 5 | 25 | 1835 | 26 | FDD | IMD24 |
|  |  |  |  |  |  | 28.75 |  |  |
|  | n78 | 3575 | 10 | 25 | 3575 | N/A | TDD | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 8.0 | FDD | IMD44 |
|  |  |  |  |  |  | 10.75 |  |  |
|  | n78 | 3435 | 10 | 25 | 3435 | N/A | TDD | N/A |
| CA\_n5-n14 | n5 | 836 | 5 | 25 | 881 | 25 | FDD | IMD34 |
|  | n14 | 791 | 5 | 25 | 761 | N/A | FDD | N/A |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | FDD | N/A |
|  | n14 | 795.5 | 5 | 25 | 765.5 | 25 | FDD | IMD3 |
| CA\_n5-n66 | n5 | 838 | 5 | 25 | 883 | 30 | FDD | IMD24 |
|  | n66 | 1721 | 5 | 25 | 2121 | N/A | FDD | N/A |
| CA\_n5-n77 | 5 | 844 | 5 | 25 | 889 | 8.3 | FDD | IMD4 |
|  | n77 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
|  | 5 | 829 | 5 | 25 | 875 | 5.5 | FDD | IMD5 |
|  | n77 | 3600 | 10 | 50 | 3600 | N/A | TDD | N/A |
| CA\_n5-n78 | n5 | 844 | 5 | 25 | 889 | 8.3 | FDD | IMD4 |
|  | n78 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
| CA\_n7-n66 | n7 | 2535 | 10 | 50 | 2655 | 15 | FDD | IMD4 |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | FDD | N/A |
| CA\_n8-n41 | n8 | 882.5 | 5 | 25 | 927.5 | 12.1 | FDD | IMD34 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| CA\_n7-n77 | n7 | 2540 | 5 | 25 | 2660 | 7.1 | FDD | IMD4 |
|  | n77 | 3870 | 10 | 50 | 3870 | N/A | TDD | N/A |
| CA\_n8-n78 | n8 | 897.5 | 5 | 25 | 942.5 | 8.3 | FDD | IMD4 |
|  | n78 | 3635 | 10 | 50 | 3635 | N/A | TDD | N/A |
| CA\_n8-n79 | n8 | 897.5 | 5 | 25 | 942.5 | 4.8 | FDD | IMD5 |
|  | n79 | 4532.5 | 40 | 216 | 4532.5 | N/A | TDD | N/A |
| CA\_n12-n66 | n12 | 707.5 | 5 | 25 | 737.5 | N/A | FDD | N/A |
|  | n66 | 1765 | 5 | 25 | 2115 | 5.0 | FDD | IMD4 |
| CA\_n12-n77 | n12 | 705.5 | 5 | 20 | 760.5 | 5.5 | FDD | IMD5 |
|  | n77 | 3582.5 | 10 | 50 | 3582.5 | N/A | TDD | N/A |
| CA\_n13-n77 | n13 | 782 | 5 | 20 | 751 | 5.5 | FDD | IMD5 |
|  | n77 | 3880 | 10 | 50 | 3880 | N/A | TDD | N/A |
| CA\_n14-n77 | n14 | 793 | 5 | 20 | 763 | 5.5 | FDD | IMD5 |
|  | n77 | 3935 | 10 | 50 | 3935 | N/A | TDD | N/A |
| CA\_n18-n778 | n18 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4/5 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n18-n789 | n18 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4 |
|  | n78 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n20-n78 | n20 | 850 | 5 | 25 | 809 | 11 | FDD | IMD4 |
|  | n78 | 3359 | 10 | 50 | 3359 | N/A | TDD | N/A |
| CA\_n24-n7710 | n24 | N/A | N/A | N/A | N/A | N/A | FDD | IMD4 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n25-n41 | n25 | N/A | 5 | N/A |  | [8.5] | FDD | IMD7 |
|  | n41 | 2545 | 90 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | [2460] | 100 | 1 (RBstart=[226-229]) | [2460] |  |  |  |
| CA\_n25-n48 | n25 | 1852.5 | 5 | 25 | 1932.5 | 12 | FDD | IMD4 |
|  | n48 | 3625 | 20 | 100 | 3625 | N/A | TDD | N/A |
| CA\_n25-n66 | n66 | 1775 | 5 | 25 | 2175 | N/A | FDD | N/A |
|  | n25 | 1855 | 5 | 25 | 1935 | 20 | FDD | IMD3 |
|  | n66 | 1712.5 | 5 | 25 | 2112.5 | 23 | FDD | IMD3 |
|  | n25 | 1912.5 | 5 | 25 | 1992.5 | N/A | FDD | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 4 | FDD | IMD5 |
|  | n25 | 1883.3 | 5 | 25 | 1963.3 | N/A | FDD | N/A |
| CA\_n25-n77 | n25 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD2 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
|  | n25 | 1885 | 5 | 25 | 1965 | 8.0 | FDD | IMD4 |
|  | n77 | 3690 | 10 | 50 | 3690 | N/A | TDD | N/A |
|  | n25 | 1885 | 5 | 25 | 1965 | 5 | FDD | IMD5 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n25-n78 | n25 | 1855 | 5 | 25 | 1935 | 26 | FDD | IMD24 |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| CA\_n28-n50 | n28 | 730 | 10 | 50 | 775 | 15.3 | FDD | IMD2 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | TDD | N/A |
|  | n28 | 740 | 10 | 50 | 785 | 6.0 | FDD | IMD44 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | TDD | N/A |
| CA\_n28-n74 | n28 | 705.5 | 5 | 25 | 760.5 | 24.6 | FDD | IMD2 |
|  | n74 | 1466 | 5 | 25 | 1514 | N/A | FDD | N/A |
|  | n28 | 743 | 5 | 25 | 798 | 11.3 | FDD | IMD411 |
|  | n74 | 1431 | 5 | 25 | 1479 | N/A | FDD | N/A |
|  | n28 | 709 | 5 | 25 | 764 | N/A | FDD | N/A |
|  | n74 | 1466 | 5 | 25 | 1514 | 14.6 | FDD | IMD4 |
|  | n28 | 735.5 | 5 | 25 | 790.5 | N/A | FDD | N/A |
|  | n74 | 1450.4 | 5 | 25 | 1498.4 | 2.5 | FDD | IMD5 |
| CA\_n28-n77 | n28 | N/A | N/A | N/A | N/A | N/A7 | FDD | IMD2 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | TDD | N/A |
| CA\_n28-n77 | n28 | 705.5 | 5 | 25 | 760.5 | 5.5 | FDD | IMD5 |
|  | n77/n78 | 3582.5 | 10 | 50 | 3582.5 | N/A | TDD | N/A |
| CA\_n30-n77 | n30 | 2310 | 5 | 25 | 2355 | 8.0 | FDD | IMD4 |
|  | n77 | 3487.5 | 10 | 50 | 3487.5 | N/A | TDD | N/A |
|  | n30 | N/A | 5 | N/A | 2352.5 | [3.2] | FDD | IMD7 |
|  | n77 | 3455 | 10 | 1 (RBstart=17) | 3455 | N/A | TDD | N/A |
|  |  | 3825 | 10 | 1 (RBstart=0) | 3825 |  |  |  |
| CA\_n41-n66 | n41 | 2545 | 90 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | 2640 | 100 | 1 (RBstart=171) | 2640 |  |  |  |
|  | n66 | N/A | 5 | N/A | 2197.5 | [32.5] | FDD | IMD5 |
| CA\_n41-n71 | n41 | 2614 | 5 | 25 | 2614 | N/A | TDD | N/A |
|  | n71 | 665 | 5 | 25 | 619 | 11 | FDD | IMD4 |
| CA\_n41-n77 | n41 | 2545 | 60 | 1 (RBstart=0) | 2545 | N/A | TDD | N/A |
|  |  | 2625 | 100 | 1 (RBstart=272) | 2625 |  |  |  |
|  | n77 | N/A | 10 | N/A | 3305 | [2.7] | FDD | IMD9 |
| CA\_n48-n66 | n48 | 3660 | 5 | 25 | 3660 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | 5.0 | FDD | IMD5 |
| CA\_n66-n71 | n66 | 1750 | 5 | 25 | 2150 | 5 | FDD | IMD4 |
|  | n71 | 675 | 5 | 25 | 629 | N/A | FDD | N/A |
| CA\_n66-n77 | n66 | 1775 | 5 | 25 | 2175 | 31 | FDD | IMD2 |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | 5.0 | FDD | IMD5 |
|  | n77 | 3660 | 10 | 50 | 3660 | N/A | TDD | N/A |
|  | n66 | 1730 | 5 | 25 | 2130 | [1.7] | FDD | IMD7 |
|  | n77 | 3455 | 10 | 1 (RBstart=10) | 3455 | N/A | TDD | N/A |
|  |  | 3875 | 10 | 1 (RBstart=0) | 3875 |  |  |  |
| CA\_n66-n78 | n66 | 1730 | 5 | 25 | 2130 | 5.0 | FDD | IMD5 |
|  | n78 | 3660 | 10 | 50 | 3660 | N/A | TDD | N/A |
| CA\_n70-n71 | n70 | 1697.5 | 5 | 25 | 1997.5 | 5 | FDD | IMD4 |
|  | n71 | 695.5 | 5 | 25 | 649.5 | N/A | FDD | N/A |
| CA\_n71-n77 | n71 | 671 | 5 | 25 | 625 | 5.5 | FDD | IMD5 |
|  | n77 | 3300 | 10 | 50 | 3300 | N/A | TDD | N/A |
| CA\_n71-n78 | n71 | 681.5 | 5 | 25 | 635.5 | 5.5 | FDD | IMD5 |
|  | n78 | 3361.5 | 10 | 50 | 3582.5 | N/A | TDD | N/A |
| NOTE 1: Both of the transmitters shall be set min(+20 dBm, PCMAX\_L,f,c) as defined in clause 6.2A.4NOTE 2: RBSTART = 0, 15 kHz SCS is assumed.NOTE 3: No requirements apply when there is at least one individual RE within the intermodulation generated by the dual uplink is within the downlink transmission bandwidth of the FDD band. The reference sensitivity should only be verified when this is not the case (the requirements specified in clause 7.3 apply).NOTE 4: This band is subject to IMD5 also which MSD is not specified.NOTE 5: Applicable only if operation with 4 antenna ports is supported in the band with carrier aggregation configured.NOTE 6: Considering the spectrum holdings of the operator for CA\_n77(2A) (when one uplink sub block is assigned within 3300-3400MHz, the other uplink sub block is not assigned within 4000-4200MHz or vice versa), no IMD5 result will fall in Rx frequency range of band n3. Therefore, no MSD requirement apply for this CA configuration when two uplink sub blocks are assigned within CA\_77(2A).NOTE 7: Considering the spectrum holdings of the operator for CA\_n77(2A) (when one uplink sub block is assigned within 3300-3400MHz, the other uplink sub block is not assigned within 4000-4200MHz or vice versa), no IMD2 result will fall in Rx frequency range of band n28. Therefore, no MSD requirement apply for this CA configuration when two uplink sub blocks are assigned within CA\_77(2A).NOTE8: There is no IMD4/5 products in band n18 downlink for n77 operating in 3520 – 3560 MHz, 3700 – 3800MHz and 4000 - 4100MHz frequency range.NOTE 9: There is no IMD4 product in band n18 downlink for n78 operating in 3520 – 3560MHz and 3700-3800MHz frequency range.NOTE 10: There is no IMD4 product in band n24 downlink for n77 operating in 3450 – 3980 MHz and n24 uplink restricted to between 1627.5 – 1637.5 MHz and between 1646.5 – 1656.5 MHz.NOTE 11: This band is subject to IMD5 also which MSD is not specified.. |

<<< End of changed sections >>>