**3GPP TSG-RAN WG4 Meeting #100-e R4-210xxxx**

**Electronic Meeting, 16 – 27 August, 2021**

**Agenda item:** 9.15.6

**Source:** Moderator (Huawei, HiSilicon)

**Title:** Email discussion summary for [100-e][136] NRSL\_enh\_Part\_3

**Document for:** Information

# Introduction

This email thread discuss Rel-17 PC2 HPUE for NR sidelink enhancements. The contributions are in agenda 9.15.6, which includes:

* Topic #1: Issues related to PC2 HPUE for SL enhancements
	1. Issue 1-1: Clarification of PC2 HPUE operating bands
	2. Issue 1-2: NR V2X power class capability
	3. Issue 1-3: power class capability for NR V2X intra-band concurrent operation
* Topic #2: MPR/A-MPR requirements
	1. Issue 2-1: MPR/A-MPR requirements for PC2 NR V2X UE
* Topic #3: Co-existence study
	1. Issue 3-1: Co-existence study for n38 (SL) and adjacent band n7 (Uu)
	2. Issue 3-2: Configured output power for intra-band con-current operation
	3. Issue 3-3: Co-channel co-existence

# Topic #1: Issues related to PC2 HPUE for SL enhancements

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [**R4-2112608**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112608.zip) | Xiaomi | **Observation 1: For single band and single antenna case, no new capability design for PC2 V2X is needed.****Observation 2: For single band and multi antenna, no new capability design for PC2 V2X TXD is needed.****Observation 3: For inter-band concurrent operation case, no new capability design for PC2 V2X is needed.****Observation 4: For intra-band concurrent operation, power class signalling for each interface is needed.****Proposal 1: It is proposed to define power class signalling for intra-band concurrent operation.****Proposal 2: For other scenario of PC2 V2X, no new PC2 capability signalling is needed.****Proposal 3: Send an LS to RAN2 to inform the capability design request.** |
| [**R4-2112612**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112612.zip) | Xiaomi | **Current design of power class report is per band basis. However, for intra-band concurrent operation, UE can work on both Uu and PC5 interface within the same band. In this case, the per band basis power class signaling cannot correctly report the two power class for each interface of one UE in the same band.****To this extend, RAN4 has agreed to introduce the power class capability signaling for intra-band concurrent operation. Besides the original per band capability signaling, additional capability signaling per band per interface is recommended.** |
| [**R4-2112992**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112992.zip) | vivo | **Proposal 1: Clarify the feasibility of HPUE for sidelink operating bands based on the information in Table 1.****Proposal 2: No need to introduce PC2 power class capability for NR V2X.****Proposal 3: Remove the restriction ‘when the UE is not associated with a serving cell on the NR V2X carrier’ to cover the scenario of Uu and SL co-existence.****Proposal 4: No need to consider the co-channel existence issues for intra-band V2X operation.** |
| [**R4-2114507**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114507.zip) | Huawei, HiSilicon | ***Observation 1: Power class 2 UE capability for LTE-V2X is reported via Uu RRC message.******Proposal 1: Specific PC2 power class for NR V2X needs to be defined.******Proposal 2: The new PC2 power class for NR-V2X should be reported via Uu RRC message.******Proposal 3: The new PC2 power class for NR-V2X should be introduced from Rel-16.******Proposal 4: LS should be sent to RAN2 on the agreements for the new PC2 power class capability for NR-V2X.*** |
| [**R4-2114508**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114508.zip) | Huawei, HiSilicon | **draft LS on new power class 2 capability for NR-V2X** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Issue 1-1: Clarification of PC2 HPUE operating bands

***Clarify which operating bands should support PC2 HPUE in Rel-17*** *(R4-2112992, vivo)*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| V2X Operating Band | Sidelink (SL) Transmission/ Reception operating band | Single Antenna 26 dBm | Multi antenna(TxD, SL-MIMO) 26 dBm | Note |
| FUL\_low – FUL\_high |
| n14 | 788 MHz | - | 798 MHz  |  |  | More discussion is needed whether to introduce PC1 for this band. |
| n79 | 4400 MHz | - | 5000 MHz |  |  | For Uu transmission, band n79 can support PC2 other than PC3. |
| n38 | 2570 MHz | - | 2620 MHz |  |  | RAN4 concluded the co-existence study, however not decide whether to support HPUE in this band. |
| n47 | 5855 MHz | - | 5925 MHz | 🗹 | 🗹 | It is feasible to support HPUE in this band. |

***Moderator’s recommendation:***

* Recommended WF
	+ Collect views for the supported HPUE bands in Rel-17 in 1st round discussion

### Issue 1-2: NR V2X power class capability

***Whether need to define specific NR V2X PC2 capability signalling?***

* ***Option 1: Yes***
* ***Option 2: No***

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion

### Issue 1-3: power class capability for NR V2X intra-band concurrent operation

***Whether need to define specific power class capability signalling for NR V2X intra-band concurrent operation?***

* ***Option 1: Yes***
* ***Option 2: No***

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Issues** | **Company Comments** |
| 1-1: Clarification of PC2 HPUE operating bands | ***Clarify which operating bands should support PC2 HPUE in Rel-17***Xiaomi: At least for band n47 and band n79, PC2 can be agreed. Other bands depend on operator request.CATT: In principle, whether licensed bands can support PC2 should be based on operator request. LGE: For n47, n79, we also support PC2 V2X operation. For n14, they only request PC1/PC3, so it can be discussed in [134] e-mail thread. For n38, we also prefer that RAN4 can study PC2 V2X operation by operator request based on each regional regulation.Ericsson: PC1 in n14 should be based on the coexisting study discussion in [134] to protect B13 and operator request for sure. For PC2 in other licensed band, it should be based on operator request.Huawei: For PC2, we support n47 and n79, one is ITS band and the other one is licensed band. For other bands, it depends on requests. But it would be better to focus on these two bands firstly in Rel-17.Vivo: For now, only band n47 is clear to support HPUE for both single antenna and multi antenna operation. For other bands, we don’t have conclusion.OPPO: n79/n47 are ok, and n38 can be considered also which is similar as n41 license band. |
| 1-2: NR V2X power class capability | ***Whether need to define specific NR V2X PC2 capability signalling?***Xiaomi: Based on our discussion paper, we think for intra-band concurrent operation, the HUPE capability signaling is needed. However, for other cases as single band and inter-band cases, the signaling is not needed.CATT: Option 1.LGE: Prefer option 1. Single band PC2 V2X operation and PC2 intra-band/inter-band V2X operation will be needed for the PC2 capability. Ericsson: Option 1.The signaling is for network and thus it must be reported over Uu interface using the licensed band. If the UE power class of a UE for Uu operation would be the same with the NR V2X operation, there is no need to be reported and the UE power class framework can be directly reused by NR V2X. However, as per band basis, in n38, there is a PC2 introduced for NR V2X but there is no PC2 UE power class in Uu and as thus the above assumption of same power class of NR V2X and NR Uu will is not valid any more. Therefore, there is a need to report PC2 NR V2X and PC3 NR Uu power class separately even for the same band. This seems what Huawei propose, but as the LTE signaling is only 1 bit on HPUE, there is aslo an ambiguity whether it is PC2 or PC1 NR V2X. So if the LS is to be sent, maybe it is good to indicate if there is different HPUE power class to RAN2 may be needed to be aware. This seems the case for the intra-band (NR V2X + NR Uu ).For inter-band, perhaps the current signaling would be ok. The V2X band and Uu band would be indicated as combination and thus the power class is reported also separately. Huawei: Option 1. Similar to LTE-V2X, additional power class reported via Uu RRC message is needed. Noted that PC3 is the default V2X power class, no need to introduce the additional V2X capability.Xiaomi2: We share similar understanding of Ericsson as currently, the ambiguity exists when intra-band concurrent operation with different power class of each interface (Uu and PC5). For other cases as analyzed in our paper, the specific PC2 V2X capability per-band is not needed. But for intra-band concurrent operation, separate power class per interface within one band should be defined.Vivo: Option 2.OPPO: Option 1.QCOM: Option 1. Our understand is signaling is needed. |
| 1-3: power class capability for NR V2X intra-band concurrent operation | ***Whether need to define specific power class capability signalling for NR V2X intra-band concurrent operation?***Xiaomi: We believe the capability is needed as explained in our paper R4-2112608.CATT: Option 1.LGE: prefer option 1Ericsson: Option 1. See above.Huawei: Option 1. Vivo: For now, only unlicensed band n47 is clear to support HPUE. We can clarify Issue 1-1 and then decide for the intra-band concurrent operation.OPPO: Option 1.QCOM: Option 1 |
| Others |  |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
|  | Company A |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Topic#1** | **Issue 1-1: Clarification of PC2 HPUE operating bands***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 1-2: NR V2X power class capability***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 1-3: power class capability for NR V2X intra-band concurrent operation***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |
| #2 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
|  |  |  |
|  |  |  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
|  |  |
|  |  |

# Topic #2: MPR/A-MPR requirements

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [**R4-2112678**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112678.zip) | LG Electronics | **TP for TR 38.785 on MPR and AMPR for NR V2X PC2** |
|  |  |  |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Issue 2-1: MPR/A-MPR requirements for PC2 NR V2X

***2-1-1: TP on MPR/A-MPR requirements for PC2 NR V2X UE*** *(R4-2112678 LGE)*

* ***Option 1****: Agree the TP.*
* ***Option 2****: FFS*

***Moderator’s recommendation:***

* Recommended WF
	+ Option 1

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Issues** | **Company Comments** |
| Issue 2-1: MPR/A-MPR requirements for PC2 NR V2X  | **LGE:** For the MPR/A-MPR of PC2 NR V2X UE, RAN4 can captured the approved contents in WF (R4-2107873) at last RAN4 meeting.The MPR/A-MPR for PC2 PSFCH, PC2 S-SSB will be captured based on WF(R4-2107873).Huawei: Agree to capture the TP based on agreed WF.QCOM: TP is agreeable |
|  |  |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| [**R4-2112678**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112678.zip)(TP for TR 38.785 on MPR and AMPR for NR V2X PC2) | Company A |
| Company B |
|  |
|  | Company A |
| Company B |
|  |
|  | Company A |
| Company B |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Topic#2** | **Issue 2-1-1: MPR/A-MPR requirements for PC2 NR V2X***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
|  |  |  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
|  |  |

# Topic #3: Co-existence study

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [**R4-2111946**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2111946.zip) | CATT | **Observation 1: RAN4 have specified adjacent channel coexistence scenarios for PC2 NR V2X. Adjacent channel coexistence for band n38 (2.6GHz) is being evaluated, in which coexistence between band n38 and band n7 can be covered.****Proposal 1: To specify ACLR by coexistence evaluation to protect adjacent band n7 instead of A-MPR.** |
| [**R4-2112602**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112602.zip) | Xiaomi | **draft CR for TS 38.101-3 PEMAX for intra-band concurrent operation (R16)** |
| [**R4-2112603**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112603.zip) | Xiaomi | **draft CR for TS 38.101-3 PEMAX for intra-band concurrent operation (R17)** |
| [**R4-2112611**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2112611.zip) | Xiaomi | **Observation 1: Using sl-maxTxPower instead of maxTxPower is acceptable for sidelink only operation.****Observation 2: Only using sl-maxTxPower or maxTxPower will cause problem for intra-band concurrent operation.****Observation 3: Inter-band concurrent operation configured output power scheme can be used as starting point for intra-band concurrent operation configured output power.****Proposal 1: For intra-band concurrent FDM operation, reuse the inter-band concurrent operation configured power scheme.****Proposal 2: For intra-band concurrent TDM operation, the configured power of NR apply for Uu interface while the configure power of NR SL apply for PC5 interface.** |
| [**R4-2113409**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113409.zip) | Huawei, HiSilicon | **TP to 38.785 to capture NR V2X PC2 coexistence results** |
| [**R4-2114336**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114336.zip) | Ericsson | **Proposal-1: update the** PEMAX,*c* **to consider the coexisting of NR V2X and NR Uu within the same licensed band.****Observation-1: The power control formula in TS 38.213 for NR V2X UE is associated with the serving cell and controlled by the network to activate/deactivate the PL compensation.****Proposal-2: use the wording of the associated cell c to define the Pcmax behavior of which maximum output power is limited by the IE P-max as the same as the NR Uu UE.****Observation-2: The co-channel coexistence between NR network and SL UE operating in out-of-coverage (Scenario #1) should be revisited when network IE p-max for NR Uu UE is configured with a lower value than IE maxTxPower. This corresponding the case where PC2 SL UE coexisting with PC3 NR Uu in band n38.****Observation-3: RAN4 should investigate the same/co-channel coexisting according to WID[3].****Proposal-3: Scenario #1 should be investigated for the co-channel coexisting between SL and NR Uu.** **Observation-4: The highest supported power class for V2X is difference with highest supported power class for Uu in band n38.****Observation#5: PC2 V2X UE could generate the co-channel interference before detecting in-coverage of network using current in-coverage detection criteria.****Proposal-3: LS could be sent to RAN2 asking for solution on the co-channel interference issue.** |
| [**R4-2114509**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2114509.zip) | Huawei, HiSilicon | ***Observation 1: New NS as well as A-MPR requirements need to be defined to guarantee the co-existence between adjacent band n38 and n7.******Proposal 1: Whether to continue the study of PC2 requirements for n38 especially for co-existence requirements between n38 and n7 depends on requests from operators.*** ***Proposal 2: The PC2 Uu requirements for n38 should be studied in a separate WI.*** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Issue 3-1: Co-existence study for n38 (SL) and adjacent band n7 (Uu)

***3-1-1: co-existence between n38(SL) and n7(Uu).***

* ***Option 1****: To specify ACLR by coexistence evaluation to protect adjacent band n7 instead of A-MPR.*
* ***Option 2****: Whether to continue the study of PC2 requirements for n38 especially for co-existence requirements between n38 and n7 depends on whether there are requests from operators.*

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion for above sub-issues

### Issue 3-2: configured output power for intra-band con-current operation

***3-2-1: Differentiate configured output power for TDM and FDM intra-band con-current operation*** *(R4-2112611, Xiaomi)*

* ***Option 1****: For intra-band concurrent FDM operation, reuse the inter-band concurrent operation configured power scheme. For intra-band concurrent TDM operation, the configured power of NR apply for Uu interface while the configure power of NR SL apply for PC5 interface.*
* ***Option 2****: FFS.*

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion for above sub-issues

***3-2-2: Update PCMAX for Uu and SL intra-band con-current operation***

* ***Option 1****: Proposal in draft CR R4-2112602 (Xiaomi).*
* ***Option 2****: use the wording of the associated cell c to define the Pcmax behavior of which maximum output power is limited by the IE P-max as the same as the NR Uu UE (R4-2114336, Ericsson).*
* ***Option 3****: FFS.*

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion for above sub-issues

***3-2-3: Update PEMAX for Uu and SL intra-band con-current operation***

* ***Option 1****: Proposal in (R4-2114336, Ericsson),* PEMAX,c is the value given by IE *maxTxPower*, defined by [TS 38.331], when the UE is not associated with a serving cell on the NR V2X carrier*.*
* ***Option 2****:FFS.*

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion for above sub-issues

### Issue 3-3: Co-channel co-existence

***3-3-1: Whether need to continue the study the of co-channel co-existence issues***

* ***Option 1****: Yes*
* ***Option 2****: No*

***Moderator’s recommendation:***

* Recommended WF
	+ TBA based on 1st round discussion for above sub-issues

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Issues** | **Company Comments** |
| 3-1: Co-existence study for n38 (SL) and adjacent band n7 (Uu) | ***3-1-1: co-existence between n38(SL) and n7(Uu).***CATT: Option 1.LGE: Prefer Option 2Ericsson: Option 3 (A-MPR needs be specified/studied to introduce the n38 band). Can we ignore A-MPR for regulatory requirement when introducing a new band?Huawei: Option 2. Co-existence mechanism between n38 and n7 is specified for Uu, which can be considered for NR V2X for n38, but there are no requirements for PC2 n38 yet. It is expected that interference would be larger for HPUE. Whether to have PC2 V2X for n38, it would be better to be based on request from operators. Vivo: Option 2.OPPO: Option 2. |
| 3-2: configured output power for intra-band con-current operation | ***3-2-1: Differentiate configured output power for TDM and FDM intra-band con-current operation***Xiaomi: As proponent of option 1, we think this method can help to overcome the ambiguity for intra-band concurrent operation as different power class for different interface.LGE: This issue will be treated in [135] e-mail thread for intra-band V2X con-current operation regardless of PC3/PC2 V2X UE. LGE provided TP for configured Tx power for intra-band V2X con-current operation in [135] email thread.Huawei: We think that same configured output power should be used for both TDM and FDM intra-band concurrent operation. Xiaomi2: To clarify, the TDM and FDM here is to differentiate same carrier and different carrier cases. So maybe same carrier and different carrier to be the justification condition is more appropriate as even for TDM still there can be different carrier cases. Vivo: In email thread [134]. Issue 2-3-1 relates to the issue here. They can be discussed together.***3-2-2: Update PCMAX for Uu and SL intra-band con-current operation***Xiaomi: As proponent of option 1, the method is to re-use the inter-band con-current operation method to derive the correct Pcmax for different carrier. CATT: Several comments on option 1:1. Subclause 6.2E.4.1 is specified for intra-band LTE V2X and NR V2X TDM operation (without Uu). It would be ambiguous to include intra-band Uu and V2X con-current operation in the same subclause.2. In Rel-16, common understanding is that only NR Uu & NR V2X con-current operation is specified in 38.101-1 and NR Uu & LTE V2X and LTE Uu & NR V2X con-current operation are specified in 38.101-3. Based on this principle, intra-band NR Uu and NR V2X should be included in 38.101-1 instead of 38.101-3.3. Both contiguous and non-contiguous cases should be considered.LGE: Generally, it shall be treated in [135] e-mail thread. The Pemax definition for intra-band V2X operation in licensed band, can be added additional Pemax definition. And The configured Tx power will be captured in TS38.101-1 for NR SL+ NR Uu in licensed band.LGE also provided configured Tx power in [135] e0mail thread to define configured Tx power for intra-band V2X con-current operation.Ericsson: Option 2 . Do we have a LTE uplink carrier for intra-band NR v2X operation in scope of the Rel-17 SL enh? For 2nd thing, the total Pcmax will depend on whether UE is dual PA or singla PA. Should clarify that In 38.101-3, the configured power for p, q overlapping depending whether the power sharing will be enabledHuawei: As commented for issue 3-2-1, we think that same configured output power should be applied for both TDM and FDM operation, which is the way we adopted for LTE V2X.Xiaomi 2: Reply to Ericsson, the inter-band concurrent operation of NR SL and LTE SL is used as an example, we are not adding LTE uplink carrier here. To Huawei, we might need to decide if same power class for Uu and PC5 interface for concurrent operation. If the same power class is applied then there should be no problem, but if different power class can be applied, then we might need to figure out how to handle the issue.QCOM: I think this is a thread 135 issue and any discussion should probably occur there.***3-2-3: Update PEMAX for Uu and SL intra-band con-current operation***CATT: Option 1.LGE : Option 1Ericsson: Option 1Huawei：The meaning of *sl*-*maxTxPower* is different from that of *maxTxPowerfor Uu,* instead *sl-MaxTransPower-r16* is defined by RAN2. In addition, to consider both coverage and out-of-coverage scenarios, “when the UE is not associated with a serving cell on the NR V2X carrier” should be removed. |
| 3-3: Co-channel co-existence | ***3-3-1: Whether need to continue the study the of co-channel co-existence issues***LGE: prefer option 2. The co-channel coexistence is not scope of RAN4. If it is needed, then RAN4 can send LS to RAN1 for the co-channel coexistence necessity.Ericsson: This topic has been discussed in several meetings and I am not sure companies are on the same page. Here I make some short introduction on this issue itself:The issue is related to the different power class definition for NR V2X and NR Uu. As the same discussion ongoing in the signalling side: the reason to define the new signalling is that there is a case where UE have two different power class for NR Uu operation and NR V2X operation. Companies may see this as an only signalling issue as traditionally it is RAN4 responsibility to notify RAN2 if there is a need to do so. We also see there is potential other RAN2 specification impact , e.g TS 38.304 which is a RAN2 specification. The issue relates to potential co-channel interference between NR Uu UE and NR V2X UE when V2X is configured in out-of-coverage operation. If companies think it is out of RAN4 scope to agree the TS 38.304 impact, it is ok to trigger a question to RAN2 at the same time the signalling is sent like the text below:*RAN4 would like to inform RAN2 that RAN4 decide to define different power class for NR V2X operation and NR Uu operation in one licensed operating band (n38) and thus UE can report different power class for NR V2X operation and NR Uu operation, for example, the PC2 for NR V2X and PC3 for NR Uu in n38, RAN4 kindly ask RAN2 to evaluate the RAN2 specification impact, if there are any.* Huawei: Option 2. It’s not clear by the clarification by Ericsson for the interference scenario where V2X is out-of-coverage. Besides, the example may not be appropriate using n38. Whether to consider PC2 for n38 is not decided yet. Xiaomi: The co-channel co-existence issue exists even without considering the signalling issue. For example as below figure 1: For UE2 and UE3 with sidelink communication, as UE2 and UE3 are out-of-coverage, it has no information about the cell situation. Then it might have interference to the network. How to trigger this interference issue might be RAN1 responsibility.Figure 1vivo: Option 2.OPPO: Option 2 maybe.Ericsson: The issue is the definition of the criteria for out-of-coverage and in-coverage. Using Xiaomi Figure 1 for example, It should be no interference from out-of-coverage to in-coverage even UE2 and UE1 is configured with the same carrier if such definition correctly reflects the different power class of NR V2X and NR Uu operation. For high power class NR V2X, if it sees the same in-coverage criteria with PC3 NR V2X, it could generate interference to the network. But we understand also it may belong to RAN2 discussion domain and thus a LS to ask them to investigate maybe more suitable.  |
| Others |  |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| [**R4-2113409**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_100-e/Docs/R4-2113409.zip)(TP to 38.785 to capture NR V2X PC2 coexistence results) | Company A |
| Company B |
|  |
|  | Company A |
| Company B |
|  |
|  | Company A |
| Company B |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Topic#3** | **Issue 3-1-1: co-existence between n38(SL) and n7(Uu)***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 3-2-1: configured output power for TDM and FDM intra-band con-current operation***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 3-2-2: Update PCMAX for Uu and SL co-existence scenario***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 3-2-3: Update PEMAX for Uu and SL co-existence scenario***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:***Issue 3-3-1: Whether need to continue the study the of co-channel co-existence issues***Tentative agreements:* *Candidate options:* *Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
|  |  |  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
|  |  |

# Recommendations for Tdocs

## 1st round

**New tdocs**

|  |  |  |
| --- | --- | --- |
| **Title** | **Source** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |

**Existing tdocs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics incl. existing and new tdocs.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. For new LS documents, please include information on To/Cc WGs in the comments column
4. Do not include hyper-links in the documents

## 2nd round

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
| R4-210xxxx | WF on … | YYY | Agreeable, Revised, Noted |  |
| R4-210xxxx | LS on … | ZZZ | Agreeable, Revised, Noted |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. Do not include hyper-links in the documents