**3GPP TSG-RAN WG4 Meeting # 100-e R4-2115321**

**Electronic Meeting, August 16-27, 2021**

**Agenda item:** 6.1.8

**Source:** CATT

**Title:** WF on CSI-RS based L3 measurement requirements

**Document for:** Approval

### Sub-topic 1-1 Time domain restriction for CSI-RS configuration

**Issue 1-1-1: Whether the conclusions in FR1 are applied to FR2?**

**Issue 1-1-2: The applicability condition of CSI-RS measurement window alignment for CSSF requirements?**

Agreements:

* The conclusions of time domain restriction for FR1in RAN4#99e meeting are also applied to FR2.
* For FR2 intra-frequency CSI-RS measurement, use the same applicability condition regarding measurement window alignment as SSB measurement.

### Sub-topic 1-2 UE behavior when the timing offset exceeds the threshold with single FFT assumption

Agreements:

* No spec updates are needed for UE behavior when the timing offset exceeds the threshold with single FFT assumption.
* Common understanding is that the measurement reporting for CSI-RS based L3 measurements shall fulfil the requirements in section 9.10.2.4 and 9.10.3.4 in TS 38.133.