3GPP TSG-RAN WG4 Meeting # 100-e Draft R4-2115665

**Electronic Meeting, August. 16-27, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.113** | **CR** |  | **rev** |  | **Current version:** | **15.14.0** |  |
|  | | | | | | | | |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)*** *on using this form: comprehensive instructions can be found at  <http://www.3gpp.org/Change-Requests>.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to TS 38.113 on Spatial Exclusion description, Release 15 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2021-08-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Clarification in the definition of spatial exclusion. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This Cat. F updates the definition of spatial exclusion for Release 15. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Lack of clarity in the definition of spatial exclusion migh lead to wrong testing procedures. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

------------------------------ Start of new section ------------------------------

### 9.2.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑3 [18], which specified test methodology based on anechoic chamber. The use of reverberation chamber test method according to IEC 61000-4-21 [29], clause 6.1 and Annex D as alternative method is allowed.

For transmitters, receivers and transceivers the following requirements shall apply:

- The test level shall be 3 V/m amplitude modulated to a depth of 80 % by a sinusoidal audio signal of 1 kHz;

- The stepped frequency increments shall be 1 % of the momentary frequency;

- The test shall be performed over the frequency range 80 MHz - 6000 MHz; with the exception of the exclusion band for receivers (see clause 4.4);

- Responses in stand-alone receivers or receivers which are part of transceivers occurring at discrete frequencies which are narrow band responses, shall be disregarded, see clause 4.3;

- The frequencies selected during the test shall be recorded in the test report.

- For the test method in accordance with IEC 61000-4-3[18], the *spatial exclusion zone* can be chosen to protect the base station receiver. For the frequency arrange above 690 MHz (according to the test method in ETSI EN 301 489-50 [28]), the EMC RF electromagnetic field immunity requirement applies on the non-radiating faces of the *BS type 1-O* and *BS type 2-O, as depicted on figure 9.2.2-1*. In other cases, to protect the *BS type 1-O* and *BS type 2-O*, exclusion band sizes as depicted in Table 4.4.2-1 shall be considered.




Figure 9.2.2-1: EMC RF electromagnetic field immunity requirement testing directions for *BS type 1-O* and *BS type 2-O* (horizontal plane depicted) with the *spatial exclusion zone* applied

----------------------------- End of proposed text ------------------------------