**3GPP TSG-WG4 Meeting #102-e *R4-2206524***

**Electronic Meeting, Feb 21- Mar 03, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** |  | **rev** | **1** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  draft CR for 38.101-1: introduction of PC2 TxD for SL |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core |  | ***Date:*** | 2022-02-13 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Introduce necessary changes to enable PC2 TxD for SL based on the endorsed CR in R4-2201953. |
|  |  |
| ***Summary of change:*** | Implement all relevant changes to the NR V2X clauses, inclusing:* UE maximum output power reduction for V2X
* MPR for V2X UE

 Note: some further update is needed once the PC2 requirements for V2X are agreed. The changes in this meeting on top of endorsed CR R4-2201953 use the change mark of Huawei RAN4#102e.  |
|  |  |
| ***Consequences if not approved:*** | PC2 TxD is not supported by NR V2X. |
|  |  |
| ***Clauses affected:*** | 6.2E.1.1, 6.2E.2.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-1 |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Separate PC2 MPR requirement for 1Tx and 2Tx. |

## **<Start of Change>**

### 6.2E.2 UE maximum output power reduction for V2X

#### 6.2E.1.1 General

When NR V2X UE is configured for NR V2X sidelink transmissions non-concurrent with NR uplink transmissions for NR V2X operating bands specified in Table 5.2E.1-1, the allowed NR V2X UE maximum output power is specified in Table 6.2.1-1 in clause 6.2.1.

When a UE is configured for NR V2X sidelink transmissions in NR Band n47, the V2X UE shall meet the following additional requirements for transmission within the frequency ranges 5855-5925 MHz:

- The maximum mean power spectral density shall be restricted to 23 dBm/MHz EIRP when the network signaling value NS\_33 is indicated.

where the network signaling values are specified in clause 6.2E.3.

NOTE: The PSD limit in EIRP shall be converted to conducted requirement depend on the supported post antenna connector gain Gpost connector declared by the UE following the principle described in annex I in [11].

For NR V2X UE supporting SL MIMO or Tx diversity, the maximum output power requirements in Table 6.2E.1.1-1 is defined as the sum of the maximum output power from each UE antenna connector. The period of measurement shall be at least one sub frame (1 ms). For UE supporting SL MIMO, the requirements shall be met with the SL MIMO configurations specified in Table 6.2D.1-2

Table 6.2E.1.1-1: NR V2X UE Power Class for SL-MIMO

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR band | Class 1 (dBm) | Tolerance (dB) | Class 2 (dBm) | Tolerance (dB) | Class 3 (dBm) | Tolerance (dB) | Class 4 (dBm) | Tolerance (dB) |
| n38 |  |  |  |  | 23 | +2/-3 |  |  |
| n47 |  |  | 26 | +2/-3 | 23 | +2/-3 |  |  |

If the UE transmits on one antenna connector at a time, the requirements in Table 6.2.1-1 shall apply to the active antenna connector.

### **<Next Change>**

#### 6.2E.2.2 MPR for V2X UE

For contiguous allocation of PSCCH and PSSCH simultaneous transmission, the allowed MPR for the maximum output power for NR V2X physical channels PSCCH and PSSCH shall be as specified in Table 6.2E.2.2-1 for Power class 3 and in Table 6.2E.2.2-2 for Power class 2 NR V2X UE.

Table 6.2E.2.2-1: Maximum Power Reduction (MPR) for power class 3 NR V2X

|  |  |
| --- | --- |
| Modulation | Channel bandwidth/MPR (dB) |
|  | Outer RB allocations | Inner RB allocations |
| CP-OFDM | QPSK | ≤ 4.5 | ≤ 2.5 |
|  | 16QAM | ≤ 4.5 | ≤ 2.5 |
|  | 64 QAM | ≤ 4.5 |
|  | 256 QAM | ≤ 7.0 |

Table 6.2E.2.2-2: Maximum Power Reduction (MPR) for power class 2 NR V2X

|  |  |
| --- | --- |
| **Modulation** | **Channel bandwidth/MPR (dB)** |
| **Outer RB allocations** | **Inner RB allocations** |
| CP-OFDM  | QPSK | ≤ 5.5 | ≤ 2.5 |
| 16QAM |
| 64 QAM | ≤ 6.0 | ≤ 4.5 |
| 256 QAM | ≤ 7.0 |

For NR V2X UE supporting SL MIMO or Tx diversity, the allowed MPR for the maximum output power for NR V2X physical channels PSCCH and PSSCH are specified in Table 6.2E.2.2-3 for power class 2 UE.

Table 6.2E.2.2-3: Maximum Power Reduction (MPR) for power class 2 NR V2X with dual Tx

|  |  |
| --- | --- |
| **Modulation** | **Channel bandwidth/MPR (dB)** |
| **Outer RB allocations** | **Inner RB allocations** |
| CP-OFDM  | QPSK | [≤ 6.0] | [≤ 3.0] |
| 16QAM |
| 64 QAM | [≤ 7.0] | [≤ 5.5] |
| 256 QAM | [≤ 9.0] |

Where the following parameters are defined to specify valid RB allocation ranges for Outer and Inner RB allocations:

NRB is the maximum number of RBs for a given Channel bandwidth and sub-carrier spacing defined in Table 5.3.2-1.

RBStart,Low = max(1, floor(LCRB/2))

where max() indicates the largest value of all arguments and floor(x) is the greatest integer less than or equal to x.

RBStart,High = NRB – RBStart,Low – LCRB

The RB allocation is an Inner RB allocation if the following conditions are met

RBStart,Low ≤ RBStart ≤ RBStart,High,and

LCRB ≤ ceil(NRB/2)

where ceil(x) is the smallest integer greater than or equal to x.

The RB allocation is an Outer RB allocation for all other allocations which are not an Inner RB allocation.

For PSFCH with single RB transmission for PC3 and PC2 NR V2X UE, the required MPR is defined as follow

MPR\_PSFCH = 3.5 dB

For contiguous and non-contiguous allocation for simultaneous PSFCH transmission for PC3 and PC2 NR V2X UE, the required MPR are specified as follow

MPR\_PSFCH = CEIL {MA\_PSFCH, 0.5}

Where MA\_PSFCH is defined as follows

MA\_PSFCH = 7.5 ; 0.00< NGap/NRB ≤ 0.55

= 12.0 ; 0.55< NGap/NRB ≤1.0

Where,

NGap is the gap RB amount between RBstart and RBend for contiguous and non-contiguous allocation simultaneous PSFCH transmission. (NGap = RBend - RBstart)

CEIL{MA, 0.5} means rounding upwards to closest 0.5dB.

The allowed MPR for the maximum output power for NR V2X physical channels on S-SSB transmission shall be specified in Table 6.2E.2.2-2.

Table 6.2E.2.2-2: Maximum Power Reduction (MPR) for S-SSB transmission for NR V2X

|  |  |
| --- | --- |
| Channel | MPRS-SSB (dB) |
|  | Outer RB allocations | Inner RB allocations |
| S-SSB | ≤ 6.0 | ≤ 2.5 |

For NR V2X UE with two transmit antenna connectors, the allowed Maximum Power Reduction (MPR) values specified in clause 6.2E.2 for PC3 and PC2 shall apply to the maximum output power specified in Table 6.2E.1.1-1. For UE supporting SL MIMO, the requirements shall be met with SL MIMO configurations defined in Table 6.2D.1-2. For UE supporting SL MIMO or Tx diversity, the maximum output power is defined as the sum of the maximum output power from each UE antenna connector.

For the UE maximum output power modified by MPR, the power limits specified in clause 6.2E.4 apply.

## **<End of Change>**