**3GPP TSG-RAN WG4 Meeting #103-e *R4-2209265***

**Electronic Meeting, 9 - 20 May, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **1090** | **rev** | **-** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Big CR on Introduction of completed 5 bands inter-band CA into TS 38.101-1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R17\_5BDL\_xBUL -Core | | | | |  | ***Date:*** | | | 2022-05-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Based on the TR 38.862, it’s agreed to simplify the configuration table. Thus, the configuration table format is simplified in Table 5.5A.3.4-1.  Correcting 5DL configuration table | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | the configuration table format is simplified in Table 5.5A.3.4-1.  Removing redundant CA\_n2A-n5A-n48B-n66A-n77A BCS1 since n48 wrongly referred to n48A and the other bands where exactly like BCS0 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The simplified configuration table can not be implemented.  5DL configuration table not corrected | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A.3.4 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## **<<Start of Change>>**

#### 5.5A.3.4 Configurations for inter-band CA (five bands)

Table 5.5A.3.4-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (five bands)

| NR CA configuration | Uplink configuration | NR Band | Channel bandwidth (MHz) (NOTE 1) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n1A-n3A-n5A-n7A-n78A | CA\_n1A-n3A CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A CA\_n5A-n7A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n5A-n78A CA\_n7A-n78A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n5A-n7B-n78A | CA\_n1A-n3A CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A CA\_n5A-n7A | n7 | See CA\_n7B bandwidth combination set 0 in Table 5.5A.1-1 |  |
|  | CA\_n5A-n78A CA\_n7A-n78A  CA\_n7B | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n28A-n78A | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7B-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | See CA\_n7B bandwidth combination set 0 in Table 5.5A.1-1 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n1A-n28A  CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n78A  CA\_n7A-n28A | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n7A-n78A  CA\_n28A-n78A | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 |  |
| CA\_n2A-n5A-n48A-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48B-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n48B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | See CA\_n48B Bandwidth Combination Set 2 in Table 5.5A.1-1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A-n66A-n77C | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | See CA\_n77C Bandwidth Combination Set 1 in Table 5.5A.1-1 |  |
| NOTE 1: The SCS of each channel bandwidth for NR FR1 and NR FR2 band refers to Table 5.3.5-1 of TS 38.101-1 and TS 38.101-2 respectively. | | | | |



## **<<End of Change>>**