**3GPP TSG-RAN WG4 Meeting #104-e draft R4-22xxxxx**

**<Electronic Meeting>, 15 ‒ 26 August, 2022**

**Title:** WF on testability aspect of BC in RRC\_INACTIVE and initial access

**Agenda Item:** 11.7.4

**Source: Nokia**

**Document for:** Approval

# Sub-topic 1: Rel-18 Beam Correspondence Test Issues

**Way forward/Agreement:**

* BC test for RRC\_INACTIVE and IA is at UE maximum output power
* BEAM\_LOCK is not available in RRC\_INACTIVE and IA mode

**Way forward/FFS:**

* FFS: discuss if and how UE Tx beam should/would change during IA and what are the impact on the test method.
* FFS: Feasibility of testing UEs in Inactive mode
* FFS: Feasibility of triggering SDT in test mode
* FFS: Without beam lock function, achieving UE max output power may be done by holding RAR message to enable power ramping until maximum output power and implication on UE implementation of beam/panel choice during IA.
* FFS: Number of tests, test time implications and proposed test time reductions
* FFS: polarization aspects in testing

|  |  |
| --- | --- |
| Company | Agree/Disagree, include justification |
|  |  |
|  |  |
|  |  |
|  |  |