**3GPP TSG-RAN WG4 Meeting # 104-e R4-2214326**

**Electronic Meeting, Aug.15-26, 2022**

**Agenda item:** 9.4.7

**Source:** Moderator (Nokia, Nokia Shanghai Bell)

**Title:** WF on RRM requirements for FR2 Inter-band DL CA and UL CA

**Document for:** Approval

# Topic #1: RRM performance requirement

**Issue 1-1 Test cases for FR2 inter-band UL CA for IBM**

*Agreements on GTW (Aug. 22):*

*Regarding test cases for FR2 inter-band UL CA for IBM*

* *In FR2 inter-band UL CA, an SCell is assumed always configured with DL+UL.*
* *Existing SCell activation TCs in FR2 inter-band scenarios can be applied.*

# References

[1] R4-2214256, Email discussion summary for [104-e][204] NR\_RF\_FR2\_req\_enh2\_RRM