3GPP TSG-RAN WG4 Meeting # 104-e R4-2214560

Electronic Meeting, August 15 – August 26, 2022

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | 2419 | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | FR2 HST Scheduling restriction on SSB |
|  |  |
| ***Source to WG:*** | Qualcomm Inc. |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_HST\_FR2-Core |  | ***Date:*** | 08/10/2022 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | We have the following agreement from RAN4#103e meeting WF (R4-2210608):**Issue 2-1-1: Scheduling restriction on SSB****Agreement**:FR2 HST requirement is applicable only when the two SSBs from adjacent RRHs are not on the adjacent symbols.And the following agreement from RAN4#100e meeting WF (R4-2115335):**Non-overlapping SSB location** * RRM requirements specified in RAN4 will NOT consider SSB overlapping case.

This CR captures the above agreements. |
|  |  |
| ***Summary of change:*** | Capture WF agreement on scheduling restrictions on SSB |
|  |  |
| ***Consequences if not approved:*** | Spec is contradict to the previous agreement |
|  |  |
| ***Clauses affected:*** | 3.6.14 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.533 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### 3.6.14 Applicability of requirements for FR2 Power Class 6

For Rel-17 FR2 power class 6 for the UE type of high speed train roof-mounted UE, UE shall only be in NR SA operation. Measurement and evaluation period requirements with highSpeedMeasFlagFR2-r17 configured in clause 4.2.2.3, 8.1.2.2, 8.5.2.2, 9.2.5, 9.2.6, 9.5.4, [9.8.4], delay requirements in clause 6.2.1.2.1, 8.10.3A, and UL timing adjustment in clause 7.1.2.3, are only applicable when any two SSBs from adjacent [RRHs] [21, clause B.3] are not on the same or consecutive symbols.