3GPP TSG-RAN WG4 Meeting # 104-e R4-2214560

Electronic Meeting, August 15 – August 26, 2022

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | 2419 | **rev** | **1** | **Current version:** | **17.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | FR2 HST Scheduling restriction on SSB |
|  |  |
| ***Source to WG:*** | Qualcomm Inc. |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_HST\_FR2-Core |  | ***Date:*** | 08/10/2022 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | We have the following agreement from RAN4#103e meeting WF (R4-2210608):**Issue 2-1-1: Scheduling restriction on SSB****Agreement**:FR2 HST requirement is applicable only when the two SSBs from adjacent RRHs are not on the adjacent symbols.And the following agreement from RAN4#100e meeting WF (R4-2115335):**Non-overlapping SSB location** * RRM requirements specified in RAN4 will NOT consider SSB overlapping case.

This CR captures the above agreements. |
|  |  |
| ***Summary of change:*** | Capture WF agreement on scheduling restrictions on SSB and add abbreviation |
|  |  |
| ***Consequences if not approved:*** | Spec is contradict to the previous agreement |
|  |  |
| ***Clauses affected:*** | 3.3, 3.6.14 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.533 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [11] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [11].

AoA Angle of Arrival

AoD Angle of Departure

BFD Beam Failure Detection

BFD-RS BFD Reference Signal

BLER Block Error Rate

BM-RS Beam Management Reference Signal

BWP Bandwidth Part

CA Carrier Aggregation

CBD Candidate Beam Detection

CBW Channel Bandwidth

CC Component Carrier

CCA Clear Channel Assessment

CG-SDT Configured Grant Small Data Transmisison

CLI Cross Link Interference

CMR Channel Measurement Resource

CORESET Control Resource Set

CP Cyclic Prefix

CSI Channel-State Information

CSI-RS CSI Reference Signal

CSI-RSRP CSI Reference Signal based Reference Signal Received Power

CSI-RSRQ CSI Reference Signal based Reference Signal Received Quality

CSI-SINR CSI Reference Signal based Signal to Noise and Interference Ratio

CSI\_RP Received (linear) average power of the resource elements that carry NR CSI-RS signals and channels, measured at the UE antenna connector

DBT Discovery Burst Transmission

DC Dual Connectivity

DCI Downlink Control Information

DL Downlink

DL-AoD Downlink Angle-of-Departure

DL-TDOA Downlink Time Difference Of Arrival

DMRS Demodulation Reference Signal

DRX Discontinuous Reception

E-CID Enhanced Cell ID

E-UTRA Evolved UTRA

E-UTRAN Evolved UTRAN

EN-DC E-UTRA-NR Dual Connectivity

FDD Frequency Division Duplex

FR Frequency Range

HARQ Hybrid Automatic Repeat Request

HO Handover

GAP Refers to any of the measurement gap pattern, activated Pre-MG and NCSG

IMR Interference Measurement Resource

L1-RSRP Layer 1 RSRP

L1 SL-RSRP Layer 1 Sidelink RSRP which corresponds to PSCCH-RSRP and/or PSSCH-RSRP

LMF Location Management Function

LPP LTE Positioning Protocol

MAC Medium Access Control

MCG Master Cell Group

MDT Minimization of Drive Tests

MG Measurement Gap

MGL Measurement Gap Length

MGRP Measurement Gap Repetition Period

MIB Master Information Block

ML Measurement Length

MN Master Node

MR-DC Multi-Radio Dual Connectivity

MUSIM Multi-Universal Subscriber Identity Module

NCSG Network Controlled Small Gap

NE-DC NR-E-UTRA Dual Connectivity

NGEN-DC NG-RAN E-UTRA-NR Dual Connectivity

NR New Radio

NR-DC NR-NR Dual Connectivity

OFDM Orthogonal Frequency Division Multiplexing

OFDMA Orthogonal Frequency Division Multiple Access

OTDOA Observed Time Difference Of Arrival

PBCH Physical Broadcast Channel

PCC Primary Component Carrier

PCell Primary Cell

PDCCH Physical Downlink Control Channel

PDSCH Physical Downlink Shared Channel

PLMN Public Land Mobile Network

PRACH Physical RACH

Pre-MG Pre-configured Measurenent Gap

PRP PRS Received Power

PRS Positioning Reference Signal

PRS-RSRP Positioning Reference Signal based Reference Signal Received Power

PSBCH Physical Sidelink Broadcast Channel

PSBCH-RSRP Physical Sidelink Broadcast Channel DMRS based Reference Signal Received Power

PSCCH Physical Sidelink Control Channel

PSCCH-RSRP Physical Sidelink Control Channel DMRS based Reference Signal Received Power

PSCell Primary SCell

PSS Primary Synchronization Signal

PSSCH Physical Sidelink Shared Channel

PSSCH-RSRP Physical Sidelink Shared Channel DMRS based Reference Signal Received Power

pTAG Primary Timing Advance Group

PUCCH Physical Uplink Control Channel

PUSCH Physical Uplink Shared Channel

QCL Quasi Co-Location

RACH Random Access Channel

RAT Radio Access Technology

RLM Radio Link Monitoring

RLM-RS Reference Signal for RLM

RMSI Remaining Minimum System Information

RRC Radio Resource Control

RRH Remote Radio Head

RRM Radio Resource Management

RSSI Received Signal Strength Indicator

RSRP Reference Signal Received Power

RSRQ Reference Signal Received Quality

RSTD Reference Signal Time Difference

RTT Round Trip Time

S-SSB Sidelink Synchronization Signal Block

SSB\_RP Received (linear) average power of the resource elements that carry NR SSB signals and channels, measured at the UE antenna connector or radiated interface boundary.

SA Standalone operation mode

SCC Secondary Component Carrier

SCell Secondary Cell

SCG Secondary Cell Group

SCS Subcarrier Spacing

SCSSSB SSB subcarrier spacing

SDL Supplementary Downlink

SDT Small Data Transmission

SFN System Frame Number

SFTD SFN and Frame Timing DifferenceSI System Information

SIB System Information Block

SL-RSSI Sidelink Received Signal Strength Indicator

SLSS Sidelink Synchronization Signal

SMTC SSB-based Measurement Timing configuration

SpCell Special Cell

SRS Sounding Reference Signal

SRS-RSRP Sounding Reference Signal based Reference Signal Received Power

SS-RSRP Synchronization Signal based Reference Signal Received Power

SS-RSRQ Synchronization Signal based Reference Signal Received Quality

SS-SINR Synchronization Signal based Signal to Noise and Interference Ratio

SSB Synchronization Signal Block

SSB\_RP Received (linear) average power of the resource elements that carry NR SSB signals and channels, measured at the UE antenna connector.

SSS Secondary Synchronization Signal

sTAG Secondary Timing Advance Group

SUL Supplementary Uplink

TA Timing Advance

TAG Timing Advance Group

TCI Transmission Configuration Indicator

TDD Time Division Duplex

TDOA Time Difference Of Arrival

TRP Transmission-Reception Point

TTI Transmission Time Interval

UE User Equipment

UL Uplink

VIL Visible Interruption Length

VIRP Visible Interruption Repetition Period

### 3.6.14 Applicability of requirements for FR2 Power Class 6

For Rel-17 FR2 power class 6 for the UE type of high speed train roof-mounted UE, UE shall only be in NR SA operation. Measurement and evaluation period requirements with highSpeedMeasFlagFR2-r17 configured in clause 4.2.2.3, 8.1.2.2, 8.5.2.2, 9.2.5, 9.2.6, 9.5.4, [9.8.4], delay requirements in clause 6.2.1.2.1, 8.10.3A, and UL timing adjustment in clause 7.1.2.3, are only applicable when any two SSBs from adjacent [RRHs] are not on the same or consecutive symbols.