{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Simulation Assumption for BS ","Parameters","PUSCH ","UL timing ajustment ","PRACH"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #104-e",null,null,null,null,null,null,null,"R4-2213659"]
[null,"Electronic meeting, 15 Aug - 26, Aug, 2022"]
[]
[null,"Source: Samsung"]
[null,"Title: Simulation results summary for Rel-17 FR2 HST BS demod"]
[null,"Agenda: 9.7.4.2"]
[null,"Document for: Information"]

{"sheet":"Simulation Assumption for BS ","index":1,"n_rows":80,"n_cols":4,"rows_kept":80,"cut":false,"hidden":false,"merged":[[9,1,17,1],[11,2,13,2],[2,1,2,2],[3,1,3,2],[4,1,5,2],[6,1,6,2],[7,1,8,1],[45,1,47,1],[45,2,47,2],[18,1,20,1],[21,1,23,1],[24,1,24,2],[25,1,26,1],[27,1,27,2],[28,1,29,2],[34,1,34,2],[35,1,35,2],[36,1,37,2],[38,1,38,2],[39,1,39,2],[79,1,80,1],[51,1,52,1],[51,2,52,2],[55,1,56,1],[55,2,56,2],[57,1,58,1],[57,2,58,2],[60,1,61,1],[60,2,61,2],[62,1,64,1],[62,2,64,2],[65,1,65,3]]}
[]
["PUSCH "]
[null,"Parameter",null,"Value"]
[null,"Transform precoding",null,"Disabled"]
[null,"Default TDD UL-DL pattern (Note 1)",null,"120kHz SCS:"]
[null,null,null,"3D1S1U, S=10D:2G:2U"]
[null,"Antenna layout",null,"1T2R, ULA Low Correlation"]
[null,"HARQ","Maximum number of HARQ transmissions",4]
[null,null,"RV sequence","0, 2, 3, 1"]
[null,"DM-RS","DM-RS configuration type",1]
[null,null,"DM-RS duration","single-symbol DM-RS"]
[null,null,"Additional DM-RS symbols","Option1: 1+0"]
[null,null,null,"Option2: 1+1"]
[null,null,null,"Option3: 1+1+1"]
[null,null,"Number of DM-RS CDM group(s) without data",2]
[null,null,"Ratio of PUSCH EPRE to DM-RS EPRE","-3 dB"]
[null,null,"DM-RS port(s)",0]
[null,null,"DM-RS sequence generation","NID=0, nSCID =0"]
[null,"Time domain resource","PUSCH mapping type","B"]
[null,null,"Start symbol index",0]
[null,null,"Allocation length",10]
[null,"Frequency domain resource","RB assignment","Full applicable test bandwidth"]
[null,null,"Frequency hopping","Disabled"]
[null,null,"Bandwidth","50MHz and 200MHz"]
[null,"Code block group based PUSCH transmission",null,"Disabled"]
[null,"PT-RS configuration","Frequency density (KPT-RS)","KPT-RS=2"]
[null,null,"Time density (LPT-RS)","LPT-RS = 1"]
[null,"MCS",null," MCS19(64 QAM table)"]
[null,"Propagation channel",null,"Bi-directional with sceanro B"]
[]
[]
[]
["UL Timing adjustment "]
[]
[null,"Parameter",null,"Value"]
[null,"Transform precoding",null,"Disabled"]
[null,"Uplink-downlink allocation for TDD",null,"120kHz SCS:"]
[null,null,null,"3D1S1U, S=10D:2G:2U"]
[null,"Channel bandwidth",null,"120KHz SCS:   50MHz and 200MHz"]
[null,"MCS",null,16]
[null,"HARQ","Maximum number of HARQ transmissions",4]
[null,null,"RV sequence","0, 2, 3, 1"]
[null,"DM-RS","DM-RS configuration type",1]
[null,null,"DM-RS duration","single-symbol DM-RS"]
[null,null,"DM-RS position (l0)",0]
[null,null,"Additional DM-RS position","option 1: 1+0"]
[null,null,null,"option 2: 1+1"]
[null,null,null,"option 3: 1+1+1"]
[null,null,"Number of DM-RS CDM group(s) without data",2]
[null,null,"Ratio of PUSCH EPRE to DM-RS EPRE","-3 dB"]
[null,null,"DM-RS port","{0}"]
[null,"Time domain resource assignment","DM-RS sequence generation","NID0=0, nSCID =0 for moving UE"]
[null,null,null,"NID0=1, nSCID =1 for stationary UE"]
[null,null,"PUSCH mapping type","B"]
[null,null,"Allocation length",10]
[null,"Frequency domain resource assignment","RB assignment","50MHz CBW:   16RBs for each UE, Moving UE RBs: 0~15; Stationary UE RBs: 16~31"]
[null,null,null,"200MHz CBW:  66RBs for each UE, Moving UE RBs: 0~65, Stationary UE RBs: 66~131"]
[null,null,"Starting PRB index","Moving UE: 0 "]
[null,null,null,"Stationary UE: 16 for 50MHz and 66 for 200MHz"]
[null,null,"Frequency hopping","Disabled"]
[null,"SRS resource allocation","Slots in which sounding RS is transmitted (Note 1)","For TDD: "]
[null,null,null,"  - last symbol in slot #3 in radio frames for 120KHz"]
[null,null,"SRS resource allocation","120 kHz SCS: "]
[null,null,null,"  - 50MHz CBW (32RBs)~C_SRS =9, B_SRS=0"]
[null,null,null,"  - 200MHz CBW (132RBs)~C_SRS =33, B_SRS=0"]
[null,"NOTE 1. The transmission of SRS is optional. And the transmission comb and SRS periodic are configured as KTC = 2, and TSRS= 10 respectively."]
[]
[]
[]
["PRACH"]
[]
[null,"Parameters","Value"]
[null,"Ncs",0]
[null,"Logical sequence index ",0]
[null,"v",0]
[null,"Channel ","AWGN"]
[null,"Antenna configuration","1T2R"]
[null,"SCS","120KHz"]
[null,"Frequency offset ","19444Hz"]
[null,"Timing offset ","0:0.48:4.8"]

{"sheet":"Parameters","index":2,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH ","index":3,"n_rows":8,"n_cols":27,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,8],[0,21,0,22],[0,25,0,26],[0,9,1,9],[0,11,0,12],[0,13,0,14],[0,10,1,10],[0,15,0,16],[0,17,0,18],[0,23,0,24],[0,19,0,20],[2,2,7,2],[2,3,7,3],[2,0,7,0],[2,4,7,4],[2,5,7,5],[2,1,7,1]]}
["  PUSCH",null,null,null,null,null,null,null,null,"38.104 req","38.141 req","Samsung",null,"Nokia",null,"Huawei",null,"Ericcson",null,"Intel",null,"CATT",null,"SPAN",null,"AVERAGE"]
["Scenario","FOE method","Channel","Frequency offset","DMRS mapping type ","PUSCH data length ","BW","MCS","RS configuration",null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Bi-directional B","Post-FFT","AWGN",9722,"B",10,"120kHz, 50MHz","MCS19","DMRS 1+0",{"$f":"DerivingPerfReq(L3:W3)","v":12.9},{"$f":"IF(J3>-100,J3+0.6,J3)","v":13.5},11.1,13.6,9.1199999999999992,12.22,10.29,12.79,10.3,12.5,12.6,null,10.94,13.44,{"$f":"MAX(L3,N3,P3,R3,T3,V3)-MIN(L3,N3,P3,R3,T3,V3)","v":3.4800000000000004},{"$f":"MAX(M3,O3,Q3,S3,U3,W3)-MIN(M3,O3,Q3,S3,U3,W3)","v":1.379999999999999},{"$f":"AVERAGE(L3,N3,P3,R3,T3,V3)","v":10.725000000000001},{"$f":" AVERAGE(M3,O3,Q3,S3,U3,W3)","v":12.91}]
[null,null,null,null,null,null,"120kHz, 50MHz","MCS19","DMRS 1+1",12.5,13.1,10.8,13.3,8.94,12.04,9.65,12.15,9.5,11.5,12.3,null,10.89,13.39,3.3600000000000012,1.8900000000000006,10.346666666666666,12.476000000000001]
[null,null,null,null,null,null,"120kHz, 50MHz","MCS19","DMRS 1+1+1",12.1,12.7,10.6,13.1,8.73,11.83,9.41,11.91,9.4,11.4,null,null,10.89,13.39,2.16,1.9900000000000002,9.8060000000000009,12.326000000000001]
[null,null,null,null,null,null,"120kHz, 200MHz","MCS19","DMRS 1+0",12.8,13.4,11.1,13.6,8.61,11.95,10.25,12.75,9.8000000000000007,12,10.4,null,10.45,12.95,2.4900000000000002,1.6500000000000004,10.101666666666667,12.65]
[null,null,null,null,null,null,"120kHz, 200MHz","MCS19","DMRS 1+1",12.3,12.9,10.7,13.2,8.7100000000000009,11.81,9.41,11.91,9.4,11.4,10.4,null,10.67,13.17,1.9899999999999984,1.7999999999999989,9.8816666666666659,12.298]
[null,null,null,null,null,null,"120kHz, 200MHz","MCS19","DMRS 1+1+1",12.4,13,11,13.5,9.02,12.12,9.51,12.01,9.4,11.4,null,null,10.62,13.12,1.9800000000000004,2.0999999999999996,9.91,12.429999999999998]

{"sheet":"UL timing ajustment ","index":4,"n_rows":8,"n_cols":24,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,8,0,9],[0,0,0,5],[0,20,0,21],[0,22,0,23],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19]]}
["PUSCH",null,null,null,null,null,"38.104 req","38.141 req","Samsung",null,"Nokia",null,"Huawei",null,"Ericcson",null,"Intel",null,"CATT",null,"SPAN",null,"AVERAGE"]
["SCS and BW","MCS","Channel ","DMRS mapping","Length of data","RS",null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["120kHz, 50MHz","MCS16","AWGN","B",10,"DMRS 1+0",{"$f":"DerivingPerfReq(I3:T3)","v":9.1},{"$f":"IF(G3>-100,G3+0.6,G3)","v":9.6999999999999993},7.5,10,6.75,9.85,6.56,9.0599999999999987,6.5,9,5.5,7.5,6.4,8.9,{"$f":"MAX(I3,K3,M3,O3,Q3,S3)-MIN(I3,K3,M3,O3,Q3,S3)","v":2},{"$f":"MAX(J3,L3,N3,P3,R3,T3)-MIN(J3,L3,N3,P3,R3,T3)","v":2.5},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3)","v":6.5350000000000001},{"$f":"AVERAGE(J3,L3,N3,P3,R3,T3)","v":9.0516666666666659}]
["120kHz, 50MHz","MCS16","AWGN","B",10,"DMRS 1+1",{"$f":"DerivingPerfReq(I4:T4)","v":8.8000000000000007},9.4,7.1,9.6,6.46,9.56,6.41,8.91,6.3,8.8000000000000007,5.8,7.8,5.89,8.39,{"$f":"MAX(I4,K4,M4,O4,Q4,S4)-MIN(I4,K4,M4,O4,Q4,S4)","v":1.2999999999999998},{"$f":"MAX(J4,L4,N4,P4,R4,T4)-MIN(J4,L4,N4,P4,R4,T4)","v":1.7999999999999998},{"$f":"AVERAGE(I4,K4,M4,O4,Q4,S4)","v":6.3266666666666671},{"$f":"AVERAGE(J4,L4,N4,P4,R4,T4)","v":8.8433333333333337}]
["120kHz, 50MHz","MCS16","AWGN","B",10,"DMRS 1+1+1",9.1999999999999993,9.7999999999999989,7.3,9.8000000000000007,6.73,9.83,6.4,8.9,6.4,8.9,null,null,6.05,8.5500000000000007,1.25,1.2799999999999994,6.5759999999999987,9.1960000000000015]
["120kHz, 200MHz","MCS16","AWGN","B",10,"DMRS 1+0",9,9.6,7.2,9.6999999999999993,6.6,9.6999999999999993,6.4,8.9,6.5,9,6.1,8.1,6.36,8.86,1.1000000000000005,1.5999999999999996,6.5266666666666673,9.043333333333333]
["120kHz, 200MHz","MCS16","AWGN","B",10,"DMRS 1+1",8.9,9.5,7.2,9.6999999999999993,6.47,9.57,6.4,8.9,6.4,8.9,5.6,7.6,5.98,8.48,1.6000000000000005,2.0999999999999996,6.3416666666666659,8.8583333333333343]
["120kHz, 200MHz","MCS16","AWGN","B",10,"DMRS 1+1+1",9.1,9.6999999999999993,7.2,9.6999999999999993,6.47,9.57,6.4,8.9,6.4,8.9,null,null,5.89,8.39,1.3100000000000005,1.3099999999999987,6.4719999999999995,9.0920000000000005]

{"sheet":"PRACH","index":5,"n_rows":3,"n_cols":24,"rows_kept":3,"cut":false,"hidden":false,"merged":[[0,22,0,23],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,12,0,13],[0,8,0,9],[0,10,0,11],[0,0,0,5],[0,20,0,21],[0,6,1,6],[0,7,1,7]]}
["PRACH",null,null,null,null,null,"38.104 req","38.141 req","Samsung",null,"Huawei",null,"Ericsson",null,"Nokia",null,"Intel",null,"CATT",null,"SPAN",null,"AVERAGE"]
["Number of Tx","Number of Rx","Format","Channel ","Frequency offset","Timing offset range",null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,2,"C2","AWGN","19444Hz","0:0.48:4.8",{"$f":"DerivingPerfReq(I3:T3)","v":-10.4},{"$f":"IF(G3>-100,G3+0.6,G3)","v":-9.8000000000000007},-12.55,-10.55,-14.07,-11.57,-12.6,-10.1,-12.48,-9.3800000000000008,-13.2,-10.7,-12.59,-10.09,{"$f":"MAX(I3,K3,M3,O3,Q3,S3)-MIN(I3,K3,M3,O3,Q3,S3)","v":1.5899999999999999},{"$f":"MAX(J3,L3,N3,P3,R3,T3)-MIN(J3,L3,N3,P3,R3,T3)","v":2.1899999999999995},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3)","v":-12.915000000000001},{"$f":"AVERAGE(J3,L3,N3,P3,R3,T3)","v":-10.398333333333333}]