**3GPP TSG-RAN WG4 Meeting #104-e R4-2212445**

**Electronic Meeting, 15-26 August 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** |  | **Current version:** | **17.6.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Big CR 38.101-1 new combinations Rel-18 NR Inter-band CA/DC for yDL/xUL (y=4,5,6, x=1,2) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_yBDL\_xBUL | | | | |  | ***Date:*** | | | 2022-08-15 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)*  *Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding new combinations Rel-18 NR Inter-band CA/DC for yDL/xUL (y=4,5,6, x=1,2) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | New table format for configuration table as in endorsed in draftCR R4-2213601 and R4-2213604  New Combinations:  CA\_n2(2A)-n12A-n30A-n77A  CA\_n2A-n12A-n30A-n77(2A)  CA\_n2A-n5A-n66(2A)-n77A  CA\_n2(2A)-n5A-n66A-n77A  CA\_n2(2A)-n12A-n30A-n77A  CA\_n2A-n12A-n30A-n77(2A)  CA\_n2A-n12A-n66(2A)-n77A  CA\_n2(2A)-n12A-n66A-n77A  CA\_n2A-n12A-n66A-n77(2A)  CA\_n2(2A)-n14A-n30A-n77A  CA\_n2A-n14A-n66(2A)-n77A  CA\_n2(2A)-n14A-n66A-n77A  CA\_n5A-n30A-n66(2A)-n77A  CA\_n12A-n30A-n66(2A)-n77A  CA\_n12A-n30A-n66A-n77(2A)  CA\_n14A-n30A-n66(2A)-n77A  CA\_n1A-n28A-n38A-n78A  CA\_n1A-n3A-n7A-n8A  CA\_n3A-n7A-n8A-n78A  CA\_n25A-n41A-n66(2A)-n77A  CA\_n25(2A)-n41A-n66A-n77A  CA\_n25A-n41A-n71A-n77(2A)  CA\_n25(2A)-n41A-n71A-n77A  CA\_n25A-n66A-n71A-n77(2A)  CA\_n25A-n66A-n71A-n77(2A)  CA\_n1A-n3A-n28A-n77(2A)  CA\_n1A-n3A-n41A-n77(2A)  CA\_n1A-n28A-n41A-n77(2A)  CA\_n1A-n3A-n28A-n41A-n77A  CA\_n1A-n3A-n28A-n77A-n79A  CA\_n25A-n41A-n66A-n71A-n77A  DC\_n1A-n3A-n28A-n41A  DC\_n1A-n3A-n41A-n77A  DC\_n1A-n28A-n41A-n77A | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Approved combinations Rel-18 NR Inter-band CA/DC for yDL/xUL (y=4,5,6, x=1,2) are not added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2A.2.3, 5.2A.2.4, 5.5A.3.3, 5.5A.3.4, Table 5.5B.1-3, 6.2A.4.2.5, 6.2A.4.2.6, 7.3A.3.2.4, 7.3A.3.2.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-3 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

#### 5.2A.2.3 Inter-band CA (four bands)

Table 5.2A.2.3-1: Inter-band CA operating bands involving FR1 (four bands)

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n1-n3-n5-n7 | n1, n3, n5, n7 |
| CA\_n1-n3-n5-n78 | n1, n3, n5, n78 |
| CA\_n1-n3-n7-n28 | n1, n3, n7, n28 |
| CA\_n1-n3-n7-n78 | n1, n3, n7, n78 |
| CA\_n1-n3-n8-n77 | n1, n3, n8, n77 |
| CA\_n1-n3-n8-n78 | n1, n3, n8, n78 |
| CA\_n1-n3-n18-n28 | n1, n3, n18, n28 |
| CA\_n1-n3-n18-n41 | n1, n3, n18, n41 |
| CA\_n1-n3-n18-n77 | n1, n3, n18, n77 |
| CA\_n1-n3-n28-n41 | n1, n3, n28, n41 |
| CA\_n1-n3-n28-n771 | n1, n3, n28, n77 |
| CA\_n1-n3-n28-n78 | n1, n3, n28, n78 |
| CA\_n1-n3-n28-n791 | n1, n3, n28, n79 |
| CA\_n1-n3-n41-n77 | n1, n3, n41, n77 |
| CA\_n1-n3-n77-n79 | n1, n3, n77, n79 |
| CA\_n1-n5-n7-n78 | n1, n5, n7, n78 |
| CA\_n1-n7-n8-n40 | n1, n7, n8, n40 |
| CA\_n1-n7-n8-n78 | n1, n7, n8, n78 |
| CA\_n1-n7-n28-n78 | n1, n7, n28, n78 |
| CA\_n1-n7-n40-n78 | n1, n7, n40, n78 |
| CA\_n1-n8-n40-n78 | n1, n8, n40, n78 |
| CA\_n1-n8-n78-n79 | n1, n8, n78, n79 |
| CA\_n1-n18-n28-n41 | n1, n18, n28, n41 |
| CA\_n1-n18-n28-n77 | n1, n18, n28, n77 |
| CA\_n1-n18-n41-n77 | n1, n18, n41, n77 |
| CA\_n1-n28-n38-n78 | n1, n28, n38, n78 |
| CA\_n1-n28-n40-n78 | n1, n28, n40, n78 |
| CA\_n1-n28-n41-n77 | n1, n28, n41, n77 |
| CA\_n1-n28-n77-n79 | n1, n28, n77, n79 |
| CA\_n2-n5-n30-n66 | n2, n5, n30, n66 |
| CA\_n2-n5-n30-n77 | n2, n5, n30, n77 |
| CA\_n2-n5-n48-n66 | n2, n5, n48, n66 |
| CA\_n2-n5-n48-n77 | n2, n5, n48, n77 |
| CA\_n2-n5-n66-n77 | n2, n5, n66, n77 |
| CA\_n2-n12-n30-n66 | n2, n12, n30, n66 |
| CA\_n2-n12-n30-n77 | n2, n12, n30, n77 |
| CA\_n2-n12-n66-n77 | n2, n12, n66, n77 |
| CA\_n2-n14-n30-n66 | n2, n14, n30, n66 |
| CA\_n2-n14-n30-n77 | n2, n14, n30, n77 |
| CA\_n2-n14-n66-n77 | n2, n14, n66, n77 |
| CA\_n2-n29-n30-n66 | n2, n29, n30, n66 |
| CA\_n2-n29-n30-n77 | n2, n29, n30, n77 |
| CA\_n2-n29-n66-n77 | n2, n29, n66, n77 |
| CA\_n2-n48-n66-n77 | n2, n48, n66, n77 |
| CA\_n2-n66-n71-n78 | n2, n66, n71, n78 |
| CA\_n3-n5-n7-n78 | n3, n5, n7, n78 |
| CA\_n3-n7-n28-n78 | n3, n7, n28, n78 |
| CA\_n3-n18-n28-n41 | n3, n18, n28, n41 |
| CA\_n3-n18-n28-n77 | n3, n18, n28, n77 |
| CA\_n3-n18-n41-n77 | n3, n18, n41, n77 |
| CA\_n3-n28-n41-n77 | n3, n28, n41, n77 |
| CA\_n3-n28-n77-n79 | n3, n28, n77, n79 |
| CA\_n3-n28-n41-n78 | n3, n28, n41, n78 |
| CA\_n5-n25-n66-n77 | n5, n25, n66, n77 |
| CA\_n5-n25-n66-n78 | n5, n25, n66, n78 |
| CA\_n5-n30-n66-n77 | n5, n30, n66, n77 |
| CA\_n5-n48-n66-n77 | n5, n48, n66, n77 |
| CA\_n7-n8-n40-n78 | n7, n8, n40, n78 |
| CA\_n7-n25-n66-n77 | n7, n25, n66, n77 |
| CA\_n7-n25-n66-n78 | n7, n25, n66, n78 |
| CA\_n12-n30-n66-n77 | n12, n30, n66, n77 |
| CA\_n13-n25-n66-n77 | n13, n25, n66, n77 |
| CA\_n14-n30-n66-n77 | n14, n30, n66, n77 |
| CA\_n18-n28-n41-n77 | n18, n28, n41, n77 |
| CA\_n25-n38-n66-n78 | n25, n38, n66, n78 |
| CA\_n25-n41-n66-n71 | n25, n41, n66, n71 |
| CA\_n25-n41-n66-n77 | n25, n41, n66, n77 |
| CA\_n25-n41-n66-n78 | n25, n41, n66, n78 |
| CA\_n25-n41-n71-n77 | n25, n41, n71, n77 |
| CA\_n25-n41-n71-n78 | n25, n41, n71, n78 |
| CA\_n25-n66-n71-n77 | n25, n66, n71, n77 |
| CA\_n25-n66-n71-n78 | n25, n66, n71, n78 |
| CA\_n29-n30-n66-n77 | n29, n30, n66, n77 |
| CA\_n41-n66-n70-n78 | n41, n66, n70, n78 |
| CA\_n41-n66-n71-n77 | n41, n66, n71, n77 |
| CA\_n41-n66-n71-n78 | n41, n66, n71, n78 |
| NOTE 1: Applicable for UE supporting inter-band carrier aggregation with mandatory simultaneous Rx/Tx capability. | |

#### 5.2A.2.4 Inter-band CA (five bands)

Table 5.2A.2.4-1: Inter-band CA operating bands involving FR1 (five bands)

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n1-n3-n5-n7-n78 | n1, n3, n5, n7, n78 |
| CA\_n1-n3-n7-n28-n78 | n1, n3, n7, n28, n78 |
| CA\_ n1-n3-n28-n41-n77 | n1, n3, n28, n41, n77 |
| CA\_ n1-n3-n28-n41-n79 | n1, n3, n28, n41, n79 |

### ---Text omitted---

#### 5.5A.3.3 Configurations for inter-band CA (four bands)

Table 5.5A.3.3-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (four bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NR CA configuration** | **Uplink CA configuration**  **or single uplink carrier 4** | **NR Band** | **Channel bandwidth (MHz) (NOTE 3)** | **Bandwidth combination set** |
| CA\_n1A-n3A-n5A-n7A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n1A-n3A-n5A-n7B | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
| CA\_n1A-n3A-n5A-n78A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n8A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
| CA\_n1A-n3A-n7B-n28A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7B  CA\_n7A-n28A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
| CA\_n1A-n3A-n7A-n78A |  | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7B-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n8A-n77A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n8A-n77(2A) | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n1A-n3A-n8A-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
| CA\_n1A-n3A-n18A-n28A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n3A-n18A  CA\_n3A-n28A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
| CA\_n1A-n3A-n18A-n41A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n41A  CA\_n3A-n18A  CA\_n3A-n41A  CA\_n18A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n18A-n77A | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n77A  CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n41A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n77A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A) |  |
| CA\_n1A-n3A-n28A-n78A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 901, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 2 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202,302 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202, 302 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n28A-n79A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n41A-n77A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n41A-n77(2A) | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) |  |
| CA\_n1A-n3A-n77A-n79A | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25,30 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n5A-n7A-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n5A-n7B-n78A | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n8A-n40A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n40A  CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
| CA\_n1A-n7A-n8A-n78A | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n28A-n78A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7B-n28A-n78A | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n28A-n78(2A) | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n7A-n40A-n78A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n8A-n40A-n78A | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n8A-n78A-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n8A-n78(2A)-n79A | - | n1 | 5, 10, 15, 20 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n18A-n28A-n41A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n18A-n28A-n77A | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n18A-n41A-n77A | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40A-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n40B-n78A | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n40 | CA\_n40B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n41A-n77A | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n28A-n41A-n77(2A) | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A) |  |
| CA\_n1A-n28A-n77A-n79A | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n5A-n30A-n66A | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n5A-n30A-n66(2A) | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n5 | 5, 10, 15, 20 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n5A-n30A-n77A | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n30A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48A-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48B-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48(2A)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48(A-B)-n66A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(A-B)\_BCS1 |  |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n5A-n48A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n5A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A-n77C | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n5A-n48B-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48(2A)-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n5 | 5, 10, 15, 20, 25 |  |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66A-n77A | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n5A-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A) BCS0 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30,40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66(2A)-n77A | CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n66A-n77(2A) | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n66A-n77C | CA\_n2A-n5A  CA\_n2A-n77A  CA\_n2A-n66A  CA\_n5A-n77A  CA\_n5A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n12A-n30A-n66A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n12A-n30A-n66(2A) | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n12A-n30A-n77A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A  CA\_n12A-n30A  CA\_n12A-n77A  CA\_n30A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n30A-n77A | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A  CA\_n12A-n30A  CA\_n12A-n77A  CA\_n30A-n77A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A-n77(2A) | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A  CA\_n12A-n30A  CA\_n12A-n77A  CA\_n30A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n12A-n66A-n77A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n12A-n66A-n77A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66(2A)-n77A | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n66A-n77(2A) | CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n14A-n30A-n66A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | 5, 10, 15, 20, 25, 30, 40 |
| CA\_n2A-n14A-n30A-n66(2A) | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  | n14 | 5, 10 |
|  | n30 | 5, 10 |
|  | n66 | CA\_n66(2A)\_BCS1 |
| CA\_n2A-n14A-n30A-n77A | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n30A-n77A | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A  CA\_n14A-n30A  CA\_n14A-n77A  CA\_n30A-n77A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n30A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n66A-n77A | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2(2A)-n14A-n66A-n77A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n14A-n66A  CA\_n14A-n77A  CA\_n66A-n77A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66(2A)-n77A | CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n14A-n66A  CA\_n14A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n66A-n77(2A) | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2(2A)-n29A-n30A-n66A | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | CA\_n2(2A)\_BCS0 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n2A-n29A-n30A-n66(2A) | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n77A | CA\_n2A-n30A  CA\_n2A-n77A  CA\_n30A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n66A-n77A | CA\_n2A-n66A  CA\_n2A-n77A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n66A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48B-n66A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 3 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48(2A)-n66A-n77A | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n48A-n66A-n77C | - | n2 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
|  | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n2 | 5, 10, 15, 20, 25, 30, 40 | 2 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n66A-n71A-n78A | - | n2 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n7A-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n5A-n7B-n78A | - | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40, 50 | 1 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n8A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n7A-n28A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n7A CA\_n3A-n28A  CA\_n3A-n78A CA\_n7A-n28A  CA\_n7A-n78A CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n28A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 202 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n7B-n28A-n78A | - | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n3 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n18A-n28A-n41A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
| CA\_n3A-n18A-n28A-n77A | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n18A-n41A-n77A | CA\_n3A-n18A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n18 | 5, 10, 15 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n77A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n77(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n3 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n28A-n41A-n78A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n28A-n41A-n78(2A) | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n3A-n28A-n77A-n79A | CA\_n3A-n28A CA\_n3A-n77A CA\_n3A-n79A CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n3A-n28A-n77(2A)-n79A | CA\_n3A-n28A CA\_n3A-n77A CA\_n3A-n79A CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n79 | 40, 50, 80, 100 |  |
| CA\_n5A-n25A-n66A-n77A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n77A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66(2A)-n77A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66A-n77(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A)-n77A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n77(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66(2A)-n77(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25(2A)-n66(2A)-n77(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n25A-n66A-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25A-n66A-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n66(2A)-n78A | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n25(2A)-n66A-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25A-n66(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n25(2A)-n66(2A)-n78(2A) | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n5A-n30A-n66A-n77A | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n66(2A)-n77A | CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A) BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n30A-n66A-n77(2A) | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n5 | 5, 10, 15, 20 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n5A-n48A-n66A-n77A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48A-n66A-n77C | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n5A-n48B-n66A-n77A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | CA\_n48B\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 2 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 3 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n5A-n48(2A)-n66A-n77A | - | n5 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n5 | 5, 10, 15, 20, 25 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n5 | 5, 10, 15, 20, 25 | 2 |
|  |  | n48 | CA\_n48(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n8A-n40A-n78A | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66A-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n66(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66A-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25(2A)-n66(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n7A-n25A-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25A-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25(2A)-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n25(2A)-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7A-n25A-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66A-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7A-n25(2A)-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66A-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78A | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n7(2A)-n25A-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78(2A) | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | n7 | CA\_n7(2A)\_BCS0 | 0 |
|  |  | n25 | CA\_n25(2A)\_BCS0 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n12A-n30A-n66A-n77A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n66(2A)-n77A | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n12A-n30A-n66A-n77(2A) | CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A  CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n12 | 5, 10,15 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n13A-n25A-n66A-n77A | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n13A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | n13 | 5, 10 | 0 |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n66A-n77A | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n66(2A)-n77A | CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A  CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n14A-n30A-n66A-n77(2A) | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | n14 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n18A-n28A-n41A-n77A | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n18 | 5, 10, 15 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n66A-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n66A-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n66(2A)-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n38A-n66A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n66(2A)-n78A | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25(2A)-n38A-n66A-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n38A-n66(2A)-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25(2A)-n38A-n66(2A)-n78(2A) | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 4 and 5 in Table 5.5A.2-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n71A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 4 and 5 in Table 5.5A.1-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 4 and 5 in Table 5.5A.1-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 4 and 5 in Table 5.5A.1-2 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n77(2A) | - | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See CA\_n77(2A) Bandwidth Combination Set 4 and 5 in Table 5.5A.2-1 |  |
| CA\_n25A-n41A-n66(2A)-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | See CA\_n66(2A) BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | n25 | See CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n78A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n41A-n66A-n78(2A) | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n41A-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A-n77(2A) | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25(2A)-n41A-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | See CA\_n25(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 4 and 5 in Table 5.5A.1-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 4 and 5 in Table 5.5A.1-2 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n71A-n78A | - | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n71A-n77A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66A-n71A-n77(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n25A-n66A-n71A-n78A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66(2A)-n71A-n78A | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n25A-n66A-n71A-n78(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n25A-n66(2A)-n71A-n78(2A) | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n29A-n30A-n66A-n77A | CA\_n30A-n66A  CA\_n30A-n77A  CA\_n66A-n77A | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n70A-n78A | CA\_n41A-n66A  CA\_n41A-n70A  CA\_n41A-n78A  CA\_n66A-n78A  CA\_n70A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 10, 15, 20, 25, 30, 40 |  |
|  |  | n70 | 5, 10, 15, 20, 25 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n71A-n77A | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A  CA\_n41A-n71A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66A-n71A-n77A | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A  CA\_n41A-n71A | n41 | CA\_n41C\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | See CA\_n41C Bandwidth Combination Set 4 and 5 in Table 5.5A.1-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A-n71A-n77A | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A  CA\_n41A-n71A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | See CA\_n41(2A) Bandwidth Combination Set 4 and 5 in Table 5.5A.2-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A)-n71A-n77A | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n71A-n77A  CA\_n41A-n71A  CA\_n66A-n77A  CA\_n41A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | See CA\_n66(2A) Bbandwidth Ccombination Sset 4 and 5 in Table 5.5A.2-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66A-n71A-n77(2A) | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n71A-n77A  CA\_n41A-n71A  CA\_n66A-n77A  CA\_n41A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | See CA\_n77(2A) Bbandwidth Ccombination Sset 4 and 5 in Table 5.5A.2-1 |  |
| CA\_n41A-n66(2A)-n71A-n77(2A) | CA\_n41A-n66A  CA\_n66A-n71A  CA\_n71A-n77A  CA\_n41A-n71A  CA\_n66A-n77A  CA\_n41A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n41A-n66A-n71A-n78A | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66(2A)-n71A-n78A | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41A-n66A-n71A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n41A-n66(2A)-n71A-n78(2A) | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| NOTE 1: This UE channel bandwidth is optional in this release of the specification.  NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: Only single uplink carriers with power class other than PC3 are listed.  NOTE 5: Power Class 2 is allowed for this uplink combination or single uplink carrier in this downlink/uplink combination. | | | | |

#### 5.5A.3.4 Configurations for inter-band CA (five bands)

Table 5.5A.3.4-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (five bands)

| NR CA configuration | Uplink configuration | NR Band | Channel bandwidth (MHz) (NOTE 1) | Bandwidth combination set |
| --- | --- | --- | --- | --- |
| CA\_n1A-n3A-n5A-n7A-n78A | CA\_n1A-n3A CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A CA\_n5A-n7A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n5A-n78A CA\_n7A-n78A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n5A-n7B-n78A | CA\_n1A-n3A CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A CA\_n5A-n7A | n7 | See CA\_n7B bandwidth combination set 0 in Table 5.5A.1-1 |  |
|  | CA\_n5A-n78A CA\_n7A-n78A  CA\_n7B | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n28A-n78A | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7B-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | See CA\_n7B bandwidth combination set 0 in Table 5.5A.1-1 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n1A-n28A  CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n78A  CA\_n7A-n28A | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n7A-n78A  CA\_n28A-n78A | n78 | See CA\_n78(2A) Bandwidth Combination Set 2 in Table 5.5A.2-1 |  |
| CA\_n1A-n3A-n28A-n41A-n77A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n77A-n79A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n48A-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48B-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n48B | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | See CA\_n48B Bandwidth Combination Set 2 in Table 5.5A.1-1 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A-n66A-n77C | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | See CA\_n77C Bandwidth Combination Set 1 in Table 5.5A.1-1 |  |
| CA\_n25A-n41A-n66A-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| NOTE 1: The SCS of each channel bandwidth for NR FR1 and NR FR2 band refers to Table 5.3.5-1 of TS 38.101-1 and TS 38.101-2 respectively. | | | | |

---Text Omitted---

Table 6.2A.4.2.5-1: ΔTIB,c due to NR CA (four bands)

|  |  |  |
| --- | --- | --- |
| Inter-band CA combination | NR Band | ΔTIB,c (dB) |
| CA\_n1-n3-n5-n7 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n5 | 0.3 |
| CA\_n1-n3-n5-n78 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n5 | 0.3 |
|  | n78 | 0.8 |
| CA\_n1-n3-n7-n26 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n7 | 0.6 |
|  | n26 | 0.6 |
| CA\_n1-n3-n7-n28 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n7 | 0.6 |
|  | n28 | 0.6 |
| CA\_n1-n3-n7-n78 | n1 | 0.7 |
|  | n3 | 0.7 |
|  | n7 | 0.7 |
|  | n78 | 0.8 |
| CA\_n1-n3-n8-n78 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n8 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n3-n8-n77 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n8 | 0.6 |
|  | n77 | 0.8 |
| CA\_n1-n3-n18-n28 | n1 | 0.3 |
|  | n3 | 0.3 |
|  | n18 | 0.5 |
|  | n28 | 0.5 |
| CA\_n1-n3-n18-n41 | n1 | 0.5 |
|  | n3 | 0.5 |
|  | n18 | 0.3 |
|  | n41 | 0.33 |
|  |  | 0.84 |
| CA\_n1-n3-n18-n77 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n18 | 0.3 |
|  | n77 | 0.8 |
| CA\_n1-n3-n26-n78 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n26 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n3-n28-n41 | n1 | 0.5 |
|  | n3 | 0.5 |
|  | n28 | 0.5 |
|  | n41 | 0.33 |
|  |  | 0.84 |
| CA\_n1-n3-n28-n77 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n28 | 0.6 |
|  | n77 | 0.8 |
| CA\_n1-n3-n28-n78 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n28 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n3-n28-n79 | n1 | 0.3 |
|  | n3 | 0.3 |
|  | n28 | 0.6 |
|  | n79 | 0.8 |
| CA\_n1-n3-n41-n77 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n41 | 0.33 |
|  |  | 0.84 |
|  | n77 | 0.8 |
| CA\_n1-n3-n77-n79 | n1 | 0.6 |
|  | n3 | 0.6 |
|  | n77 | 0.8 |
|  | n79 | 0.8 |
| CA\_n1-n5-n7-n78 | n1 | 0.6 |
|  | n5 | 0.6 |
|  | n7 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n7-n8-n40 | n1 | 0.6 |
|  | n7 | 0.8 |
|  | n8 | 0.6 |
|  | n40 | 0.9 |
| CA\_n1-n7-n8-n78 | n1 | 0.6 |
|  | n7 | 0.6 |
|  | n8 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n7-n26-n78 | n1 | 0.6 |
|  | n7 | 0.6 |
|  | n26 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n7-n28-n78 | n1 | 0.6 |
|  | n7 | 0.6 |
|  | n28 | 0.6 |
|  | n78 | 0.8 |
| CA\_n1-n7-n40-n78 | n1 | 0.6 |
|  | n7 | 0.5 |
|  | n40 | 0.5 |
|  | n78 | 0.8 |
| CA\_n1-n8-n40-n78 | n1 | 0.5 |
|  | n8 | 0.3 |
|  | n40 | 0.5 |
|  | n78 | 0.8 |
| CA\_n1-n8-n78-n79 | n1 | 0.3 |
|  | n8 | 0.6 |
|  | n78 | 0.8 |
|  | n79 | 0.5 |
| CA\_n1-n18-n28-n41 | n1 | 0.6 |
|  | n18 | 0.5 |
|  | n28 | 0.6 |
|  | n41 | 0.5 |
| CA\_n1-n18-n28-n77 | n1 | 0.6 |
|  | n18 | 0.5 |
|  | n28 | 0.6 |
|  | n77 | 0.8 |
| CA\_n1-n18-n41-n77 | n1 | 0.5 |
|  | n18 | 0.5 |
|  | n41 | 0.5 |
|  | n77 | 0.8 |
| CA\_n1-n28-n40-n78 | n1 | 0.3 |
|  | n28 | 0.6 |
|  | n40 | 0.5 |
|  | n78 | 0.8 |
| CA\_n1-n28-n41-n77 | n1 | 0.6 |
|  | n28 | 0.6 |
|  | n41 | 0.6 |
|  | n77 | 0.8 |
| CA\_n1-n28-n77-n79 | n1 | 0.6 |
|  | n28 | 0.6 |
|  | n77 | 0.8 |
|  | n79 | 0.8 |
| CA\_n2-n5-n30-n66 | n2 | 0.5 |
|  | n5 | 0.3 |
|  | n30 | 0.3 |
|  | n66 | 0.5 |
| CA\_n2-n5-n30-n77 | n2 | 0.6 |
|  | n5 | 0.6 |
|  | n30 | 0.3 |
|  | n77 | 0.8 |
| CA\_n2-n5-n48-n66 | n2 | 0.6 |
|  | n5 | 0.3 |
|  | n48 | 0.8 |
|  | n66 | 0.6 |
| CA\_n2-n5-n48-n77 | n2 | 0.6 |
|  | n5 | 0.3 |
|  | n48 | 0.8 |
|  | n77 | 0.8 |
| CA\_n2-n5-n66-n77 | n2 | 0.5 |
|  | n5 | 0.3 |
|  | n66 | 0.5 |
|  | n77 | 0.8 |
| CA\_n2-n12-n30-n66 | n2 | 0.5 |
|  | n12 | 0.8 |
|  | n30 | 0.3 |
|  | n66 | 0.5 |
| CA\_n2-n12-n30-n77 | n2 | 0.6 |
|  | n12 | 0.5 |
|  | n30 | 0.3 |
|  | n77 | 0.8 |
| CA\_n2-n12-n66-n77 | n2 | 0.6 |
|  | n12 | 0.8 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n2-n14-n30-n66 | n2 | 0.5 |
|  | n14 | 0.3 |
|  | n30 | 0.3 |
|  | n66 | 0.5 |
| CA\_n2-n14-n30-n77 | n2 | 0.6 |
|  | n14 | 0.5 |
|  | n30 | 0.3 |
|  | n77 | 0.8 |
| CA\_n2-n14-n66-n77 | n2 | 0.6 |
|  | n14 | 0.6 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n2-n29-n30-n66 | n2 | 0.5 |
|  | n30 | 0.3 |
|  | n66 | 0.5 |
| CA\_n2-n29-n30-n77 | n2 | 0.6 |
|  | n30 | 0.3 |
|  | n77 | 0.8 |
| CA\_n2-n29-n66-n77 | n2 | 0.6 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n2-n48-n66-n77 | n2 | 0.6 |
|  | n48 | 0.8 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n2-n66-n71-n78 | n2 | 0.5 |
|  | n66 | 0.5 |
|  | n71 | 0.3 |
|  | n78 | 0.5 |
| CA\_n3-n5-n7-n78 | n3 | 0.6 |
|  | n5 | 0.6 |
|  | n7 | 0.6 |
|  | n78 | 0.8 |
| CA\_n3-n7-n26-n78 | n3 | 0.6 |
|  | n7 | 0.6 |
|  | n26 | 0.6 |
|  | n78 | 0.6 |
| CA\_n3-n7-n28-n78 | n3 | 0.6 |
|  | n7 | 0.6 |
|  | n28 | 0.6 |
|  | n78 | 0.6 |
| CA\_n3-n18-n28-n41 | n3 | 0.5 |
|  | n18 | 0.4 |
|  | n28 | 0.4 |
|  | n41 | 0.33 |
|  |  | 0.84 |
| CA\_n3-n18-n28-n77 | n3 | 0.6 |
|  | n18 | 0.5 |
|  | n28 | 0.5 |
|  | n77 | 0.8 |
| CA\_n3-n18-n41-n77 | n3 | 0.6 |
|  | n18 | 0.4 |
|  | n41 | 0.33 |
|  |  | 0.84 |
|  | n77 | 0.8 |
| CA\_n3-n28-n41-n77 | n3 | 1 |
|  | n28 | 0.5 |
|  | n41 | 0.31/0.82 |
|  | n77 | 0.8 |
| CA\_n3-n28-n41-n78 | n3 | 1 |
|  | n28 | 0.5 |
|  | n41 | 0.31/0.82 |
|  | n78 | 0.8 |
| CA\_n3-n28-n77-n79 | n3 | 0.6 |
|  | n28 | 0.5 |
|  | n77 | 0.8 |
|  | n79 | 0.8 |
| CA\_n5-n25-n66-n77 | n5 | 0.6 |
|  | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n5-n25-n66-n78 | n5 | 0.6 |
|  | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n78 | 0.8 |
| CA\_n5-n30-n66-n77 | n5 | 0.6 |
|  | n30 | 0.3 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n5-n48-n66-n77 | n5 | 0.6 |
|  | n48 | 0.8 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n7-n8-n40-n78 | n7 | 0.5 |
|  | n8 | 0.3 |
|  | n40 | 0.5 |
|  | n78 | 0.8 |
| CA\_n7-n25-n66-n77 | n7 | 0.5 |
|  | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n7-n25-n66-n78 | n7 | 0.5 |
|  | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n78 | 0.8 |
| CA\_n12-n30-n66-n77 | n12 | 0.8 |
|  | n30 | 0.3 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n13-n25-n66-n77 | n13 | 0.5 |
|  | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n14-n30-n66-n77 | n14 | 0.6 |
|  | n30 | 0.3 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n18-n28-n41-n77 | n18 | 0.5 |
|  | n28 | 0.5 |
|  | n41 | 0.33 |
|  | 0.84 |
|  | n77 | 0.8 |
| CA\_n25-n38-n66-n78 | n25 | 0.6 |
|  | n38 | 0.6 |
|  | n66 | 0.6 |
|  | n78 | 0.8 |
| CA\_n25-n41-n66-n71 | n25 | 0.5 |
|  | n41 | 0.5 |
|  | n66 | 0.5 |
|  | n71 | 0.3 |
| CA\_n25-n41-n66-n77 | n25 | 0.5 |
|  | n41 | 0.83/1.34 |
|  | n66 | 0.5 |
|  | n77 | 0.8 |
| CA\_n25-n41-n66-n78 | n25 | 0.5 |
|  | n41 | 0.83/1.34 |
|  | n66 | 0.5 |
|  | n78 | 0.8 |
| CA\_n25-n41-n71-n77 | n25 | 0.5 |
|  | n41 | 0.5 |
|  | n71 | 0.6 |
|  | n77 | 0.8 |
| CA\_n25-n41-n71-n78 | n25 | 0.5 |
|  | n41 | 0.5 |
|  | n71 | 0.6 |
|  | n78 | 0.8 |
| CA\_n25-n66-n71-n77 | n25 | 0.5 |
|  | n66 | 0.5 |
|  | n71 | 0.6 |
|  | n77 | 0.8 |
| CA\_n25-n66-n71-n78 | n25 | 0.6 |
|  | n66 | 0.6 |
|  | n71 | 0.6 |
|  | n78 | 0.8 |
| CA\_n29-n30-n66-n77 | n30 | 0.3 |
|  | n66 | 0.6 |
|  | n77 | 0.8 |
| CA\_n41-n66-n70-n78 | n41 | 0.5 |
|  | n66 | 0.6 |
|  | n70 | 0.6 |
|  | n78 | 0.8 |
| CA\_n41-n66-n71-n77 | n41 | 0.33/0.84 |
|  | n66 | 1 |
|  | n71 | 0.5 |
|  | n77 | 0.8 |
| CA\_n41-n66-n71-n78 | n41 | 0.33/0.84 |
|  | n66 | 1 |
|  | n71 | 0.5 |
|  | n78 | 0.8 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz | | |

### ---Text omitted---

Table 5.5B.1-3: Inter-band NR DC configurations (four bands)

| NR DC  configuration | Uplink NR DC  configuration |
| --- | --- |
| DC\_n1A-n3A-n28A-n41A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n41A  DC\_n3A-n28A  DC\_n3A-n41A  DC\_n28A-n41A |
| DC\_n1A-n3A-n28A-n77A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n77A  DC\_n3A-n28A  DC\_n3A-n77A  DC\_n28A-n77A |
| DC\_n1A-n3A-n28A-n79A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n79A  DC\_n3A-n28A  DC\_n3A-n79A  DC\_n28A-n79A |
| DC\_n1A-n3A-n41A-n77A | DC\_n1A-n3A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n41A-n77A |
| DC\_n1A-n3A-n77A-n79A | DC\_n1A-n3A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n77A-n79A |
| DC\_n1A-n28A-n41A-n77A | DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n41A-n77A |
| DC\_n1A-n28A-n77A-n79A | DC\_n1A-n28A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n3A-n28A-n41A-n77A | DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n41A-n77A |
| DC\_n3A-n28A-n77A-n79A | DC\_n3A-n28A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n3A-n28A-n77(2A)-n79A | DC\_n3A-n28A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |

### ---Text omitted---

##### 6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands)

Table 6.2A.4.2.5-1: ΔTIB,c due to NR CA (four bands)



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)5 | | | |
| Component band in order of bands in configuration6 | | | |
| CA\_n1-n3-n5-n7 | 0.6 | 0.6 | 0.3 | - |
| CA\_n1-n3-n5-n78 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n7-n8 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n28 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n78 | 0.7 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n8-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n18-n28 | 0.3 | 0.3 | 0.5 | 0.5 |
| CA\_n1-n3-n18-n41 | 0.5 | 0.5 | 0.3 | 0.33 / 0.84 |
| CA\_n1-n3-n18-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n28-n41 | 0.5 | 0.5 | 0.5 | 0.33 / 0.84 |
| CA\_n1-n3-n28-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n79 | 0.3 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n3-n41-n77 | 0.6 | 0.6 | 0.33 / 0.84 | 0.8 |
| CA\_n1-n3-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n8-n40 | 0.6 | 0.8 | 0.6 | 0.9 |
| CA\_n1-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n40-n78 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n1-n8-n78-n79 | 0.3 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n18-n28-n41 | 0.6 | 0.5 | 0.6 | 0.5 |
| CA\_n1-n18-n28-n77 | 0.6 | 0.5 | 0.6 | 0.8 |
| CA\_n1-n18-n41-n77 | 0.5 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n28-n38-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n40-n78 | 0.3 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n28-n41-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n2-n5-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n5-n30-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n5-n48-n66 | 0.6 | 0.3 | 0.8 | 0.6 |
| CA\_n2-n5-n48-n77 | 0.6 | 0.3 | 0.8 | 0.8 |
| CA\_n2-n5-n66-n77 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n2-n12-n30-n66 | 0.5 | 0.8 | 0.3 | 0.5 |
| CA\_n2-n12-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n12-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n14-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n14-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n14-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n2-n29-n30-n66 | 0.5 | - | 0.3 | 0.5 |
| CA\_n2-n29-n30-n77 | 0.6 | - | 0.3 | 0.8 |
| CA\_n2-n29-n66-n77 | 0.6 | - | 0.6 | 0.8 |
| CA\_n2-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n66-n71-n78 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n3-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n18-n28-n41 | 0.5 | 0.4 | 0.4 | 0.33 / 0.84 |
| CA\_n3-n18-n28-n77 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n3-n18-n41-n77 | 0.6 | 0.4 | 0.33 / 0.84 | 0.8 |
| CA\_n3-n28-n41-n77 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n41-n78 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n77-n79 | 0.6 | 0.5 | 0.8 | 0.8 |
| CA\_n5-n25-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n25-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n5-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n7-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n7-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n25-n66-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n12-n30-n66-n77 | 0.8 | 0.3 | 0.6 | 0.8 |
| CA\_n13-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n14-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n18-n28-n41-n77 | 0.5 | 0.5 | 0.33 / 0.84 | 0.8 |
| CA\_n25-n38-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n41-n66-n71 | 0.5 | 0.5 | 0.5 | 0.3 |
| CA\_n25-n41-n66-n77 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n66-n78 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n41-n71-n78 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n66-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n66-n71-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n29-n30-n66-n77 | - | 0.3 | 0.6 | 0.8 |
| CA\_n41-n66-n70-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n41-n66-n71-n77 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| CA\_n41-n66-n71-n78 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz.  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz.  NOTE 5: “-” denotes ΔTIB,c = 0.  NOTE 6: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n78 the band order from left to right is n1, n3, n5 and n78. | | | | |

##### 6.2A.4.2.6 ΔTIB,c for Inter-band CA (five bands)

Table 6.2A.4.2.6-1: ΔTIB,c due to NR CA (five bands)



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)1 | | | | |
| Component band in order of bands in configuration2 | | | | |
| CA\_n1-n3-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n7-n28-n78 | 0.7 | 0.7 | 0.7 | 0.6 | 0.8 |
| CA\_n2-n5-n48-n66-n77 | 0.6 | 0.3 | 0.8 | 0.6 | 0.8 |
| NOTE 1: “-” denotes ΔTIB,c = 0.  NOTE 2: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n7-n78 the band order from left to right is n1, n3, n5, n7 and n78. | | | | | |

### ---Text omitted---

##### 7.3A.3.2.4 ΔRIB,c for four bands

Table 7.3A.3.2.4-1: ΔRIB,c due to CA (four bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Inter-band CA combination | | ΔRIB,c for NR bands (dB)7 | | | | | |
| Component band in order of bands in configuration8 | | | | | |
| CA\_n1-n3-n5-n78 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n1-n3-n7-n8 | | - | - | | - | 0.2 | |
| CA\_n1-n3-n7-n28 | | - | - | | - | 0.2 | |
| CA\_n1-n3-n7-n78 | | 0.3 | 0.3 | | 0.3 | 0.5 | |
| CA\_n1-n3-n8-n77 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n3-n8-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n3-n18-n28 | | - | - | | - | 0.2 | |
| CA\_n1-n3-n18-n41 | | - | - | | - | 05 / 0.56 | |
| CA\_n1-n3-n18-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n1-n3-n28-n41 | | - | - | | 0.2 | 05 / 0.56 | |
| CA\_n1-n3-n28-n77 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n3-n28-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n3-n28-n79 | | - | - | | 0.2 | 0.5 | |
| CA\_n1-n3-n41-n77 | | 0.2 | 0.2 | | 05 / 0.56 | 0.5 | |
| CA\_n1-n3-n77-n79 | | 0.2 | 0.2 | | 0.5 | 0.5 | |
| CA\_n1-n5-n7-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n7-n8-n40 | | - | - | | 0.3 | 0.8 | |
| CA\_n1-n7-n8-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n1-n7-n28-n78 | | 0.2 | 0.2 | | - | - | |
| CA\_n1-n7-n40-n78 | | 0.2 | - | | 0.4 | 0.5 | |
| CA\_n1-n8-n40-n78 | | 0.2 | - | | 0.4 | 0.5 | |
| CA\_n1-n8-n78-n79 | | 0.3 | 0.3 | | 0.5 | - | |
| CA\_n1-n18-n28-n41 | | 0.2 | - | | 0.2 | - | |
| CA\_n1-n18-n28-n77 | | 0.2 | - | | 0.2 | 0.5 | |
| CA\_n1-n18-n41-n77 | | 0.2 | - | | - | 0.5 | |
| CA\_n1-n28-n38-n78 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n1-n28-n40-n78 | | - | 0.2 | | - | 0.5 | |
| CA\_n1-n28-n41-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n1-n28-n77-n79 | | 0.2 | 0.2 | | 0.5 | 0.5 | |
| CA\_n2-n5-n30-n66 | | 0.4 | - | | 0.5 | 0.4 | |
| CA\_n2-n5-n30-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n2-n5-n48-n66 | | 0.2 | - | | 0.5 | 0.2 | |
| CA\_n2-n5-n48-n77 | | 0.2 | - | | 0.5 | 0.5 | |
| CA\_n2-n5-n66-n77 | | 0.3 | - | | 0.3 | 0.5 | |
| CA\_n2-n12-n30-n66 | | 0.4 | 0.5 | | 0.5 | 0.4 | |
| CA\_n2-n12-n30-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n2-n12-n66-n77 | | 0.2 | 0.5 | | 0.5 | 0.5 | |
| CA\_n2-n14-n30-n66 | | 0.4 | - | | 0.5 | 0.4 | |
| CA\_n2-n14-n30-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n2-n14-n66-n77 | | 0.2 | 0.2 | | 0.5 | 0.5 | |
| CA\_n2-n29-n30-n66 | | 0.4 | - | | 0.5 | 0.4 | |
| CA\_n2-n29-n30-n77 | | 0.2 | 0.2 | | - | 0.5 | |
| CA\_n2-n29-n66-n77 | | 0.2 | 0.5 | | 0.5 | 0.5 | |
| CA\_n2-n48-n66-n77 | | 0.3 | 0.5 | | 0.3 | 0.5 | |
| CA\_n2-n66-n71-n78 | | 0.3 | 0.5 | | - | 0.5 | |
| CA\_n3-n5-n7-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n3-n7-n8-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n3-n7-n28-n78 | | 0.2 | 0.2 | | 0.2 | 0.5 | |
| CA\_n3-n18-n28-n41 | | - | - | | - | 05 / 0.56 | |
| CA\_n3-n18-n28-n77 | | 0.2 | - | | 0.2 | 0.5 | |
| CA\_n3-n18-n41-n77 | | 0.2 | - | | 05 / 0.56 | 0.5 | |
| CA\_n3-n28-n41-n77 | | 0.5 | 0.2 | | 01 / 0.52 | 0.5 | |
| CA\_n3-n28-n41-n78 | | 0.5 | 0.2 | | 01 / 0.52 | 0.5 | |
| CA\_n3-n28-n77-n79 | | 0.2 | 0.2 | | 0.5 | 0.5 | |
| CA\_n5-n25-n66-n77 | | 0.5 | 0.3 | | 0.3 | 0.5 | |
| CA\_n5-n25-n66-n78 | | 0.5 | 0.3 | | 0.3 | 0.5 | |
| CA\_n5-n30-n66-n77 | | 0.2 | 0.4 | | 0.4 | 0.5 | |
| CA\_n5-n48-n66-n77 | | 0.2 | 0.5 | | 0.2 | 0.5 | |
| CA\_n7-n8-n40-n78 | | - | 0.2 | | 0.4 | 0.5 | |
| CA\_n7-n25-n66-n77 | | 0.5 | 0.6 | | 0.6 | 0.8 | |
| CA\_n7-n25-n66-n78 | | 0.5 | 0.6 | | 0.6 | 0.8 | |
| CA\_n12-n30-n66-n77 | | 0.5 | 0.5 | | 0.5 | 0.5 | |
| CA\_n13-n25-n66-n77 | | 0.3 | 0.3 | | 0.3 | 0.5 | |
| CA\_n14-n30-n66-n77 | | 0.2 | 0.5 | | 0.5 | 0.5 | |
| CA\_n18-n28-n41-n77 | | - | 0.2 | | 05 / 0.56 | 0.5 | |
| CA\_n25-n38-n66-n78 | | 0.3 | 0.4 | | 0.3 | 0.5 | |
| CA\_n25-n41-n66-n71 | | 0.3 | 0.5 | | 0.5 | - | |
| CA\_n25-n41-n66-n77 | | 0.3 | 0.53 / 1.04 | | 0.3 | 0.5 | |
| CA\_n25-n41-n66-n78 | | 0.3 | 0.53 / 1.04 | | 0.3 | 0.5 | |
| CA\_n25-n41-n71-n77 | | - | - | | 0.2 | 0.5 | |
| CA\_n25-n41-n71-n78 | | - | - | | 0.2 | 0.5 | |
| CA\_n25-n66-n71-n77 | | 0.3 | 0.3 | | 0.3 | 0.5 | |
| CA\_n25-n66-n71-n78 | | 0.3 | 0.3 | | 0.3 | 0.5 | |
| CA\_n29-n30-n66-n77 | | 0.5 | 0.5 | | 0.5 | 0.5 | |
| CA\_n41-n66-n70-n78 | | - | 0.2 | | 0.2 | 0.5 | |
| CA\_n41-n66-n71-n77 | | 03 / 0.54 | 0.5 | | 0.2 | 0.5 | |
| CA\_n41-n66-n71-n78 | | 03 / 0.54 | 0.5 | | 0.2 | 0.5 | |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz  NOTE 5: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 6: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz  NOTE 7: “-” denotes ΔRIB,c = 0.  NOTE 8: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n7-n78 the band order from left to right is n1 n3, n7 and n78. | | | | | | | |

##### 7.3A.3.2.5 ΔRIB,c for five bands

Table 7.3A.3.2.5-1: ΔRIB,c due to CA (five bands)



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔRIB,c for NR bands (dB)1 | | | | |
| Component band in order of bands in configuration2 | | | | |
| CA\_n1-n3-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n7-n28-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n2-n5-n48-n66-n77 | 0.2 | - | 0.5 | 0.2 | 0.5 |
| NOTE 1: “-” denotes ΔRIB,c = 0.  NOTE 2: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n7-n78 the band order from left to right is n1 n3, n5, n7 and n78. | | | | | |

--- End of changes---