{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Cover","Parameters","PUSCH TBoMS","PUSCH JCE (1T2R)","PUSCH JCE (1T4R)","PUSCH JCE (1T8R)","TBoMS simulation assumption","PUSCH JCE simulation assumption"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH TBoMS","index":2,"n_rows":12,"n_cols":31,"rows_kept":12,"cut":false,"hidden":false,"merged":[[2,1,11,1],[2,3,9,3],[10,3,11,3],[8,0,9,0],[8,2,9,2],[4,0,5,0],[2,2,3,2],[4,2,5,2],[6,0,7,0],[6,2,7,2],[2,0,3,0],[0,11,0,12],[0,5,1,5],[0,6,1,6],[0,7,0,8],[0,9,0,10],[0,25,0,26],[0,27,0,28],[0,29,0,30],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24]]}
["  PUSCH TBoMS ",null,null,null,null,"38.104 req","38.141 req","China Telecom",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Samsung",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["TBoMS over",null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["4 available slots","1T2R","FDD 15kHz SCS","TDLB100-400 Low","PUSCH Mapping type A",{"$f":"DerivingPerfReq(H3:AA3)","v":-2.2999999999999998},{"$f":"IF(F3>-100,F3+0.6,F3)","v":-1.6999999999999997},-7.1,-5.0999999999999996,"-4,37","-1,87",-4.53,-2.5299999999999998,-4.3499999999999996,-2.35,-3.9,-1.9,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":3.1999999999999997},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":3.1999999999999997},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-4.97},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-2.9699999999999998}]
[null,null,null,null,"PUSCH Mapping type B",-2.1,-1.5,-7.2,-5.2,"-4,15","-1,65",-4.5,-2.5,-4.16,-2.16,-3.7,-1.7,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)-MIN(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":3.5},3.5,{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":-4.8899999999999997},-2.8899999999999997]
["2 available slots",null,"TDD 15kHz SCS",null,"PUSCH Mapping type A",-2.5,{"$f":"IF(F5>-100,F5+0.6,F5)","v":-1.9},-5.6,-3.6,"-4,52","-2,02",-4.46,-2.46,-4.16,-2.16,-3.8,-1.8,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H5,J5,L5,N5,P5,R5,T5,V5,X5,Z5)-MIN(H5,J5,L5,N5,P5,R5,T5,V5,X5,Z5)","v":1.7999999999999998},{"$f":"MAX(I5,K5,M5,O5,Q5,S5,U5,W5,Y5,AA5)-MIN(I5,K5,M5,O5,Q5,S5,U5,W5,Y5,AA5)","v":1.8},{"$f":"AVERAGE(H5,J5,L5,N5,P5,R5,T5,V5,X5,Z5)","v":-4.5049999999999999},{"$f":"AVERAGE(I5,K5,M5,O5,Q5,S5,U5,W5,Y5,AA5)","v":-2.5050000000000003}]
[null,null,null,null,"PUSCH Mapping type B",-2.5,-1.9,-5.7,-3.7,"-4,38","-1,88",-4.41,-2.41,-4.09,-2.09,-3.7,-1.7,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H6,J6,L6,N6,P6,R6,T6,V6,X6,Z6)-MIN(H6,J6,L6,N6,P6,R6,T6,V6,X6,Z6)","v":2},{"$f":"MAX(I6,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)-MIN(I6,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)","v":2},{"$f":"AVERAGE(H6,J6,L6,N6,P6,R6,T6,V6,X6,Z6)","v":-4.4749999999999996},{"$f":"AVERAGE(I6,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)","v":-2.4749999999999996}]
["4 available slots",null,"FDD 30kHz SCS",null,"PUSCH Mapping type A",-2.4,-1.7999999999999998,-6.8,-4.8,"-4,38","-1,88",-4.5199999999999996,-2.5199999999999996,-4.47,-2.4700000000000002,-4.3,-2.2999999999999998,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)-MIN(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)","v":2.5},{"$f":"MAX(I7,K7,M7,O7,Q7,S7,U7,W7,Y7,AA7)-MIN(I7,K7,M7,O7,Q7,S7,U7,W7,Y7,AA7)","v":2.5},{"$f":"AVERAGE(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)","v":-5.0225},{"$f":"AVERAGE(I7,K7,M7,O7,Q7,S7,U7,W7,Y7,AA7)","v":-3.0225}]
[null,null,null,null,"PUSCH Mapping type B",-2.4,-1.7999999999999998,-7.1,-5.0999999999999996,"-4,36","-1,86",-4.4800000000000004,-2.4800000000000004,-4.43,-2.4300000000000002,-4.3,-2.2999999999999998,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H8,J8,L8,N8,P8,R8,T8,V8,X8,Z8)-MIN(H8,J8,L8,N8,P8,R8,T8,V8,X8,Z8)","v":2.8},{"$f":"MAX(I8,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)-MIN(I8,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)","v":2.8},{"$f":"AVERAGE(H8,J8,L8,N8,P8,R8,T8,V8,X8,Z8)","v":-5.0774999999999997},{"$f":"AVERAGE(I8,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)","v":-3.0774999999999997}]
["2 available slots",null,"TDD 30kHz SCS",null,"PUSCH Mapping type A",-2.5,{"$f":"IF(F9>-100,F9+0.6,F9)","v":-1.9},-5.4,-3.4,"-4,30","-1,80",-4.2699999999999996,-2.2699999999999996,-4.32,-2.3199999999999998,-4.2,-2.2000000000000002,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H9,J9,L9,N9,P9,R9,T9,V9,X9,Z9)-MIN(H9,J9,L9,N9,P9,R9,T9,V9,X9,Z9)","v":1.2000000000000002},{"$f":"MAX(I9,K9,M9,O9,Q9,S9,U9,W9,Y9,AA9)-MIN(I9,K9,M9,O9,Q9,S9,U9,W9,Y9,AA9)","v":1.1999999999999997},{"$f":"AVERAGE(H9,J9,L9,N9,P9,R9,T9,V9,X9,Z9)","v":-4.5475000000000003},{"$f":"AVERAGE(I9,K9,M9,O9,Q9,S9,U9,W9,Y9,AA9)","v":-2.5475000000000003}]
[null,null,null,null,"PUSCH Mapping type B",-2.5,-1.9,-5.5,-3.5,"-4,26","-1,76",-4.24,-2.2400000000000002,-4.3,-2.2999999999999998,-4.0999999999999996,-2.1,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H10,J10,L10,N10,P10,R10,T10,V10,X10,Z10)-MIN(H10,J10,L10,N10,P10,R10,T10,V10,X10,Z10)","v":1.4000000000000004},{"$f":"MAX(I10,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)-MIN(I10,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)","v":1.4},{"$f":"AVERAGE(H10,J10,L10,N10,P10,R10,T10,V10,X10,Z10)","v":-4.5350000000000001},{"$f":"AVERAGE(I10,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)","v":-2.5349999999999997}]
["2 available slots",null,"TDD 60kHz SCS","TDLA30-300 Low","PUSCH Mapping type B",-2.6,-2,-4.9000000000000004,-2.9,"-4,40","-1,30",-4.74,-2.74,-4.6500000000000004,-2.15,-4.5,-2.5,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)-MIN(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)","v":0.40000000000000036},{"$f":"MAX(I11,K11,M11,O11,Q11,S11,U11,W11,Y11,AA11)-MIN(I11,K11,M11,O11,Q11,S11,U11,W11,Y11,AA11)","v":0.75},{"$f":"AVERAGE(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)","v":-4.6974999999999998},{"$f":"AVERAGE(I11,K11,M11,O11,Q11,S11,U11,W11,Y11,AA11)","v":-2.5725000000000002}]
["2 available slots",null,"TDD 120kHz SCS",null,"PUSCH Mapping type B",-2.4,{"$f":"IF(F12>-100,F12+0.6,F12)","v":-1.7999999999999998},-4.9000000000000004,-2.9,"-4,20","-1,10",-4.43,-2.4299999999999997,-4.37,-1.87,-4.3,-2.2999999999999998,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)-MIN(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":0.60000000000000053},{"$f":"MAX(I12,K12,M12,O12,Q12,S12,U12,W12,Y12,AA12)-MIN(I12,K12,M12,O12,Q12,S12,U12,W12,Y12,AA12)","v":1.0299999999999998},{"$f":"AVERAGE(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":-4.5},{"$f":"AVERAGE(I12,K12,M12,O12,Q12,S12,U12,W12,Y12,AA12)","v":-2.375}]

{"sheet":"PUSCH JCE (1T2R)","index":3,"n_rows":20,"n_cols":31,"rows_kept":20,"cut":false,"hidden":false,"merged":[[18,0,19,0],[18,2,19,2],[14,0,17,0],[14,1,17,1],[14,3,15,3],[16,3,17,3],[6,3,7,3],[8,3,9,3],[10,0,13,0],[10,1,13,1],[10,3,11,3],[12,3,13,3],[0,27,0,28],[0,29,0,30],[2,0,5,0],[2,1,5,1],[2,2,17,2],[2,3,3,3],[4,3,5,3],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[0,5,1,5],[6,0,9,0],[6,1,9,1],[0,6,1,6],[0,7,0,8],[0,9,0,10],[0,11,0,12],[0,13,0,14]]}
["  PUSCH JCE",null,null,null,null,"38.104 req","38.141 req","China Telecom",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Samsung",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["JCE over",null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["8 slots","FDD 15kHz SCS 5MHz ","TDLA30-10 Low","DMRS 1+0","PUSCH Mapping type A",{"$f":"DerivingPerfReq(H3:AA3)","v":-7.9},{"$f":"IF(F3>-100,F3+0.6,F3)","v":-7.3000000000000007},-9.5,-7.5,-9.3699999999999992,-6.8699999999999992,-11.38,-9.3800000000000008,-12.1,-10.1,-11.2,-9.1999999999999993,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":2.7300000000000004},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":3.2300000000000004},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-10.709999999999999},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-8.61}]
[null,null,null,null,"PUSCH Mapping type B",-8.3000000000000007,-7.7000000000000011,-9.6,-7.6,-9.43,-6.93,-11.38,-9.3800000000000008,-12.1,-10.1,-11.2,-9.1999999999999993,null,null,null,null,null,null,null,null,null,null,2.67,3.17,-10.742000000000001,-8.6419999999999995]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-9.9,-9.3000000000000007,-9.5,-7.5,-10.130000000000001,-7.6300000000000008,-11.75,-9.75,-12.3,-10.3,-11.7,-9.6999999999999993,null,null,null,null,null,null,null,null,null,null,2.8000000000000007,2.8000000000000007,-11.076000000000002,-8.9760000000000026]
[null,null,null,null,"PUSCH Mapping type B",-9.9,-9.3000000000000007,-9.5,-7.5,-10.119999999999999,-7.6199999999999992,-11.74,-9.74,-12.3,-10.3,-11.6,-9.6,null,null,null,null,null,null,null,null,null,null,2.8000000000000007,2.8000000000000007,-11.052,-8.952]
["2 slots","TDD 15kHz SCS 5MHz",null,"DMRS 1+0","PUSCH Mapping type A",-2.6,-2,-3.8,-1.8,-4.0599999999999996,-1.5599999999999996,-5.38,-3.38,-6.32,-4.32,-5.7,-3.7,null,null,null,null,null,null,null,null,null,null,2.5200000000000005,2.7600000000000007,-5.0519999999999996,-2.9519999999999995]
[null,null,null,null,"PUSCH Mapping type B",-2.6,-2,-3.9,-1.9,-4.08,-1.58,-5.37,-3.37,-6.32,-4.32,-5.7,-3.7,null,null,null,null,null,null,null,null,null,null,2.4200000000000004,2.74,-5.0739999999999998,-2.9740000000000002]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-3.6,-3,-4.4000000000000004,-2.4,-4.58,-2.08,-5.78,-3.7800000000000002,-6.47,-4.47,-6.1,-4.0999999999999996,null,null,null,null,null,null,null,null,null,null,2.0699999999999994,2.3899999999999997,-5.4659999999999993,-3.3659999999999997]
[null,null,null,null,"PUSCH Mapping type B",-3.4,-2.8,-4.5,-2.5,-4.6399999999999997,-2.1399999999999997,-5.79,-3.79,-6.48,-4.4800000000000004,-6.1,-4.0999999999999996,null,null,null,null,null,null,null,null,null,null,1.9800000000000004,2.3400000000000007,-5.5019999999999998,-3.4019999999999997]
["8 slots","FDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-9.8000000000000007,-9.2000000000000011,-9.9,-7.9,-10,-7.5,-11.57,-9.57,-12.1,-10.1,-11.6,-9.6,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)-MIN(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)","v":2.1999999999999993},2.5999999999999996,{"$f":"AVERAGE(H11,J11,L11,N11,P11,R11,T11,V11,X11,Z11)","v":-11.034000000000001},-8.9340000000000011]
[null,null,null,null,"PUSCH Mapping type B",-9.8000000000000007,-9.2000000000000011,-9.9,-7.9,-10.01,-7.51,-11.55,-9.5500000000000007,-12.1,-10.1,-11.6,-9.6,null,null,null,null,null,null,null,null,null,null,2.1999999999999993,2.59,-11.032,-8.9320000000000004]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-9.5,-8.9,-10,-8,-10.66,-8.16,-11.72,-9.7200000000000006,-12.1,-10.1,-12,-10,null,null,null,null,null,null,null,null,null,null,2.0999999999999996,{"$f":"MAX(I14,K13,M13,O13,Q13,S13,U13,W13,Y13,AA13)-MIN(I14,K13,M13,O13,Q13,S13,U13,W13,Y13,AA13)","v":2.0999999999999996},-11.296000000000001,{"$f":"AVERAGE(I14,K13,M13,O13,Q13,S13,U13,W13,Y13,AA13)","v":-9.1960000000000015}]
[null,null,null,null,"PUSCH Mapping type B",-9.5,-8.9,-10,-8,-10.62,-8.1199999999999992,-11.71,-9.7100000000000009,-12.1,-10.1,-12,-10,null,null,null,null,null,null,null,null,null,null,2.0999999999999996,{"$f":"MAX(H14,K14,M14,O14,Q14,S14,U14,W14,Y14,AA14)-MIN(H14,K14,M14,O14,Q14,S14,U14,W14,Y14,AA14)","v":1.9800000000000004},-11.286,{"$f":"AVERAGE(I14,K14,M14,O14,Q14,S14,U14,W14,Y14,AA14)","v":-9.1859999999999999}]
["2 slots","TDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-2.9,-2.2999999999999998,-4,-2,-4.47,-1.9699999999999998,-5.66,-3.66,-6.74,-4.74,-5.8,-3.8,null,null,null,null,null,null,null,null,null,null,2.74,2.7700000000000005,-5.3339999999999996,-3.2340000000000004]
[null,null,null,null,"PUSCH Mapping type B",-2.8,-2.1999999999999997,-4,-2,-4.46,-1.96,-5.64,-3.6399999999999997,-6.73,-4.7300000000000004,-5.8,-3.8,null,null,null,null,null,null,null,null,null,null,2.7300000000000004,2.7700000000000005,-5.3260000000000005,-3.226]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-3.8,-3.1999999999999997,-4.5,-2.5,-4.88,-2.38,-5.96,-3.96,-6.82,-4.82,-6.2,-4.2,null,null,null,null,null,null,null,null,null,null,2.3200000000000003,2.4400000000000004,-5.6719999999999997,-3.5720000000000001]
[null,null,null,null,"PUSCH Mapping type B",-3.3,-2.6999999999999997,-4.7,-2.7,-4.8600000000000003,-2.3600000000000003,-5.97,-3.9699999999999998,-6.82,-4.82,-6.2,-4.2,null,null,null,null,null,null,null,null,null,null,2.12,2.46,-5.71,-3.6100000000000003]
["2 slots","TDD 60kHz SCS 50MHz","TDLA30-75 Low","DMRS 1+1","PUSCH Mapping type B",{"$f":"DerivingPerfReq(H19:AA19)","v":-3.9},-3.3,-5.3,-3.3,-4.37,-1.27,-5.86,-3.8600000000000003,-6.53,-4.03,-6.3,-4.3,null,null,null,null,null,null,null,null,null,null,2.16,3.03,{"$f":"AVERAGE(H19,J19,L19,N19,P19,R19,T19,V19,X19,Z19)","v":-5.6720000000000006},-3.3520000000000003]
[null,"TDD 120kHz SCS 50MHz",null,"DMRS 1+1","PUSCH Mapping type B",-3.5,-2.9,-5.7,-3.7,-4.9400000000000004,-1.8400000000000003,-5.95,-3.95,-6.58,-4.08,-6.1,-4.0999999999999996,null,null,null,null,null,null,null,null,null,null,1.6399999999999997,2.2599999999999993,-5.854000000000001,-3.5340000000000003]

{"sheet":"PUSCH JCE (1T4R)","index":4,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[14,0,17,0],[14,1,17,1],[14,3,15,3],[16,3,17,3],[8,3,9,3],[10,0,13,0],[10,1,13,1],[10,3,11,3],[12,3,13,3],[0,27,0,28],[0,29,0,30],[2,0,5,0],[2,1,5,1],[2,2,17,2],[2,3,3,3],[4,3,5,3],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[6,0,9,0],[6,1,9,1],[6,3,7,3],[0,13,0,14],[0,5,1,5],[0,6,1,6],[0,7,0,8],[0,9,0,10],[0,11,0,12]]}
["  PUSCH JCE",null,null,null,null,"38.104 req","38.141 req","China Telecom",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Samsung",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["JCE over",null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["8 slots","FDD 15kHz SCS 5MHz ","TDLA30-10 Low","DMRS 1+0","PUSCH Mapping type A",{"$f":"DerivingPerfReq(H3:AA3)","v":-11.8},{"$f":"IF(F3>-100,F3+0.6,F3)","v":-11.200000000000001},-13.5,-11.5,-13.08,-10.58,-14.8,-12.8,-15.9,-13.9,-14.5,-12.5,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":2.8200000000000003},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":3.3200000000000003},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-14.356},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-12.255999999999998}]
[null,null,null,null,"PUSCH Mapping type B",-11.8,-11.200000000000001,-13.5,-11.5,-12.98,-10.48,-14.82,-12.82,-15.9,-13.9,-14.5,-12.5,null,null,null,null,null,null,null,null,null,null,2.92,3.42,-14.339999999999998,-12.239999999999998]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-12.3,-11.700000000000001,-13.5,-11.5,-13.79,-11.29,-15.29,-13.29,-16.100000000000001,-14.1,-15,-13,null,null,null,null,null,null,null,null,null,null,2.6000000000000014,2.8100000000000005,-14.736000000000001,-12.635999999999999]
[null,null,null,null,"PUSCH Mapping type B",-12.3,-11.700000000000001,-13.5,-11.5,-13.72,-11.22,-15.29,-13.29,-16.100000000000001,-14.1,-15,-13,null,null,null,null,null,null,null,null,null,null,2.6000000000000014,2.879999999999999,-14.722,-12.622]
["2 slots","TDD 15kHz SCS 5MHz",null,"DMRS 1+0","PUSCH Mapping type A",{"$f":"DerivingPerfReq(H7:AA7)","v":-6.2},-5.6000000000000005,-7.7,-5.7,-7.84,-5.34,-8.89,-6.8900000000000006,-11.6,-9.6,-9,-7,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)-MIN(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)","v":3.8999999999999995},4.26,{"$f":"AVERAGE(H7,J7,L7,N7,P7,R7,T7,V7,X7,Z7)","v":-9.0060000000000002},-6.9060000000000006]
[null,null,null,null,"PUSCH Mapping type B",-6.3,-5.7,-7.9,-5.9,-7.76,-5.26,-8.89,-6.8900000000000006,-11.6,-9.6,-9,-7,null,null,null,null,null,null,null,null,null,null,3.84,4.34,-9.0299999999999994,-6.93]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-6.8,-6.2,-8.5,-6.5,-8.39,-5.8900000000000006,-9.43,-7.43,-11.7,-9.6999999999999993,-9.3000000000000007,-7.3,null,null,null,null,null,null,null,null,null,null,3.3099999999999987,3.8099999999999987,-9.4639999999999986,-7.3639999999999999]
[null,null,null,null,"PUSCH Mapping type B",-6.8,-6.2,-8.6,-6.6,-8.32,-5.82,-9.43,-7.43,-11.7,-9.6999999999999993,-9.3000000000000007,-7.3,null,null,null,null,null,null,null,null,null,null,3.379999999999999,3.879999999999999,-9.4699999999999989,-7.37]
["8 slots","FDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-13,-12.4,-13.9,-11.9,-13.31,-10.81,-15.42,-13.42,-15.9,-13.9,-14.7,-12.7,null,null,null,null,null,null,null,null,null,null,2.59,3.09,-14.646000000000001,-12.546000000000001]
[null,null,null,null,"PUSCH Mapping type B",-13.3,-12.700000000000001,-13.8,-11.8,-13.36,-10.86,-15.41,-13.41,-15.9,-13.9,-14.7,-12.7,null,null,null,null,null,null,null,null,null,null,2.5400000000000009,3.0400000000000009,-14.634,-12.534000000000001]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-13.1,-12.5,-13.8,-11.8,-14.06,-11.56,-15.78,-13.78,-16,-14,-15,-13,null,null,null,null,null,null,null,null,null,null,2.1999999999999993,2.4399999999999995,-14.928000000000001,-12.827999999999999]
[null,null,null,null,"PUSCH Mapping type B",-13.1,-12.5,-13.7,-11.7,-14.11,-11.61,-15.75,-13.75,-16,-14,-15,-13,null,null,null,null,null,null,null,null,null,null,2.3000000000000007,2.3900000000000006,-14.912000000000001,-12.812000000000001]
["2 slots","TDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-6.5,-5.9,-7.9,-5.9,-8.01,-5.51,-9.02,-7.02,-9.18,-7.18,-9,-7,null,null,null,null,null,null,null,null,null,null,1.2799999999999994,1.67,-8.6219999999999999,-6.5220000000000002]
[null,null,null,null,"PUSCH Mapping type B",-6.5,-5.9,-7.9,-5.9,-8.02,-5.52,-9.01,-7.01,-9.17,-7.17,-9,-7,null,null,null,null,null,null,null,null,null,null,1.2699999999999996,1.6500000000000004,-8.620000000000001,-6.5200000000000005]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-7,-6.4,-8.6999999999999993,-6.7,-8.51,-6.01,-9.44,-7.4399999999999995,-9.34,-7.34,-9.3000000000000007,-7.3,null,null,null,null,null,null,null,null,null,null,0.92999999999999972,1.4299999999999997,-9.0579999999999981,-6.9580000000000002]
[null,null,null,null,"PUSCH Mapping type B",-7,-6.4,-8.6999999999999993,-6.7,-8.52,-6.02,-9.44,-7.4399999999999995,-9.34,-7.34,-9.3000000000000007,-7.3,null,null,null,null,null,null,null,null,null,null,0.91999999999999993,1.42,-9.0599999999999987,-6.9599999999999991]

{"sheet":"PUSCH JCE (1T8R)","index":5,"n_rows":18,"n_cols":31,"rows_kept":18,"cut":false,"hidden":false,"merged":[[14,0,17,0],[14,1,17,1],[14,3,15,3],[16,3,17,3],[8,3,9,3],[10,0,13,0],[10,1,13,1],[10,3,11,3],[12,3,13,3],[0,27,0,28],[0,29,0,30],[2,0,5,0],[2,1,5,1],[2,2,17,2],[2,3,3,3],[4,3,5,3],[0,15,0,16],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,25,0,26],[6,0,9,0],[6,1,9,1],[6,3,7,3],[0,13,0,14],[0,5,1,5],[0,6,1,6],[0,7,0,8],[0,9,0,10],[0,11,0,12]]}
["  PUSCH JCE",null,null,null,null,"38.104 req","38.141 req","China Telecom",null,"Nokia",null,"Huawei",null,"Ericsson",null,"Samsung",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["JCE over",null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["8 slots","FDD 15kHz SCS 5MHz ","TDLA30-10 Low","DMRS 1+0","PUSCH Mapping type A",{"$f":"DerivingPerfReq(H3:AA3)","v":-15},{"$f":"IF(F3>-100,F3+0.6,F3)","v":-14.4},-16.600000000000001,-14.6,-15.92,-14.42,-17.78,-15.780000000000001,-19.5,-17.5,-17.3,-15.3,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":3.58},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)-MIN(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":3.08},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-17.420000000000002},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3,W3,Y3,AA3)","v":-15.52}]
[null,null,null,null,"PUSCH Mapping type B",-15,-14.4,-16.7,-14.7,-15.89,-14.39,-17.760000000000002,-15.760000000000002,-19.5,-17.5,-17.3,-15.3,null,null,null,null,null,null,null,null,null,null,3.6099999999999994,{"$f":"MAX(I4,K4,M4,O4,Q4,S4,U4,W4,Y4,AA4)-MIN(I4,K4,M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":3.1099999999999994},-17.43,{"$f":"AVERAGE(#REF!,K4,M4,O4,Q4,S4,U4,W4,Y4,AA4)","v":{"$error":"#REF!"}}]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-15.6,-15,-16.600000000000001,-14.6,-16.86,-15.36,-18.43,-16.43,-19.5,-17.5,-18.100000000000001,-16.100000000000001,null,null,null,null,null,null,null,null,null,null,2.8999999999999986,2.9000000000000004,-17.898000000000003,-15.998000000000001]
[null,null,null,null,"PUSCH Mapping type B",-15.6,-15,-16.7,-14.7,-16.84,-15.34,-18.43,-16.43,-19.5,-17.5,-18.100000000000001,-16.100000000000001,null,null,null,null,null,null,null,null,null,null,2.8000000000000007,{"$f":"MAX(I6,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)-MIN(I6,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)","v":2.8000000000000007},-17.913999999999998,{"$f":"AVERAGE(#REF!,K6,M6,O6,Q6,S6,U6,W6,Y6,AA6)","v":{"$error":"#REF!"}}]
["2 slots","TDD 15kHz SCS 5MHz",null,"DMRS 1+0","PUSCH Mapping type A",-9.4,-8.8000000000000007,-10.9,-8.9,-10.6,-9.1,-11.86,-9.86,-13.6,-11.6,-11.8,-9.8000000000000007,null,null,null,null,null,null,null,null,null,null,3,2.6999999999999993,-11.752000000000001,-9.8520000000000003]
[null,null,null,null,"PUSCH Mapping type B",-9.4,-8.8000000000000007,-10.9,-8.9,-10.64,-9.14,-11.88,-9.8800000000000008,-13.6,-11.6,-11.8,-9.8000000000000007,null,null,null,null,null,null,null,null,null,null,2.9599999999999991,{"$f":"MAX(I4,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)-MIN(I4,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)","v":5.5599999999999987},-11.764000000000001,{"$f":"AVERAGE(I4,K8,M8,O8,Q8,S8,U8,W8,Y8,AA8)","v":-11.024000000000001}]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-10.6,-10,-11.9,-9.9,-11.44,-9.94,-12.57,-10.57,-13.7,-11.7,-12.5,-12.1,null,null,null,null,null,null,null,null,null,null,2.2599999999999998,2.1999999999999993,-12.422000000000001,-10.842000000000001]
[null,null,null,null,"PUSCH Mapping type B",-10.6,-10,-11.9,-9.9,-11.45,-9.9499999999999993,-12.56,-10.56,-13.7,-11.7,-12.5,-12.1,null,null,null,null,null,null,null,null,null,null,2.25,{"$f":"MAX(I6,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)-MIN(I6,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)","v":4.75},-12.422000000000001,{"$f":"AVERAGE(I6,K10,M10,O10,Q10,S10,U10,W10,Y10,AA10)","v":-11.802}]
["8 slots","FDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-15.3,-14.700000000000001,-16.899999999999999,-14.9,-16.149999999999999,-14.649999999999999,-18.12,-16.12,-17.399999999999999,-15.4,-17.399999999999999,-15.4,null,null,null,null,null,null,null,null,null,null,1.9700000000000024,1.4700000000000024,-17.193999999999999,-15.294]
[null,null,null,null,"PUSCH Mapping type B",-15.5,-14.9,-16.899999999999999,-14.9,-16.13,-14.629999999999999,-18.16,-16.16,-17.399999999999999,-15.4,-17.399999999999999,-15.4,null,null,null,null,null,null,null,null,null,null,2.0300000000000011,1.5300000000000011,-17.198,-15.297999999999998]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-15.8,-15.200000000000001,-16.899999999999999,-14.9,-17.059999999999999,-15.559999999999999,-18.86,-16.86,-17.600000000000001,-15.6,-18.100000000000001,-16.100000000000001,null,null,null,null,null,null,null,null,null,null,1.9600000000000009,1.9599999999999991,-17.703999999999997,-15.804000000000002]
[null,null,null,null,"PUSCH Mapping type B",-15.8,-15.200000000000001,-16.899999999999999,-14.9,-17.010000000000002,-15.510000000000002,-18.829999999999998,-16.829999999999998,-17.600000000000001,-15.6,-18.100000000000001,-16.100000000000001,null,null,null,null,null,null,null,null,null,null,1.9299999999999997,1.9299999999999979,-17.687999999999999,-15.788]
["2 slots","TDD 30kHz SCS 10MHz",null,"DMRS 1+0","PUSCH Mapping type A",-9.6999999999999993,-9.1,-11,-9,-11,-9.5,-11.94,-9.94,-12.1,-10.1,-11.8,-9.8000000000000007,null,null,null,null,null,null,null,null,null,null,1.0999999999999996,1.0999999999999996,-11.568000000000001,-9.668000000000001]
[null,null,null,null,"PUSCH Mapping type B",-9.6999999999999993,-9.1,-11,-9,-10.99,-9.49,-11.93,-9.93,-12.1,-10.1,-11.8,-9.8000000000000007,null,null,null,null,null,null,null,null,null,null,1.1099999999999994,1.0999999999999996,-11.564000000000002,-9.6640000000000015]
[null,null,null,"DMRS 1+1","PUSCH Mapping type A",-10.3,-9.7000000000000011,-11.8,-9.8000000000000007,-11.68,-10.18,-12.54,-10.54,-12.4,-10.4,-12.4,-10.4,null,null,null,null,null,null,null,null,null,null,0.85999999999999943,0.73999999999999844,-12.163999999999998,-10.263999999999999]
[null,null,null,null,"PUSCH Mapping type B",-10.3,-9.7000000000000011,-11.9,-9.9,-11.67,-10.17,-12.55,-10.55,-12.4,-10.4,-12.4,-10.4,null,null,null,null,null,null,null,null,null,null,0.88000000000000078,0.65000000000000036,-12.184000000000001,-10.284000000000001]

{"sheet":"TBoMS simulation assumption","index":6,"n_rows":34,"n_cols":3,"rows_kept":34,"cut":false,"hidden":false,"merged":[[32,0,32,1],[33,0,33,1],[17,0,17,1],[19,0,25,0],[26,0,28,0],[27,1,28,1],[29,0,30,0],[31,0,31,1],[16,0,16,1],[0,0,0,1],[1,0,1,1],[2,0,3,1],[4,0,4,1],[5,0,6,1],[7,0,8,1],[9,0,9,1],[10,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,15,1]]}
["Parameter",null,"Value"]
["Duplex mode",null,"FDD and TDD"]
["SCS",null,"15/30 kHz for FR1 (TDD and FDD)"]
[null,null,"60/120 kHz for FR2 (TDD)"]
["Antenna",null,"1T2R"]
["Channel Model",null,"TDLB100-400 Low for FR1"]
[null,null,"TDLA30-300 Low for FR2"]
["TDD UL-DL pattern",null,"7D1S2U, S=6D:4G:4U for 30kHz SCS"]
[null,null,"3D1S1U, S=10D:2G:2U for 15/60/120 kHz SCS"]
["PRB number",null,"5 PRB"]
["PUSCH mapping type",null,"Type A and type B for FR1 "]
[null,null,"Type B for FR2"]
["MCS",null,"MCS 2"]
["Inter-slot frequency hopping",null,"Disabled"]
["Physical/available slots for TBoMS",null,"4 for FDD"]
[null,null,"2 for TDD"]
["PUSCH repetition",null,"Disabled"]
["Transform precoding",null,"CP-OFDM"]
["HARQ","Maximum number of HARQ transmissions",4]
["DM-RS","DM-RS configuration type",1]
[null,"DM-RS duration","single-symbol DM-RS"]
[null,"Additional DM-RS position","pos1"]
[null,"Number of DM-RS CDM group(s) without data",2]
[null,"Ratio of PUSCH EPRE to DM-RS EPRE","-3 dB"]
[null,"DM-RS port",0]
[null,"DM-RS sequence generation","NID0=0, nSCID =0"]
["Time domain resource assignment","Start symbol",0]
[null,"Allocation length","14 for FR1"]
[null,null,"10 for FR2"]
["PT-RS configuration","Frequency density (KPT-RS)","Disabled"]
[null,"Time density (LPT-RS)","Disabled"]
["Code block group based PUSCH transmission",null,"Disabled"]
["RV sequence",null,"[0 2 3 1]"]
["Test metric",null,"Test SNR at which the PUSCH achieves 70% of throughput"]

{"sheet":"PUSCH JCE simulation assumption","index":7,"n_rows":43,"n_cols":3,"rows_kept":43,"cut":false,"hidden":false,"merged":[[37,0,38,0],[39,0,39,1],[40,0,40,1],[41,0,41,1],[42,0,42,1],[35,0,36,0],[10,0,14,1],[15,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,20,1],[21,0,22,1],[23,0,23,1],[24,0,26,0],[25,1,26,1],[27,0,34,0],[29,1,30,1],[0,0,0,1],[1,0,1,1],[2,0,3,1],[6,0,7,1],[8,0,9,1],[4,0,5,1]]}
["Parameter",null,"Value"]
["Duplex mode",null,"FDD and TDD"]
["SCS",null,"15/30 kHz for FR1 (TDD and FDD)"]
[null,null,"60/120 kHz for FR2 (TDD)"]
["Antenna",null,"For FR1: 1T2R 1T4R 1T8R"]
[null,null,"For FR2: 1T2R"]
["Channel Model",null,"TDLA30-10 for FR1"]
[null,null,"TDLA30-75 for FR2"]
["TDD UL-DL pattern",null,"7D1S2U, S=6D:4G:4U for 15/30kHz SCS"]
[null,null,"DDSUU, S=10D:2G:2U for 60/120kHz SCS"]
["PRB number",null,"Full applicable test bandwidth for"]
[null,null,"5MHz for 15kHz SCS"]
[null,null,"10MHz for 30kHz SCS"]
[null,null,"50MHz for 60/120kHz SCS"]
[null,null,"Interested companies can bring simulation results for the largest CHBW for each SCS."]
["PUSCH mapping type",null,"Type A and type B for FR1 "]
[null,null,"Type B for FR2"]
["MCS",null,"MCS 4"]
["Inter-slot frequency hopping",null,"Disabled"]
["aTDW length (same with cTDW length)",null,"2 for TDD"]
[null,null,"8 for FDD"]
["PUSCH repetition number",null,"2 for TDD"]
[null,null,"8 for FDD"]
["Transform precoding",null,"CP-OFDM"]
["HARQ","Maximum number of HARQ transmissions",4]
[null,"RV sequence","[0 3 0 3] for TDD (repetition number = 2)"]
[null,null,"[0 0 0 0] for FDD (repetition number = 8)"]
["DM-RS","DM-RS configuration type",1]
[null,"DM-RS duration","single-symbol DM-RS"]
[null,"Additional DM-RS position","For FR1: DMRS 1+1 and DMRS 1+0"]
[null,null,"For FR2: DMRS 1+1"]
[null,"Number of DM-RS CDM group(s) without data",2]
[null,"Ratio of PUSCH EPRE to DM-RS EPRE","-3 dB"]
[null,"DM-RS port",0]
[null,"DM-RS sequence generation","NID0=0, nSCID =0"]
["Time domain resource assignment","Start symbol",0]
[null,"Allocation length",14]
["PT-RS configuration","Frequency density (KPT-RS)","Disabled"]
[null,"Time density (LPT-RS)","Disabled"]
["Code block group based PUSCH transmission",null,"Disabled"]
["phase and power offset",null,"Ideal"]
["CFO modelling",null,"N/A"]
["Test metric",null,"Test SNR at which the PUSCH achieves 70% of throughput"]