{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Cover","Parameters","PUCCH Format1 JCE (1T2R) ","PUCCH Format3 JCE (1T2R) ","PUCCH JCE simulation assumption"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUCCH Format1 JCE (1T2R) ","index":2,"n_rows":14,"n_cols":30,"rows_kept":14,"cut":false,"hidden":false,"merged":[[10,0,13,0],[10,2,13,2],[8,0,9,0],[8,1,9,1],[12,1,13,1],[10,1,11,1],[2,0,3,0],[2,1,3,1],[2,2,9,2],[0,14,0,15],[0,4,1,4],[0,5,1,5],[0,6,0,7],[0,8,0,9],[6,0,7,0],[6,1,7,1],[4,0,5,0],[4,1,5,1],[0,10,0,11],[0,12,0,13],[0,26,0,27],[0,28,0,29],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25]]}
["PUCCH Format1 JCE (1T2R) ",null,null,null,"38.104 req","38.141 req","Nokia",null,"Ericsson",null,"Samsung",null,"Huawei",null,"Company 5",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["JCE over",null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["8 slots","FDD 15kHz SCS 5MHz ","TDLA30-10 Low","ACK missed detection ",{"$f":"DerivingPerfReq(G3:Z3)","v":-8.9},{"$f":"IF(E3>-100,E3+0.6,E3)","v":-8.3000000000000007},-14,-11.5,-11.3,{"$f":"I3+2","v":-9.3000000000000007},-10.8,-8.8000000000000007,-11.23,-8.73,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)-MIN(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)","v":3.1999999999999993},{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":2.7699999999999996},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)","v":-11.8325},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-9.5824999999999996}]
[null,null,null,"NACK to ACK detection",{"$f":"DerivingPerfReq(G4:Z4)","v":-9.1},{"$f":"IF(E4>-100,E4+0.6,E4)","v":-8.5},-11.7,-9.1999999999999993,-12,{"$f":"I4+2","v":-10},-10.56,-8.6,-11.16,-8.66,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)-MIN(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)","v":1.4399999999999995},{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)-MIN(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":1.4000000000000004},{"$f":"AVERAGE(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)","v":-11.355},{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":-9.1149999999999984}]
["2 slots","TDD 15kHz SCS 5MHz",null,"ACK missed detection ",{"$f":"DerivingPerfReq(G5:Z5)","v":-3.9},-3.3,-7.8,-5.3,-5.3,-3.3,-6.09,-4.09,-6.92,-4.42,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)-MIN(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)","v":2.5},2,{"$f":"AVERAGE(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)","v":-6.5274999999999999},-4.2774999999999999]
[null,null,null,"NACK to ACK detection",-3,-2.4,-4.9000000000000004,-2.4000000000000004,-6,-4,-5.24,-3.24,-5,-2.5,null,null,null,null,null,null,null,null,null,null,null,null,1.0999999999999996,1.5999999999999996,-5.2850000000000001,-3.0350000000000001]
["8 slots","FDD 30kHz SCS 10MHz",null,"ACK missed detection ",-8.5,-7.9,-13.7,-11.2,-11.2,-9.1999999999999993,-10.67,-8.67,-10.220000000000001,-7.7200000000000006,null,null,null,null,null,null,null,null,null,null,null,null,3.4799999999999986,3.4799999999999986,-11.4475,-9.1974999999999998]
[null,null,null,"NACK to ACK detection",-8.6999999999999993,-8.1,-10.6,-8.1,-11.6,-9.6,-9.93,-7.93,-11.68,-9.18,null,null,null,null,null,null,null,null,null,null,null,null,1.75,1.67,-10.952499999999999,-8.7025000000000006]
["2 slots","TDD 30kHz SCS 10MHz",null,"ACK missed detection ",-3.8,-3.1999999999999997,-7.6,-5.0999999999999996,-5.4,-3.4000000000000004,-6.25,-4.25,-6.18,-3.6799999999999997,null,null,null,null,null,null,null,null,null,null,null,null,2.1999999999999993,1.6999999999999993,-6.3574999999999999,-4.1074999999999999]
[null,null,null,"NACK to ACK detection",-3,-2.4,-4.8,-2.2999999999999998,-5.7,-3.7,-4.8499999999999996,-2.85,-5.5,-3,null,null,null,null,null,null,null,null,null,null,null,null,0.90000000000000036,1.4000000000000004,-5.2125000000000004,-2.9624999999999999]
["2 slots","TDD 60kHz SCS 50MHz","TDLA30-75 Low","ACK missed detection ",-103,-103,-8.3000000000000007,-5.2000000000000011,-5.2,{"$f":"I11+2.5","v":-2.7},-6.16,-4.16,-10.09,-7.59,null,null,null,null,null,null,null,null,null,null,null,null,4.8899999999999997,4.8899999999999997,-7.4375,-4.9125000000000005]
[null,null,null,"NACK to ACK detection",{"$f":"DerivingPerfReq(G12:Z12)","v":-2.9},{"$f":"IF(E12>-100,E12+0.6,E12)","v":-2.2999999999999998},-5.6,-2.4999999999999996,-5.3,{"$f":"I12+2.5","v":-2.8},-5.4,-3.4,-8.99,-6.49,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)-MIN(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)","v":3.6900000000000004},{"$f":"MAX(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)-MIN(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":3.9900000000000007},{"$f":"AVERAGE(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)","v":-6.3224999999999998},{"$f":"AVERAGE(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":-3.7974999999999999}]
[null,"TDD 120kHz SCS 50MHz",null,"ACK missed detection ",-4.8,-4.2,-8.1,-5,-5.2,-2.7,-6.21,-4.2,-7.66,-5.16,null,null,null,null,null,null,null,null,null,null,null,null,2.8999999999999995,2.46,-6.7925000000000004,-4.2650000000000006]
[null,null,null,"NACK to ACK detection",{"$f":"DerivingPerfReq(G14:Z14)","v":-3},-2.4,-5.5,-2.4,-5.3,-2.8,-5.81,-3.8,-7.63,-5.13,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)-MIN(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)","v":2.33},2.73,{"$f":"AVERAGE(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)","v":-6.06},-3.5324999999999998]

{"sheet":"PUCCH Format3 JCE (1T2R) ","index":3,"n_rows":14,"n_cols":30,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,26,0,27],[0,28,0,29],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25],[0,4,1,4],[0,5,1,5],[0,6,0,7],[12,1,13,1],[10,0,13,0],[10,2,13,2],[10,1,11,1],[6,0,7,0],[6,1,7,1],[8,0,9,0],[8,1,9,1],[2,0,3,0],[2,1,3,1],[2,2,9,2],[4,0,5,0],[4,1,5,1]]}
["PUCCH Format3 JCE (1T2R) ",null,null,null,"38.104 req","38.141 req","Nokia",null,"Ericsson",null,"Samsung",null,"Huawei",null,"Company 5",null,"Company 6",null,"Company 7",null,"Company 8",null,"Company 9",null,"Company 10",null,"SPAN",null,"AVERAGE"]
["JCE over",null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["8 slots","FDD 15kHz SCS 5MHz ","TDLA30-10 Low","DMRS 1+0",{"$f":"DerivingPerfReq(G3:Z3)","v":-5.3},{"$f":"IF(E3>-100,E3+0.6,E3)","v":-4.7},-6.8,-4.3,-8.1999999999999993,{"$f":"I3+2","v":-6.1999999999999993},-6.93,-4.93,-8.34,-5.84,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)-MIN(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)","v":1.54},{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":1.8999999999999995},{"$f":"AVERAGE(G3,I3,K3,M3,O3,Q3,S3,U3,W3,Y3)","v":-7.5674999999999999},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3,V3,X3,Z3)","v":-5.3174999999999999}]
[null,null,null,"DMRS 1+1",-5.8,{"$f":"IF(E4>-100,E4+0.6,E4)","v":-5.2},-7.6,-5.0999999999999996,-8.4,{"$f":"I4+2","v":-6.4},-7.6,-5.6,-8.52,-6.02,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)-MIN(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)","v":0.91999999999999993},{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)-MIN(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":1.3000000000000007},{"$f":"AVERAGE(G4,I4,K4,M4,O4,Q4,S4,U4,W4,Y4)","v":-8.0300000000000011},{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4,V4,X4,Z4)","v":-5.78}]
["2 slots","TDD 15kHz SCS 5MHz",null,"DMRS 1+0",0.3,0.89999999999999991,-1.8,0.7,-2.2000000000000002,-0.20000000000000018,-1.7,0.3,-2.21,0.29000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)-MIN(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)","v":0.51},0.90000000000000013,{"$f":"AVERAGE(G5,I5,K5,M5,O5,Q5,S5,U5,W5,Y5)","v":-1.9775},0.27249999999999996]
[null,null,null,"DMRS 1+1",-0.1,0.5,-2.2000000000000002,0.29999999999999982,-2.6,-0.60000000000000009,-2.2999999999999998,-0.3,-2.25,0.25,null,null,null,null,null,null,null,null,null,null,null,null,0.39999999999999991,0.89999999999999991,-2.3375000000000004,-8.7500000000000078E-2]
["8 slots","FDD 30kHz SCS 10MHz",null,"DMRS 1+0",-5.2,-4.6000000000000005,-6.6,-4.0999999999999996,-8.1999999999999993,-6.1999999999999993,-7,-5,-8.08,-5.58,null,null,null,null,null,null,null,null,null,null,null,null,1.5999999999999996,2.0999999999999996,-7.4699999999999989,-5.22]
[null,null,null,"DMRS 1+1",-5.6,-5,-7.4,-4.9000000000000004,-8.5,-6.5,-7.6,-5.6,-8.01,-5.51,null,null,null,null,null,null,null,null,null,null,null,null,1.0999999999999996,1.5999999999999996,-7.8774999999999995,-5.6274999999999995]
["2 slots","TDD 30kHz SCS 10MHz",null,"DMRS 1+0",0.2,0.8,-1.6,0.89999999999999991,-2.2999999999999998,-0.29999999999999982,-2.1,-0.1,-2.0299999999999998,0.4700000000000002,null,null,null,null,null,null,null,null,null,null,null,null,0.69999999999999973,1.1999999999999997,-2.0074999999999998,0.24250000000000008]
[null,null,null,"DMRS 1+1",0,0.6,-2,0.5,-2.6,-0.60000000000000009,-2.6,-0.6,-1.95,0.55000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,0.65000000000000013,1.1500000000000001,-2.2874999999999996,-3.7500000000000006E-2]
["2 slots","TDD 60kHz SCS 50MHz","TDLA30-75 Low","DMRS 1+0",0.1,0.7,-2.5,0.60000000000000009,-2.2000000000000002,-0.20000000000000018,-2.1,-0.1,-0.06,2.44,null,null,null,null,null,null,null,null,null,null,null,null,2.44,2.64,-1.7150000000000001,0.68499999999999994]
[null,null,null,"DMRS 1+1",{"$f":"DerivingPerfReq(G12:Z12)","v":-0.2},0.39999999999999997,-3.1,0,-2.6,{"$f":"I12+2.5","v":-0.10000000000000009},-2.5,-0.5,-0.56999999999999995,1.9300000000000002,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)-MIN(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)","v":2.5300000000000002},{"$f":"MAX(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)-MIN(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":2.4300000000000002},{"$f":"AVERAGE(G12,I12,K12,M12,O12,Q12,S12,U12,W12,Y12)","v":-2.1924999999999999},{"$f":"AVERAGE(H12,J12,L12,N12,P12,R12,T12,V12,X12,Z12)","v":0.33250000000000002}]
[null,"TDD 120kHz SCS 50MHz",null,"DMRS 1+0",0.7,{"$f":"IF(E13>-100,E13+0.6,E13)","v":1.2999999999999998},-2.2000000000000002,0.89999999999999991,-2.2999999999999998,0.20000000000000018,-2.1,-0.1,-0.53,1.97,null,null,null,null,null,null,null,null,null,null,null,null,1.7699999999999998,2.0699999999999998,-1.7825,0.74249999999999994]
[null,null,null,"DMRS 1+1",{"$f":"DerivingPerfReq(G14:Z14)","v":-0.1},0.5,-2.6,0.5,-2.7,-0.20000000000000018,-2.6,-0.6,-0.64,1.8599999999999999,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)-MIN(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)","v":2.06},{"$f":"MAX(H14,J14,L14,N14,P14,R14,T14,V14,X14,Z14)-MIN(H14,J14,L14,N14,P14,R14,T14,V14,X14,Z14)","v":2.46},{"$f":"AVERAGE(G14,I14,K14,M14,O14,Q14,S14,U14,W14,Y14)","v":-2.1350000000000002},{"$f":"AVERAGE(H14,J14,L14,N14,P14,R14,T14,V14,X14,Z14)","v":0.3899999999999999}]

{"sheet":"PUCCH JCE simulation assumption","index":4,"n_rows":32,"n_cols":3,"rows_kept":32,"cut":false,"hidden":false,"merged":[[31,0,31,1],[22,0,22,1],[26,0,26,1],[27,0,27,1],[28,0,28,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[1,0,1,1],[30,0,30,1],[29,0,29,1],[10,0,10,1],[11,0,14,1],[21,0,21,1],[16,0,16,1],[15,0,15,1],[17,0,18,1],[19,0,20,1],[2,0,2,1],[3,0,4,1],[6,0,7,1],[8,0,9,1],[5,0,5,1]]}
["Parameter",null,"Value"]
["PUCCH formats",null,"Format 1 and Format 3"]
["Duplex mode",null,"FDD and TDD"]
["SCS",null,"15/30 kHz for FR1 (TDD and FDD)"]
[null,null,"60/120 kHz for FR2 (TDD)"]
["Antenna",null,"1T2R"]
["Channel Model",null,"TDLA30-10 for FR1"]
[null,null,"TDLA30-75 for FR2"]
["TDD UL-DL pattern (same as PUSCH)",null,"7D1S2U, S=6D:4G:4U for 15/30kHz SCS"]
[null,null,"DDSUU, S=10D:2G:2U for 60/120kHz SCS"]
["PRB number",null,"1 PRB"]
["CBW",null,"5MHz for 15kHz SCS"]
[null,null,"10MHz for 30kHz SCS"]
[null,null,"50MHz for 60/120kHz SCS"]
[null,null,"Interested companies can bring simulation results for the largest CHBW for each SCS."]
["Intra-slot frequency hopping",null,"Disabled"]
["Inter-slot frequency hopping",null,"Disabled"]
["aTDW length = cTDW length (same as PUSCH)",null,"2 for TDD"]
[null,null,"8 for FDD"]
["PUCCH repetition number (same as PUSCH)",null,"2 for TDD"]
[null,null,"8 for FDD"]
["Start symbol",null,0]
["Number of symbols",null,14]
["phase and power offset (same as PUSCH)",null,"Ideal"]
["Test metric",null,"format 1: Test NACK to ACK detection probability and ACK missed detection probability \n\nformat 3: Test UCI block error probability "]
["Bit payload",null,"format 1: 2 bits\n\nformat 3: 16 bits "]
["Group and sequence hopping ",null,"neither"]
["Hopping ID",null,0]
["Initial cyclic shift (format1)",null,0]
["Index of orthogonal cover code (timeDomainOCC) (format1)",null,0]
["Modulation order (format 3)",null,"QPSK"]
["DMRS configuration (format 3)",null,"DMRS1+1 , DMRS1+0"]