**3GPP TSG-RAN WG4 Meeting #106 R4-2301064**

**Athens, Greece, 27th February – 3rd March 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **-3** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for corrections for EN-DC 1 LTE + 1 NR bands |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | DC\_R18\_1BLTE\_1BNR\_2DL2UL |  | ***Date:*** | 2023-02-17 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Making corrections |
|  |  |
| ***Summary of change:*** | Placing DC\_1A\_n1A before DC\_2A\_n2APlacing DC\_40A\_n40A before DC\_41A\_n41ARemoving lower line in first column for DC\_40A\_n40ACorrecting BCS1 part of DC\_40A\_n40ACorrecting note for DC\_28A\_n20A8,11,13Adding n20 test points for DC\_3A\_n20A |
|  |  |
| ***Consequences if not approved:*** | Corrections are not made |
|  |  |
| ***Clauses affected:*** | 5.3, 5.5, 7.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

Table 5.3B.1.3-1: EN-DC configurations and bandwidth combination sets defined for intra-band non-contiguous EN-DC

|  |
| --- |
| E-UTRA – NR configuration / Bandwidth combination set |
| DownlinkEN-DC configuration | Uplink EN-DC configurations | Component carriers in order of increasing carrier frequency | Maximum aggregated bandwidth (MHz) | Bandwidth combination set |
|  |  | Channel bandwidths for E-UTRA carrier (MHz) | Channel bandwidths for NR carrier (MHz) | Channel bandwidths for E-UTRA carrier (MHz) |  |  |
| DC\_1A\_n1A | DC\_1A\_n1A2 | 5, 10, 15, 20 | 5, 10, 15, 20 |  | 40 | 0 |
| DC\_2A\_n2A | DC\_2A\_n2A2 | 5, 10, 15, 20 | 5, 10, 15, 20 |  | 40 | 0 |
|  |  |  |  |  |  |  |
| DC\_3A\_n3A | DC\_3A\_n3A |  | 5, 10, 15, 20, 25, 30 | 5, 10, 15, 20 | 50 | 0 |
|  |  |  | 5, 10, 15, 20, 25, 30 | 5, 10, 15, 20 | 50 | 1 |
|  |  | 5, 10, 15, 20 | 5, 10, 15, 20, 25, 30 |  |  |  |
| DC\_5A\_n5A | DC\_5A\_n5A2 | 5, 10 | 5, 10, 15 |  | 20 | 0 |
| DC\_7A\_n7A3 | DC\_7A\_n7A2 | 5, 10, 15, 20 | 5, 10, 15, 20 |  | 40 | 0 |
|  |  |  |  |  |  |  |
| DC\_40A\_n40A4 | DC\_40A\_n40A2 | 5, 10, 15, 20 | 5, 10, 15, 20, 25, 30, 40 |  | 60 | 0 |
|  | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20 |  |  |
|  |  |  | 40, 60, 80,100 | 20 | 120 | 1 |
|  |  | 20 | 40, 50, 60, 80,100 |  |  |  |
|  |  |  | 40, 50, 60, 80,100 | 20 |  |  |
|  |  | 20 | 10, 20, 30, 40, 50, 60, 80,100 |  | 120 | 2 |
|  |  |  | 10, 20, 30, 40, 50, 60, 80,100 | 20 |  |  |
|  |  | 10 | 20, 30, 40, 50, 60, 80,100 |  |  |  |
|  |  |  | 20, 30, 40, 50, 60, 80,100 | 10 |  |  |
| DC\_41A\_n41A | DC\_41A\_n41A | 20 | 40, 60, 80,100 |  | 120 | 0 |
| DC\_41C\_n41A | DC\_41A\_n41A | 20+20 | 40, 60, 80,100 |  | 140 | 0 |
|  |  |  | 40, 60, 80,100 | 20+20 |  |  |
|  |  | 20+20 | 40, 50, 60, 80,100 |  | 140 | 1 |
|  |  |  | 40, 50, 60, 80,100 | 20+20 |  |  |
| DC\_41D\_n41A | DC\_41A\_n41A | 20+20+20 | 40, 60, 80,100 |  | 160 | 0 |
|  |  |  | 40, 60, 80,100 | 20+20+20 |  |  |
|  |  | 20+20+20 | 40, 50, 60, 80,100 |  | 160 | 1 |
|  |  |  | 40, 50, 60, 80,100 | 20+20+20 |  |  |
| DC\_48A\_n48A4 | DC\_48A\_n48A2 | 5, 10, 15, 20 | 5, 10, 15, 20, 40 |  | 60 | 0 |
|  |  |  | 5, 10, 15, 20, 40 | 5, 10, 15, 20 |  |  |
| DC\_48A-48A\_n48A4 | DC\_48A\_n48A2 | See CA\_48A-48A Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-3 | 5, 10, 15, 20, 40 |  | 80 | 0 |
|  |  |  | 5, 10, 15, 20, 40 | See CA\_48A-48A Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-3 |  |  |
| DC\_48C\_n48A4 | DC\_48A\_n48A2 | See CA\_48C Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-1 | 5, 10, 15, 20, 40 |  | 80 | 0 |
|  |  |  | 5, 10, 15, 20, 40 | See CA\_48C Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-1 |  |  |
| DC\_48D\_n48A4 | DC\_48A\_n48A2 | See CA\_48D Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-1 | 5, 10, 15, 20, 40 |  | 100 | 0 |
|  |  |  | 5, 10, 15, 20, 40 | See CA\_48D Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-1 |  |  |
| DC\_66A\_n66A | DC\_66A\_n66A2 | 5, 10, 15, 20 | 5, 10, 15, 20, 40 |  | 50 | 0 |
| 5, 10, 15, 20 | 5, 10, 15, 20, 25, 30, 40 |  | 60 | 1 |
|  | 5, 10, 15, 20, 25, 30, 40 | 5, 10, 15, 20 |
| DC\_66A-66A\_n66A | DC\_66A\_n66A2 | See CA\_66A-66A Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-3 | 5, 10, 15, 20, 40 |  | 70 | 0 |
| See CA\_66A-66A Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-3 | 5, 10, 15, 20, 25, 30, 40 |  | 80 | 1 |
|  | 5, 10, 15, 20, 25, 30, 40 | See CA\_66A-66A Bandwidth Combination Set 0 in TS 36.101 Table 5.6A.1-3 |
| DC\_71A\_n71A | DC\_71A\_n71A2 | 15 | 5 |  | 20 | 0 |
|  |  | 10 | 5, 10 |  |  |  |
|  |  | 5 | 5, 10, 15 |  |  |  |
|  |  |  | 5 | 15 |  |  |
|  |  |  | 5, 10 | 10 |  |  |
|  |  |  | 5, 10, 15 | 5 |  |  |
|  |  | 5, 10, 15, 20 | 5, 10, 15, 20 |  | 30 | 1 |
|  |  |  | 5, 10, 15, 20 | 5, 10, 15, 20 |
| NOTE 1: Void.NOTE 2: Only single switched UL is supported.NOTE 3: Requirements in this specification apply for NR SCS of 15 kHz only.NOTE 4: The minimum requirements only apply for non-simultaneous Tx/Rx between all carriers. |

---Text omitted---

Table 5.5B.4.1-1: Inter-band EN-DC configurations within FR1 (two bands)

| **EN-DC****configuration** | **Uplink EN-DC****configuration****(NOTE 1)** | **Single UL allowed** | **DL interruption allowed****(Note 14)** |
| --- | --- | --- | --- |
| DC\_1A\_n3ADC\_1C\_n3A | DC\_1A\_n3ADC\_1C\_n3A | DC\_1\_n3 |  |
| DC\_1A\_n5A | DC\_1A\_n5A | No |  |
| DC\_1A\_n7ADC\_1A\_n7B | DC\_1A\_n7ADC\_1A\_n7B | No |  |
| DC\_1A-1A\_n7ADC\_1A-1A\_n7B | DC\_1A\_n7A | No |  |
| DC\_1A\_n8A | DC\_1A\_n8A | No |  |
| DC\_1A\_n20A | DC\_1A\_n20A | No |  |
| DC\_1A\_n28A | DC\_1A\_n28A | No |  |
| DC\_1A\_n26A | DC\_1A\_n26A | No |  |
| DC\_1A-1A\_n28A | DC\_1A\_n28A | No |  |
| DC\_1A\_n38ADC\_1C\_n38A | DC\_1A\_n38A | No |  |
| DC\_1A\_n40ADC\_1A\_n40B | DC\_1A\_n40A | No |  |
| DC\_1A\_n41A7 | DC\_1A\_n41A | No |  |
| DC\_1A\_n50A | DC\_1A\_n50A | No |  |
| DC\_1A\_n51A | DC\_1A\_n51A | No |  |
| DC\_1A\_n71ADC\_1A\_n71B | DC\_1A\_n71A | No |  |
| DC\_1A\_n77A7DC\_1A\_n77C7 | DC\_1A\_n77A | DC\_1\_n77 | No |
| DC\_1A\_n77(2A)7DC\_1A\_n77(3A)7 | DC\_1A\_n77A | DC\_1\_n77 | No |
| DC\_1A\_n78A7DC\_1A\_n78C7 | DC\_1A\_n78A | No | No |
| DC\_1A\_n78(2A)7DC\_1A\_n78(A-C)7 | DC\_1A\_n78A | No | No |
| DC\_1A-1A\_n78A | DC\_1A\_n78A | No | No |
| DC\_1A\_n79A7DC\_1A\_n79C7 | DC\_1A\_n79A | No | No |
| DC\_2A\_n5A | DC\_2A\_n5A | No |  |
| DC\_2A-2A\_n5A | DC\_2A\_n5A | No |  |
| DC\_2A\_n7A | DC\_2A\_n7A | No |  |
| DC\_2A\_n7(2A) | DC\_2A\_n7A | No |  |
| DC\_2A\_n12A | DC\_2A\_n12A | No |  |
| DC\_2A\_n25A11, 13, 20 | N/A | N/A |  |
| DC\_2A\_n28A | DC\_2A\_n28A | No |  |
| DC\_2A\_n30A | DC\_2A\_n30A | No |  |
| DC\_2A-2A\_n30A | DC\_2A\_n30A | No |  |
| DC\_2A\_n38A | DC\_2A\_n38A | No |  |
| DC\_2A-2A\_n38A | DC\_2A\_n38A | No |  |
| DC\_2A\_n41ADC\_2A\_n41CDC\_2C\_n41A | DC\_2A\_n41ADC\_2C\_n41A | No |  |
| DC\_2A\_n41(2A) | DC\_2A\_n41A | No |  |
| DC\_2A-2A\_n41A | DC\_2A\_n41A | No |  |
| DC\_2A\_n46A | DC\_2A\_n46A | No |  |
| DC\_2A\_n48ADC\_2A\_n48B | DC\_2A\_n48A | No |  |
| DC\_2A\_n66A | DC\_2A\_n66A | DC\_2\_n66 |  |
| DC\_2A\_n66(2A) | DC\_2A\_n66A | DC\_2\_n66 |  |
| DC\_2A-2A\_n66A | DC\_2A\_n66A | DC\_2\_n66 |  |
| DC\_2A\_n71ADC\_2A\_n71BDC\_2C\_n71A | DC\_2A\_n71A | No |  |
| DC\_2A-2A\_n71A | DC\_2A\_n71A | No |  |
| DC\_2A\_n77ADC\_2A\_n77C | DC\_2A\_n77A | DC\_2\_n77 |  |
| DC\_2A\_n77(2A) 21 | DC\_2A\_n77A21 | DC\_2\_n77 |  |
| DC\_2A-2A\_n77ADC\_2A-2A\_n77C | DC\_2A\_n77A | DC\_2\_n77 |  |
| DC\_2A-2A\_n77(2A) 21 | DC\_2A\_n77A21 | DC\_2\_n77 |  |
| DC\_2A\_n78A | DC\_2A\_n78A | DC\_2\_n78 |  |
| DC\_2A-2A\_n78(2A) | DC\_2A\_n78A | DC\_2\_n78 |  |
| DC\_2A\_n78(2A) | DC\_2A\_n78A | DC\_2\_n78 |  |
| DC\_2A-2A\_n78A | DC\_2A\_n78A | DC\_2\_n78 |  |
| DC\_3A\_n1ADC\_3C\_n1A | DC\_3A\_n1ADC\_3C\_n1A | DC\_3\_n1 |  |
| DC\_3A-3A\_n1A | DC\_3A\_n1A | DC\_3\_n1 |  |
| DC\_3A\_n5ADC\_3C\_n5A | DC\_3A\_n5A | DC\_3\_n5 |  |
| DC\_3A\_n7ADC\_3A\_n7BDC\_3C\_n7ADC\_3C\_n7B | DC\_3A\_n7ADC\_3A\_n7BDC\_3C\_n7A | No |  |
| DC\_3A-3A\_n7ADC\_3A-3A\_n7B | DC\_3A\_n7A | No |  |
| DC\_3A\_n8A | DC\_3A\_n8A | No |  |
| DC\_3A-3A\_n8A | DC\_3A\_n8A | No |  |
| DC\_3A\_n20ADC\_3C\_n20A | DC\_3A\_n20A | No |  |
| DC\_3A\_n26ADC\_3C\_n26A | DC\_3A\_n26ADC\_3C\_n26A | Yes |  |
| DC\_3A\_n28ADC\_3C\_n28A | DC\_3A\_n28ADC\_3C\_n28A | No |  |
| DC\_3A\_n34A | DC\_3A\_n34A | No |  |
| DC\_3A\_n38ADC\_3C\_n38A | DC\_3A\_n38A | No |  |
| DC\_3A\_n40ADC\_3A\_n40B | DC\_3A\_n40A | No |  |
| DC\_3A\_n41A7DC\_3C\_n41A | DC\_3A\_n41ADC\_3C\_n41A | DC\_3\_n41 | No |
| DC\_3A\_n50A | DC\_3A\_n50A | No |  |
| DC\_3A\_n51A | DC\_3A\_n51A | No |  |
| DC\_3A\_n71ADC\_3A\_n71B | DC\_3A\_n71A | No |  |
| DC\_3A\_n77A7DC\_3A\_n77C7DC\_3C\_n77A7 | DC\_3A\_n77ADC\_3C\_n77A | DC\_3\_n77 | No |
| DC\_3A\_n77(2A)7DC\_3A\_n77(3A)7DC\_3C\_n77(2A)7 | DC\_3A\_n77ADC\_3C\_n77A | DC\_3\_n77 | No |
| DC\_3A-3A\_n77A7 | DC\_3A\_n77A | DC\_3\_n77 | No |
| DC\_3A\_n78A7DC\_3A\_n78C7DC\_3C\_n78A7 | DC\_3A\_n78ADC\_3C\_n78A | DC\_3\_n78 | No |
| DC\_3A\_n78(2A)7DC\_3A\_n78(A-C)7DC\_3C\_n78(2A)7 | DC\_3A\_n78ADC\_3C\_n78A | DC\_3\_n78 | No |
| DC\_3A-3A\_n78A7, 21 | DC\_3A\_n78A21 | DC\_3\_n78 | No |
| DC\_3A\_n79A7DC\_3A\_n79C7DC\_3C\_n79A7 | DC\_3A\_n79ADC\_3C\_n79A | No | No |
| DC\_4A\_n2A | DC\_4A\_n2A | No |  |
| DC\_4A\_n5A | DC\_4A\_n5A | DC\_4\_n5 |  |
| DC\_4A\_n7A | DC\_4A\_n7A | No |  |
| DC\_4A\_n28A | DC\_4A\_n28A | No |  |
| DC\_4A\_n38A | DC\_4A\_n38A | No |  |
| DC\_4A\_n41A | DC\_4A\_n41A | No |  |
| DC\_4A\_n78A | DC\_4A\_n78A | No |  |
| DC\_4A\_n78(2A) | DC\_4A\_n78A | No |  |
| DC\_5A\_n1A | DC\_5A\_n1A | No |  |
| DC\_5A\_n2ADC\_5B\_n2A | DC\_5A\_n2A | No |  |
| DC\_5A-5A\_n2A | DC\_5A\_n2A | No |  |
| DC\_5A\_n3A | DC\_5A\_n3A | DC\_5\_n3 |  |
| DC\_5A\_n7A | DC\_5A\_n7A | DC\_5\_n7 |  |
| DC\_5A\_n7(2A) | DC\_5A\_n7A | DC\_5\_n7 |  |
| DC\_5A\_n12A | DC\_5A\_n12A | No |  |
| DC\_5A\_n30A | DC\_5A\_n30A | No |  |
| DC\_5A\_n38A | DC\_5A\_n38A | DC\_5\_n38 |  |
| DC\_5A\_n40A | DC\_5A\_n40A | No |  |
| DC\_5A\_n48ADC\_5A\_n48B | DC\_5A\_n48A | No |  |
| DC\_5A\_n66ADC\_5B\_n66A | DC\_5A\_n66A | DC\_5\_n66 |  |
| DC\_5A-5A\_n66A | DC\_5A\_n66A | DC\_5\_n66 |  |
| DC\_5A\_n77ADC\_5A\_n77C | DC\_5A\_n77A | No |  |
| DC\_5A\_n77(2A) 21DC\_5A\_n77(3A) | DC\_5A\_n77A21 | No |  |
| DC\_5A\_n71A | DC\_5A\_n71A | No |  |
| DC\_5A\_n78A7DC\_5A\_n78C7 | DC\_5A\_n78A | No | No |
| DC\_5A\_n78(2A)7DC\_5A\_n78(A-C)7 | DC\_5A\_n78A | No | No |
| DC\_5A\_n79A | DC\_5A\_n79A | No | No |
| DC\_7A\_n1ADC\_7C\_n1A | DC\_7A\_n1ADC\_7C\_n1A | No |  |
| DC\_7A-7A\_n1A | DC\_7A\_n1A | No |  |
| DC\_7A\_n2ADC\_7C\_n2A | DC\_7A\_n2A | No |  |
| DC\_7A\_n3ADC\_7C\_n3A | DC\_7A\_n3ADC\_7C\_n3A | No |  |
| DC\_7A\_n5ADC\_7C\_n5A | DC\_7A\_n5ADC\_7C\_n5A | DC\_7\_n5 |  |
| DC\_7A-7A\_n5A | DC\_7A\_n5A | DC\_7\_n5 |  |
| DC\_7A\_n8A | DC\_7A\_n8A | No |  |
| DC\_7A-7A\_n8A | DC\_7A\_n8A | No |  |
| DC\_7A-7A\_n78(2A)7 | DC\_7A\_n78A | No |  |
| DC\_7A\_n20A | DC\_7A\_n20A | No |  |
| DC\_7A\_n25ADC\_7C\_n25A | DC\_7A\_n25A | No |  |
| DC\_7A\_n26ADC\_7C\_n26A | DC\_7A\_n26ADC\_7C\_n26A | Yes |  |
| DC\_7A-7A\_n25A | DC\_7A\_n25A | No |  |
| DC\_7A\_n28ADC\_7C\_n28A | DC\_7A\_n28ADC\_7C\_n28A | No |  |
| DC\_7A\_n40A | DC\_7A\_n40A | Yes |  |
| DC\_7A-7A\_n28A | DC\_7A\_n28A | No |  |
| DC\_7A\_n51A | DC\_7A\_n51A | No |  |
| DC\_7A\_n66ADC\_7C\_n66A | DC\_7A\_n66A | No |  |
| DC\_7A-7A\_n66A | DC\_7A\_n66A | No |  |
| DC\_7A\_n71A | DC\_7A\_n71A | No |  |
| DC\_7A\_n77A7DC\_7C\_n77A | DC\_7A\_n77A | No |  |
| DC\_7A\_n77(2A)DC\_7A\_n77(3A)DC\_7C\_n77(2A) | DC\_7A\_n77A | No |  |
| DC\_7A-7A\_n77A7 | DC\_7A\_n77A | No |  |
| DC\_7A-7A\_n77(2A)DC\_7A-7A\_n77(3A) | DC\_7A\_n77A | No |  |
| DC\_7A\_n78A7DC\_7C\_n78A7DC\_7A\_n78C7 | DC\_7A\_n78ADC\_7C\_n78A | No |  |
| DC\_7A\_n78(2A)7DC\_7A\_n78(A-C)7DC\_7C\_n78(2A)7 | DC\_7A\_n78ADC\_7C\_n78A | No |  |
| DC\_7A-7A\_n78A7, 21DC\_7A-7A\_n78C7 | DC\_7A\_n78A21 | No |  |
| DC\_7A-7A\_n78(A-C)7 | DC\_7A\_n78A | No |  |
| DC\_7A\_n79ADC\_7A\_n79C | DC\_7A\_n79A | No |  |
| DC\_8A\_n1A | DC\_8A\_n1A | No |  |
| DC\_8A\_n2A | DC\_8A\_n2A | DC\_8\_n2 |  |
| DC\_8A\_n3A | DC\_8A\_n3A | No |  |
| DC\_8A\_n7A | DC\_8A\_n7A | No |  |
| DC\_8A\_n20A | DC\_8A\_n20A | Yes |  |
| DC\_8A\_n28A | DC\_8A\_n28A | No |  |
| DC\_8A\_n34A | DC\_8A\_n34A | No |  |
| DC\_8A\_n38A | DC\_8A\_n38A | No |  |
| DC\_8A\_n39A | DC\_8A\_n39A | No |  |
| DC\_8A\_n40A7 | DC\_8A\_n40A | No |  |
| DC\_8A\_n41A7DC\_8A\_n41C | DC\_8A\_n41A | No | No |
| DC\_8A\_n41(2A) | DC\_8A\_n41A | No | No |
| DC\_8A\_n77A7 | DC\_8A\_n77A | No | No |
| DC\_8A\_n77(2A)7DC\_8A\_n77(3A)7 | DC\_8A\_n77A | No | No |
| DC\_8A\_n78A7DC\_8B\_n78A7 | DC\_8A\_n78A | No | No |
| DC\_8A\_n78(2A)7 | DC\_8A\_n78A | No | No |
| DC\_8A\_n79A7DC\_8A\_n79C | DC\_8A\_n79ADC\_8A\_n79C | No | No |
| DC\_8A\_n93A | DC\_8A\_n93A\_ULSUP-TDM | N/A |  |
| DC\_8A\_n94A | DC\_8A\_n94A\_ULSUP-TDM | N/A |  |
| DC\_11A\_n1A | DC\_11A\_n1A | No |  |
| DC\_11A\_n3A | DC\_11A\_n3A | No |  |
| DC\_11A\_n28A | DC\_11A\_n28A | No |  |
| DC\_11A\_n41A7 | DC\_11A\_n41A | No |  |
| DC\_11A\_n77A7 | DC\_11A\_n77A | No | No |
| DC\_11A\_n77(2A)7DC\_11A\_n77(3A)7 | DC\_11A\_n77A | No | No |
| DC\_11A\_n78A7 | DC\_11A\_n78A | No | No |
| DC\_11A\_n78(2A) | DC\_11A\_n78A | No | No |
| DC\_11A\_n79A7 | DC\_11A\_n79A | No |  |
| DC\_12A\_n2A | DC\_12A\_n2A | No |  |
| DC\_12A\_n5A | DC\_12A\_n5A | No |  |
| DC\_12A\_n7A | DC\_12A\_n7A | No |  |
| DC\_12A\_n7(2A) | DC\_12A\_n7A | No |  |
| DC\_12A\_n25A | DC\_12A\_n25A | No |  |
| DC\_12A\_n30A | DC\_12A\_n30A | No |  |
| DC\_12A\_n38A | DC\_12A\_n38A | No |  |
| DC\_12A\_n41A | DC\_12A\_n41A | No |  |
| DC\_12A\_n66A | DC\_12A\_n66A | No |  |
| DC\_12A\_n66(2A) | DC\_12A\_n66A | No |  |
| DC\_12A\_n71A | DC\_12A\_n71A18,19 | DC\_12\_n71 |  |
| DC\_12A\_n77A | DC\_12A\_n77A | DC\_12\_n77 |  |
| DC\_12A\_n77(2A) 21 | DC\_12A\_n77A21 | DC\_12\_n77 |  |
| DC\_12A\_n78A | DC\_12A\_n78A | DC\_12\_n78 |  |
| DC\_12A\_n78(2A) | DC\_12A\_n78A | DC\_12\_n78 |  |
| DC\_13A\_n2A | DC\_13A\_n2A | No |  |
| DC\_13A\_n5A | DC\_13A\_n5A | DC\_13\_n5 |  |
| DC\_13A\_n7A | DC\_13A\_n7A | No |  |
| DC\_13A\_n7(2A) | DC\_13A\_n7A | No |  |
| DC\_13A\_n25A | DC\_13A\_n25A | No |  |
| DC\_13A\_n48ADC\_13A\_n48B | DC\_13A\_n48A | No |  |
| DC\_13A\_n66A | DC\_13A\_n66A | No |  |
| DC\_13A\_n71A | DC\_13A\_n71A | No |  |
| DC\_13A\_n77ADC\_13A\_n77C | DC\_13A\_n77A | No |  |
| DC\_13A\_n78A | DC\_13A\_n78A | No |  |
| DC\_13A\_n78(2A) | DC\_13A\_n78A | No |  |
| DC\_14A\_n2A | DC\_14A\_n2A | No |  |
| DC\_14A\_n5A | DC\_14A\_n5A | DC\_14\_n5 |  |
| DC\_14A\_n30A | DC\_14A\_n30A | No |  |
| DC\_14A\_n66A | DC\_14A\_n66A | No |  |
| DC\_14A\_n77A | DC\_14A\_n77A | No |  |
| DC\_14A\_n77(2A) 21 | DC\_14A\_n77A21 | No |  |
| DC\_18A\_n3A | DC\_18A\_n3A | No |  |
| DC\_18A\_n28A | DC\_18A\_n28A | No |  |
| DC\_18A\_n41A16 | DC\_18A\_n41A | No |  |
| DC\_18A\_n77A7DC\_18A\_n77(2A)7 | DC\_18A\_n77A | No | No |
| DC\_18A\_n78A7 | DC\_18A\_n78A | No | No |
| DC\_18A\_n78(2A)7 | DC\_18A\_n78A | No | No |
| DC\_20A\_n91A | DC\_20A\_n91A\_ULSUP-TDM | N/A |  |
| DC\_20A\_n92A | DC\_20A\_n92A\_ULSUP-TDM | N/A |  |
| DC\_18A\_n79A7 | DC\_18A\_n79A | No |  |
| DC\_19A\_n1A | DC\_19A\_n1A | No |  |
| DC\_19A\_n77A7DC\_19A\_n77C7 | DC\_19A\_n77A | No |  |
| DC\_19A\_n77(2A)7 | DC\_19A\_n77A | No |  |
| DC\_19A\_n78A7DC\_19A\_n78C7 | DC\_19A\_n78A | No | No |
| DC\_19A\_n78(2A)7 | DC\_19A\_n78A | No | No |
| DC\_19A\_n79A7DC\_19A\_n79C7 | DC\_19A\_n79A | No | No |
| DC\_20A\_n1A | DC\_20A\_n1A | No |  |
| DC\_20A\_n3A | DC\_20A\_n3A | No |  |
| DC\_20A\_n7A | DC\_20A\_n7A | DC\_20\_n7 |  |
| DC\_20A\_n8A | DC\_20A\_n8A | DC\_20\_n8 |  |
| DC\_20A\_n28A8,11,13 | DC\_20A\_n28A | No |  |
| DC\_20A\_n38A | DC\_20A\_n38A | No |  |
| DC\_20A\_n41A | DC\_20A\_n41A | DC\_20\_n41 |  |
| DC\_20A\_n50A | DC\_20A\_n50A | No |  |
| DC\_20A\_n51A | DC\_20A\_n51A | No |  |
| DC\_20A\_n77A7 | DC\_20A\_n77A | No |  |
| DC\_20A\_n78A7DC\_20A\_n78C7 | DC\_20A\_n78A | No |  |
| DC\_20A\_n78(2A)7 | DC\_20A\_n78A | No |  |
| DC\_21A\_n1A | DC\_21A\_n1A | No |  |
| DC\_21A\_n28A17 | DC\_21A\_n28A | DC\_21\_n28 |  |
| DC\_21A\_n77A7DC\_21A\_n77C7 | DC\_21A\_n77A | No |  |
| DC\_21A\_n77(2A)7 | DC\_21A\_n77A | No |  |
| DC\_21A\_n78A7DC\_21A\_n78C7 | DC\_21A\_n78A | No | No |
| DC\_21A\_n78(2A)7 | DC\_21A\_n78A | No | No |
| DC\_21A\_n79A7DC\_21A\_n79C7 | DC\_21A\_n79A | No | No |
| DC\_25A\_n41A | DC\_25A\_n41A | No |  |
| DC\_25A-25A\_n41A | DC\_25A\_n41A | No |  |
| DC\_25A\_n77A | DC\_25A\_n77A | DC\_25\_n77 |  |
| DC\_25A-25A\_n77A | DC\_25A\_n77A | DC\_25\_n77 |  |
| DC\_25A\_n78A | DC\_25A\_n78A | DC\_25\_n78 |  |
| DC\_25A-25A\_n78A | DC\_25A\_n78A | DC\_25\_n78 |  |
| DC\_26A\_n25A | DC\_26A\_n25A | No |  |
| DC\_26A\_n41A | DC\_26A\_n41A | No |  |
| DC\_26A\_n77A7 | DC\_26A\_n77A | No |  |
| DC\_26A\_n78A7 | DC\_26A\_n78A | No |  |
| DC\_26A\_n79A7 | DC\_26A\_n79A | No |  |
| DC\_28A\_n1A | DC\_28A\_n1A | No |  |
| DC\_28A\_n2A | DC\_28A\_n2A | No |  |
| DC\_28A\_n3A | DC\_28A\_n3A | No |  |
| DC\_28A\_n5A | DC\_28A\_n5A | No |  |
| DC\_28A\_n7ADC\_28A\_n7B | DC\_28A\_n7ADC\_28A\_n7B | No |  |
| DC\_28A\_n51A | DC\_28A\_n51A | No |  |
| DC\_28A\_n8A | DC\_28A\_n8A | No |  |
| DC\_28A\_n20A8,11,13 | DC\_28A\_n20A | No |  |
| DC\_28A\_n38A | DC\_28A\_n38A | No |  |
| DC\_28A\_n40A | DC\_28A\_n40A | No |  |
| DC\_28A\_n41A7 | DC\_28A\_n41A | No |  |
| DC\_28A\_n50A | DC\_28A\_n50A | No |  |
| DC\_28A\_n66A | DC\_28A\_n66A | No |  |
| DC\_28A\_n77A7DC\_28A\_n77C7 | DC\_28A\_n77A | No | No |
| DC\_28A\_n77(2A)7 | DC\_28A\_n77A | No | No |
| DC\_28A\_n78A7DC\_28A\_n78C7 | DC\_28A\_n78A | No | No |
| DC\_28A\_n78(2A)7 | DC\_28A\_n78A | No | No |
| DC\_28A\_n79A7DC\_28A\_n79C7 | DC\_28A\_n79A | No |  |
| DC\_30A\_n2A | DC\_30A\_n2A | No |  |
| DC\_30A\_n5A | DC\_30A\_n5A | No |  |
| DC\_30A\_n66A | DC\_30A\_n66A | No |  |
| DC\_30A\_n77A | DC\_30A\_n77A | No |  |
| DC\_30A\_n77(2A) 21 | DC\_30A\_n77A21 | No |  |
| DC\_38A\_n1A | DC\_38A\_n1A | No |  |
| DC\_38A\_n3A | DC\_38A\_n3A | No |  |
| DC\_38A\_n8A | DC\_38A\_n8A | No |  |
| DC\_38A\_n28A | DC\_38A\_n28A | No |  |
| DC\_38A\_n78A7 | DC\_38A\_n78A | No |  |
| DC\_38A\_n79ADC\_38A\_n79C | DC\_38A\_n79A | No |  |
| DC\_39A\_n40A3 | DC\_39A\_n40A | No |  |
| DC\_39A\_n41A3DC\_39C\_n41A3DC\_39A\_n41C3 | DC\_39A\_n41ADC\_39C\_n41A | No | No |
| DC\_39A\_n78A5,7 | DC\_39A\_n78A | No |  |
| DC\_39A\_n79A7DC\_39A\_n79C7 | DC\_39A\_n79A | No | No |
| DC\_40A\_n1ADC\_40C\_n1A | DC\_40A\_n1A | No |  |
| DC\_40A\_n41A3DC\_40A\_n41C3DC\_40C\_n41A3 | DC\_40A\_n41A | No |  |
| DC\_40A\_n41(2A)3 | DC\_40A\_n41A | No |  |
| DC\_40A\_n77ADC\_40A\_n77C | DC\_40A\_n77A | No |  |
| DC\_40A\_n78ADC\_40C\_n78A | DC\_40A\_n78ADC\_40C\_n78A | No |  |
| DC\_40A\_n78(2A)DC\_40C\_n78(2A) | DC\_40A\_n78ADC\_40C\_n78A | No |  |
| DC\_40A\_n79A7,12DC\_40A\_n79C7,12DC\_40C\_n79A7,12 | DC\_40A\_n79A | No | No |
| DC\_41A\_n1ADC\_41C\_n1A | DC\_41A\_n1ADC\_41C\_n1A | No | DC\_41A\_n1ADC\_41C\_n1A |
| DC\_41A\_n3A7DC\_41C\_n3A7 | DC\_41A\_n3ADC\_41C\_n3A | No |  |
| DC\_41A\_n28A7DC\_41C\_n28A7 | DC\_41A\_n28ADC\_41C\_n28A | No |  |
| DC\_41A\_n77ADC\_41C\_n77A | DC\_41A\_n77ADC\_41C\_n77A | No |  |
| DC\_41A\_n77(2A)DC\_41C\_n77(2A) | DC\_41A\_n77ADC\_41C\_n77A | No |  |
| DC\_41A\_n78ADC\_41C\_n78ADC\_41D\_n78A | DC\_41A\_n78ADC\_41C\_n78A | No |  |
| DC\_41A\_n78(2A)DC\_41C\_n78(2A) | DC\_41A\_n78ADC\_41C\_n78A | No |  |
| DC\_41A\_n79A6,7DC\_41A\_n79C6,7DC\_41C\_n79A6,7 | DC\_41A\_n79ADC\_41C\_n79A | No | No |
| DC\_42A\_n1A7DC\_42C\_n1A7 | DC\_42A\_n1ADC\_42C\_n1A | No |  |
| DC\_42A\_n3A**7**DC\_42C\_n3A7 | DC\_42A\_n3ADC\_42C\_n3A | DC\_42\_n3 |  |
| DC\_42A\_n28A7DC\_42C\_n28A7 | DC\_42A\_n28ADC\_42C\_n28A | No |  |
| DC\_42A\_n51A | DC\_42A\_n51A | No |  |
| DC\_42A\_n77A3,4,9,11DC\_42A\_n77C3,4,9,11DC\_42C\_n77A3,4,9,11DC\_42C\_n77C3,4,9,11DC\_42D\_n77A3,4,9,11DC\_42D\_n77CDC\_42E\_n77A3,4,9,11DC\_42E\_n77C | N/A | N/A |  |
| DC\_42A\_n77(2A)3,4,9,11DC\_42C\_n77(2A)3,4,9,11 | N/A | N/A |  |
| DC\_42A\_n78A3,4,9,11DC\_42A\_n78C3,4,9,11DC\_42C\_n78A3,4,9,11DC\_42C\_n78C3,4,9,11DC\_42D\_n78A3,4,9,11DC\_42D\_n78C3,4,9,11DC\_42E\_n78A3,4,9,11DC\_42E\_n78C3,4,9,11 | N/A | N/A |  |
| DC\_42A\_n79A9,15DC\_42A\_n79C9,15DC\_42C\_n79A9,15DC\_42C\_n79C9,15DC\_42D\_n79A9,15DC\_42D\_n79C9,15DC\_42E\_n79A9,15DC\_42E\_n79C9,15 | N/A | N/A |  |
| DC\_46A\_n77A2 | N/A | N/A |  |
| DC\_46A\_n78A2DC\_46C\_n78A2DC\_46D\_n78A2DC\_46E\_n78A2 | N/A | N/A |  |
| DC\_48A\_n2ADC\_48C\_n2ADC\_48D\_n2ADC\_48E\_n2A | DC\_48A\_n2A | No |  |
| DC\_48A\_n5ADC\_48C\_n5ADC\_48D\_n5ADC\_48E\_n5A | DC\_48A\_n5A | No |  |
| DC\_48A\_n12A | DC\_48A\_n12A | No |  |
| DC\_48A\_n25ADC\_48C\_n25ADC\_48D\_n25A | DC\_48A\_n25A | No |  |
| DC\_48A\_n46ADC\_48B\_n46ADC\_48C\_n46ADC\_48D\_n46ADC\_48E\_n46ADC\_48A\_n46BDC\_48B\_n46BDC\_48C\_n46BDC\_48D\_n46BDC\_48E\_n46BDC\_48A\_n46CDC\_48B\_n46CDC\_48C\_n46CDC\_48D\_n46CDC\_48E\_n46CDC\_48A\_n46DDC\_48B\_n46DDC\_48C\_n46DDC\_48D\_n46DDC\_48E\_n46DDC\_48A\_n46EDC\_48B\_n46EDC\_48C\_n46EDC\_48D\_n46EDC\_48E\_n46E | DC\_48A\_n46ADC\_48B\_n46A | No |  |
| DC\_48A\_n66ADC\_48C\_n66ADC\_48D\_n66ADC\_48E\_n66A | DC\_48A\_n66A | No |  |
| DC\_48A\_n71ADC\_48B\_n71ADC\_48C\_n71ADC\_48D\_n71A | DC\_48A\_n71A | No |  |
| DC\_48A-48A\_n71ADC\_48A-48A-48A\_n71A | DC\_48A\_n71A | No |  |
| DC\_48A\_n77A3. 4. 9, 11DC\_48C\_n77A3. 4. 9, 11DC\_48A\_n77C3. 4. 9, 11DC\_48C\_n77C3. 4. 9, 11DC\_48D\_n77A3. 4. 9, 11DC\_48D\_n77C3. 4. 9, 11DC\_48E\_n77A3. 4. 9, 11 | N/A | N/A |  |
| DC\_48A-48A\_n77A | N/A | N/A |  |
| DC\_48A-48A-48A\_n77A | N/A | N/A |  |
| DC\_66A\_n2ADC\_66B\_n2ADC\_66C\_n2A | DC\_66A\_n2A | DC\_66\_n2 |  |
| DC\_66A-66A\_n2A | DC\_66A\_n2A | DC\_66\_n2 |  |
| DC\_66A-66A-66A\_n2A | DC\_66A\_n2A | DC\_66\_n2 |  |
| DC\_66A\_n5ADC\_66B\_n5ADC\_66C\_n5A | DC\_66A\_n5A | DC\_66\_n5 |  |
| DC\_66A-66A\_n5A | DC\_66A\_n5A | DC\_66\_n5 |  |
| DC\_66A-66A-66A\_n5A | DC\_66A\_n5A | DC\_66\_n5 |  |
| DC\_66A\_n7A | DC\_66A\_n7A | No |  |
| DC\_66A\_n7(2A) | DC\_66A\_n7A | No |  |
| DC\_66A-66A\_n7A | DC\_66A\_n7A | No |  |
| DC\_66A-66A\_n7(2A) | DC\_66A\_n7A | No |  |
| DC\_66A\_n12A | DC\_66A\_n12A | No |  |
| DC\_66A\_n25A | DC\_66A\_n25A | DC\_66\_n25 |  |
| DC\_66A\_n28A | DC\_66A\_n28A | No |  |
| DC\_66A\_n30A | DC\_66A\_n30A | No |  |
| DC\_66A-66A\_n30A | DC\_66A\_n30A | No |  |
| DC\_66A\_n38A | DC\_66A\_n38A | No |  |
| DC\_66A-66A\_n38A | DC\_66A\_n38A | No |  |
| DC\_66A\_n41ADC\_66A\_n41C | DC\_66A\_n41A | No |  |
| DC\_66A\_n41(2A) | DC\_66A\_n41A | No |  |
| DC\_66A\_n46A | DC\_66A\_n46A | No |  |
| DC\_66A\_n48ADC\_66A\_n48B | DC\_66A\_n48A | No |  |
| DC\_66A-66A\_n48ADC\_66A-66A\_n48B | DC\_66A\_n48A | No |  |
| DC\_66A\_n71ADC\_66C\_n71ADC\_66A\_n71B | DC\_66A\_n71A | No |  |
| DC\_66A-66A\_n71A | DC\_66A\_n71A | No |  |
| DC\_66A\_n77ADC\_66A\_n77C | DC\_66A\_n77A | DC\_66\_n77 |  |
| DC\_66A\_n77(2A) 21 | DC\_66A\_n77A21 | DC\_66\_n77 |  |
| DC\_66A-66A\_n77ADC\_66A-66A\_n77C | DC\_66A\_n77A | DC\_66\_n77 |  |
| DC\_66A-66A\_n77(2A) 21 | DC\_66A\_n77A21 | DC\_66\_n77 |  |
| DC\_66A-66A-66A\_n77ADC\_66A-66A-66A\_n77C | DC\_66A\_n77A | DC\_66\_n77 |  |
| DC\_66A-66A-66A\_n77(2A) | DC\_66A\_n77A | DC\_66\_n77 |  |
| DC\_66A\_n78A | DC\_66A\_n78A | No |  |
| DC\_66A\_n78(2A) | DC\_66A\_n78A | No |  |
| DC\_66A-66A\_n78A | DC\_66A\_n78A | No |  |
| DC\_66A-66A\_n78(2A) | DC\_66A\_n78A | No |  |
| DC\_71A\_n2A | DC\_71A\_n2A | No |  |
| DC\_71A\_n5A | DC\_71A\_n5A | No |  |
| DC\_71A\_n38A | DC\_71A\_n38A | No |  |
| DC\_71A\_n41A | DC\_71A\_n41A | No |  |
| DC\_71A\_n48A | DC\_71A\_n48A | No |  |
| DC\_71A\_n66A | DC\_71A\_n66A | No |  |
| DC\_71A\_n77ADC\_71A\_n77C | DC\_71A\_n77A | No |  |
| DC\_71A\_n78A | DC\_71A\_n78A | No |  |
| DC\_71A\_n78(2A) | DC\_71A\_n78A | No |  |
| NOTE 1: Uplink EN-DC configurations are the configurations supported by the present release of specifications.NOTE 2: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell.NOTE 3: The minimum requirements apply only when there is non-simultaneous Tx/Rx operation between E-UTRA and NR carriers. This restriction applies also for these carriers when applicable EN-DC configuration is part of a higher order EN-DC configuration.NOTE 4: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for intra-band non-contiguous EN-DC apply for the Band 42/48 and Band n77/n78 combination. For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, when UE capability *interBandContiguousMRDC* is indicated, the minimum requirements for intra-band-contiguous EN-DC also should be met in addtion to intra-band non-contiguous EN-DC*.* The intra-band requirements also apply for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 5: The frequency range above 3600 MHz for Band n78 is not used in this combination.NOTE 6: The frequency range below 2506 MHz for Band 41 is not used in this combination.NOTE 7: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability.NOTE 8: The frequency range in band n28 / 28 is restricted for this band combination to 703 - 733 MHz for the UL and 758-788 MHz for the DL. This restriction also apply for any band combinations when DC\_20\_n28/ DC\_28\_n20/ CA\_20-28/ CA\_n20-n28 is a subset of a higher order band combination.NOTE 9: The combination is not used alone as fall back mode of other band combinations in which UL in Band 42 or Band 48 is not used.NOTE 10: Void.NOTE 11: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for apply when the maximum power spectral density imbalance between downlink carriers is within 6 dB. For UEs indicating interBandMRDC-WithOverlapDL-Bands-r16, the power imbalance requirement defined in clause 7.6B.2.6 apply. For these UEs, the power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 12: Applicable for frequency range above 4800 MHz for Band n79 in this combination.NOTE 13: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements apply for synchronized DL carriers with a maximum receive time difference ≤ 3 usec. The requirements also apply for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 14: Applicable when dynamic switching between two uplink carriers is conducted. The DL interruption requirements for NR DL carrier(s) and E-UTRA DL carrier(s) are specified in clause 8.2.1.2.14 of 38.133 [15] and clause 7.32.2.12 of 36.133 [16] respectively.NOTE 15: Simultaneous Rx/Tx capability does not apply for UEs supporting band 42 with a n77 implementation only. Same restrictions are applied to related higher order configurations.NOTE 16: The frequency range in band n41 is restricted for this band combination to 2595 – 2645 MHz.NOTE 17: The frequency range in band n28 is restricted for this band combination to 728 - 738 MHz for the UL and 783 - 793 MHz for the DL. This restriction applies also for these band combinations when applicable EN-DC configuration is part of a higher order EN-DC configuration.NOTE 18: Only single switched UL is supported.NOTE 19: The implementation with 4 antennas is targeted for FWA form factor for this band combination.NOTE 20: The combination is not used alone as fallback mode of other band combinations in which UL in Band 2 is not used.NOTE 21: PC3 or PC2 Uplink EN-DC configuration is applicable to EN-DC configurations. |

---Text omitted---

Table 7.3B.2.3.5.1-1: MSD test points for PCell due to dual uplink operation for PC3 EN-DC in NR FR1 (two bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DCConfiguration | EUTRA or NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL LCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_1\_n3 | 1 | 1950 | 5 | 25 | 2140 | 23 | IMD3 |
|  | n3 | 1760 | 5 | 25 | 1855 | N/A | N/A |
| DC\_1C\_n3 | 1C | 19501970 | 2020 | 1 (RBstart=0)1 (RBstart=67) | 21402160 | N/A | N/A |
|  | n3 | N/A | 5 | N/A | 1877.5 | 36 | IMD5 |
| DC\_1A\_n8A | 1 | 1965 | 5 | 25 | 2155 | 6.0 | IMD4 |
|  | n8 | 887.5 | 5 | 25 | 932.5 | N/A | N/A |
| DC\_1A\_n71ADC\_1A\_n71B | 1 | 1958 | 5 | 25 | 2148 | N/A | N/A |
|  | n71 | 668 | 5 | 25 | 622 | 15.1 | IMD3 |
| DC\_1A\_n77A,DC\_1A\_SUL\_n77A-n84A,DC\_1A\_n77(2A), | 1 | 1950 | 5 | 25 | 2140 | 29.8 | IMD23 |
|  |  |  |  |  |  |  |  |
|  | n77 | 4090 | 10 | 50 | 4090 | N/A | N/A |
| DC\_1A\_n77A,DC\_1A\_SUL\_n77A-n84A,DC\_1A\_n77(2A),DC\_1A\_n77(3A),DC\_1A\_n78A,DC\_1A\_SUL\_n78A-n84A,DC\_1A\_n78(2A)DC\_1A\_n78(A-C) | 1 | 1950 | 5 | 25 | 2140 | 8.0 | IMD43 |
|  |  |  |  |  |  |  |  |
|  | n77, n78 | 3710 | 10 | 50 | 3710 | N/A | N/A |
| DC\_2A\_n46A | 2 | 1880 | 5 | 25 | 1960 | 12.0 | IMD3 |
|  | n46 | 5720 | 20 | 100 | 5720 | N/A | N/A |
| DC\_2A\_n48A | 2 | 1852.5 | 5 | 25 | 1932.5 | 12 | IMD4 |
|  | n48 | 3625 | 20 | 100 | 3625 | N/A | N/A |
| DC\_2A\_n66A, DC\_2A-2A\_n66ADC\_2A\_n66(2A) | 2 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
|  | n66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| DC\_2A\_n66A, DC\_2A-2A\_n66ADC\_2A\_n66(2A) | 2 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
| DC\_2A\_n77ADC\_2A\_n77(2A)DC\_2A-2A\_n77ADC\_2A\_n77(2A)DC\_2A-2A\_n77(2A) | 2 | 1855 | 5 | 25 | 1935 | 26 | IMD2 |
|  |  |  |  |  |  |  |  |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | N/A |
|  | 2 | 1900 | 5 | 25 | 1980 | 8.0 | IMD4 |
|  |  |  |  |  |  |  |  |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | N/A |
|  | 2 | 1885 | 5 | 25 | 1965 | 5 | IMD5 |
|  |  |  |  |  |  |  |  |
|  | n77 | 3810 | 10 | 50 | 3810 | N/A | N/A |
| DC\_2A\_n78ADC\_2A\_n78(2A)DC\_2A-2A\_n78(2A) | 2 | 1855 | 5 | 25 | 1935 | 26 | IMD23 |
|  |  |  |  |  |  |  |  |
|  | n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |
|  | 2 | 1885 | 5 | 25 | 1965 | 8.0 | IMD43 |
|  |  |  |  |  |  |  |  |
|  | n78 | 3690 | 10 | 50 | 3690 | N/A | N/A |
| DC\_3\_n1 | 3 | 1760 | 5 | 25 | 1855 | N/A | N/A |
|  | n1 | 1950 | 5 | 25 | 2140 | 23 | IMD3 |
| DC\_3\_n5 | 3 | 1771 | 10 | 50 | 1866 | 4 | IMD4 |
|  | n5 | 838 | 5 | 25 | 883 | N/A | N/A |
|  | 3 | 1721 | 10 | 50 | 1816 | N/A | N/A |
|  | n5 | 838 | 5 | 25 | 883 | 24 | IMD23 |
| DC\_3A\_n7ADC\_3C\_n7A | 3 | 1730 | 5 | 25 | 1825 | N/A | N/A |
|  | n7 | 2535 | 10 | 50 | 2655 | 10.2 | IMD4 |
| DC\_3\_n8 | n8 | 900 | 5 | 25 | 945 | 8 | IMD43 |
|  | 3 | 1755 | 10 | 50 | 1850 | N/A | N/A |
|  | n8 | 897.5 | 5 | 25 | 942.5 | N/A | N/A |
|  | 3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | IMD5 |
| DC\_3A\_n20ADC\_3C\_n20A | 3 | 1775 | 5 | 25 | 1870 | 4 | IMD4 |
|  | n20 | 840 | 5 | 25 | 799 | N/A | N/A |
|  | 3 | 1735 | 5 | 25 | 1830 | N/A | N/A |
|  | n20 | 847 | 5 | 25 | 806 | 9 | IMD4 |
| DC\_3A\_n26A | 3 | 1771 | 10 | 50 | 1866 | 4 | IMD4 |
|  | n26 | 838 | 5 | 25 | 883 | N/A | N/A |
|  | 3 | 1721 | 10 | 50 | 1816 | N/A | N/A |
|  | n26 | 838 | 5 | 25 | 883 | 24 | IMD23 |
| DC\_3C\_n26A | 3 | 1720 | 20 | 1 (RBSTART=0) | 1815 | N/A | N/A |
|  |  | 1739.8 | 20 | 1 (RBSTART=99) | 1834.8 | N/A |  |
|  | n26 | 841.5 | 15 | 25(RBSTART=54) | 886.5 | 18.9 | IMD3 |
| DC\_3C\_n28A | n28 | 715.5 | 25 | 25(RBSTART=108) | 770.5 | 11 | 1st order triple beat α (TX22TX1) i.e. IMD3 |
|  | 3 | 1720 | 20 | 1 (RBSTART=0) | 1815 | N/A | N/A |
| DC\_3C\_n20A | n20 | 840 | 5 | 25 | 799 | N/A | N/A |
|  | 3 | 1735 | 5 | 25 | 1830 | N/A | N/A |
|  | n20 | 847 | 5 | 25 | 806 | 9 | IMD4 |
| DC\_3A\_n38A | 3 | 1712.8 | 5 | 25 | 1807.8 | 8.2 | IMD4 |
|  | n38 | 2616.7 | 10 | 50 | 2616.7 | N/A | N/A |
| DC\_3A\_n41ADC\_3C\_n41ADC\_3A\_SUL\_n41A-n80A, DC\_3C\_SUL\_n41A-n80A | 3 | 1740 | 5 | 25 | 1835 | 8.2 | IMD4 |
|  | n41 | 2657.5 | 10 | 50 | 2657.5 | N/A | N/A |
| DC\_3A\_n77A,DC\_3A\_n77(2A),DC\_3A\_n77(3A),DC\_3A\_SUL\_n77A-n80A,DC\_3A\_n78A,DC\_3A\_SUL\_n78A-n80A,DC\_3A\_n78(2A),DC\_3A\_n78(A-C)DC\_3C\_n78ADC\_3C\_n78(2A) | 3 | 1740 | 5 | 25 | 1835 | 26 | IMD23 |
|  |  |  |  |  |  |  |  |
|  | n77, n78 | 3575 | 10 | 50 | 3575 | N/A | N/A |
| DC\_3A\_n77A,DC\_3A\_n77(2A),DC\_3C\_n77A,DC\_3C\_n77(2A),DC\_3A\_SUL\_n77A-n80A,DC\_3A\_n78A, DC\_3A\_SUL\_n78A-n80A,DC\_3A\_n78(2A),DC\_3C\_n78ADC\_3C\_n78(2A) | 3 | 1765 | 5 | 25 | 1860 | 8.0 | IMD43 |
|  |  |  |  |  |  |  |  |
|  | n77, n78 | 3435 | 10 | 50 | 3435 | N/A | N/A |
| DC\_4A\_n2A | 2 | 1860 | 20 | 502 | 1940 | 5 | IMD3 |
|  | 4 | 1752.5 | 5 | 25 | 2152.5 | N/A | N/A |
|  | 2 | 1868.3 | 5 | 25 | 1948.3 | N/A | N/A |
|  | 4 | 1735 | 5 | 25 | 2135 | 5 | IMD5 |
| DC\_4A\_n5A | n5 | 838 | 5 | 25 | 883 | 30 | IMD23 |
|  | 4 | 1721 | 5 | 25 | 2121 | N/A | N/A |
| DC\_4A\_n7A | 4 | 1730 | 5 | 25 | 2130 | N/A | N/A |
|  | n7 | 2535 | 10 | 50 | 2655 | 15 | IMD4 |
| DC\_5A\_n3A | 5 | 838 | 5 | 25 | 883 | N/A | N/A |
|  | n3 | 1771 | 10 | 50 | 1866 | 4 | IMD4 |
|  | 5 | 838 | 5 | 25 | 883 | 24 | IMD23 |
|  | n3 | 1721 | 10 | 50 | 1816 | N/A | N/A |
| DC\_5\_n7 | n7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
|  | 5 | 834 | 5 | 25 | 879 | 12 | IMD33 |
| DC\_5\_n38 | 5 | 844 | 5 | 25 | 889 | 12 | IMD33 |
|  | n38 | 2577 | 10 | 50 | 2577 | N/A | N/A |
| DC\_5A\_n66A | 5 | 838 | 5 | 25 | 883 | 30 | IMD23 |
|  | n66 | 1721 | 5 | 25 | 2121 | N/A | N/A |
| DC\_5A\_n77A8DC\_5A\_n77(2A)8DC\_5A\_n77(3A)8 | 5 | 844 | 5 | 25 | 889 | 8.3 | IMD4 |
|  | n77 | 3421 | 10 | 50 | 3421 | N/A | N/A |
|  | 5 | 826.5 | 5 | 25 | 871.5 | 5.5 | IMD5 |
|  | n77 | 4177.5 | 10 | 50 | 4177.5 | N/A | N/A |
| DC\_5A\_n78ADC\_5A\_n78(2A)DC\_5A\_n78(A-C)DC\_5A\_n78C | 5 | 844 | 5 | 25 | 889 | 8.3 | IMD4 |
|  | n78 | 3421 | 10 | 50 | 3421 | N/A | N/A |
| DC\_7\_n3 | 7 | 2535 | 10 | 50 | 2655 | 13 | IMD4 |
|  | n3 | 1730 | 5 | 25 | 1825 | N/A | N/A |
| DC\_7\_n5 | 7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
|  | n5 | 834 | 5 | 25 | 879 | 12 | IMD33 |
| DC\_7A\_n20A | 7 | 2512 | 10 | 50 | 2632 | N/A | N/A |
|  | n20 | 851 | 5 | 25 | 810 | 12 | IMD33 |
| DC\_7A\_n26ADC\_7C\_n26A | 7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
|  | n26 | 834 | 5 | 25 | 879 | 12 | IMD33 |
|  | 7 | 2567.5 | 5 | 25 | 2687.5 | 2.5 | IMD5 |
|  | n26 | 816.5 | 5 | 25 | 861.5 | N/A | N/A |
| DC\_7\_n40 | 7 | 2510 | 5 | 25 | 2630 | 23 | IMD3 |
|  | n40 | 2390 | 5 | 25 | 2390 | N/A | N/A |
| DC\_7A\_n66ADC\_7A-7A\_n66ADC\_7C\_n66A | 7 | 2535 | 10 | 50 | 2655 | 15 | IMD4 |
|  | n66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| DC\_7A\_n77ADC\_7A-7A\_n77(2A)DC\_7A-7A\_n77(3A)DC\_7A\_n77(2A)DC\_7A\_n77(3A)DC\_7C\_n77ADC\_7C\_n77(2A) | 7 | 2540 | 5 | 25 | 2660 | 7.1 | IMD4 |
|  | n77 | 3870 | 10 | 50 | 3870 | N/A | N/A |
| DC\_7\_n79 | 7 | 2510 | 5 | 25 | 2630 | [8] | IMD4 |
| n79 | 4900 | 40 | 216 | 4900 | N/A | N/A |
| DC\_8A\_n1A | 8 | 887.5 | 5 | 25 | 932.5 | N/A | N/A |
|  | n1 | 1965 | 5 | 25 | 2155 | 6 | IMD4 |
| DC\_8A\_n3A | 8 | 900 | 5 | 25 | 945 | 8 | IMD43 |
|  | n3 | 1755 | 10 | 50 | 1850 | N/A | N/A |
|  | 8 | 897.5 | 5 | 25 | 942.5 | N/A | N/A |
|  | n3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | IMD5 |
| DC\_8A\_n20A | n20 | 849.5 | 5 | 25 | 808.5 | 25 | IMD33 |
|  | 8 | 890.5 | 5 | 25 | 935.5 | N/A | N/A |
|  | n20 | 847.5 | 5 | 25 | 806.5 | N/A | N/A |
|  | 8 | 892.5 | 5 | 25 | 937.5 | 25 | IMD33 |
| DC\_8A\_n38A | 8 | 887.5 | 5 | 25 | 932.5 | 8.1 | IMD5 |
|  | n38 | 2617.5 | 5 | 25 | 2617.5 | N/A | N/A |
| DC\_8A\_n41ADC\_8A\_SUL\_n41A-n81A | 8 | 882.5 | 5 | 25 | 927.5 | 12.1 | IMD33 |
|  | n41 | 2685 | 10 | 50 | 2685 | N/A | N/A |
| DC\_8A\_n77A,DC\_8A\_n78A,DC\_8B\_n78ADC\_8A\_n78(2A),DC\_8A\_n77(3A),DC\_8A\_SUL\_n78A-n81A | 8 | 897.5 | 5 | 25 | 942.5 | 8.3 | IMD4 |
|  | n77, n78 | 3635 | 10 | 50 | 3635 | N/A | N/A |
| DC\_8A\_n79A,DC\_8A\_n79C,DC\_8A\_SUL\_n79A-n81A | 8 | 897.5 | 5 | 25 | 942.5 | 4.8 | IMD5 |
|  | n79 | 4532.5 | 40 | 216 | 4532.5 | N/A | N/A |
| DC\_11A\_n28A | 11 | 1430.5 | 5 | 25 | 1478.5 | N/A | N/A |
|  | n28 | 743 | 5 | 25 | 798 | 10.4 | IMD4 |
| DC\_12A\_n77ADC\_12A\_n77(2A) | 12 | 702 | 5 | 20 | 732 | 5.5 | IMD5 |
|  | n77 | 3540 | 10 | 50 | 3540 | N/A | N/A |
| DC\_12A\_n78A | 12 | 710 | 5 | 25 | 740 | 5.5 | IMD5 |
|  | n78 | 3580 | 10 | 50 | 3580 | N/A | N/A |
| DC\_13A\_n5A | 13 | 783 | 5 | 25 | 752 | N/A | N/A |
|  | n5 | 828 | 5 | 25 | 873 | 25 | IMD3 |
| DC\_13A\_n7ADC\_13A\_n7(2A) | 13 | 784.5 | 5 | 25 | 753.5 | N/A | N/A |
|  | n7 | 2520 | 40 | 216 | 2640 | 2.5 | IMD5 |
| DC\_13A\_n77A | 13 | 784.5 | 5 | 20 | 753.5 | 5.5 | IMD5 |
|  | n77 | 3891.5 | 10 | 50 | 3891.5 | N/A | N/A |
| DC\_14A\_n5A | 14 | 791 | 5 | 25 | 761 | N/A | N/A |
|  | n5 | 836 | 5 | 25 | 881 | 25 | IMD3 |
|  | 14 | 795.5 | 5 | 25 | 765.5 | 25 | IMD3 |
|  | n5 | 826.5 | 5 | 25 | 871.5 | N/A | N/A |
| DC\_14A\_n77ADC\_14A\_n77(2A) | 14 | 795.5 | 5 | 15 | 765.5 | 5.5 | IMD5 |
|  | n77 | 3947.5 | 10 | 50 | 3947.5 | N/A | N/A |
| DC\_18A\_n3A | 18 | 823 | 5 | 25 | 868 | N/A | N/A |
|  | n3 | 1721 | 5 | 25 | 1816 | 4 | IMD4 |
| DC\_18A\_n77ADC\_18A\_n78A | 18 | N/A | N/A | N/A | N/A | N/A | IMD4 |
|  | n77, n78 | N/A | N/A | N/A | N/A | N/A | N/A |
| DC\_19A\_n78A | 19 | N/A | N/A | N/A | N/A | N/A | IMD4 |
|  | n78 | N/A | N/A | N/A | N/A | N/A | N/A |
| DC\_20A\_n3A | 20 | 840 | 5 | 25 | 799 | N/A | N/A |
|  | n3 | 1775 | 5 | 25 | 1870 | 4 | IMD4 |
|  | 20 | 847 | 5 | 25 | 806 | 9 | IMD4 |
|  | n3 | 1735 | 5 | 25 | 1830 | N/A | N/A |
| DC\_20A\_n38A | 20 | N/A | N/A | N/A | N/A | N/A | IMD5 |
|  | n38 | N/A | N/A | N/A | N/A | N/A | N/A |
| DC\_20\_n7 | 20 | 851 | 5 | 25 | 810 | 12 | IMD33 |
|  | n7 | 2512 | 10 | 50 | 2632 | N/A | N/A |
| DC\_20A\_n8A | 20 | 849.5 | 5 | 25 | 808.5 | 25 | IMD3 |
|  | n8 | 892.5 | 5 | 25 | 937.5 | 25 | IMD3 |
| DC\_20\_n41 | 20 | 851 | 5 | 25 | 810 | 12.1 | IMD3 |
|  | n41 | 2512 | 10 | 50 | 2512 | N/A | N/A |
| DC\_20\_n41 | 20 | 841 | 5 | 25 | 800 | 8.1 | IMD5 |
|  | n41 | 2564 | 10 | 50 | 2564 | N/A | N/A |
| DC\_20A\_n77A,DC\_20A\_n78ADC\_20A\_n78C7,DC\_20A\_n78(2A),DC\_20A\_SUL\_n78A-n82A | 20 | 850 | 5 | 25 | 809 | 11 | IMD4 |
|  | n77, n78 | 3359 | 10 | 50 | 3359 | N/A | N/A |
| DC\_20A\_n77A | 20 | 840 | 5 | 25 | 799 | 6.5 | IMD5 |
|  | n77 | 4159 | 10 | 50 | 4159 | N/A | N/A |
| DC\_21A\_n28A7 | 21 | 1450.4 | 5 | 25 | 1498.4 | 2.5 | IMD5 |
| n28 | 735.5 | 5 | 25 | 790.5 | N/A | N/A |
| DC\_21A\_n79A | 21 | 1457.5 | 5 | 25 | 1505.5 | 18.4 | IMD3 |
|  | n79 | 4420.5 | 40 | 216 | 4420.5 | N/A | N/A |
| DC\_25A\_n77ADC\_25A-25A\_n77A | 25 | 1855 | 5 | 25 | 1935 | 26 | IMD2 |
|  | n77 | 3790 | 10 | 50 | 3790 | N/A | N/A |
|  | 25 | 1900 | 5 | 25 | 1980 | 8 | IMD4 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | N/A |
|  | 25 | 1885 | 5 | 25 | 1965 | 5 | IMD5 |
|  | n77 | 3810 | 10 | 50 | 3810 | N/A | N/A |
| DC\_25A\_n78ADC\_25A-25A\_n78A | 25 | 1855 | 5 | 25 | 1935 | 26 | IMD2 |
| n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |
| 25 | 1885 | 5 | 25 | 1965 | 8 | IMD4 |
| n78 | 3690 | 10 | 50 | 3690 | N/A | N/A |
| 25 | 1875 | 5 | 25 | 1955 | 5 | IMD5 |
| n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |
| DC\_26A\_n41A | 26 | 839 | 5 | 25 | 884 | 15.6 | IMD33 |
|  | n41 | 2562 | 10 | 50 | 2562 | N/A | N/A |
| DC\_28\_n50 | 28 | 730 | 10 | 50 | 775 | 15.3 | IMD 2 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
|  | 28 | 740 | 10 | 50 | 785 | 6 | IMD 4 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
|  | 28 | 740 | 10 | 50 | 785 | 0.5 | IMD 5 |
|  | n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
| DC\_28A\_n51A | 28 | 742.3 | 5 | 25 | 797.3 | 5 | IMD4 |
|  | n51 | 1429.5 | 5 | 25 | 1429.5 | N/A | N/A |
| DC\_26A\_n77A,DC\_26A\_n78A | 26 | 836.5 | 5 | 25 | 881.5 | 11.1 | IMD4 |
|  | n77, n78 | 3391 | 10 | 50 | 3391 | N/A | N/A |
| DC\_28A\_n77A,DC\_28A\_n78A,DC\_28A\_n78(2A),DC\_28A\_SUL\_n78A-n83A | 28 | 705.5 | 5 | 25 | 760.5 | 5.5 | IMD5 |
|  | n77, n78 | 3582.5 | 10 | 50 | 3582.5 | N/A | N/A |
| DC\_30A\_n77ADC\_30A\_n77(2A) | 30 | 2310 | 5 | 25 | 2355 | 8.0 | IMD4 |
|  | n77 | 3487.5 | 10 | 50 | 3487.5 | N/A | N/A |
| DC\_38A\_n3A | n3 | 1713 | 5 | 25 | 1808 | 8.2 | IMD4 |
|  | 38 | 2617 | 5 | 25 | 2617 | N/A | N/A |
| DC\_38A\_n8A | 38 | 2617.5 | 5 | 25 | 2617.5 | N/A | N/A |
|  | n8 | 887.5 | 5 | 25 | 932.5 | 8.1 | IMD5 |
| DC\_41A\_n3ADC\_41C\_n3A | n3 | 1740 | 5 | 25 | 1835 | 8.2 | IMD4 |
|  | 41 | 2657.5 | 5 | 25 | 2657.5 | N/A | N/A |
| DC\_42\_n3 | 42 | 3575 | 10 | 50 | 3575 | N/A | N/A |
|  | n3 | 1740 | 5 | 25 | 1835 | 26 | 2nd3 |
|  |  |  |  |  |  |  |  |
|  | 42 | 3435 | 10 | 50 | 3435 | N/A | N/A |
|  | n3 | 1765 | 5 | 25 | 1860 | 8.0 | IMD4 |
|  |  |  |  |  |  |  |  |
| DC\_42\_n28 | 42 | 3582.5 | 10 | 50 | 3582.5 | N/A | N/A |
|  | n28 | 705.5 | 5 | 25 | 760.5 | 5.5 | IMD5 |
| DC\_48A\_n2ADC\_48C\_n2ADC\_48D\_n2ADC\_48E\_n2A | 48 | 3625 | 20 | 100 | 3625 | N/A | N/A |
|  | n2 | 1852.5 | 5 | 25 | 1932.5 | 12 | IMD4 |
| DC\_48A\_n12A | 48 | 3557.5 | 10 | 50 | 3557.5 | N/A | N/A |
|  | n12 | 705.5 | 5 | 25 | 735.5 | 5.5 | IMD5 |
| DC\_48A\_n25ADC\_48C\_n25ADC\_48D\_n25A | 48 | 3625 | 20 | 100 | 3625 | N/A | N/A |
|  | n25 | 1852.5 | 5 | 25 | 1932.5 | 12 | IMD4 |
| DC\_48A\_n66ADC\_48C\_n66ADC\_48D\_n66A | 48 | 3630 | 20 | 100 | 3630 | N/A | N/A |
|  | n66 | 1715 | 5 | 25 | 2115 | 4 | IMD5 |
| DC\_66A\_n2A, DC\_66A-66A\_n2A | 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
|  | n2 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
|  | 66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
|  | n2 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| DC\_66A\_n5A | n5 | 838 | 5 | 25 | 883 | 30 | IMD23 |
|  | 66 | 1721 | 5 | 25 | 2121 | N/A | N/A |
| DC\_66A\_n7ADC\_66A-66A\_n7ADC\_66A\_n7(2A)DC\_66A-66A\_n7(2A) | 66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
|  | n7 | 2535 | 10 | 50 | 2655 | 15 | IMD4 |
| DC\_66A\_n25A | 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
|  | n25 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
|  | 66 | 1712.5 | 5 | 25 | 2112.5 | 23 | IMD3 |
|  | n25 | 1912.5 | 5 | 25 | 1992.5 | N/A | N/A |
|  | 66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
|  | n25 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| DC\_66A\_n46A | 66 | 1735 | 5 | 25 | 2135 | 12.0 | IMD3 |
|  | n46 | 5605 | 20 | 100 | 5605 | N/A | N/A |
| DC\_66A\_n48A | 66 | 1715 | 5 | 25 | 2115 | 4 | IMD5 |
|  | n48 | 3630 | 20 | 100 | 3630 | N/A | N/A |
| DC\_66A\_n71A | 66 | 1750 | 5 | 25 | 2150 | 5 | IMD4 |
|  | n71 | 675 | 5 | 25 | 629 | N/A | N/A |
| DC\_66A\_n77ADC\_66A\_n77(2A)DC\_66A-66A\_n77ADC\_66A-66A\_n77(2A)DC\_66A-66A-66A\_n77ADC\_66A-66A-66A\_n77(2A) | 66 | 1775 | 5 | 25 | 2175 | 31.0 | IMD2 |
|  | n77 | 3950 | 10 | 50 | 3950 | N/A | N/A |
|  | 66 | 1760 | 5 | 25 | 2160 | 5.0 | IMD5 |
|  | n77 | 3720 | 10 | 50 | 3720 | N/A | N/A |
| DC\_66A\_n78A | 66 | 1730 | 5 | 25 | 2150 | 5.0 | IMD5 |
|  | n78 | 3660 | 10 | 50 | 3660 | N/A | N/A |
| DC\_71A\_n38A | 71 | 665 | 5 | 25 | 619 | 11 | IMD4 |
|  | n38 | 2614 | 10 | 50 | 2614 | N/A | N/A |
| DC\_71A\_n41A | 71 | 666 | 5 | 25 | 620 | 11 | IMD4 |
| n41 | 2618 | 5 | 25 | 2618 | N/A | N/A |
| DC\_71A\_n66A | 71 | 675 | 5 | 25 | 629 | N/A | N/A |
|  | n66 | 1750 | 5 | 25 | 2150 | 5 | IMD4 |
| DC\_71A\_n77A8 | 71 | 671 | 5 | 25 | 625 | 5.5 | IMD5 |
|  | n77 | 3309 | 10 | 50 | 3309 | N/A | N/A |
| DC\_71A\_n78A | 71 | 681.5 | 5 | 25 | 635.5 | 5.5 | IMD5 |
| DC\_71A\_n78(2A) | n78 | 3361.5 | 10 | 50 | 3361.5 | N/A | N/A |
| NOTE 1: E-UTRA carrier shall be set to min(+20 dBm, PCMAX\_L\_E-UTRA,c) and NR carrier shall be set to min(+20 dBm, PCMAX\_L,f,c,NR) as defined in clause 6.2B.4.1.3.NOTE 2: RBstart = 0NOTE 3: This band is subject to IMD5 also which MSD is not specified.NOTE 4: VoidNOTE 5: VoidNOTE 6: For NR band, UL/DL BW and UL LCRB can be adjusted according to the supported BW and lowest SCS supported by the UE.NOTE 7: The frequency range in band n28 is restricted for this band combination to 728 - 738 MHz for the UL and 783 - 793 MHz for the DL. This band is subject to IMD2, IMD4 and IMD5 fall in n28 also which MSD is not specified. In addition, this band is subject to IMD4 fall in B21 also which MSD is not specified.NOTE 8: For a UE which supports this band combination only when the Band n77 frequency range restriction defined in NOTE 12 of Table 5.2-1 from TS 38.101-1 applies, the MSD test point(s) cannot be verified for the band combination and the test point(s) can be skipped. |

---End of changes---