**3GPP TSG-RAN4 Meeting #108-bis *R4-2317370***

**Xiamen, China, 9 – 13 October, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **xxxx** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | draftCR on NW A L1 measurement requirements with MUSIM gaps |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_DualTxRx\_MUSIM-Core |  | ***Date:*** | 2023-09-19 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Based on WF R4-2314364, RAN4 should define L1 measurement requirements for NW A when MUSIM gaps are configured. |
|  |  |
| ***Summary of change:*** | Introdcue L1 measurement requirements for NW A when MUSIM gaps are configured. |
|  |  |
| ***Consequences if not approved:*** | Requirements for MUSIM gaps are incomplete. |
|  |  |
| ***Clauses affected:*** | 9.5.4.1, 9.5.4.2, 9.8.4.1, 9.13.4.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

#### 9.5.4.1 SSB based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB.

The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in Table 9.5.4.1-1 for FR1. The value of TL1-RSRP\_Measurement\_Period\_SSB is defined in Table 9.5.4.1-2 for FR2 when *highSpeedMeasFlagFR2-r17* is not configured, and defined in Table 9.5.4.1-3 for FR2 power class 6 UE when *highSpeedMeasFlagFR2-r17* is configured, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- N= 8 in Table 9.5.4.1-2.

When UE supports concurrent measurement gap or *musim-GapPreference-r17* or both concurrent measurement gap and *musim-GapPreference-r17*, and concurrent gaps or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- P value for SSB resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gaps, MUSIM gap(s) and per-FR measurement gaps within the same FR as serving cell, and starting at the beginning of any SSB resource occasion:

- Ntotal is the total number of SSB resource occasions within the window, including those overlapped with measurement gap occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of SSB resource occasions that are not overlapped with any non-dropped measurement gap occasion nor non-dropped MUSIM gap occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8 and 9.1.10, and

- Navailable is the number of SSB resource occasions that are not overlapped with any non-dropped measurement gap occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8 and 9.1.10.

- TL1 is periodicity of the target SSB.

Otherwise, for a UE not supporting *concurrentMeasGap-r17* or when concurrent gaps are not configured, and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

*Editor Note: FFS whether and how to update definition of GAP to include MUSIM gap.*

*Editor Note: FFS for the case when Navailable = 0 due to fully overlapping between SSB occasions and the union of MUSIM gap and measurement gap occasions within the window W.*

For FR1,

- P=$\frac{1}{1-\frac{T\_{SSB}}{xGP}}$, when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the SSB.

For FR2,

 P1=$ \frac{1}{1-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when SSB is not overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod).

- P is PL1\_sharing\*Psharing factor, when SSB is not overlapped with measurement gap and SSB is fully overlapped with SMTC period (TSSB = TSMTCperiod).

- P1=$\frac{1}{1-\frac{T\_{SSB}}{xRP}-\frac{T\_{SSB}}{T\_{SMTCperiod}}}$, when SSB is partially overlapped with GAP and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TSSB < 0.5\*TSMTCperiod

- P is $\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{xRP}}$, when SSB is partially overlapped with GAP and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TSSB = 0.5\*TSMTCperiod

- P1=$ \frac{1}{1-\frac{T\_{SSB}}{min(T\_{SMTCperiod},xRP)}}$, when SSB is partially overlapped with GAP (TSSB < xRP) and SSB is partially overlapped with SMTC occasion (TSSB < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- P is $ P\_{L1\\_sharing}\*\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{xRP}}$, when SSB is partially overlapped with measurement gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

-

- If SSB resource from the cell with different PCI is configured for L1-RSRP measurement, and P2 is valid accoding to 9.13.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain)

- P = $\frac{P\_{1}}{1-\frac{P\_{1}\*T\_{SSB}}{P\_{2}\*T\_{SSB\\_CDP}}}$ , if P1\*TSSB < P2\*TSSB\_CDP.

- P = P1, if P1\*TSSB > P2\*TSSB\_CDP.

- P = 2\*P1, if P1\*TSSB = P2\*TSSB\_CDP.

- Otherwise, P = P1

Where:

- TSSB = ssb-periodicityServingCell of the serving cell

- TSMTCperiod = the configured SMTC period

- TSSB\_CDP = SSB periodicity of the cell with PCI different from serving cell

- Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- PL1\_sharing = 2, if SSB resource from the cell with different PCI is configured for L1-RSRP measurement, and Psharing\_factor,CDP is used in 9.13.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain). PL1\_sharing = 1, otherwise.

- TSSB = ssb-periodicityServingCell

- TSMTCperiod = the configured SMTC period

- If the UE is configured with Pre-MG, an SSB or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When a measurement gap is configured and the measurement gap is not NCSG,

- an SSB or an SMTC occasion is considered to be overlapped with the GAP if it overlaps a measurement gap occasion, and

- xRP = MGRP

- Otherwise, when NCSG measurement gap is configured,

- an SSB or an SMTC occasion is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

- When concurrent gaps are configured, an SSB or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to 9.1.8.

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and GAP configurations does not meet pervious conditions.

When UE is configured with aperiodic MUSIM gap via *MUSIM-GapConfig-r17* and the aperiodic MUSIM gap is overlapping with SSB resource occasion for L1-RSRP, longer evaluation period would be expected.

When UE is configured with periodic MUSIM gap(s), and if SSB resource occasions for L1-RSRP are fully overlapped with MUSIM gap(s), no requirement applies for the SSB based L1-RSRP measurement.

For either an FR1 or FR2 serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

For either an FR1 or FR2 serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.5.4.1-1: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: K = 1 when TSSB ≤ 40 ms and *highSpeedMeasFlag-r16 or highSpeedMeasCA-Scell-r17* are configured; otherwise K = 1.5.Note 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16. or measurementEnhancementCA-r17* |

Table 9.5.4.1-2: Measurement period TL1-RSRP\_Measurement\_Period\_SSB for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. |

Table 9.5.4.1-3: Measurement period TL1-RSRP\_Measurement\_Period\_SSB configured with *highSpeedMeasFlagFR2-r17* for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N1Note2)\*TSSB) |
| DRX cycle ≤ 80ms | max(TReport, ceil(M\*P\*N1Note2\*M2)\*max(TDRX,TSSB))  |
| 80ms< DRX ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB)) |
| DRX cycle > 320ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note1: TSSB = ssb-periodicityServingCell is the periodicity of the SSB-Index configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: N1 = 2 when *highSpeedMeasFlagFR2-r17* = set1; N1 = 6 when *highSpeedMeasFlagFR2-r17* = [set2].Note 3: M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2 = 1 |

#### 9.5.4.2 CSI-RS based L1-RSRP Reporting

The UE shall be capable of performing L1-RSRP measurements based on the configured CSI-RS resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_CSI-RS.

The value of TL1-RSRP\_Measurement\_Period\_CSI-RS is defined in Table 9.5.4.2-1 for FR1 and in Table 9.5.4.2-2 for FR2, where

- For periodic and semi-persistent CSI-RS resources, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- For aperiodic CSI-RS resources M=1

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured with QCL-TypeD for all resources in the resource set.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided with QCL-TypeD for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided *qcl-info* is configured for all resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clause 10.1.19.2 and 10.1.20.2 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requirements apply provided *qcl-info* is configured with QCL-TypeD for all resources in the resource set.

When UE supports [concurrent measurement gap] or *musim-GapPreference-r17* or both concurrent measurement gap and *musim-GapPreference-r17*, and concurrent gaps or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- P value for a CSI-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gaps, MUSIM gap(s) and per-FR measurement gaps within the same FR as serving cell, and starting at the beginning of any CSI-RS resource occasion:

- Ntotal is the total number of CSI-RS resource occasions within the window, including those overlapped with measurement gap occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of CSI-RS resource occasions that are not overlapped with any non-dropped measurement gap occasion nor non-dropped MUSIM gap occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8 and 9.1.10, and

- Navailable is the number of CSI-RS resource occasions that are not overlapped with any non-dropped measurement gap occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8 and 9.1.10.

TL1 is periodicity of the target CSI-RS.

Otherwise, for a UE not supporting *concurrentMeasGap-r17* or when concurrent gaps are not configured, and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

*Editor Note: FFS whether and how to update definition of GAP to include MUSIM gap.*

*Editor Note: FFS for the case when Navailable = 0 due to fully overlapping between CSI-RS occasions and the union of MUSIM gap and measurement gap occasions within the window W.*

For FR1,

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{xRP}}$, when in the monitored cell there are GAPs configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For FR2,

- P=1, when CSI-RS is not overlapped with a GAP and also not overlapped with SMTC occasion.

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{xRP}}$, when CSI-RS is partially overlapped with GAP and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{T\_{SMTCperiod}}}$, when CSI-RS is not overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P=Psharing factor, when CSI-RS is not overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=1, when aperiodic CSI-RS resource is not overlapped with GAP

- P=$ \frac{1}{1-\frac{T\_{CSI-RS}}{xRP}-\frac{T\_{CSI-RS}}{T\_{SMTCperiod}}}$, when CSI-RS is partially overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=$\frac{3}{1-\frac{T\_{CSI-RS}}{xRP}}$, when CSI-RS is partially overlapped with [measurement gap] and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=$ \frac{1}{1-\frac{T\_{CSI-RS}}{T\_{SMTCperiod}}}$, when CSI-RS is partially overlapped with GAP (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP.

- P=$\frac{P\_{sharing factor}}{1-\frac{T\_{CSI-RS}}{xRP}}$, when CSI-RS is partially overlapped with GAP and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

Where:

- Psharing factor = 1, if the CSI-RS configured for L1-RSRP measurement outside gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

TSMTCperiod = the configured SMTC period.

 TCSI-RS = the periodicity of CSI-RS configured for L1-RSRP measurement

 If the UE is configured with Pre-MG, a CSI-RS or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When a measurement gap is configured and the measurement gap is not NCSG,

- a CSI-RS or an SMTC occasion is considered to be as overlapped with the GAP if it overlapps a measurement gap occasion, and

- xRP = MGRP

- Otherwise, when NCSG measurement gap is configured,

- a CSI-RS or an SMTC occasion is considered to be as overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

When UE is configured with aperiodic MUSIM gap via *MUSIM-GapConfig-r17* and the aperiodic MUSIM gap is overlapping with CSI-RS resource occasion for L1-RSRP, longer evaluation period would be expected.

When UE is configured with periodic MUSIM gap(s), and if CSI-RS resource occasions for L1-RSRP are fully overlapped with MUSIM gap(s), no requirement applies for the CSI-RS based L1-RSRP measurement.

When concurrent gaps are configured, a CSI-RS or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to 9.1.8.

Table 9.5.4.2-1: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3.Note 3: K = 1 when TCSI-RS ≤ 40 ms and *highSpeedMeasFlag-r16 or highSpeedMeasCA-Scell-r17* are configured; otherwise K = 1.5.Note 4: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16 or measurementEnhancementCA-r17.* |

Table 9.5.4.2-2: Measurement period TL1-RSRP\_Measurement\_Period\_CSI-RS for FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_CSI-RS (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P\*N)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-RSRP measurement is transmitted with Density = 3. |

<End of Change 1>

#### 9.8.4.1 L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured

edicated resource configured as IMR for L1-SINR computation, and the UE physical layer shall be capable of reporting L1-SINR measured over the measurement period of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only.

The value of TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only is defined in Table 9.8.4.1-1 for FR1 and in Table 9.8.4.1-2 for FR2, where

For the value of M,

- For periodic and semi-persistent CSI-RS resources as CMR, M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise;

- For aperiodic CSI-RS resources as CMR, M=1.

For the value of N in FR2

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply if *qcl-InfoPeriodicCSI-RS* is configured for all the resources in the resource set and for each resource one RS has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For periodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided *qcl-InfoPeriodicCSI-RS* is configured for all resources in the resource set.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For semi-persistent CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=ceil(*maxNumberRxBeam* / Nres\_per\_set), where Nres\_per\_set is number of resources in the resource set. The requirements apply provided TCI state is provided for all resources in the resource set in the MAC CE activating the resource set.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to OFF, N=1. The requriements apply provided *qcl-info* is configured for all resources in the resource set and for each resource has QCL-TypeD with

- SSB for L1-RSRP or L1-SINR measurement, or

- another CSI-RS in resource set configured with repetition ON.

- For aperiodic CSI-RS resources as CMR in a resource set configured with higher layer parameter *repetition* set to ON, N=1. UE is not required to meet the accuracy requirements in clause 10.1.28.1 and 10.1.28.3 if number of resources in the resource set is smaller than *maxNumberRxBeam*. The requriements apply provided *qcl-info* is configured for all resources in the resource set.

When UE supports concurrent measurement gap or *musim-GapPreference-r17* or both concurrent measurement gap and *musim-GapPreference-r17*, and concurrent gaps or periodic MUSIM gaps or both concurrent gaps and periodic MUSIM gaps are configured,

- P value for a CSI-RS resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- Psharing factor \* Ntotal / Noutside\_MG in FR2 with Navailable = 0

- Ntotal / Navailable in FR2 with Navailable > 0

- For a window W of duration max(TL1, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gaps, periodic MUSIM gap(s) and per-FR measurement gaps within the same FR as serving cell, and starting at the beginning of any CSI-RS resource occasion:

- Ntotal is the total number of CSI-RS resource occasions within the window, including those overlapped with measurement gap occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of CSI-RS resource occasions that are not overlapped with any non-dropped measurement gap occasion nor non-dropped MUSIM gap occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8, and 9.1.10, and

- Navailable is the number of CSI-RS resource occasions that are not overlapped with any non-dropped measurement gap occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8, and 9.1.10

- TL1 is periodicity of the target CSI-RS.

Otherwise, for a UE not supporting *concurrentMeasGap-r17* or when concurrent gaps are not configured, and UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

*Editor Note: FFS whether and how to update definition of GAP to include MUSIM gap.*

*Editor Note: FFS for the case when Navailable = 0 due to fully overlapping between CSI-RS occasions and the union of MUSIM gap and measurement gap occasions within the window W.*

For the value of P in FR1,

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{xGP}}$, when in the monitored cell there are [measurement gaps] configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the CSI-RS; and

- P=1 when in the monitored cell there are no GAPs overlapping with any occasion of the CSI-RS.

For the value of P in FR2,

- P=1, when CSI-RS is not overlapped with GAP and also not overlapped with SMTC occasion.

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{xGP}}$, when CSI-RS is partially overlapped with GAP and CSI-RS is not overlapped with SMTC occasion (TCSI-RS < xRP)

- P=$\frac{1}{1-\frac{T\_{CSI-RS}}{T\_{SMTCperiod}}}$, when CSI-RS is not overlapped with GAP and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod).

- P is Psharing factor,, when CSI-RS is not overlapped with [measurement gap] and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod).

- P=$ \frac{1}{1-\frac{T\_{CSI-RS}}{xGP}-\frac{T\_{CSI-RS}}{T\_{SMTCperiod}}}$, when CSI-RS is partially overlapped with [measurement gap] and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and

- TSMTCperiod ≠ xRP or

- TSMTCperiod = xRP and TCSI-RS < 0.5\*TSMTCperiod

- P=$\frac{P\_{sharing factor}}{1-\frac{T\_{CSI-RS}}{xGP}}$, when CSI-RS is partially overlapped with [measurement gap] and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is not overlapped with GAP and TSMTCperiod = xRP and TCSI-RS = 0.5\*TSMTCperiod

- P=$ \frac{1}{1-\frac{T\_{CSI-RS}}{min⁡(T\_{SMTCperiod},xRP)}}$, when CSI-RS is partially overlapped with [measurement gap] (TCSI-RS < xRP) and CSI-RS is partially overlapped with SMTC occasion (TCSI-RS < TSMTCperiod) and SMTC occasion is partially or fully overlapped with GAP .

- P=$\frac{P\_{sharing factor}}{1-\frac{T\_{CSI-RS}}{xGP}}$, when CSI-RS is partially overlapped with [measurement gap] and CSI-RS is fully overlapped with SMTC occasion (TCSI-RS = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP)

Where:

 Psharing factor = 1, if the CSI-RS configured for L1-SINR measurement outside gap is

 not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

 not overlapped by the RSSI symbols indicated by *ss-RSSI-Measurement* and 1 data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured.

- Psharing factor = 3, otherwise.

- TSMTCperiod = the configured SMTC1 period or SMTC2 period if configured.

- TCSI-RS = the periodicity of CSI-RS configured for L1-SINR measurement

- If the UE is configured with Pre-MG, a CSI-RS reourse or an SMTC occasion is only considered to be overlapped by the Pre-MG if the Pre-MG is activated.

- When a measurement gap is configured and the measurement gap is not NCSG,

- a CSI-RS is considered to be overlapped with the GAP if it overlaps a measurement gap occasion, and

- xRP = MGRP

- Otherwise, when NCSG measurement gap is configured,

- a CSI-RS is considered to be overlapped with the GAP if

- it overlaps the VIL1 or VIL2 of NCSG, or

- it overlaps the ML of NCSG in FR2, and there exists a target carrier to be measured within NCSG that is intra-frequency carrier or inter-frequency carrier in the same band as the serving cell, or inter-frequency carrier in different band as the serving cell and UE does not support IBM between the target carrier and the serving cell,

- and

- xRP = VIRP

- When concurrent gaps are configured, a CSI-RS or an SMTC occasion is not considered to be overlapped by a gap occasion if the gap occasion is dropped according to 9.1.8.

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*.

Note: The overlap between CSI-RS for L1-SINR measurement and SMTC means that CSI-RS for L1-SINR measurement is within the SMTC window duration.

When UE is configured with aperiodic MUSIM gap via *MUSIM-GapConfig-r17* and the aperiodic MUSIM gap is overlapping with CSI-RS resource occasion for L1-SINR, longer evaluation period would be expected.

When UE is configured with periodic MUSIM gap(s), and if CSI-RS resource occasions for L1-SINR are fully overlapped with MUSIM gap(s), no requirement applies for the CSI-RS based L1-SINR measurement.

Longer evaluation period would be expected if the combination of CSI-RS, SMTC occasion and GAP configurations does not meet pervious conditions.

Table 9.8.4.1-1: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR1

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. |

Table 9.8.4.1-2: Measurement period TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only for FR2

|  |  |
| --- | --- |
| Configuration | TL1-SINR\_Measurement\_Period\_CSI-RS\_CMR\_Only (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TCSI-RS) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TCSI-RS)) |
| DRX cycle > 320ms | ceil(M\*P\*N)\*TDRX |
| Note 1: TCSI-RS is the periodicity of CSI-RS configured for L1-SINR measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: the requirements are applicable provided that the CSI-RS resource configured for L1-SINR measurement is transmitted with Density = 3. |

<Start of Change 2>

<End of Change 2>

<Start of Change 3>

#### 9.13.4.1 Inter-cell SSB based L1-RSRP Reporting

If a cell with PCI different from serving cell is known according 9.13.2, the UE shall be capable of performing L1-RSRP measurements based on the configured SSB resource for L1-RSRP computation, and the UE physical layer shall be capable of reporting L1-RSRP measured over the measurement period of TL1-RSRP\_Measurement\_Period\_SSB\_CDP. The requirements specified in this clause are only applicable when

- *highSpeedMeasFlag-r16* is not configured, and

- *highSpeedMeasFlagFR2-r17* is not configured, and

- highSpeedMeasCA-Scell-r17 is not configured, and

- SSBs of CDP outside SMTCs for L1-RSRP measurement are not overlapped with concurrent gaps.

The value of TL1-RSRP\_Measurement\_Period\_SSB\_CDP is defined in Table 9.13.4.1-1 for FR1, The value of TL1-RSRP\_Measurement\_Period\_SSB\_CDP is defined in Table 9.13.4.1-2 for FR2 when *highSpeedMeasFlagFR2-r17* is not configured, where

- M=1 if higher layer parameter *timeRestrictionForChannelMeasurement* is configured, and M=3 otherwise

- N= 8.

When UE supports *musim-GapPreference-r17*, and periodic MUSIM gaps are configured,

- P value for SSB resource to be measured is defined as

- Ntotal / Noutside\_MG in FR1

- P = PL1\_sharing factor \* Psharing factor \* Ntotal / Noutside\_MG in FR2, if Navailable = 0

- P is defined as below based on P2, where P2 = Ntotal / Navailable in FR2, if Navailable > 0

- For a window W of duration max(TL1, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gaps, MUSIM gap(s) and/or per-FR measurement gaps within the same FR as serving cell, and starting at the beginning of any SSB resource occasion:

- Ntotal is the total number of SSB resource occasions within the window, including those overlapped with measurement gap occasions, MUSIM gap occasions or SMTC occasions within the window, and

- Noutside\_MG is the number of SSB resource occasions that are not overlapped with any non-dropped measurement gap occasion nor non-dropped MUSIM gap occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8, and

- Navailable is the number of SSB resource occasions that are not overlapped with any non-dropped measurement gap occasion, non-dropped MUSIM gap occasion nor any SMTC occasion within the window W, after accounting for measurement gap and MUSIM gap collisions as defined in clause 9.1.8.

- TL1 is periodicity of the target SSB.

Otherwise, when UE does not support *musim-GapPreference-r17* or when no MUSIM gaps are configured,

*Editor Note: FFS for the case when Navailable = 0 due to fully overlapping between SSB occasions and the union of MUSIM gap and measurement gap occasions within the window W.*

For FR1,

- P=$\frac{1}{1-\frac{T\_{SSB\\_CDP}}{MRGP}}$, when in the monitored cell there are measurement gaps configured for intra-frequency, inter-frequency or inter-RAT measurements, which are overlapping with some but not all occasions of the SSB; and

- P=1 when in the monitored cell there are no measurement gaps overlapping with any occasion of the SSB.

For FR2,

- P is PL1\_sharing\*Psharing factor, CDP, when SSB is not overlapped with measurement gap and SSB is fully overlapped with SMTC period (TSSB\_CDP = TSMTCperiod), and TSSB\_SC = TSMTCperiod.

- P is $ P\_{L1\\_sharing}\*\frac{P\_{sharing factor}}{1-\frac{T\_{SSB}}{xRP}}$, when SSB is partially overlapped with measurement gap and SSB is fully overlapped with SMTC occasion (TSSB = TSMTCperiod) and SMTC occasion is partially overlapped with GAP (TSMTCperiod < xRP), and TSSB\_SC = TSMTCperiod.

- P2=$\frac{1}{1-\frac{T\_{SSB\\_CDP}}{T\_{SMTCperiod}}}$, when SSB is not overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB\_CDP < TSMTCperiod).

- P2=$ \frac{1}{1-\frac{T\_{SSB\\_CDP}}{MGRP}-\frac{T\_{SSB\\_CDP}}{T\_{SMTCperiod}}}$, when SSB is partially overlapped with measurement gap and SSB is partially overlapped with SMTC occasion (TSSB\_CDP < TSMTCperiod) and SMTC occasion is not overlapped with measurement gap and

- TSMTCperiod ≠ MGRP or

- TSMTCperiod = MGRP and TSSB\_CDP < 0.5\*TSMTCperiod

- P2= $\frac{1}{1-\frac{T\_{SSB\\_CDP}}{min(T\_{SMTCperiod},MGRP)}}$,when SSB is partially overlapped with measurement gap (TSSB\_CDP <MGRP) and SSB is partially overlapped with SMTC occasion (TSSB\_CDP < TSMTCperiod) and SMTC occasion is partially or fully overlapped with measurement gap.

- If SSB resource from serving cell is configured for L1-RSRP measurements, and P1 is valid accoding to 9.5.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain)

- P = $\frac{P\_{2}}{1-\frac{P\_{2}\*T\_{SSB\\_CDP}}{P\_{1}\*T\_{SSB\\_SC}}}$ , if P2\*TSSB\_CDP < P1\*TSSB\_SC.

- P = P2, if P2\*TSSB\_CDP> P1\*TSSB\_SC.

- P = 2\*P2, if P1\*TSSB\_SC = P2\*TSSB\_CDP.

 - Otherwise, P = P2

- TSSB\_CDP = SSB periodicity of the cell with PCI different from serving cell

- TSMTCperiod = the configured SMTC period

- TSSB\_SC = ssb-periodicityServingCell of the serving cell

Psharing factor = 1, if the SSB configured for L1-RSRP measurement outside measurement gap is

- not overlapped with the SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol before each consecutive SSB symbols indicated by *SSB-ToMeasure* and 1 data symbol after each consecutive SSB symbols indicated by *SSB-ToMeasure*, given that *SSB-ToMeasure* is configured, where the *SSB-ToMeasure* is the union set of *SSB-ToMeasure* from all the configured measurement objects merged on the same serving carrier, and,

- not overlapped with the RSSI symbols indicated by *ss-RSSI-Measurement* and 1data symbol before each RSSI symbol indicated by *ss-RSSI-Measurement* and 1 data symbol after each RSSI symbol indicated by *ss-RSSI-Measurement*, given that *ss-RSSI-Measurement* is configured,

Psharing factor = 3, otherwise.

PL1\_sharing = 2, if SSB resource from serving cell is configured for L1-RSRP measurements, and Psharing\_factor is used in 9.5.4.1, and any symbol of the SSBs from serving cell and cell with different PCI are overlapping or adjacent (in time domain). PL1\_sharing = 1, otherwise.

If the high layer in TS 38.331 [2] signaling of *smtc2* is configured, TSMTCperiod corresponds to the value of higher layer parameter *smtc2*; Otherwise TSMTCperiod corresponds to the value of higher layer parameter *smtc1*. TSMTCperiod is the shortest SMTC period among all CCs in the same FR2 band, provided the SMTC offset of all CCs in FR2 have the same offset.

Longer evaluation period would be expected if the combination of SSB, SMTC occasion and measurement gap configurations does not meet pervious conditions.

For either an FR1 or FR2 cell with PCI different from serving cell, longer evaluation period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

When UE is configured with aperiodic MUSIM gap via *MUSIM-GapConfig-r17* and the aperiodic MUSIM gap is overlapping with SSB resource occasion for inter-cell L1-RSRP, longer evaluation period would be expected.

When UE is configured with periodic MUSIM gap(s), and if SSB resource occasions for inter-cell L1-RSRP are fully overlapped with MUSIM gap(s), no requirement applies for the SSB based inter-cell L1-RSRP measurement.

For either an FR1 or FR2 cell with PCI different from serving cell, longer L1 RSRP measurement period would be expected during the period Tidentify\_CGI,E-UTRAN when the UE is requested to decode an LTE CGI.

Table 9.13.4.1-1: Inter-cell L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_CDP for known cells with different PCIs in FR1

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_CDP (ms)  |
| non-DRX | max(TReport, ceil(M\*P)\*TSSB\_CDP) |
| DRX cycle ≤ 320ms | max(TReport, ceil(K \*M\*P)\*max(TDRX,TSSB\_CDP)) |
| DRX cycle > 320ms | ceil(M\*P)\*TDRX |
| Note 1: TSSB\_CDP is the periodicity of the SSB-Index configured for inter-cell L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting.Note 2: K = 1.5.  |

Table 9.13.4.1-2: Inter-cell L1-RSRP measurement period TL1-RSRP\_Measurement\_Period\_SSB\_CDP for known cells with different PCIs in FR2

|  |  |
| --- | --- |
| Configuration | TL1-RSRP\_Measurement\_Period\_SSB\_CDP (ms)  |
| non-DRX | max(TReport, ceil(M\*P\*N)\*TSSB\_CDP) |
| DRX cycle ≤ 320ms | max(TReport, ceil(1.5\*M\*P\*N)\*max(TDRX,TSSB\_CDP)) |
| DRX cycle > 320ms | ceil(1.5\*M\*P\*N)\*TDRX |
| Note: TSSB\_CDP is the periodicity of the SSB-Index configured for inter-cell L1-RSRP measurement. TDRX is the DRX cycle length. TReport is configured periodicity for reporting. |

<End of Change 3>