**3GPP TSG-RAN WG4 Meeting #109 *R4-2319154***

Chicago, US, November 13 – 17, 2023

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **3719** | **rev** | **-** | **Current version:** | **17.11.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR on ConMGs |
|  |  |
| ***Source to WG:*** | Ericsson, ZTE |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_MG\_enh-Core |  | ***Date:*** | 2023-11-03 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | *<This CR shall be implemented before Rel-18 MG CR>*In Rel-15, when UE performs intra-frequency without gaps measurement and fully overlapping with MG, UE will perform the measurement within the MG. The scenario is captured in section ‘intra-frequency measurement without measurement gaps’ since SMTC = MGRP.However, from Rel-17, RAN4 introduced the Con-MGs, intra-frequency SMTC may partially overlap with the measurement gap and fully overlap with the union of the gaps. In this case, UE shall perform measurement within the associated gap. The measurement period shall follow MGRP other than SMTC. |
|  |  |
| ***Summary of change:*** | Introduce a new structure to define the intra-frequency measurements without measurement gaps.If the intrafrequency MO will be measured within measurement gap, it refer on the related sections of intrafrequency measurements with measurement gap.The new structure can also be applied to other gap combinations, such as MUSIM gaps, NeedForGaps, Pre-MG, NCSG etc. |
|  |  |
| ***Consequences if not approved:*** | The requirements will be missing and their performance cannot be guaranteed. |
|  |  |
| ***Clauses affected:*** |  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.533  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**------------------------------------ CHANGE --------------------------------**

## 9.2 NR intra-frequency measurements

### 9.2.1 Introduction

A measurement is defined as a SSB based intra-frequency measurement provided the centre frequency of the SSB of the serving cell indicated for measurement and the centre frequency of the SSB of the neighbour cell are the same, and the subcarrier spacing of the two SSBs are also the same.

The UE shall be able to identify new intra-frequency cells and perform SS-RSRP, SS-RSRQ, and SS-SINR measurements of identified intra-frequency cells if carrier frequency information is provided by PCell or the PSCell, even if no explicit neighbour list with physical layer cell identities is provided.

The UE can perform intra-frequency SSB based measurements without measurement gaps (either legacy measurement gap or NCSG) if

- the UE indicates ‘no-gap’ via *intraFreq-needForGap* for intra-frequency measurement, or

- the SSB is completely contained in the active BWP of the UE, or

- the active downlink BWP is initial BWP[3].

Besides the conditions listed above, for UE supporting *nr-NeedForGapNCSG-reporting-r17* and indicating *NeedForGapNCSG-InfoNR* for intra-frequency measurement,

- An intra-frequency SSB measurement is defined as measurement without gap if

- the UE indicates ‘nogap-noncsg’ via *NeedForGapNCSG-InfoNR* for the intra-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE, and

- the active downlink BWP is not an initial BWP [3].

 - An intra-frequency SSB measurement is defined as measurement with NCSG if

- the UE indicates ‘ncsg’ via *NeedForGapNCSG-InfoNR* for the intra-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE, and

- the active downlink BWP is not an initial BWP [3]

- An intra-frequency SSB measurement is defined as measurement with gap if

- the UE indicates ‘gap’ via *NeedForGapNCSG-InfoNR* for the intra-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE, and

- the active downlink BWP is not an initial BWP [3]

- The UE can perform intra-frequency SSB based measurement corresponding to a deactivated SCell or dormant SCell with NCSG.

- For intra-frequency SSB based measurements with NCSG, UE may cause scheduling restriction as specified in clause 9.2.7.3.

For intra-frequency SSB based measurements without measurement gaps, UE may cause scheduling restriction as specified in clause 9.2.5.3.SSB based measurements are configured along with one or two measurement timing configuration(s) (SMTC(s)) which provides periodicity, duration and offset information on a window of up to 5ms where the measurements are to be performed. For intra-frequency connected mode measurements, up to two measurement window periodicities may be configured. A single measurement window offset and measurement duration are configured per intra-frequency measurement object.

When measurement gaps are needed, the UE is not expected to detect SSB and measure RSSI of RSRQ which start earlier than the gap starting time + switching time, nor detect SSB and measure RSSI of RSRQ which end later than the gap end – switching time. Switching time is 0.5ms for frequency range FR1 and 0.25ms for frequency range FR2.

The requirements in this clause shall also apply, when the UE is configured to perform SRS carrier based switching and using measurement gaps.

The measurement requirements defined for an activated SCell with a non-dormant active BWP defined in this clause shall also apply to an activated SCell with dormant BWP as active BWP.

The intra-frequency measurement requirements in 9.2.5 applies for SSB based intra-frequency measurements without measurement gaps if the intra-frequency measurement object satisfies one of the following conditions,

- For a UE supporting concurrent gaps and when concurrent gaps are configured:

- When none of the SMTC occasions of this intra-frequency measurement object are overlapped by the union of concurrent measurement gaps.

- When part of the SMTC occasions of this intra-frequency measurement object are overlapped by the union of concurrent measurement gaps.

- Otherwise, for a UE not supporting concurrent gaps or if concurrent gaps are not configured:

- When none of the SMTC occasions of this intra-frequency measurement object are overlapped by the measurement gaps.

- SSB-based intra-frequency measurement with no measurement gap when part of the SMTC occasions of this intra-frequency measurement object are overlapped by the measurement gaps.

The intra-frequency measurement requirements in 9.2.6 applies for SSB based intra-frequency measurements without measurement gaps if the intra-frequency measurement object satisfies one of the following conditions,

- For a UE supporting concurrent gaps and when concurrent gaps are configured:

- When all of the SMTC occasions of this intra-frequency measurement object are overlapped with the associated measurement gap in the concurrent measurement gaps, or

- part of the SMTC occasions of this intra-frequency measurement object are overlapped with the associated measurement gap and all the SMTC occasions of this intra-frequency measurement object are overlapped with the union of all the measurement gaps in concurrent measurement gaps.

- Otherwise, for a UE not supporting concurrent gaps or if concurrent gaps are not configured:

- When all of the SMTC occasions of this intra-frequency measurement object are overlapped with the measurement gap, or

- SSB-based intra-frequency measurement object with NCSG, when UE supporting nr-NeedForGapNCSG-reporting-r17 and indicating ‘ncsg’ in NeedForGapNCSG-InfoNR for intra-frequency measurement but measurement gap is configured.

The intra-frequency measurement requirements in 9.2.7 applies for SSB based intra-frequency measurements without measurement gaps if the intra-frequency measurement object satisfies one of the following conditions,

- Wwhen all of the SMTC occasions of this intra-frequency measurement object are overlapped by the NCSG;

- SSB-based intra-frequency measurement object with NCSG corresponding to an activated serving cell (in non-dormancy);

- SSB-based intra-frequency measurement object corresponding to a deactivated serving cell or to an activated serving cell in dormancy, when all or part of the SMTC occasions of this intra-frequency measurement object are overlapped by the NCSG.

**--------------------END OF CHANGES--------------------------**

**------------------------------------ CHANGE --------------------------------**

### 9.2.5 Intrafrequency measurements without measurement gaps

#### 9.2.5.1 Intrafrequency cell identification

The UE shall be able to identify a new detectable intra-frequency cell within Tidentify\_intra\_without\_index if the UE is not indicated to report SSB based RRM measurement result with the associated SSB index(*reportQuantityRsIndexes* or *maxNrofRSIndexesToReport* is not configured), or the UE is indicated that the neighbour cell is synchronous with the serving cell (*deriveSSB-IndexFromCell* is enabled). Otherwise UE shall be able to identify a new detectable intra frequency cell within Tidentify\_intra\_with\_index. The UE shall be able to identify a new detectable intra frequency SS block of an already detected cell within Tidentify\_intra\_without\_index. It is assumed that *deriveSSB-IndexFromCell* is always enabled for FR1 TDD and FR2 with SCS smaller or equal to 480 kHz.

Tidentify\_intra\_without\_index = (TPSS/SSS\_sync\_intra + T SSB\_measurement\_period\_intra) ms

Tidentify\_intra\_with\_index = (TPSS/SSS\_sync\_intra + T SSB\_measurement\_period\_intra + TSSB\_time\_index\_intra) ms

Where:

 TPSS/SSS\_sync\_intra: it is the time period used in PSS/SSS detection given in table 9.2.5.1-1, 9.2.5.1-2, 9.2.5.1-4 (deactivated SCell) or 9.2.5.1-5 (deactivated SCell) or 9.2.5.1-9 (deactivated SCell) or 9.2.5.1-11 or 9.2.5.1-12 (deactivated PSCell) or 9.2.5.1-13 (deactivated PSCell).

- For UE supporting power class 6 with *highSpeedMeasFlagFR2-r17* configured, if SMTC <= 40ms, TPSS/SSS\_sync\_intra is given in Table 9.2.5.1-11; otherwise, TPSS/SSS\_sync\_intra is given in Table 9.2.5.1-2.

 TSSB\_time\_index\_intra: it is the time period used to acquire the index of the SSB being measured given in table 9.2.5.1-3, 9.2.5.1-15 (FR2-2), 9.2.5.1-6 (deactivated SCell), 9.2.5.1-10(deactivated SCell) or 9.2.5.1-14 (deactivated PSCell).

 T SSB\_measurement\_period\_intra: equal to a measurement period of SSB based measurement given in table 9.2.5.2-1, table 9.2.5.2-2 table 9.2.5.2-3 (deactivated SCell), 9.2.5.2-4(deactivated SCell), 9.2.5.2-5 or 9.2.5.2-6(deactivated SCell), 9.2.5.2-8(deactivated PSCell) or 9.2.5.2-9(deactivated PSCell).

- For UE supporting power class 6 with *highSpeedMeasFlagFR2-r17* configured, if SMTC <= 40ms, TSSB\_measurement\_period\_intra is given in Table 9.2.5.2-7; otherwise, T SSB\_measurement\_period\_intra is given in Table 9.2.5.2-2.

 CSSFintra: it is a carrier specific scaling factor and is determined according to CSSFoutside\_gap,i in clause 9.1.5.1 for measurement conducted outside measurement gaps, i.e. when intra-frequency SMTC is fully non overlapping or partially overlapping with GAP.

 For a UE that supports Pre-MG, an SMTC occasion is only considered to be overlapped by Pre-MG if the Pre-MG is activated.

 if the high layer in TS 38.331 [2] signalling of *smtc2* is configured, the assumed periodicity of intra-frequency SMTC occasions corresponds to the value of higher layer parameter *smtc2*; Otherwise the assumed periodicity of intra-frequency SMTC occasions corresponds to the value of higher layer parameter *smtc1*.

 Mpss/sss\_sync\_w/o\_gaps: For a UE supporting FR2-1 power class 1 or 5, Mpss/sss\_sync\_w/o\_gaps =40. For a UE supporting power class 2, Mpss/sss\_sync\_w/o\_gaps =24. For a UE supporting FR2-1 power class 3, Mpss/sss\_sync\_w/o\_gaps =24. For a UE supporting FR2-1 power class 4, Mpss/sss\_sync\_w/o\_gaps =24. For a UE supporting FR2-2 power class 1, Mpss/sss\_sync\_w/o\_gaps = 60. For a UE supporting FR2-2 power class 2, Mpss/sss\_sync\_w/o\_gaps = 36. For a UE supporting FR2-2 power class 3, Mpss/sss\_sync\_w/o\_gaps = 36.

 Mmeas\_period\_w/o\_gaps: For a UE supporting FR2-1 power class 1 or 5, Mmeas\_period\_w/o\_gaps =40. For a UE supporting FR2-1 power class 2, Mmeas\_period\_w/o\_gaps =24. For a UE supporting FR2-1 power class 3, Mmeas\_period\_w/o\_gaps =24. For a UE supporting power class 4, Mmeas\_period\_w/o\_gaps =24. For a UE supporting FR2-2 power class 1, Mmeas\_period\_w/o\_gaps = 60. For a UE supporting FR2-2 power class 2, Mmeas\_period\_w/o\_gaps = 36. For a UE supporting FR2-2 power class 3, Mmeas\_period\_w/o\_gaps = 36.

MSSB\_index\_intra: For a UE supporting FR2-2 power class 1, MSSB\_index\_intra = 72 samples. For a UE supporting FR2-2 power class 2, MSSB\_index\_intra = 48 samples. For a UE supporting FR2 power class 3, MSSB\_index\_intra = 48 samples.

When UE supports *concurrentMeasGap-r17* and is configured with concurrent measurement gaps,

 Kp is the scaling factor for an SSB frequency layer to be measured without measurement gaps. Kp = Ntotal / Navailable, where Navailable and Ntotal are calculated as follows:

- For a window W of duration max(SMTC period, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE measurement gap and/or per-FR measurement gap within the same FR as the SSB frequency layer, and starting from the beginning of any SMTC occasion:

- Ntotal is the total number of SMTC occasions within the window, including those overlapped with measurement gap occasions within the window, and

- Navailable is the number of SMTC occasions that are not overlapped with any non-dropped MG occasion within the window W, after accounting for measurement gap collisions by applying the measurement gap collision rule in section 9.1.8.3.

 Kp = 1 when Navailable = 0.

Otherwise, when UE is not configured with or UE does not support concurrent measurement gaps:

 When intra-frequency SMTC is fully non overlapping with GAP, Kp=1

 When intra-frequency SMTC is partially overlapping with measurement gaps, Kp = 1/(1- (SMTC period /MGRP)), where SMTC period < MGRP. When intra-frequency SMTC is partially overlapping with NCSG, Kp = 1/(1- (SMTC period /VIRP)), where SMTC period < VIRP. For calculation of Kp, if the high layer signalling (TS 38.331 [2]) of *smtc2* is configured, for cells indicated in the *pci-List* parameter in *smtc2*, the SMTC periodicity corresponds to the value of higher layer parameter *smtc2*; for the other cells, the SMTC periodicity corresponds to the value of higher layer parameter *smtc1.*

If the higher layer signaling in TS38.331 [2] signalling of *smtc2* is present and smtc1 is fully overlapping with measurement gaps and smtc2 is partially overlapping with measurement gaps, requirements are not specified for Tidentify\_intra\_without\_index or Tidentify\_intra\_with\_index.

 For FR2,

 Klayer1\_measurement=1,

- if all of the reference signals configured for RLM, BFD, CBD or L1-RSRP for beam reporting on any FR2 serving frequency in the same band outside measurement gap are not fully overlapped by intra-frequency SMTC occasions, or

- if all of the reference signal configured for RLM, BFD, CBD or L1-RSRP for beam reporting on any FR2 serving frequency in the same band outside measurement gap and fully-overlapped by intra-frequency SMTC occasions are not overlapped with any of the SSB symbols and the RSSI symbols, and 1 symbol before each consecutive SSB symbols and the RSSI symbols, and 1 symbol after each consecutive SSB symbols and the RSSI symbols, given that *SSB-ToMeasure* and *SS-RSSI-Measurement* are configured, where SSB symbols are indicated by the union set of SSB-ToMeasure from all the configured measurement objects on the same serving carrier which can be merged.and RSSI symbols are indicated by *SS-RSSI-Measurement*;

 Klayer1\_measurement=1.5, otherwise.

 If the above-mentioned reference signal configured for L1-RSRP measurement is aperiodic CSI-RS resource, longer cell identification delay would be expected.

 If MCG DRX is in use, cell identification requirements for intra-frequency measurement in MCG specified in Table 9.2.5.1-1, Table 9.2.5.1-2, Table 9.2.5.1-3, Table 9.2.5.1-4, Table 9.2.5.1-5 and Table 9.2.5.1-6 shall depend on the MCG DRX cycle. If SCG DRX is in use, cell identification requirements for intra-frequency measurement in SCG specified in Table 9.2.5.1-1, Table 9.2.5.1-2, Table 9.2.5.1-3, Table 9.2.5.1-4, Table 9.2.5.1-5, Table 9.2.5.1-6, Table 9.2.5.1-12, Table 9.2.5.1-13 and Table 9.2.5.1-14 shall depend on the SCG DRX cycle. Otherwise, the requirements for when DRX is not in use shall apply.

Table 9.2.5.1-1: Time period for PSS/SSS detection, (Frequency range FR1)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | max( 600ms, ceil( 5 x Kp) x SMTC period )Note 1 x CSSFintra |
| DRX cycle≤ 320ms | max( 600ms, ceil(M2 Note 2x 5 x Kp) x max(SMTC period,DRX cycle)) x CSSFintra |
| DRX cycle>320ms | ceil(5 x Kp) x DRX cycle x CSSFintra |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: When *highSpeedMeasFlag-r16* is not configured, M2 = 1.5; When *highSpeedMeasFlag-r16* is configured, M2 = 1.5 if SMTC periodicity > 40 ms;,otherwise M2=1.NOTE 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16* on measurements of the primary component carrier and do not apply to measurements of a secondary component carrier with active SCell.NOTE 4: When *highSpeedMeasCA-Scell-r17* is configured and UE supports *measurementEnhancementCA-r17*, M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2=1. |

Table 9.2.5.1-2: Time period for PSS/SSS detection, (Frequency range FR2)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | max(600ms, ceil(Mpss/sss\_sync\_w/o\_gaps x KFR x Kp x Klayer1\_measurement)x SMTC period)Note 1 x CSSFintra |
| DRX cycle≤ 320ms | max(600ms, ceil(1.5 x Mpss/sss\_sync\_w/o\_gaps x KFR x Kp x Klayer1\_measurement)x max(SMTC period,DRX cycle)) x CSSFintra |
| DRX cycle>320ms | ceil(Mpss/sss\_sync\_w/o\_gaps x KFR x Kp x Klayer1\_measurement) x DRX cycle x CSSFintra |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: KFR is a scaling factor depending on the frequency range and the SSB SCS. For FR2-1, KFR = 1. For FR2-2: KFR = 1 if the SCS of the SSB of the cell being detected is 120 kHz, KFR = 2 if the SCS of the SSB of the cell being detected is 480 kHz, and KFR = 3 if the SCS of the SSB of the cell being detected is 960 kHz. |

Table 9.2.5.1-3: Time period for time index detection (FR1)

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_intra |
| No DRX | max(120ms, ceil( 3 x Kp )x SMTC period)Note 1 x CSSFintra |
| DRX cycle≤ 320ms | max(120ms, ceil (M2 Note 2 x 3 x Kp) x max(SMTC period,DRX cycle)) x CSSFintra |
| DRX cycle>320ms | Ceil(3 x Kp) x DRX cycle x CSSFintra |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: When *highSpeedMeasFlag-r16* is not configured, M2 = 1.5; When *highSpeedMeasFlag-r16* is configured, M2 = 1.5 if SMTC periodicity > 40 ms;,otherwise M2=1NOTE 3: When *highSpeedMeasFlag-r16* is configured, the requirements apply only to UE supporting either *measurementEnhancement-r16* or *intraNR-MeasurementEnhancement-r16* on measurements of the primary component carrier and do not apply to measurements of a secondary component carrier with active SCell.NOTE 4: When *highSpeedMeasCA-Scell-r17* is configured and UE supports *measurementEnhancementCA-r17*, M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2=1 |

Table 9.2.5.1-4: Time period for PSS/SSS detection, deactivated SCell (FR1)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | Ceil(5 x Kp) x measCycleSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(5 x Kp) x max(measCycleSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(5 x Kp) x max(measCycleSCell, DRX cycle) x CSSFintra |
| NOTE 1: The requirements also apply to deactivated SCG SCell. |

Table 9.2.5.1-5: Time period for PSS/SSS detection, deactivated SCell (FR2)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x measCycleSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x max(measCycleSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x max(measCycleSCell, DRX cycle) x CSSFintra |
| NOTE 1: The requirements also apply to deactivated SCG SCell. |

Table 9.2.5.1-6: Time period for time index detection, deactivated SCell (FR1)

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_intra |
| No DRX | Ceil(3 x Kp) x measCycleSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(3 x Kp) x max(measCycleSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(3 x Kp) x max(measCycleSCell, DRX cycle) x CSSFintra |
| NOTE 1: The requirements also apply to deactivated SCG SCell. |

Table 9.2.5.1-7: Void

Table 9.2.5.1-8: Void

Table 9.2.5.1-9: Time period for PSS/SSS detection, deactivated SCell (FR1), when *highSpeedMeasCA-Scell-r17* is configured

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | Ceil(5 x Kp) x measCycleSCell x CSSFintra |
| DRX cycle≤ 320ms |  Ceil(5 x Kp) x max(measCycleSCell, M2 Note 1xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(5 x Kp) x max(measCycleSCell, DRX cycle) x CSSFintra |
| NOTE 1: M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2=1 |

Table 9.2.5.1-10: Time period for time index detection, deactivated SCell (FR1)，when *highSpeedMeasCA-Scell-r17* is configured

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_intra |
| No DRX | Ceil(3 x Kp) x measCycleSCell x CSSFintra |
| DRX cycle≤ 320ms |  Ceil(3 x Kp) x max(measCycleSCell, M2 Note 1xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(3 x Kp)x max(measCycleSCell, DRX cycle) x CSSFintra |
| NOTE 1: M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2=1 |

Table 9.2.5.1-11: Time period for PSS/SSS detection when *highSpeedMeasFlagFR2-r17* is configured, (Frequency range FR2) when SMTC period <= 40ms

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | max(600ms, ceil(M1Note 2 x Kp x Klayer1\_measurement)x SMTC period)Note 1 x CSSFintra |
| DRX cycle≤ 80ms | max(600ms, ceil(M1Note 2 x Kp x Klayer1\_measurement)x max(SMTC period,DRX cycle)) x CSSFintra |
| 80ms< DRX cycle≤ 320ms | ceil(1.5x Mpss/sss\_sync\_w/o\_gaps Note 3 x Kp x Klayer1\_measurement)x max(SMTC period,DRX cycle) x CSSFintra |
| DRX cycle>320ms | ceil(Mpss/sss\_sync\_w/o\_gaps Note 3 x Kp x Klayer1\_measurement) x DRX cycle x CSSFintra |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: For UE supporting power class 6, M1= 6 if *highSpeedMeasFlagFR2-r17* = set1 or M1= 18 if *highSpeedMeasFlagFR2-r17* = set2NOTE 3: Void |

Table 9.2.5.1-12: Time period for PSS/SSS detection, deactivated PSCell (FR1)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | Ceil(5 x Kp) x measCyclePSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(5 x Kp) x max(measCyclePSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(5 x Kp) x max(measCyclePSCell, DRX cycle) x CSSFintra |

Table 9.2.5.1-13: Time period for PSS/SSS detection, deactivated PSCell (FR2)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_intra |
| No DRX | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x measCyclePSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x max(measCyclePSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(Mpss/sss\_sync\_w/o\_gaps x Kp) x max(measCyclePSCell, DRX cycle) x CSSFintra |

Table 9.2.5.1-14: Time period for time index detection, deactivated PSCell (FR1)

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_intra |
| No DRX | Ceil(3 x Kp) x measCyclePSCell x CSSFintra |
| DRX cycle≤ 320ms | Ceil(3 x Kp) x max(measCyclePSCell, 1.5xDRX cycle) x CSSFintra |
| DRX cycle> 320ms | Ceil(3 x Kp) x max(measCyclePSCell, DRX cycle) x CSSFintra |

Table 9.2.5.1-15: Time period for time index detection (Frequency range FR2-2)

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_intra |
| No DRX | max(200ms, ceil(MSSB\_index\_intra x Kp x SMTC period) x CSSFintra |
| DRX cycle≤ 320ms | max(200ms, ceil(1.5 x MSSB\_index\_intra x Kp) x max(SMTC period, DRX cycle) x CSSFintra) |
| DRX cycle>320ms | Ceil(MSSB\_index\_intra x Kp )x DRX cycle x CSSFintra |

**--------------------END OF CHANGES--------------------------**

**------------------------------------ CHANGE --------------------------------**

## 9.3 NR inter-frequency measurements

### 9.3.1 Introduction

A measurement is defined as an SSB based inter-frequency measurement provided it is not defined as an intra-frequency measurement according to clause 9.2.

The UE shall be able to identify new inter-frequency cells and perform SS-RSRP, SS-RSRQ, and SS-SINR measurements of identified inter-frequency cells if carrier frequency information is provided by PCell or PSCell, even if no explicit neighbour list with physical layer cell identities is provided.

A measurement is defined as an inter-frequency SSB based measurements without measurement gaps (either legacy measurement gap or NCSG) in active BWP, for UE capable of *interFrequencyMeas-NoGap* provided that

- the UE supports *interFrequencyMeas-Nogap-r16* [15], and

- the SSB is completely contained in the active BWP of the UE.

Besides the conditions listed above, for UE supporting *nr-NeedForGapNCSG-reporting-r17* and indicating *NeedForGapNCSG-InfoNR* for inter-frequency measurement,

- An inter-frequency SSB measurement is defined as measurement without gap if

- the UE indicates ‘nogap-noncsg’ via *NeedForGapNCSG-InfoNR* for the inter-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE

- An inter-frequency SSB measurement is defined as measurement with NCSG if

- the UE indicates ‘ncsg’ via *NeedForGapNCSG-InfoNR* for the inter-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE

- An inter-frequency SSB measurement is defined as measurement with gap if

- the UE indicates ‘gap’ via *NeedForGapNCSG-InfoNR* for the inter-frequency measurement, and

- the SSB is not completely contained in the active BWP of the UE

- For inter-frequency SSB based measurements with NCSG, UE may cause scheduling restriction as specified in clause 9.3.10.3.

For inter-frequency SSB based measurements without measurement gaps, UE may cause scheduling restriction as specified in clause 9.3.5.3.

Note: Non-CA capable UE is not expected to indicate support of *interFrequencyMeas-Nogap-r16* [15].

SSB based measurements are configured along with a measurement timing configuration (SMTC) per carrier, which provides periodicity, duration and offset information on a window of up to 5ms where the measurements on the configured inter-frequency carrier are to be performed. For inter-frequency connected mode measurements, one measurement window periodicity may be configured per inter-frequency measurement object.

When measurement gaps are needed, the UE is not expected to detect SSB and measure RSSI of RSRQ on an inter-frequency measurement object which start earlier than the gap starting time + switching time, nor detect SSB and measure RSSI of RSRQ which ends later than the gap end – switching time. When the inter-frequency cells are in FR2 and the per-FR gap is configured to the UE in EN-DC, SA NR, NE-DC and NR-DC, or the serving cells are in FR2, the inter-frequency cells are in FR2 and the per-UE gap is configured to the UE in SA NR and NR-DC, the switching time is 0.25ms. Otherwise the switching time is 0.5ms.

The requirements in this clause shall also apply, when the UE is configured to perform SRS carrier based switching and using measurement gaps.

Longer measurement period would be expected during the period Tidentify\_CGI when the UE is requested to decode an NR CGI.

The measurement reporting delay can be longer for the measurement reporting requirements in this clause when IDC autonomous denial is configured.

The inter-frequency measurement requirements in 9.3.4 and 9.3.5 applies if the inter-frequency measurement object satisfies one of the following conditions,

- SSB-based inter-frequency measurement object with measurement gap.

- SSB-based inter-frequency measurement object without measurement gap for UE capable of *interFrequencyMeas-NoGap*, when

- all of the SMTC occasions of this inter-frequency measurement object are overlapped with the measurement gap or associated measurement gap in concurrent measurement gaps, or

- part of the SMTC occasions of this inter-frequency measurement object are overlapped with the associated measurement gap and all the SMTC occasions of this inter-frequency measurement object are overlapped with the union of all the measurement gaps in concurrent measurement gaps, or

- part of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap or associated measurement gap in concurrent measurement gaps and the flag *interFrequencyConfig-NoGap-r16* is not configured by the Network.

The inter-frequency measurement requirements in 9.3.10 applies if the inter-frequency measurement object satisfies one of the following conditions,

- SSB-based inter-frequency measurement object without measurement gap, when all of the SMTC occasions of this inter-frequency measurement object are overlapped by the NCSG;

- SSB-based inter-frequency measurement object with NCSG.

The inter-frequency measurement requirements in 9.3.9 applies if the inter-frequency measurement object satisfies one of the following conditions,

- SSB-based inter-frequency measurement with no measurement gap, when none of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap or the union of concurrent measurement gaps, if UE supports *interFrequencyMeas-NoGap-r16* and the flag *interFrequencyConfig-NoGap-r16* is configured by the Network.

- SSB-based inter-frequency measurement with no measurement gap, when part of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap or the union of concurrent measurement gaps, if UE supports *interFrequencyMeas-NoGap-r16* and the flag *interFrequencyConfig-NoGap-r16* is configured by the Network.

**--------------------END OF CHANGES--------------------------**

**------------------------------------ CHANGE --------------------------------**

### 9.3.9 Inter frequency measurements without measurement gaps

#### 9.3.9.1 Inter frequency Cell identification

UE satisfying the applicability conditions specified in 9.3.1 on the requirement in this clause shall be able to identify a new detectable inter frequency cell within Tidentify\_inter\_without\_index if UE is not indicated to report SSB based RRM measurement result with the associated SSB index (*reportQuantityRsIndexes* or *maxNrofRSIndexesToReport* is not configured) or *deriveSSB-IndexFromCellInter-r17* is configured for the FR1 and FR2-1 target frequency layers and and UE supporting *deriveSSB-IndexFromCellInterNon-NCSG-r17*. Otherwise UE shall be able to identify a new detectable inter frequency cell within Tidentify\_inter\_with\_index. The UE shall be able to identify a new detectable inter frequency SS block of an already detected cell within Tidentify\_inter\_without\_index.

- For inter-frequency SSB based measurements without measurement gaps in active BWP, it is assumed that when UE performs inter-frequency measurements without measurement gaps in a TDD bands on FR1 and FR2, SFN and frame boundary across serving cell and inter-frequency neighbor cells is aligned

 Tidentify\_inter\_without\_index = (TPSS/SSS\_sync\_inter + T SSB\_measurement\_period\_inter) ms

 Tidentify\_inter\_with\_index = (TPSS/SSS\_sync\_inter + T SSB\_measurement\_period\_inter + TSSB\_time\_index\_inter) ms

Where:

 TPSS/SSS\_sync\_inter: it is the time period used in PSS/SSS detection given in table 9.3.9.1-1 and table 9.3.9.1-2.

 TSSB\_time\_index\_inter: it is the time period used to acquire the index of the SSB being measured given in table 9.3.9.1-3 and table 9.3.9.1-4.

 T SSB\_measurement\_period\_inter: equal to a measurement period of SSB based measurement given in table 9.3.9.2-1, table 9.3.9.2-2, table 9.3.9.2-3 and table 9.3.9.2-3a when *highSpeedMeasInterFreq-r17* is configured and UE supports measurementEnhancementInterFreq-r17, and table 9.3.9.2-4 when *highSpeedMeasFlagFR2-r17* is configured and UE supports [*measurementEnhancementCAInterFreqFR2-r18*].

- For UE supporting power class 6 and [*measurementEnhancementCAInterFreqFR2-r18*] with *highSpeedMeasFlagFR2-r17* configured, if SMTC <= 40ms, TSSB\_measurement\_period\_inter is given in Table 9.3.9.2-x; otherwise, TSSB\_measurement\_period\_inter is given in Table 9.3.9.2-2.

 CSSFinter: it is a carrier specific scaling factor and is determined according to CSSFoutside\_gap,i in clause 9.1.5.1 for measurement conducted outside measurement gaps or NCSG, i.e. when interfrequency SMTC is fully non overlapping or partially overlapping with measurement gaps.

For inter-frequency SSB based measurements without measurement gaps in active BWP

 Mpss/sss\_sync\_inter: For a UE supporting FR2-1 power class 1 or 5, Mpss/sss\_sync\_inter = 40. For a UE supporting FR2-1 power class 2, Mpss/sss\_sync\_inter = 24. For a UE supporting FR2-1 power class 3, Mpss/sss\_sync\_inter = 24. For a UE supporting FR2-1 power class 4, Mpss/sss\_sync = 24. For a UE supporting FR2-2 power class 1, Mpss/sss\_sync\_inter = 60. For a UE supporting FR2-2 power class 2, Mpss/sss\_sync\_inter = 36. For a UE supporting FR2-2 power class 3, Mpss/sss\_sync\_inter = 36. For FR1, Mpss/sss\_sync\_inter = 5.

 MSSB\_index\_inter: For a UE supporting FR2-2 power class 1, MSSB\_index\_inter = 72. For a UE supporting FR2-2 power class 2, MSSB\_index\_inter = 48. For a UE supporting FR2-2 power class 3, MSSB\_index\_inter = 48. For FR1, MSSB\_index\_inter = 3.

 Mmeas\_period\_inter: For a UE supporting FR2-1 power class 1 or 5, Mmeas\_period\_inter = 40. For a vehicle mounted UE supporting FR2-1 power class 2, Mpss/sss\_sync\_inter=24. For a UE supporting FR2-1 power class 3, Mmeas\_period\_inter = 24. For a UE supporting FR2-1 power class 4, Mmeas\_period\_inter = 24. For a UE supporting FR2-2 power class 1, Mmeas\_period\_inter = 60. For a UE supporting FR2-2 power class 2, Mpss/sss\_sync\_inter = 36. For a UE supporting FR2-2 power class 3, Mmeas\_period\_inter = 36. For FR1, Mmeas\_period\_inter = 5.

If the UE indicates ‘nogap-noncsg’ via *NeedForGapNCSG-InfoNR* for the inter-frequency measurement,

 Mpss/sss\_sync\_inter: For a UE supporting FR2-1 power class 1 or 5, Mpss/sss\_sync\_inter = 64 samples. For a UE supporting FR2-1 power class 2, Mpss/sss\_sync\_inter = 40 samples. For a UE supporting FR2-1 power class 3, Mpss/sss\_sync\_inter = 40 samples. For a UE supporting FR2-1 power class 4, Mpss/sss\_sync\_inter = 40 samples. For a UE supporting FR2-2 power class 1, Mpss/sss\_sync\_inter = 96. For a UE supporting FR2-2 power class 2, Mpss/sss\_sync\_inter = 60. For a UE supporting FR2-2 power class 3, Mpss/sss\_sync\_inter = 60. For FR1, Mpss/sss\_sync\_inter = 8.

 MSSB\_index\_inter: For a UE supporting FR2-1 power class 1 or 5, MSSB\_index\_inter = 40 samples. For a UE supporting FR2 power class 2, MSSB\_index\_inter = 24 samples. For a UE supporting FR2-1 power class 3, MSSB\_index\_inter = 24 samples. For a UE supporting FR2-1 power class 4, MSSB\_index\_inter = 24 samples. For a UE supporting FR2-2 power class 2 or 3, MSSB\_index\_inter = 48 samples. For a UE supporting FR2 power class 1, MSSB\_index\_inter = 72 samples. For FR1, MSSB\_index\_inter = 3.

 Mmeas\_period\_inter: For a UE supporting FR2-1 power class 1 or 5, Mmeas\_period\_inter =64. For a UE supporting FR2-1 power class 2, Mmeas\_period\_inter=40. For a UE supporting FR2-1 power class 3, Mmeas\_period\_inter =40. For a UE supporting FR2-1 power class 4, Mmeas\_period\_inter = 40. For a UE supporting FR2-2 power class 1, Mmeas\_period\_inter = 96. For a UE supporting FR2-2 power class 2, Mmeas\_period\_inter = 60. For a UE supporting FR2-2 power class 3, Mmeas\_period\_inter = 60. For FR1, Mmeas\_period\_inter = 8.When UE supports *concurrentMeasGap-r17* and is configured with concurrent measurement gaps,

Kp is a scaling factor for an SSB frequency layer to be measured without measurement gaps. Kp = Ntotal / Navailable, where Navailable and Ntotal are calculated as follows:

 For a window W of duration max(SMTC period, MGRP\_max), where MGRP max is the maximum MGRP across all configured per-UE MG and per-FR MG within the same FR as the SSB frequency layer, and starting at the beginning of any SMTC occasion:

 Ntotal is the total number of SMTC occasions within the window, including those overlapped with MG occasions within the window, and

 Navailable is the number of SMTC occasions that are not overlapped with any non-dropped MG occasion within the window W, after accounting for MG collisions by applying the selected gap collision rule provided that concurrent measurement gaps are configured.

 Kp = 1 when Navailable = 0.

Otherwise, when UE is not configured with or UE does not support concurrent measurement gaps:

 When interfrequency SMTC is fully non overlapping with measurement gaps or NCSG, or interfrequency SMTC is fully overlapping with MGs or NCSG, Kp =1.

 When interfrequency SMTC is partially overlapping with measurement gaps, Kp = 1/(1- (SMTC period /MGRP)), where SMTC period < MGRP. When inter-frequency SMTC is partially overlapping with NCSG, Kp = 1/(1- (SMTC period /VIRP)), where SMTC period < VIRP.

For FR2,

 Klayer1\_measurement=1,

- if all of the reference signals configured for RLM, BFD, CBD or L1-RSRP for beam reporting on any FR2 serving frequency in the same band outside measurement gap are not fully overlapped by inter-frequency SMTC occasions, or

- if all of the reference signal configured for RLM, BFD, CBD or L1-RSRP for beam reporting on any FR2 serving frequency in the same band outside measurement gap and fully-overlapped by inter-frequency SMTC occasions are not overlapped with any of the SSB symbols and the RSSI symbols, and 1 symbol before each consecutive SSB symbols and the RSSI symbols, and 1 symbol after each consecutive SSB symbols and the RSSI symbols, given that *SSB-ToMeasure* and *SS-RSSI-Measurement* are configured, where SSB symbols are indicated by *SSB-ToMeasure* and RSSI symbols are indicated by *SS-RSSI-Measurement*;

 Klayer1\_measurement=1.5, otherwise.

 If the above-mentioned reference signal configured for L1-RSRP measurement is aperiodic CSI-RS resource, longer cell identification delay would be expected.

For calculation of Kp, if the high layer signalling (TS 38.331 [2]) of *smtc2* is configured, for cells indicated in the *pci-List* parameter in *smtc2*, the SMTC periodicity corresponds to the value of higher layer parameter *smtc2*; for the other cells, the SMTC periodicity corresponds to the value of higher layer parameter *smtc1.*

Table 9.3.9.1-1: Time period for PSS/SSS detection, (FR1)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_inter |
| No DRX | max( 600ms, ceil(Mpss/sss\_sync\_inter x Kp) x SMTC period )Note 1 x CSSFinter |
| DRX cycle≤ 320ms | max( 600ms, ceil(M2x Mpss/sss\_sync\_inter x Kp) x max(SMTC period,DRX cycle)) x CSSFinter |
| DRX cycle>320ms | ceil(Mpss/sss\_sync\_inter x Kp) x DRX cycle x CSSFinter |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: VoidNOTE 3: When *highSpeedMeasInterFreq-r17* is not configured, M2 = 1.5; When *highSpeedMeasInterFreq-r17* is configured, M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2 = 1 |

Table 9.3.9.1-2: Time period for PSS/SSS detection, (FR2)

|  |  |
| --- | --- |
| DRX cycle | TPSS/SSS\_sync\_inter |
| No DRX | max(600ms, ceil(Mpss/sss\_sync\_inter x Kp x Klayer1\_measurement)x SMTC period)Note 1 x CSSFinter |
| DRX cycle≤ 320ms | max(600ms, ceil(1.5 x Mpss/sss\_sync\_inter x Kp x Klayer1\_measurement)x max(SMTC period,DRX cycle)) x CSSFinter |
| DRX cycle>320ms | ceil(Mpss/sss\_sync\_inter x Kp x Klayer1\_measurement) x DRX cycle x CSSFinter |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: Void |

Table 9.3.9.1-3: Time period for time index detection (FR1)

|  |  |
| --- | --- |
| DRX cycle | TSSB\_time\_index\_inter |
| No DRX | max(120ms, ceil(MSSB\_index\_inter x Kp )x SMTC period)Note 1 x CSSFinter |
| DRX cycle≤ 320ms | max(120ms, ceil (M2 x MSSB\_index\_inter x Kp) x max(SMTC period,DRX cycle)) x CSSFinter |
| DRX cycle>320ms | Ceil(MSSB\_index\_inter x Kp) x DRX cycle x CSSFinter |
| NOTE 1: If different SMTC periodicities are configured for different cells, the SMTC period in the requirement is the one used by the cell being identifiedNOTE 2: VoidNOTE 3: When *highSpeedMeasInterFreq-r17* is not configured, M2 = 1.5; When *highSpeedMeasInterFreq-r17* is configured, M2 = 1.5 if SMTC periodicity > 40 ms; otherwise M2 = 1 |

Table 9.3.9.1-4: Time period for time index detection (FR2)

|  |  |
| --- | --- |
| **Condition NOTE1,2** | **TSSB\_time\_index\_inter** |
| No DRX | Max(200ms, Ceil(MSSB\_index\_inter x Kp)× SMTC period) × CSSFinter |
| DRX cycle ≤ 320ms | Max(200ms, Ceil(1.5 × MSSB\_index\_inter x Kp) × Max(SMTC period, DRX cycle)) × CSSFinter |
| DRX cycle > 320ms | Ceil(MSSB\_index\_inter x Kp) × DRX cycle × CSSFinter |
| NOTE 1: DRX or non DRX requirements apply according to the conditions described in clause 3.6.1NOTE 2: Kp is applicable for UE supporting *concurrentMeasGap-r17* |

**--------------------END OF CHANGES--------------------------**