**3GPP TSG-RAN WG4 Meeting #109 R4-2321838**

**Chicago, USA, 13 - 17 November 2023**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **1918** | **rev** | **1** | **Current version:** | **18.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | big CR 38.101-1 new combinations Rel-18 NR Inter-band CA/DC for y bands DL with x bands UL (y=4,5,6, x=1,2) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_yBDL\_xBUL | | | | |  | ***Date:*** | | | 2023-11-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding new combinations and configurtions | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Implemented draft CRs endorsed in meeting #108-bis:  Draft CR R4-2317679:  CA\_n48A-n66(2A)-n71A-n77A  Draft CR R4-2317703:  CA\_n1A-n3A-n7A-n75A  CA\_n1A-n3A-n7A-n78A  CA\_n1A-n3A-n75A-n78A  CA\_n1A-n7A-n75A-n78A  CA\_n3A-n7A-n75A-n78A  CA\_n1A-n3A-n7A-n75A-n78A  Draft CR R4-2316192:  CA\_n1(2A)-n3A-n7A-n38A  CA\_n1A-n3B-n7A-n38A  CA\_n1(2A)-n3B-n7A-n38A  CA\_n1A-n3(2A)-n7A-n38A  CA\_n1(2A)-n3(2A)-n7A-n38A  Draft CR R4-2317696:  CA\_n1A-n3A-n40A-n105A  CA\_n1A-n7A-n40A-n105A  CA\_n1A-n7A-n78A-n105A  CA\_n7A-n40A-n78A-n105A  CA\_n3A-n7A-n40A-n105A  CA\_n3A-n7A-n78A-n105A  Draft CR R4-2315466:  CA\_n5A-n25A-n29A-n66A  Draft CR R4-2316763:  Replace n41 with n66 for CA\_n25A-n66A-n71(2A)-n77(2A) and CA\_n25A-n66A-n71B-n77(2A).  Implemented draft CRs endorsed in meeting #109:  Draft CR R4-2318541:  Cell borders are corrected, and missing ULs added, and other errors are corrected.  Draft CR R4-2318503:  CA\_n2A-n41A-n66A-n71A  CA\_n7A-n12A-n25A-n66A  CA\_n7A-n25A-n66A-n71A  Draft CR R4-2318803:  Add UL CA\_n77C configuration to follow DL inter band CA:  CA\_n2A-n5A-n48A-n77C  CA\_n2A-n5A-n66A-n77C  CA\_n2A-n48A-n66A-n77C  Draft CR R4-2321837:  The delta T with the following special constituted bands for 4, 5 and 6 bands NR inter-band CA configurations are corrected to “N/A”.  Draft CR R4-2321839:  CA\_n1A-n3A-n5A-n28A  CA\_n1A-n5A-n28A-n78A  CA\_n1A-n5A-n28A-n79A  CA\_n1A-n5A-n78A-n79A  CA\_n1A-n28A-n78A-n79A  CA\_n3A-n5A-n28A-n78A  CA\_n3A-n5A-n28A-n79A  CA\_n5A-n28A-n78A-n79A  CA\_n1A-n3A-n5A-n28A-n78A  CA\_n1A-n5A-n28A-n78A-n79A  Draft CR R4-2319674:  CA\_n25A-n41(3A)-n66A-n71A  CA\_n25A-n41(A-C)-n66A-n71A  CA\_n25(2A)-n41(2A)-n66A-n77A  CA\_n25(2A)-n41A-n66A-n77(2A)  CA\_n25(2A)-n41C-n66A-n77A  CA\_n25A-n41(2A)-n66(2A)-n77A  CA\_n25A-n41A-n66(2A)-n77(2A)  CA\_n25A-n41C-n66(2A)-n77A  CA\_n25(2A)-n41(2A)-n71A-n77A  CA\_n25(2A)-n41A-n71A-n77(2A)  CA\_n25(2A)-n41C-n71A-n77A  CA\_n25A-n41(2A)-n71(2A)-n77A  CA\_n25A-n41(2A)-n71B-n77A  CA\_n25A-n41A-n71(2A)-n77(2A)  CA\_n25A-n41A-n71B-n77(2A)  CA\_n25A-n41C-n71(2A)-n77A  CA\_n25A-n41C-n71B-n77A  CA\_n25A-n41A-n77A-n85A  CA\_n41(2A)-n66(2A)-n71A-n77A  CA\_n41(2A)-n66A-n71(2A)-n77A  CA\_n41(2A)-n66A-n71B-n77A  CA\_n41A-n66(2A)-n71A-n77(2A)  CA\_n41A-n66A-n71(2A)-n77(2A)  CA\_n41A-n66A-n71B-n77(2A)  CA\_n41C-n66(2A)-n71A-n77A  CA\_n41C-n66A-n71(2A)-n77A  CA\_n41C-n66A-n71B-n77A  CA\_n41A-n66A-n77A-n85A  CA\_n25A-n41(2A)-n66A-n71A-n77A  CA\_n25A-n41A-n66A-n71A-n77(2A)  CA\_n25A-n41C-n66A-n71A-n77A  Draft CR R4-2319857:  CA\_n1A-n28A-n75A-n78A  Draft CR R4-2321858:  CA\_n1A-n3A-n40A-n78A-n105A  CA\_n1A-n7A-n40A-n78A-n105A  CA\_n3A-n7A-n40A-n78A-n105A  Draft CR R4-2321869:  CA\_n1A-n3A-n20A-n67A  CA\_n3A-n7A-n20A-n67A  CA\_n3A-n7A-n20A-n78A  CA\_n3A-n7A-n20A-n78(2A)  CA\_n3A-n20A-n67A-n78A  CA\_n3A-n20A-n67A-n78(2A)  CA\_n7A-n20A-n67A-n78A  CA\_n7A-n20A-n67A-n78(2A)  CA\_n3A-n7A-n20A-n67A-n78A  CA\_n3A-n7A-n20A-n67A-n78(2A)  DC\_n1A-n3A-n20A-n67A  DC\_n3A-n7A-n20A-n67A  DC\_n3A-n7A-n20A-n78A  DC\_n3A-n7A-n20A-n78(2A)  DC\_n3A-n20A-n67A-n78A  DC\_n3A-n20A-n67A-n78(2A)  DC\_n7A-n20A-n67A-n78A  DC\_n7A-n20A-n67A-n78(2A)  DC\_n3A-n7A-n20A-n67A-n78A  DC\_n3A-n7A-n20A-n67A-n78(2A)  Draft CR R4-2320316:  Correcting NR CA FR1 4 bands combinations  Draft CR R4-2319858:  CA\_n8A-n20A-n28A-n75A | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | New combinations and configurations are not included in the specification. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.2A.2.3, 5.2A.2.4, 5.5A.3.3, 5.5A.3.4, Table 5.5B.1-3, Table 5.5B.1-4, 6.2A.4.2.5, 6.2A.4.2.6, 7.3A.3.2.4 and 7.3A.3.2.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

#### 5.2A.2.3 Inter-band CA (four bands)

Table 5.2A.2.3-1: Inter-band CA operating bands involving FR1 (four bands)

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n1-n3-n5-n7 | n1, n3, n5, n7 |
| CA\_n1-n3-n5-n28 | n1, n3, n5, n28 |
| CA\_n1-n3-n5-n78 | n1, n3, n5, n78 |
| CA\_n1-n3-n7-n8 | n1, n3, n7, n8 |
| CA\_n1-n3-n7-n26 | n1, n3, n7, n26 |
| CA\_n1-n3-n7-n28 | n1, n3, n7, n28 |
| CA\_n1-n3-n7-n38 | n1, n3, n7, n38 |
| CA\_n1-n3-n7-n67 | n1, n3, n7, n67 |
| CA\_n1-n3-n7-n75 | n1, n3, n7, n75 |
| CA\_n1-n3-n7-n79 | n1, n3, n7, n79 |
| CA\_n1-n3-n7-n78 | n1, n3, n7, n78 |
| CA\_n1-n3-n8-n77 | n1, n3, n8, n77 |
| CA\_n1-n3-n8-n78 | n1, n3, n8, n78 |
| CA\_n1-n3-n18-n28 | n1, n3, n18, n28 |
| CA\_n1-n3-n18-n41 | n1, n3, n18, n41 |
| CA\_n1-n3-n18-n77 | n1, n3, n18, n77 |
| CA\_n1-n3-n20-n67 | n1, n3, n20, n67 |
| CA\_n1-n3-n26-n78 | n1, n3, n26, n78 |
| CA\_n1-n3-n28-n38 | n1, n3, n28, n38 |
| CA\_n1-n3-n28-n41 | n1, n3, n28, n41 |
| CA\_n1-n3-n28-n771 | n1, n3, n28, n77 |
| CA\_n1-n3-n28-n78 | n1, n3, n28, n78 |
| CA\_n1-n3-n28-n791 | n1, n3, n28, n79 |
| CA\_n1-n3-n40-n77 | n1, n3, n40, n77 |
| CA\_n1-n3-n40-n105 | n1, n3, n40, n105 |
| CA\_n1-n3-n41-n77 | n1, n3, n41, n77 |
| CA\_n1-n3-n41-n79 | n1, n3, n41, n79 |
| CA\_n1-n3-n67-n78 | n1, n3, n67, n78 |
| CA\_n1-n3-n75-n78 | n1, n3, n75, n78 |
| CA\_n1-n3-n77-n79 | n1, n3, n77, n79 |
| CA\_n1-n5-n7-n78 | n1, n5, n7, n78 |
| CA\_n1-n5-n28-n78 | n1, n5, n28, n78 |
| CA\_n1-n5-n28-n79 | n1, n5, n28, n79 |
| CA\_n1-n5-n78-n79 | n1, n5, n78, n79 |
| CA\_n1-n7-n8-n40 | n1, n7, n8, n40 |
| CA\_n1-n7-n8-n78 | n1, n7, n8, n78 |
| CA\_n1-n7-n26-n78 | n1, n7, n26, n78 |
| CA\_n1-n7-n28-n38 | n1, n7, n28, n38 |
| CA\_n1-n7-n28-n78 | n1, n7, n28, n78 |
| CA\_n1-n7-n40-n78 | n1, n7, n40, n78 |
| CA\_n1-n7-n40-n105 | n1, n7, n40, n105 |
| CA\_n1-n7-n67-n78 | n1, n7, n67, n78 |
| CA\_n1-n7-n75-n78 | n1, n7, n75, n78 |
| CA\_n1-n7-n78-n105 | n1, n7, n78, n105 |
| CA\_n1-n8-n40-n78 | n1, n8, n40, n78 |
| CA\_n1-n8-n78-n79 | n1, n8, n78, n79 |
| CA\_n1-n18-n28-n41 | n1, n18, n28, n41 |
| CA\_n1-n18-n28-n77 | n1, n18, n28, n77 |
| CA\_n1-n18-n41-n77 | n1, n18, n41, n77 |
| CA\_n1-n28-n38-n78 | n1, n28, n38, n78 |
| CA\_n1-n28-n40-n77 | n1, n28, n40, n77 |
| CA\_n1-n28-n40-n78 | n1, n28, n40, n78 |
| CA\_n1-n28-n41-n77 | n1, n28, n41, n77 |
| CA\_n1-n28-n41-n79 | n1, n28, n41, n79 |
| CA\_n1-n28-n75-n78 | n1, n28, n75, n78 |
| CA\_n1-n28-n77-n79 | n1, n28, n77, n79 |
| CA\_n1-n28-n78-n79 | n1, n28, n78, n79 |
| CA\_n1-n41-n77-n79 | n1, n41, n77, n79 |
| CA\_n2-n5-n30-n66 | n2, n5, n30, n66 |
| CA\_n2-n5-n30-n77 | n2, n5, n30, n77 |
| CA\_n2-n5-n48-n66 | n2, n5, n48, n66 |
| CA\_n2-n5-n48-n77 | n2, n5, n48, n77 |
| CA\_n2-n5-n66-n77 | n2, n5, n66, n77 |
| CA\_n2-n12-n30-n66 | n2, n12, n30, n66 |
| CA\_n2-n12-n30-n77 | n2, n12, n30, n77 |
| CA\_n2-n12-n66-n77 | n2, n12, n66, n77 |
| CA\_n2-n14-n30-n66 | n2, n14, n30, n66 |
| CA\_n2-n14-n30-n77 | n2, n14, n30, n77 |
| CA\_n2-n14-n66-n77 | n2, n14, n66, n77 |
| CA\_n2-n29-n30-n66 | n2, n29, n30, n66 |
| CA\_n2-n29-n30-n77 | n2, n29, n30, n77 |
| CA\_n2-n29-n66-n77 | n2, n29, n66, n77 |
| CA\_n2-n30-n66-n77 | n2, n30, n66, n77 |
| CA\_n2-n41-n66-n71 | n2, n41, n66, n71 |
| CA\_n2-n48-n66-n77 | n2, n48, n66, n77 |
| CA\_n2-n66-n71-n77 | n2, n66, n71, n77 |
| CA\_n2-n66-n71-n78 | n2, n66, n71, n78 |
| CA\_n3-n5-n7-n78 | n3, n5, n7, n78 |
| CA\_n3-n5-n28-n78 | n3, n5, n28, n78 |
| CA\_n3-n5-n28-n79 | n3, n5, n28, n79 |
| CA\_n3-n7-n8-n781 | n3, n7, n8, n78 |
| CA\_n3-n7-n20-n67 | n3, n7, n20, n67 |
| CA\_n3-n7-n20-n78 | n3, n7, n20, n78 |
| CA\_n3-n7-n26-n78 | n3, n7, n26, n78 |
| CA\_n3-n7-n28-n38 | n3, n7, n28, n38 |
| CA\_n3-n7-n28-n78 | n3, n7, n28, n78 |
| CA\_n3-n7-n40-n105 | n3, n7, n40, n105 |
| CA\_n3-n7-n67-n78 | n3, n7, n67, n78 |
| CA\_n3-n7-n75-n78 | n3, n7, n75, n78 |
| CA\_n3-n7-n78-n105 | n3, n7, n78, n105 |
| CA\_n3-n18-n28-n41 | n3, n18, n28, n41 |
| CA\_n3-n18-n28-n77 | n3, n18, n28, n77 |
| CA\_n3-n20-n67-n78 | n3, n20, n67, n78 |
| CA\_n3-n28-n40-n77 | n3, n28, n40, n77 |
| CA\_n3-n18-n41-n77 | n3, n18, n41, n77 |
| CA\_n3-n28-n41-n77 | n3, n28, n41, n77 |
| CA\_n3-n28-n41-n79 | n3, n28, n41, n79 |
| CA\_n3-n28-n77-n79 | n3, n28, n77, n79 |
| CA\_n3-n28-n41-n78 | n3, n28, n41, n78 |
| CA\_n3-n41-n77-n79 | n3, n41, n77, n79 |
| CA\_n5-n25-n29-n66 | n5, n25, n29, n66 |
| CA\_n5-n25-n66-n77 | n5, n25, n66, n77 |
| CA\_n5-n25-n66-n78 | n5, n25, n66, n78 |
| CA\_n5-n28-n78-n79 | n5, n28, n78, n79 |
| CA\_n5-n30-n66-n77 | n5, n30, n66, n77 |
| CA\_n5-n48-n66-n77 | n5, n48, n66, n77 |
| CA\_n7-n8-n40-n78 | n7, n8, n40, n78 |
| CA\_n7-n12-n25-n66 | n7, n12, n25, n66 |
| CA\_n7-n20-n67-n78 | n7, n20, n67, n78 |
| CA\_n7-n25-n66-n71 | n7, n25, n66, n71 |
| CA\_n7-n25-n66-n77 | n7, n25, n66, n77 |
| CA\_n7-n25-n66-n78 | n7, n25, n66, n78 |
| CA\_n7-n40-n78-n105 | n7, n40, n78, n105 |
| CA\_n8-n20-n28-n75 | n8, n20, n28, n75 |
| CA\_n12-n30-n66-n77 | n12, n30, n66, n77 |
| CA\_n13-n25-n66-n77 | n13, n25, n66, n77 |
| CA\_n14-n30-n66-n77 | n14, n30, n66, n77 |
| CA\_n18-n28-n41-n77 | n18, n28, n41, n77 |
| CA\_n25-n38-n66-n78 | n25, n38, n66, n78 |
| CA\_n25-n41-n66-n71 | n25, n41, n66, n71 |
| CA\_n25-n41-n66-n77 | n25, n41, n66, n77 |
| CA\_n25-n41-n66-n78 | n25, n41, n66, n78 |
| CA\_n25-n41-n71-n77 | n25, n41, n71, n77 |
| CA\_n25-n41-n71-n78 | n25, n41, n71, n78 |
| CA\_n25-n41-n77-n85 | n25, n41, n77, n85 |
| CA\_n25-n66-n71-n77 | n25, n66, n71, n77 |
| CA\_n25-n66-n71-n78 | n25, n66, n71, n78 |
| CA\_n28-n41-n77-n79 | n28, n41, n77, n79 |
| CA\_n29-n30-n66-n77 | n29, n30, n66, n77 |
| CA\_n41-n66-n70-n78 | n41, n66, n70, n78 |
| CA\_n41-n66-n71-n77 | n41, n66, n71, n77 |
| CA\_n41-n66-n71-n78 | n41, n66, n71, n78 |
| CA\_n41-n66-n77-n85 | n41, n66, n77, n85 |
| CA\_n48-n66-n70-n71 | n48, n66, n70, n71 |
| CA\_n48-n66-n70-n77 | n48, n66, n70, n77 |
| CA\_n48-n66-n71-n77 | n48, n66, n71, n77 |
| CA\_n48-n70-n71-n77 | n48, n70, n71, n77 |
| NOTE 1: Applicable for UE supporting inter-band carrier aggregation with mandatory simultaneous Rx/Tx capability. | |

#### 5.2A.2.4 Inter-band CA (five bands)

Table 5.2A.2.4-1: Inter-band CA operating bands involving FR1 (five bands)

|  |  |
| --- | --- |
| NR CA Band | NR Band  (Table 5.2-1) |
| CA\_n1-n3-n5-n7-n78 | n1, n3, n5, n7, n78 |
| CA\_n1-n3-n5-n28-n78 | n1, n3, n5, n28, n78 |
| CA\_n1-n3-n7-n8-n781 | n1, n3, n7, n8, n78 |
| CA\_n1-n3-n7-n26-n78 | n1, n3, n7, n26, n78 |
| CA\_n1-n3-n7-n28-n38 | n1, n3, n7, n28, n38 |
| CA\_n1-n3-n7-n28-n78 | n1, n3, n7, n28, n78 |
| CA\_n1-n3-n7-n67-n78 | n1, n3, n7, n67, n78 |
| CA\_n1-n3-n7-n75-n78 | n1, n3, n7, n75, n78 |
| CA\_ n1-n3-n28-n41-n77 | n1, n3, n28, n41, n77 |
| CA\_n1-n3-n28-n41-n79 | n1, n3, n28, n41, n79 |
| CA\_n1-n3-n28-n77-n79 | n1, n3, n28, n77, n79 |
| CA\_n1-n3-n40-n78-n105 | n1, n3, n40, n78, n105 |
| CA\_n1-n3-n41-n77-n79 | n1, n3, n41, n77, n79 |
| CA\_n1-n5-n28-n78-n79 | n1, n5, n28, n78, n79 |
| CA\_n1-n7-n40-n78-n105 | n1, n7, n40, n78, n105 |
| CA\_n1-n28-n41-n77-n79 | n1, n28, n41, n77, n79 |
| CA\_n2-n5-n30-n66-n77 | n2, n5, n30, n66, n77 |
| CA\_n2-n5-n48-n66-n77 | n2, n5, n48, n66, n77 |
| CA\_n2-n12-n30-n66-n77 | n2, n12, n30, n66, n77 |
| CA\_n2-n14-n30-n66-n77 | n2, n14, n30, n66, n77 |
| CA\_n2-n29-n30-n66-n77 | n2, n29, n30, n66, n77 |
| CA\_n3-n7-n20-n67-n78 | n3, n7, n20, n67, n78 |
| CA\_n3-n7-n40-n78-n105 | n3, n7, n40, n78, n105 |
| CA\_n3-n28-n41-n77-n79 | n3, n28, n41, n77, n79 |
| NOTE 1: Applicable for UE supporting inter-band carrier aggregation with mandatory simultaneous Rx/Tx capability. | |

---Text omitted---

#### 5.5A.3.3 Configurations for inter-band CA (four bands)

Table 5.5A.3.3-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (four bands)

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NR CA configuration** | | **Uplink CA configuration**  **or single uplink carrier 4** | | **NR Band** | | **Channel bandwidth (MHz) (NOTE 3)** | | **Bandwidth combination set** | |
| CA\_n1A-n3A-n5A-n7A | | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
| CA\_n1A-n3A-n5A-n7B | | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n7A  CA\_n3A-n5A  CA\_n3A-n7A  CA\_n5A-n7A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
| CA\_n1A-n3A-n5A-n28A | | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n28A  CA\_n3A-n5A  CA\_n3A-n28A  CA\_n5A-n28A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n3A-n5A-n78A | | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n78A  CA\_n3A-n5A  CA\_n3A-n78A  CA\_n5A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n7A-n8A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n7A-n8A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3A-n7A-n26A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3B-n7A-n26A | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3A-n7B-n26A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3B-n7B-n26A | | CA\_n3B  CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3A-n7A-n26(2A) | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
| CA\_n1A-n3B-n7A-n26(2A) | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n7B-n26(2A) | | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
| CA\_n1A-n3B-n7B-n26(2A) | | CA\_n3B  CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n26A  CA\_n3A-n7A  CA\_n3A-n26A  CA\_n7A-n26A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n7A-n28A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | | n1 | | 5, 10, 15, 20 | | 1 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
| CA\_n1A-n3A-n7B-n28A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | | n1 | | 5, 10, 15, 20 | | 1 | |
|  | | CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3B-n7A-n28A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3B-n7B-n28A | | CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n7A-n28A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3A-n7A-n38A7 | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1(2A)-n3A-n7A-n38A7 | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1A-n3B-n7A-n38A7 | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1(2A)-n3B-n7A-n38A7 | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1A-n3(2A)-n7A-n38A7 | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS1 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1(2A)-n3(2A)-n7A-n38A7 | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS1 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1A-n3A-n7A-n67A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n3A-n7A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
| CA\_n1A-n3A-n7A-n75A | | - | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n75 | | n75 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n3A-n7A-n78A | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n1 | | 5, 10, 15, 20 | | 1 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 2 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n3B-n7A-n78A | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3B-n7B-n78A | | CA\_n3B  CA\_n7B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n7A-n78(2A) | | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3A-n7B-n78A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 1 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3B-n7A-n78(2A) | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3A-n7B-n78(2A) | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3B-n7B-n78(2A) | | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n3B  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n7A-n79A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3A-n7A-n79C | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1(2A)-n3A-n7A-n79A | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1(2A)-n3A-n7A-n79C | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1A-n3B-n7A-n79A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3B-n7A-n79C | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1(2A)-n3B-n7A-n79A | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1(2A)-n3B-n7A-n79C | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1A-n3(2A)-n7A-n79A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3(2A)-n7A-n79C | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1(2A)-n3(2A)-n7A-n79A | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1(2A)-n3(2A)-n7A-n79C | | - | | n1 | | CA\_n1(2A)\_BCS0 | | 0 | |
|  | |  | | n3 | | CA\_n3(2A)\_BCS0 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n79 | | CA\_n79C\_BCS0 | |  | |
| CA\_n1A-n3A-n8A-n77A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n8A-n77(2A) | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n1A-n3A-n8A-n78A | | CA\_n1A-n3A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n8A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 40, 50, 60, 80, 901, 100 | |  | |
| CA\_n1A-n3A-n18A-n28A | | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n28A  CA\_n3A-n18A  CA\_n3A-n28A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
| CA\_n1A-n3A-n18A-n41A | | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n41A  CA\_n3A-n18A  CA\_n3A-n41A  CA\_n18A-n41A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n18A-n77A | | CA\_n1A-n3A  CA\_n1A-n18A  CA\_n1A-n77A  CA\_n3A-n18A  CA\_n3A-n77A  CA\_n18A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n20A-n67A | | CA\_n1A-n3A  CA\_n1A-n20A  CA\_n3A-n20A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n3A-n26A-n78A | | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n26(2A)-n78A | | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n26A-n78(2A) | | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A) BCS0 | |  | |
| CA\_n1A-n3A-n26(2A)-n78(2A) | | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n3B-n26A-n78A | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3B-n26(2A)-n78A | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3B-n26A-n78(2A) | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n3B-n26(2A)-n78(2A) | | CA\_n3B  CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n26A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n28A-n38A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1A-n3A-n28A-n41A | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n28A-n41A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n28A-n77A | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | | n1 | | 5, 10, 15, 20 | | 1 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n28A-n77(2A) | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n28A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n28A-n78A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
|  | |  | | n78 | | 10, 15, 20, 40, 50, 60, 80, 901, 100 | |  | |
|  | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 1 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 2 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202,302 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n28A-n78(2A) | | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202, 302 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3B-n28A-n78A | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3B-n28A-n78(2A) | | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | CA\_n3B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3A-n28A-n79A | | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n28A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25,30 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3A-n38A-n78A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n40A-n77A | | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n40A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n40A-n105A | | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n40A-n105A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n1A-n3A-n41A-n77A | | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n41A-n77(2A) | | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n41A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
| CA\_n1A-n3A-n41A-n79A | | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n41A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3A-n67A-n78A | | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n3A-n67A-n78(2A) | | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n3A-n78A  CA\_n78(2A) | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n3A-n75A-n78A | | - | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n75 | | n75 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n3A-n77A-n79A | | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25,30 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3A-n77(2A)-n79A | | CA\_n1A-n3A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25,30 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n3A-n78A-n105A | | CA\_n1A-n3A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n78A-n105A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n3 | | 5, 10, 15, 20, 25,30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25,30, 35 | |  | |
| CA\_n1A-n5A-n7A-n78A | | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n5A-n7B-n78A | | CA\_n1A-n5A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n5A-n28A-n78A | | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n5A-n28A  CA\_n5A-n78A  CA\_n28A-n78A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n5A-n28A-n79A | | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n79 | | n79 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n5A-n78A-n79A | | CA\_n1A-n5A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n78A-n79A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n79 | | n79 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n7A-n8A-n40A | | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n40A  CA\_n7A-n8A  CA\_n7A-n40A  CA\_n8A-n40A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
| CA\_n1A-n7A-n8A-n78A | | CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n26A-n78A | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7B-n26A-n78A | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n26(2A)-n78A | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n26A-n78(2A) | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A) BCS0 | |  | |
| CA\_n1A-n7A-n26(2A)-n78(2A) | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n7B-n26(2A)-n78A | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7B-n26A-n78(2A) | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n7B-n26(2A)-n78(2A) | | CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n1A-n7A-n28A-n38A7 | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n1A-n7A-n28A-n78A | | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7B-n28A-n78A | | CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7B-n28A-n78(2A) | | CA\_n7B  CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n7A-n28A-n78(2A) | | CA\_n78(2A)  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n7A-n38A-n78A7 | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n40A-n78A | | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n40A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n40A-n105A | | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n1A-n7A-n67A-n78A | | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n7A-n67A-n78(2A) | | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n7A-n78A  CA\_n78(2A) | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n1A-n7A-n75A-n78A | | - | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n75 | | n75 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n7A-n78A-n105A | | CA\_n1A-n7A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n1A-n8A-n40A-n78A | | CA\_n1A-n8A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n8A-n78A-n79A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n8A-n78(2A)-n79A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS1 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n18A-n28A-n41A | | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n1A-n18A-n28A-n77A | | CA\_n1A-n18A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n18A-n41A-n77A | | CA\_n1A-n18A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n38A-n78A | | - | | n1 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n40A-n77A | | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n40A-n78A | | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n40B-n78A | | CA\_n1A-n28A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n28A-n40A  CA\_n28A-n78A  CA\_n40A-n78A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | CA\_n40B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n41A-n77A | | n41**7**  n77**7**  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n41A-n77(2A) | | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
| CA\_n1A-n28A-n41A-n79A | | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n28A-n75A-n78A | | - | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n75 | | 5, 10, 15, 20, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n1A-n28A-n77A-n79A | | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n28A-n78A-n79A | | CA\_n1A-n28A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | | n1 | | n1 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n79 | | n79 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n1A-n28A-n77(2A)-n79A | | CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n40A-n78A-n105A | | CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n1A-n41A-n77A-n79A | | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n1A-n41A-n77(2A)-n79A | | CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n1 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n2A-n5A-n30A-n66A | | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2(2A)-n5A-n30A-n66A | | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | | n5 | | 5, 10, 15, 20 | |
|  | | n30 | | 5, 10 | |
|  | | n66 | | 10, 15, 20, 25, 30, 40 | |
| CA\_n2A-n5A-n30A-n66(2A) | | CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | | n5 | | 5, 10, 15, 20 | |
|  | | n30 | | 5, 10 | |
|  | | n66 | | CA\_n66(2A)\_BCS1 | |
| CA\_n2A-n5A-n30A-n77A | | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n5A-n30A-n77A | | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n5A-n30A-n77(2A) | | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n5A-n30A-n77(2A) | | n775  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n5A-n30A  CA\_n5A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n5A-n48A-n66A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n5A-n48B-n66A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 3 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n5A-n48(2A)-n66A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n48A-n66A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n5A-n48(A-B)-n66A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | CA\_n48(A-B)\_BCS1 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n5A-n48A-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n5A-n48A-n77C | | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS0 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS1 | |  | |
| CA\_n2A-n5A-n48B-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS0 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 3 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n5A-n48(2A)-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS0 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n5A-n66A-n77A | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n5A-n66A-n77A | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30,40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n5A-n66(2A)-n77A | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n5A-n66A-n77(2A) | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n5A-n66(2A)-n77(2A) | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | CA\_n66(2A) BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n5A-n66A-n77(2A) | | n775  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n5A-n66A-n77C | | CA\_n77C  CA\_n2A-n5A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n77A  CA\_n5A-n66A  CA\_n66A-n77A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS1 | |  | |
| CA\_n2A-n12A-n30A-n66A | | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2(2A)-n12A-n30A-n66A | | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n12A-n30A-n66(2A) | | CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
| CA\_n2A-n12A-n30A-n77A | | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n12A-n30A-n77A | | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n12A-n30A-n77(2A) | | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n12A-n30A-n77(2A) | | n775  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n12A-n30A  CA\_n12A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n12A-n66A-n77A | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n12A-n66A-n77A | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n12A-n66(2A)-n77A | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n12A-n66A-n77(2A) | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n12A-n66(2A)-n77(2A) | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | CA\_n66(2A) BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n12A-n66A-n77(2A) | | n775  CA\_n2A-n12A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n14A-n30A-n66A | | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2(2A)-n14A-n30A-n66A | | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | | n14 | | 5, 10 | |
|  | | n30 | | 5, 10 | |
|  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |
| CA\_n2A-n14A-n30A-n66(2A) | | CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | | n14 | | 5, 10 | |
|  | | n30 | | 5, 10 | |
|  | | n66 | | CA\_n66(2A)\_BCS1 | |
| CA\_n2A-n14A-n30A-n77A | | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n14A-n30A-n77A | | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n14A-n30A-n77(2A) | | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n14A-n30A-n77(2A) | | n775  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n14A-n30A  CA\_n14A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n14A-n66A-n77A | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n14A-n66A-n77A | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n14A-n66(2A)-n77A | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n14A-n66A-n77(2A) | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n14A-n66(2A)-n77(2A) | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A) BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n14A-n66A-n77(2A) | | n775  CA\_n2A-n14A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n14 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n29A-n30A-n66A | | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2(2A)-n29A-n30A-n66A | | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n2A-n29A-n30A-n66(2A) | | CA\_n2A-n30A  CA\_n2A-n66A  CA\_n30A-n66A | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
| CA\_n2A-n29A-n30A-n77A | | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n29A-n30A-n77A | | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n29A-n30A-n77(2A) | | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n29A-n30A-n77(2A) | | n775  CA\_n2A-n30A  CA\_n2A-n77A5  CA\_n30A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n29A-n66A-n77A | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n29A-n66A-n77A | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n29A-n66(2A)-n77A | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n29A-n66A-n77(2A) | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n29A-n66A-n77(2A) | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n29A-n66(2A)-n77(2A) | | n775  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n30A-n66A-n77A | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2(2A)-n30A-n66A-n77A | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n30A-n66(2A)-n77A | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n30A-n66A-n77(2A) | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n30A-n66(2A)-n77(2A) | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A) BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2(2A)-n30A-n66A-n77(2A) | | n775  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n2 | | CA\_n2(2A)\_BCS0 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n2A-n41A-n66A-n71A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
| CA\_n2A-n48A-n66A-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n48B-n66A-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n48 | | CA\_n48B\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 3 | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n48(2A)-n66A-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n48A-n66A-n77C | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS0 | |  | |
|  | | CA\_n77C  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS1 | |  | |
|  | |  | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 2 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS1 | |  | |
| CA\_n2A-n66A-n71A-n77A | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n66A-n71A-n77(2A) | | - | | n2 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A) BCS1 | |  | |
| CA\_n2A-n66A-n71A-n78A | | - | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n2A-n66A-n71A-n78(2A) | | - | | n2 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3A-n5A-n7A-n78A | | - | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n5A-n7B-n78A | | - | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n3A-n5A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n5A-n7A  CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 1 | |
|  | |  | | n5 | | 5, 10, 15, 20 | |  | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n5A-n28A-n78A | | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n5A-n28A-n79A | | CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n79 | | n79 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n7A-n8A-n78A | | CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n20A-n67A | | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n7A-n20A | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n7A-n20A-n78A | | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n7A-n20A-n78(2A) | | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS 4 and 5 | |  | |
| CA\_n3A-n7A-n26A-n78A | | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7B-n26A-n78A | | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n26(2A)-n78A | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n26A-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A) BCS0 | |  | |
| CA\_n3A-n7A-n26(2A)-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3A-n7B-n26(2A)-n78A | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7B-n26A-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3A-n7B-n26(2A)-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | CA\_n7B BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3B-n7A-n26A-n78A | | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n3B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7A-n26(2A)-n78A | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7A-n26A-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3B-n7A-n26(2A)-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 35, 40, 50 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3B-n7B-n26A-n78A | | CA\_n3A-n7A  CA\_n3A-n26A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n7A-n78A  CA\_n26A-n78A  CA\_n3B  CA\_n7B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7B-n26(2A)-n78A | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B  CA\_n7B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7B-n26A-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B  CA\_n7B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3B-n7B-n26(2A)-n78(2A) | | CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B  CA\_n7B | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n26 | | CA\_n26(2A)\_BCS0 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS0 | |  | |
| CA\_n3A-n7A-n28A-n38A7 | | - | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n3A-n7A-n28A-n78A | | - | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n3A-n7A CA\_n3A-n28A  CA\_n3A-n78A CA\_n7A-n28A  CA\_n7A-n78A CA\_n28A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n28A-n78(2A) | | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 202 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3A-n7B-n28A-n78A | | - | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7B-n28A-n78(2A) | | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3B-n7A-n28A-n78A | | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7A-n28A-n78(2A) | | CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3B-n7B-n28A-n78A | | CA\_n7B  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3B-n7B-n28A-n78(2A) | | CA\_n7B  CA\_n78(2A)  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n28A-n78A | | n3 | | CA\_n3B\_BCS0 | | 0 | |
|  | |  | | n7 | | CA\_n7B\_BCS0 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3A-n7A-n38A-n78A7 | | - | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n40A-n105A | | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n105A  CA\_n7A-n40A  CA\_n7A-n105A  CA\_n40A-n105A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n3A-n7A-n67A-n78A | | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n7A-n67A-n78(2A) | | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78(2A) | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n67 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3A-n7A-n75A-n78A | | - | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n75 | | n75 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n7A-n78A-n105A | | CA\_n3A-n7A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n78A-n105A | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n3A-n18A-n28A-n41A | | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n18A-n28A  CA\_n18A-n41A  CA\_n28A-n41A | | n3 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
| CA\_n3A-n18A-n28A-n77A | | CA\_n3A-n18A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n18A-n28A  CA\_n18A-n77A  CA\_n28A-n77A | | n3 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n18A-n41A-n77A | | CA\_n3A-n18A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n41A-n77A | | n3 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n18 | | 5, 10, 15 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n20A-n67A-n78A | | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n3A-n20A-n67A-n78(2A) | | CA\_n3A-n20A  CA\_n3A-n78A  CA\_n20A-n78A  CA\_n78(2A) | | n3 | | n3 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS 4 and 5 | |  | |
| CA\_n3A-n28A-n38A-n78A | | - | | n3 | | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n28A-n40A-n77A | | CA\_n3A-n28A  CA\_n3A-n40A  CA\_n3A-n77A  CA\_n28A-n40A  CA\_n28A-n77A  CA\_n40A-n77A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20, 30 | |  | |
|  | |  | | n40 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n28A-n41A-n77A | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20, 30 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n28A-n41A-n77(2A) | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n3 | | 5, 10, 15, 20 | | 1 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n3A-n28A-n41A-n78A | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n3A-n28A-n41A-n78(2A) | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n78A  CA\_n28A-n41A  CA\_n28A-n78A  CA\_n41A-n78A | | n3 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n3A-n28A-n41A-n79A | | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n3A-n28A-n77A-n79A | | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 80, 100 | |  | |
| CA\_n3A-n28A-n77(2A)-n79A | | CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | |  | | n79 | | 40, 50, 80, 100 | |  | |
| CA\_n3A-n40A-n78A-n105A | | CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | | n3 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25,30, 35 | |  | |
| CA\_n3A-n41A-n77A-n79A | | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n3A-n41A-n77(2A)-n79A | | CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n3 | | 5, 10, 15, 20, 25, 30 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n5A-n25A-n29A-n66A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n25A-n66A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n29 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 30, 40 | |  | |
| CA\_n5A-n25A-n66A-n77A | | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25(2A)-n66A-n77A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25A-n66(2A)-n77A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25A-n66A-n77(2A) | | n775,6  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n5A-n25(2A)-n66(2A)-n77A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25(2A)-n66A-n77(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n5A-n25A-n66(2A)-n77(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n5A-n25(2A)-n66(2A)-n77(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n5A-n25A-n66A-n78A | | n785  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A5  CA\_n25A-n66A  CA\_n25A-n78A5  CA\_n66A-n78A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25(2A)-n66A-n78A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25A-n66(2A)-n78A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25A-n66A-n78(2A) | | n785  CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A5  CA\_n25A-n66A  CA\_n25A-n78A5  CA\_n66A-n78A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n5A-n25(2A)-n66(2A)-n78A | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n25(2A)-n66A-n78(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n5A-n25A-n66(2A)-n78(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n5A-n25(2A)-n66(2A)-n78(2A) | | CA\_n5A-n25A  CA\_n5A-n66A  CA\_n5A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n5A-n28A-n78A-n79A | | CA\_n5A-n28A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | | n5 | | n5 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n28 | | n28 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n79 | | n79 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n5A-n30A-n66A-n77A | | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n30A-n66(2A)-n77A | | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n30A-n66(2A)-n77(2A) | | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A) BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A) BCS1 | |  | |
| CA\_n5A-n30A-n66A-n77(2A) | | n775  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n5A-n48A-n66A-n77A | | - | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20, 25 | | 1 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n48A-n66A-n77C | | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77C\_BCS1 | |  | |
| CA\_n5A-n48B-n66A-n77A | | - | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20, 25 | | 1 | |
|  | |  | | n48 | | CA\_n48B\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | | 2 | |
|  | |  | | n48 | | CA\_n48B\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | | 3 | |
|  | |  | | n48 | | CA\_n48B\_BCS2 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n5A-n48(2A)-n66A-n77A | | - | | n5 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | | CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | | n5 | | 5, 10, 15, 20, 25 | | 1 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n5 | | 5, 10, 15, 20, 25 | | 2 | |
|  | |  | | n48 | | CA\_n48(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n8A-n40A-n78A | | CA\_n7A-n8A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n8A-n40A  CA\_n8A-n78A  CA\_n40A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n8 | | 5, 10, 15, 20 | |  | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n12A-n25A-n66A | | - | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n12 | | 5, 10, 15 | |  | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
| CA\_n7A-n20A-n67A-n78A | | CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | n78 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n7A-n20A-n67A-n78(2A) | | CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | | n7 | | n7 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n20 | | n20 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n67 | | n67 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS 4 and 5 | |  | |
| CA\_n7A-n25A-n66A-n71A | | - | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
| CA\_n7A-n25A-n66A-n77A | | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66A-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25(2A)-n66A-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25A-n66(2A)-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25A-n66A-n77(2A) | | n775,6  CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n66A-n77A5 | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7(2A)-n25(2A)-n66A-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66(2A)-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66A-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7A-n25(2A)-n66(2A)-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25(2A)-n66A-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7A-n25A-n66(2A)-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66(2A)-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7(2A)-n25(2A)-n66A-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7A-n25(2A)-n66(2A)-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7(2A)-n25(2A)-n66(2A)-n77(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n7A-n25A-n66A-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25(2A)-n66A-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25A-n66(2A)-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25A-n66A-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7(2A)-n25A-n66A-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25(2A)-n66A-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7A-n25(2A)-n66(2A)-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n25A-n66(2A)-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7(2A)-n25(2A)-n66A-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66(2A)-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66A-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7A-n25(2A)-n66(2A)-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7(2A)-n25(2A)-n66A-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78A | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7(2A)-n25A-n66(2A)-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7(2A)-n25(2A)-n66(2A)-n78(2A) | | CA\_n7A-n25A  CA\_n7A-n66A  CA\_n7A-n78A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n66A-n78A | | n7 | | CA\_n7(2A)\_BCS0 | | 0 | |
|  | |  | | n25 | | CA\_n25(2A)\_BCS0 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n7A-n28A-n38A-n78A7 | | - | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n28 | | 5, 10, 15, 20, 25, 30 | |  | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n7A-n40A-n78A-n105A | | CA\_n7A-n40A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | | n7 | | 5, 10, 15, 20, 25, 30, 40, 50 | | 0 | |
|  | |  | | n40 | | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | |  | |
|  | |  | | n78 | | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n105 | | 5, 10, 15, 20, 25, 30, 35 | |  | |
| CA\_n8A-n20A-n28A-n75A | | - | | n8 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n20 | | 5, 10, 15, 20 | |  | |
|  | |  | | n28 | | 5, 10, 15, 20 | |  | |
|  | |  | | n75 | | 5, 10, 15, 20, 25, 30, 40, 50 | |  | |
| CA\_n12A-n30A-n66A-n77A | | n775  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n12 | | 5, 10,15 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n12A-n30A-n66(2A)-n77A | | n775  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n12 | | 5, 10,15 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n12A-n30A-n66A-n77(2A) | | n775  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n12 | | 5, 10,15 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n12A-n30A-n66(2A)-n77(2A) | | n775  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n12 | | 5, 10,15 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n13A-n25A-n66A-n77A | | CA\_n13A-n25A  CA\_n13A-n66A  CA\_n13A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n13 | | 5, 10 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n13A-n25A-n66A-n77(2A) | | CA\_n77(2A)  CA\_n13A-n25A  CA\_n13A-n66A  CA\_n13A-n77A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n66A-n77A | | n13 | | 5, 10 | | 0 | |
|  | |  | | n25 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n14A-n30A-n66A-n77A | | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n14 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n14A-n30A-n66(2A)-n77A | | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n14 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n14A-n30A-n66A-n77(2A) | | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n14 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n14A-n30A-n66(2A)-n77(2A) | | n775  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A5  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n14 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n18A-n28A-n41A-n77A | | CA\_n18A-n28A  CA\_n18A-n41A  CA\_n18A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | | n18 | | 5, 10, 15 | | 0 | |
|  | |  | | n28 | | 5, 10 | |  | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n38A-n66A-n78A | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25(2A)-n38A-n66A-n78A | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | CA\_n25(2A)\_BCS0 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n38A-n66(2A)-n78A | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n38A-n66A-n78(2A) | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25(2A)-n38A-n66(2A)-n78A | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | CA\_n25(2A)\_BCS0 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25(2A)-n38A-n66A-n78(2A) | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | CA\_n25(2A)\_BCS0 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25A-n38A-n66(2A)-n78(2A) | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25(2A)-n38A-n66(2A)-n78(2A) | | CA\_n25A-n38A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n38A-n66A  CA\_n38A-n78A  CA\_n66A-n78A | | n25 | | CA\_n25(2A)\_BCS0 | | 0 | |
|  | |  | | n38 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25A-n41A-n66A-n71A | | - | | n25 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | | n415,6  CA\_n25A-n41A  CA\_n25A-n66A5  CA\_n25A-n71A  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(A-C)-n66A-n71A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A CA\_n41A-n71A CA\_n41C CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(A-C)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66(2A)-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66A-n71(2A) | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41A-n66A-n71B | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
| CA\_n25A-n41(2A)-n66A-n71A | | - | | n25 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | | n415,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n66A-n71A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(2A)-n66A-n71(2A) | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41(2A)-n66A-n71B | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
| CA\_n25A-n41(2A)-n66(2A)-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n66A-n71A | | - | | n25 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | CA\_n41C\_BCS0 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | | n415,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41C5  CA\_n66A-n71A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 1 | |
|  | |  | | n41 | | CA\_n41C\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n66A-n71(2A) | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41C-n66A-n71B | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
| CA\_n25A-n41C-n66(2A)-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n66A-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41(2A)-n66A-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n66A-n71A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41C-n66A-n71A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41C  CA\_n66A-n71A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(3A)-n66A-n71A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n71A CA\_n41A-n66A CA\_n41A-n71A CA\_n66A-n71A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(3A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n66A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n66A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | CA\_n41C\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n66(2A)-n77A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n41C CA\_n66A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | | CA\_n25A-n41A-n66A-n77(2A) | |
| CA\_n25A-n41(2A)-n66A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS1 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66(2A)-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5CA\_n66A-n77A5 | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66A-n77(2A) | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41A-n66(2A)-n77(2A) | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n66A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41(2A)-n66(2A)-n77A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n66A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n66A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n66A  CA\_n25A-n77A5  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n66A-n77A5 | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n66A-n77(2A) | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n66A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25(2A)-n41A-n66(2A)-n77A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n77A  CA\_n66A-n77A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41C-n66A-n77A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n66A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41(2A)-n66A-n77A | | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n77A CA\_n66A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n66A-n78A | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n41A-n66A-n78(2A) | | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n78A  CA\_n41A-n66A  CA\_n41A-n78A  CA\_n66A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25A-n41A-n71A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n71A-n77(2A) | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41A-n71B-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n71B-n77(2A) | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41A-n71(2A)-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n71(2A)-n77(2A) | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n41C-n71A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n71A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | CA\_n41C\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n71B-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n41C CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41C-n71(2A)-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n41C CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(2A)-n71A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(2A)-n71B-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41(2A)-n71(2A)-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | CA\_41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n71A-n77A | | n415,6  n775,6  CA\_n25A-n41A5  CA\_n25A-n71A5  CA\_n25A-n77A  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n71A-n77A5 | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n71(2A)-n77A | | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n71B-n77A | | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n71A-n77A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41A-n71A-n77(2A) | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25(2A)-n41C-n71A-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n41(2A)-n71A-n77A | | CA\_n25A-n41A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n71A CA\_n41A-n77A CA\_n71A-n77A | | n25 | | CA\_25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n41 | | CA\_41(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n41A-n71A-n78A | | CA\_n25A-n41A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n71A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n41A-n77A-n85A | | CA\_n25A-n41A CA\_n25A-n77A CA\_n25A-n85A CA\_n41A-n77A CA\_n41A-n85A CA\_n77A-n85A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n85 | | n85 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n66A-n71A-n77A | | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n66(2A)-n71A-n77A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n66(2A)-n71A-n77(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n66A-n71B-n77A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n66A-n71(2A)-n77A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25A-n66A-n71A-n77(2A) | | n775,6  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n66A-n71(2A)-n77(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n66A-n71B-n77(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | n25 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25(2A)-n66A-n71A-n77A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n25(2A)-n66A-n71A-n77(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n25 | | CA\_n25(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 | |  | |
| CA\_n25A-n66A-n71A-n78A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n66(2A)-n71A-n78A | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n25A-n66A-n71A-n78(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n25A-n66(2A)-n71A-n78(2A) | | CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n25 | | 5, 10, 15, 20, 25, 30, 40 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n28A-n41A-n77A-n79A | | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n28 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | 10, 15, 20, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n28A-n41A-n77(2A)-n79A | | CA\_n28A-n41A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | | n28 | | 5, 10, 15, 20 | | 0 | |
|  | |  | | n41 | | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS0 | |  | |
|  | |  | | n79 | | 40, 50, 60, 80, 100 | |  | |
| CA\_n29A-n30A-n66A-n77A | | n775  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n29 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n29A-n30A-n66(2A)-n77A | | n775  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n29 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n29A-n30A-n66A-n77(2A) | | n775  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n29 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n29A-n30A-n66(2A)-n77(2A) | | n775  CA\_n30A-n66A  CA\_n30A-n77A5  CA\_n66A-n77A5 | | n29 | | 5, 10 | | 0 | |
|  | |  | | n30 | | 5, 10 | |  | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
| CA\_n41A-n66A-n70A-n78A | | CA\_n41A-n66A  CA\_n41A-n70A  CA\_n41A-n78A  CA\_n66A-n78A  CA\_n70A-n78A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n70 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n41A-n66A-n71A-n77A | | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66A-n71B-n77A | | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66A-n71B-n77(2A) | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n41A-n66A-n71(2A)-n77A | | n415,6  n775,6  CA\_n41A-n66A5CA\_n41A-n71A5CA\_n41A-n77A5CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66A-n71(2A)-n77(2A) | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n41A-n66(2A)-n71A-n77(2A) | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_77(2A)\_BCS 4 and 5 | |  | |
| CA\_n41C-n66A-n71A-n77A | | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n41C5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | CA\_n41C\_BCS1 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n41 | | CA\_n41C\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41C-n66A-n71B-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_n41C\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41C-n66A-n71(2A)-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_n41C\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41C-n66(2A)-n71A-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_n41C\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41(2A)-n66A-n71A-n77A | | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n71A5  CA\_n41A-n77A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | CA\_n41(2A)\_BCS1 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n41 | | CA\_n41(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41(2A)-n66A-n71B-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_41(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41(2A)-n66A-n71(2A)-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_41(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | CA\_71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41(2A)-n66(2A)-n71A-n77A | | CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n41 | | CA\_41(2A)\_BCS 4 and 5 | | 4 and 5 | |
|  | |  | | n66 | | CA\_66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66(2A)-n71A-n77A | | n415,6  n775,6  CA\_n41A-n66A5CA\_n41A-n71A5CA\_n41A-n77A5CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66(2A)-n71(2A)-n77A | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_n71(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66(2A)-n71B-n77A | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS 4 and 5 | |  | |
|  | |  | | n71 | | CA\_n71B\_BCS 4 and 5 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n41A-n66A-n71A-n77(2A) | | n415,6  n775,6  CA\_n41A-n66A5  CA\_n41A-n77A5  CA\_n41A-n71A5  CA\_n66A-n71A  CA\_n66A-n77A5  CA\_n71A-n77A5 | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS1 | |  | |
|  | |  | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n71 | | n71 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | CA\_n77(2A)\_BCS 4 and 5 in | |  | |
| CA\_n41A-n66A-n71A-n78A | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n41A-n66(2A)-n71A-n78A | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n41A-n66A-n71A-n78(2A) | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n41A-n66(2A)-n71A-n78(2A) | | CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n78A  CA\_n66A-n71A  CA\_n66A-n78A  CA\_n71A-n78A | | n41 | | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n78 | | CA\_n78(2A)\_BCS2 | |  | |
| CA\_n41A-n66A-n77A-n85A | | CA\_n41A-n66A CA\_n41A-n77A CA\_n41A-n85A CA\_n66A-n77A CA\_n66A-n85A CA\_n77A-n85A | | n41 | | n41 channel bandwidths in Table 5.3.5-1 | | 4 and 5 | |
|  | |  | | n66 | | n66 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n77 | | n77 channel bandwidths in Table 5.3.5-1 | |  | |
|  | |  | | n85 | | n85 channel bandwidths in Table 5.3.5-1 | |  | |
| CA\_n48A-n66A-n70A-n71A | | CA\_n48A-n66A CA\_n48A-n70A CA\_n48A-n71A CA\_n66A-n71A CA\_n70A-n71A | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 35, 40 | |  | |
|  | |  | | n70 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
| CA\_n48A-n66A-n70A-n77A | | CA\_n48A-n66A CA\_n48A-n70A CA\_n66A-n77A CA\_n70A-n77A | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 35, 40 | |  | |
|  | |  | | n70 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n48A-n66A-n71A-n77A | | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | 5, 10, 15, 20, 25, 30, 35, 40 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n48A-n66(2A)-n71A-n77A | | CA\_n48A-n66A CA\_n48A-n71A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS0 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
|  | |  | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 1 | |
|  | |  | | n66 | | CA\_n66(2A)\_BCS1 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n48A-n70A-n71A-n77A | | CA\_n48A-n70A CA\_n48A-n71A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | | n48 | | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | | 0 | |
|  | |  | | n70 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| CA\_n66A-n70A-n71A-n77A | | CA\_n66A-n71A CA\_n66A-n77A CA\_n70A-n71A CA\_n70A-n77A CA\_n71A-n77A | | n66 | | 5, 10, 15, 20, 25, 30, 35, 40 | | 0 | |
|  | |  | | n70 | | 5, 10, 15, 20, 25 | |  | |
|  | |  | | n71 | | 5, 10, 15, 20 | |  | |
|  | |  | | n77 | | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | |  | |
| NOTE 1: This UE channel bandwidth is optional in this release of the specification.  NOTE 2: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.  NOTE 3: The SCS of each channel bandwidth for NR band refers to Table 5.3.5-1.  NOTE 4: Only single uplink carriers with power class other than PC3 are listed.  NOTE 5: Minimum requirements for Power Class 2 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination.  NOTE 6: Minimum requirements for Power Class 1.5 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination.  NOTE 7: For a band combination which includes band n7 and n38 simultaneously, carriers in band n7 and n38 can only be configured as downlink carriers. Power imbalance between downlink carriers on Band n7 and Band n38 is assumed to be within 6dB. | | | | | | | | | |

#### 5.5A.3.4 Configurations for inter-band CA (five bands)

Table 5.5A.3.4-1: NR CA configurations and bandwidth combinations sets defined for inter-band CA (five bands)

| **NR CA configuration** | **Uplink configuration**  **or single uplink carrier 2** | **NR Band** | **Channel bandwidth (MHz) (NOTE 1)** | **Bandwidth combination set** |
| --- | --- | --- | --- | --- |
| CA\_n1A-n3A-n5A-n7A-n78A | CA\_n1A-n3A  CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A  CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A  CA\_n5A-n7A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n5A-n78A  CA\_n7A-n78A | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n5A-n7B-n78A | CA\_n1A-n3A  CA\_n1A-n5A | n1 | 5, 10, 15, 20 | 0 |
|  | CA\_n1A-n7A  CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n3A-n5A  CA\_n3A-n7A | n5 | 5, 10, 15, 20 |  |
|  | CA\_n3A-n78A  CA\_n5A-n7A | n7 | CA\_n7B\_BCS0 |  |
|  | CA\_n5A-n78A  CA\_n7A-n78A  CA\_n7B | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n5A-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n79A  CA\_n3A-n5A  CA\_n3A-n28A  CA\_n3A-n79A  CA\_n5A-n28A  CA\_n5A-n79A  CA\_n28A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n7A-n8A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n8A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n8A  CA\_n3A-n78A  CA\_n7A-n8A  CA\_n7A-n78A  CA\_n8A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n8 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7A-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7A-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7A-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7A-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7A-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3B-n7B-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7B-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7B-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A) BCS0 |  |
| CA\_n1A-n3B-n7B-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n3B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7B-n26A-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7B-n26(2A)-n78A | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7B-n26A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7B-n26(2A)-n78(2A) | CA\_n1A-n3A  CA\_n1A-n26A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n26A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n26A  CA\_n26A-n78A  CA\_n7A-n78A  CA\_n7B | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n26 | CA\_n26(2A)\_BCS0 |  |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n1A-n3A-n7A-n28A-n38A4 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n1A-n3A-n7A-n28A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A | n1 | 5, 10, 15, 20 | 1 |
|  | CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | CA\_n7A-n28A  CA\_n7A-n78A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n28A-n78A | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7B-n28A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n28A  CA\_n3A-n78A  CA\_n7A-n28A  CA\_n7A-n78A  CA\_n7B  CA\_n28A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n28A-n78(2A) | CA\_n78(2A)  CA\_n1A-n3A  CA\_n1A-n7A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  | CA\_n1A-n28A  CA\_n1A-n78A | n3 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n7A  CA\_n3A-n28A | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  | CA\_n3A-n78A  CA\_n7A-n28A | n28 | 5, 10, 15, 20, 30 |  |
|  | CA\_n7A-n78A  CA\_n28A-n78A | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7B-n28A-n78(2A) | CA\_n7B CA\_n78(2A) CA\_n1A-n3A CA\_n1A-n7A CA\_n1A-n28A CA\_n1A-n78A CA\_n3A-n7A CA\_n3A-n28A CA\_n3A-n78A CA\_n7A-n28A CA\_n7A-n78A CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n7A-n28A-n78A | CA\_n1A-n3A CA\_n1A-n7A CA\_n1A-n28A CA\_n1A-n78A CA\_n3A-n7A CA\_n3A-n28A CA\_n3A-n78A CA\_n7A-n28A CA\_n7A-n78A CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7A-n28A-n78(2A) | CA\_n78(2A) CA\_n1A-n3A CA\_n1A-n7A CA\_n1A-n28A CA\_n1A-n78A CA\_n3A-n7A CA\_n3A-n28A CA\_n3A-n78A CA\_n7A-n28A CA\_n7A-n78A CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3B-n7B-n28A-n78A | CA\_n7B CA\_n1A-n3A CA\_n1A-n7A CA\_n1A-n28A CA\_n1A-n78A CA\_n3A-n7A CA\_n3A-n28A CA\_n3A-n78A CA\_n7A-n28A CA\_n7A-n78A CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3B-n7B-n28A-n78(2A) | CA\_n7B CA\_n78(2A) CA\_n1A-n3A CA\_n1A-n7A CA\_n1A-n28A CA\_n1A-n78A CA\_n3A-n7A CA\_n3A-n28A CA\_n3A-n78A CA\_n7A-n28A CA\_n7A-n78A CA\_n28A-n78A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | CA\_n3B\_BCS0 |  |
|  |  | n7 | CA\_n7B\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7A-n38A-n78A4 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n67A-n78A | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | 10, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n7A-n67A-n78(2A) | CA\_n1A-n3A  CA\_n1A-n7A  CA\_n1A-n78A  CA\_n3A-n7A  CA\_n3A-n78A  CA\_n7A-n78A  CA\_n78(2A) | n1 | 5, 10, 15, 20, 25, 30, 40, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 35, 40, 45, 50 |  |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n1A-n3A-n7A-n75A-n78A | - | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n3 | n3 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n75 | n75 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n3A-n28A-n38A-n78A | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n41A-n77A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n41A-n77A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n3A-n28A-n41A-n79A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n79A  CA\_n28A-n41A  CA\_n28A-n79A  CA\_n41A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n28A-n77A-n79A | CA\_n1A-n3A  CA\_n1A-n28A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n28A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n3A-n40A-n78A-n105A | CA\_n1A-n3A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n3A-n41A-n77A-n79A | CA\_n1A-n3A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n3 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n1A-n5A-n28A-n78A-n79A | CA\_n1A-n5A  CA\_n1A-n28A  CA\_n1A-n78A  CA\_n1A-n79A  CA\_n5A-n28A  CA\_n5A-n78A  CA\_n5A-n79A  CA\_n28A-n78A  CA\_n28A-n79A  CA\_n78A-n79A | n1 | n1 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n5 | n5 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n28 | n28 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n79 | n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n1A-n7A-n28A-n38A-n78A4 | - | n1 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n1A-n7A-n40A-n78A-n105A | CA\_n1A-n7A  CA\_n1A-n40A  CA\_n1A-n78A  CA\_n1A-n105A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n1A-n28A-n41A-n77A-n79A | CA\_n1A-n28A  CA\_n1A-n41A  CA\_n1A-n77A  CA\_n1A-n79A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n1 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n2A-n5A-n30A-n66A-n77A | n773  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n30A-n66A-n77(2A) | n773  CA\_n2A-n5A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n5A-n30A  CA\_n5A-n66A  CA\_n5A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n5A-n48A-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48B-n66A-n77A | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n48B  CA\_n66A-n77A | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | CA\_n48B\_BCS2 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n5A-n48A-n66A-n77C | CA\_n2A-n5A  CA\_n2A-n48A  CA\_n2A-n66A  CA\_n2A-n77A  CA\_n5A-n48A  CA\_n5A-n66A  CA\_n5A-n77A  CA\_n48A-n66A  CA\_n66A-n77A  CA\_n77C | n2 | 5, 10, 15, 20 | 0 |
|  |  | n5 | 5, 10, 15, 20 |  |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n2A-n12A-n30A-n66A-n77A | n773  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n12A-n30A-n66A-n77(2A) | n773  CA\_n2A-n12A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n12A-n30A  CA\_n12A-n66A  CA\_n12A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n12 | 5, 10, 15 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n14A-n30A-n66A-n77A | n773  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n14A-n30A-n66A-n77(2A) | n773  CA\_n2A-n14A  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n14A-n30A  CA\_n14A-n66A  CA\_n14A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n14 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n2A-n29A-n30A-n66A-n77A | n773  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n2A-n29A-n30A-n66A-n77(2A) | n773  CA\_n2A-n30A  CA\_n2A-n66A  CA\_n2A-n77A3  CA\_n30A-n66A  CA\_n30A-n77A3  CA\_n66A-n77A3 | n2 | 5, 10, 15, 20 | 0 |
|  |  | n29 | 5, 10 |  |
|  |  | n30 | 5, 10 |  |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n3A-n7A-n20A-n67A-n78A | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n3A-n7A-n20A-n67A-n78(2A) | CA\_n3A-n7A  CA\_n3A-n20A  CA\_n3A-n78A  CA\_n7A-n20A  CA\_n7A-n78A  CA\_n20A-n78A  CA\_n78(2A) | n3 | n3 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n7 | n7 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n78 | CA\_n78(2A)\_BCS 4 and 5 |  |
| CA\_n3A-n7A-n28A-n38A-n78A4 | - | n3 | 5, 10, 15, 20, 25, 30, 40, 45, 50 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n3A-n7A-n40A-n78A-n105A | CA\_n3A-n7A  CA\_n3A-n40A  CA\_n3A-n78A  CA\_n3A-n105A  CA\_n7A-n40A  CA\_n7A-n78A  CA\_n7A-n105A  CA\_n40A-n78A  CA\_n40A-n105A  CA\_n78A-n105A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n7 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n3A-n28A-n41A-n77A-n79A | CA\_n3A-n28A  CA\_n3A-n41A  CA\_n3A-n77A  CA\_n3A-n79A  CA\_n28A-n41A  CA\_n28A-n77A  CA\_n28A-n79A  CA\_n41A-n77A  CA\_n41A-n79A  CA\_n77A-n79A | n3 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
| CA\_n25A-n41A-n66A-n71A-n77A | n413,4  n773,4  CA\_n25A-n41A3  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A3  CA\_n41A-n66A3  CA\_n41A-n71A3CA\_n41A-n77A3  CA\_n66A-n71A  CA\_n66A-n77A3  CA\_n71A-n77A3 | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n71A-n77(2A) | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | CA\_77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41A-n66(2A)-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n71(2A)-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41A-n66A-n71B-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41C-n66A-n71A-n77A | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n41C CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n41(2A)-n66A-n71A-n77A | CA\_n25A-n41A CA\_n25A-n66A CA\_n25A-n71A CA\_n25A-n77A CA\_n41A-n66A CA\_n41A-n71A CA\_n41A-n77A CA\_n66A-n71A CA\_n66A-n77A CA\_n71A-n77A | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_41(2A)\_BCS 4 and 5 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A-n66A-n71A-n77A | CA\_n25A-n41A  CA\_n25A-n66A  CA\_n25A-n71A  CA\_n25A-n77A  CA\_n41A-n66A  CA\_n41A-n71A  CA\_n41A-n77A  CA\_n66A-n71A  CA\_n66A-n77A  CA\_n71A-n77A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| NOTE 1: The SCS of each channel bandwidth for NR FR1 and NR FR2 band refers to Table 5.3.5-1 of TS 38.101-1 and TS 38.101-2 respectively.  NOTE 2: Only single uplink carriers with power class other than PC3 are listed.  NOTE 3: Minimum requirements for Power Class 2 are applicable for this uplink combination or single uplink carrier in this downlink/uplink combination.  NOTE 4: For a band combination which includes band n7 and n38 simultaneously, carriers in band n7 and n38 can only be configured as downlink carriers. Power imbalance between downlink carriers on Band n7 and Band n38 is assumed to be within 6dB.  NOTE 5: Power Class 1.5 is allowed for this single uplink carrier in this downlink/uplink combination. | | | | |

---Text omitted---

Table 5.5B.1-3: Inter-band NR DC configurations (four bands)

| NR DC  configuration | Uplink NR DC  configuration |
| --- | --- |
| DC\_n1A-n3A-n7A-n67A | DC\_n1A-n3A  DC\_n1A-n7A  DC\_n3A-n7A |
| DC\_n1A-n3A-n7A-n78A | DC\_n1A-n3A  DC\_n1A-n7A  DC\_n1A-n78A  DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n1A-n3A-n7A-n78(2A) | DC\_n1A-n3A  DC\_n1A-n7A  DC\_n1A-n78A  DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n1A-n3A-n20A-n67A | DC\_n1A-n3A  DC\_n1A-n20A  DC\_n3A-n20A |
| DC\_n1A-n3A-n28A-n41A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n41A  DC\_n3A-n28A  DC\_n3A-n41A  DC\_n28A-n41A |
| DC\_n1A-n3A-n28A-n77A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n77A  DC\_n3A-n28A  DC\_n3A-n77A  DC\_n28A-n77A |
| DC\_n1A-n3A-n28A-n79A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n79A  DC\_n3A-n28A  DC\_n3A-n79A  DC\_n28A-n79A |
| DC\_n1A-n3A-n41A-n77A | DC\_n1A-n3A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n41A-n77A |
| DC\_n1A-n3A-n41A-n79A | DC\_n1A-n3A  DC\_n1A-n41A  DC\_n1A-n79A  DC\_n3A-n41A  DC\_n3A-n79A  DC\_n41A-n79A |
| DC\_n1A-n3A-n67A-n78A | DC\_n1A-n3A  DC\_n1A-n78A  DC\_n3A-n78A |
| DC\_n1A-n3A-n67A-n78(2A) | DC\_n1A-n3A  DC\_n1A-n78A  DC\_n3A-n78A |
| DC\_n1A-n3A-n77A-n79A | DC\_n1A-n3A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n77A-n79A |
| DC\_n1A-n7A-n28A-n78A | DC\_n1A-n7A DC\_n1A-n28A DC\_n1A-n78A DC\_n7A-n28A DC\_n7A-n78A DC\_n28A-n78A |
| DC\_n1A-n7A-n28A-n78(2A) | DC\_n1A-n7A DC\_n1A-n28A DC\_n1A-n78A DC\_n7A-n28A DC\_n7A-n78A DC\_n28A-n78A |
| DC\_n1A-n7A-n67A-n78A | DC\_n1A-n7A  DC\_n1A-n78A  DC\_n7A-n78A |
| DC\_n1A-n7A-n67A-n78(2A) | DC\_n1A-n7A  DC\_n1A-n78A  DC\_n7A-n78A |
| DC\_n1A-n28A-n41A-n77A | DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n41A-n77A |
| DC\_n1A-n28A-n41A-n79A | DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n79A  DC\_n28A-n41A  DC\_n28A-n79A  DC\_n41A-n79A |
| DC\_n1A-n28A-n77A-n79A | DC\_n1A-n28A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n1A-n41A-n77A-n79A | DC\_n1A-n41A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |
| DC\_n3A-n7A-n20A-n67A | DC\_n3A-n7A  DC\_n3A-n20A  DC\_n7A-n20A |
| DC\_n3A-n7A-n20A-n78A | DC\_n3A-n7A  DC\_n3A-n20A  DC\_n3A-n78A  DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n3A-n7A-n20A-n78(2A) | DC\_n3A-n7A  DC\_n3A-n20A  DC\_n3A-n78A  DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n3A-n7A-n28A-n78A | DC\_n3A-n7A  DC\_n3A-n28A  DC\_n3A-n78A  DC\_n7A-n28A  DC\_n7A-n78A  DC\_n28A-n78A |
| DC\_n3A-n7A-n28A-n78(2A) | DC\_n3A-n7A  DC\_n3A-n28A  DC\_n3A-n78A  DC\_n7A-n28A  DC\_n7A-n78A  DC\_n28A-n78A |
| DC\_n3A-n7A-n67A-n78A | DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n3A-n7A-n67A-n78(2A) | DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n3A-n20A-n67A-n78A | DC\_n3A-n20A  DC\_n3A-n78A  DC\_n20A-n78A |
| DC\_n3A-n20A-n67A-n78(2A) | DC\_n3A-n20A  DC\_n3A-n78A  DC\_n20A-n78A |
| DC\_n3A-n28A-n41A-n77A | DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n41A-n77A |
| DC\_n3A-n28A-n41A-n79A | DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n79A  DC\_n28A-n41A  DC\_n28A-n79A  DC\_n41A-n79A |
| DC\_n3A-n28A-n77A-n79A | DC\_n3A-n28A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n3A-n28A-n77(2A)-n79A | DC\_n3A-n28A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n3A-n41A-n77A-n79A | DC\_n3A-n41A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |
| DC\_n7A-n20A-n67A-n78A | DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n7A-n20A-n67A-n78(2A) | DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n28A-n41A-n77A-n79A | DC\_n28A-n41A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |

Table 5.5B.1-4: Inter-band NR DC configurations (five bands)

| NR DC  configuration | Uplink NR DC  configuration |
| --- | --- |
| DC\_n1A-n3A-n7A-n67A-n78A | DC\_n1A-n3A  DC\_n1A-n7A  DC\_n1A-n78A  DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n1A-n3A-n7A-n67A-n78(2A) | DC\_n1A-n3A  DC\_n1A-n7A  DC\_n1A-n78A  DC\_n3A-n7A  DC\_n3A-n78A  DC\_n7A-n78A |
| DC\_n1A-n3A-n28A-n41A-n77A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n41A-n77A |
| DC\_n1A-n3A-n28A-n41A-n79A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n79A  DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n79A  DC\_n28A-n41A  DC\_n28A-n79A  DC\_n41A-n79A |
| DC\_n1A-n3A-n28A-n77A-n79A | DC\_n1A-n3A  DC\_n1A-n28A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n3A-n28A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n77A-n79A |
| DC\_n1A-n3A-n41A-n77A-n79A | DC\_n1A-n3A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |
| DC\_n1A-n28A-n41A-n77A-n79A | DC\_n1A-n28A  DC\_n1A-n41A  DC\_n1A-n77A  DC\_n1A-n79A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |
| DC\_n3A-n7A-n20A-n67A-n78A | DC\_n3A-n7A  DC\_n3A-n20A  DC\_n3A-n78A  DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n3A-n7A-n20A-n67A-n78(2A) | DC\_n3A-n7A  DC\_n3A-n20A  DC\_n3A-n78A  DC\_n7A-n20A  DC\_n7A-n78A  DC\_n20A-n78A |
| DC\_n3A-n28A-n41A-n77A-n79A | DC\_n3A-n28A  DC\_n3A-n41A  DC\_n3A-n77A  DC\_n3A-n79A  DC\_n28A-n41A  DC\_n28A-n77A  DC\_n28A-n79A  DC\_n41A-n77A  DC\_n41A-n79A  DC\_n77A-n79A |

---Text omitted---

##### 6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands)

Table 6.2A.4.2.5-1: ΔTIB,c due to NR CA (four bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)5 | | | |
| Component band in order of bands in configuration6 | | | |
| CA\_n1-n3-n5-n7 | 0.6 | 0.6 | 0.3 | - |
| CA\_n1-n3-n5-n28 | 0.3 | 0.3 | 0.7 | 0.7 |
| CA\_n1-n3-n5-n78 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n7-n8 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n26 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n28 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n7-n38 | 0.6 | 0.6 | N/A | N/A |
| CA\_n1-n3-n7-n67 | 0.6 | 0.6 | 0.6 | N/A |
| CA\_n1-n3-n7-n75 | 0.6 | 0.6 | 0.6 | N/A |
| CA\_n1-n3-n7-n78 | 0.7 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n7-n79 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n8-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n18-n28 | 0.3 | 0.3 | 0.5 | 0.5 |
| CA\_n1-n3-n18-n41 | 0.5 | 0.5 | 0.3 | 0.33 / 0.84 |
| CA\_n1-n3-n18-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n1-n3-n20-n67 | 0.3 | 0.3 | 0.3 | - |
| CA\_n1-n3-n26-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n38 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n1-n3-n28-n41 | 0.5 | 0.5 | 0.5 | 0.33 / 0.84 |
| CA\_n1-n3-n28-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n28-n79 | 0.3 | 0.3 | 0.6 | 0.8 |
| CA\_n1-n3-n40-n77 | 0.7 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n40-n105 | 0.7 | 0.7 | 0.7 | 0.5 |
| CA\_n1-n3-n41-n77 | 0.6 | 0.6 | 0.33 / 0.84 | 0.8 |
| CA\_n1-n3-n41-n79 | 0.5 | 0.5 | 0.53 / 0.84 | 0.8 |
| CA\_n1-n3-n67-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n3-n75-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n3-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n5-n28-n78 | 0.3 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n5-n28-n79 | 0.3 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n5-n78-n79 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n7-n8-n40 | 0.6 | 0.8 | 0.6 | 0.9 |
| CA\_n1-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n26-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n28-n38 | 0.5 | N/A | 0.6 | N/A |
| CA\_n1-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n7-n40-n78 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n7-n40-n105 | 0.6 | 0.5 | 0.5 | 0.5 |
| CA\_n1-n7-n67-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n7-n75-n78 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_n1-n7-n78-n105 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n1-n8-n78-n79 | 0.3 | 0.6 | 0.8 | 0.5 |
| CA\_n1-n18-n28-n41 | 0.6 | 0.5 | 0.6 | 0.5 |
| CA\_n1-n18-n28-n77 | 0.6 | 0.5 | 0.6 | 0.8 |
| CA\_n1-n18-n41-n77 | 0.5 | 0.5 | 0.5 | 0.8 |
| CA\_n1-n28-n38-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n40-n77 | 0.3 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n28-n40-n78 | 0.3 | 0.6 | 0.5 | 0.8 |
| CA\_n1-n28-n41-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n41-n79 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n28-n75-n78 | 0.5 | 0.6 | - | 0.8 |
| CA\_n1-n28-n77-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n28-n78-n79 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n41-n77-n79 | 0.6 | 0.5 | 0.8 | 0.8 |
| CA\_n2-n5-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n5-n30-n77 | 0.6 | 0.6 | 0.3 | 0.8 |
| CA\_n2-n5-n48-n66 | 0.6 | 0.3 | 0.8 | 0.6 |
| CA\_n2-n5-n48-n77 | 0.6 | 0.3 | 0.8 | 0.8 |
| CA\_n2-n5-n66-n77 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n2-n12-n30-n66 | 0.5 | 0.8 | 0.3 | 0.5 |
| CA\_n2-n12-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n12-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n14-n30-n66 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n2-n14-n30-n77 | 0.6 | 0.5 | 0.3 | 0.8 |
| CA\_n2-n14-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n2-n29-n30-n66 | 0.5 | N/A | 0.3 | 0.5 |
| CA\_n2-n29-n30-n77 | 0.6 | N/A | 0.3 | 0.8 |
| CA\_n2-n29-n66-n77 | 0.6 | N/A | 0.6 | 0.8 |
| CA\_n2-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n2-n41-n66-n71 | 0.5 | 0.83 / 1.34 | 0.5 | 0.6 |
| CA\_n2-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n66-n71-n77 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n66-n71-n78 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n3-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n5-n28-n78 | 0.6 | 0.7 | 0.7 | 0.8 |
| CA\_n3-n5-n28-n79 | 0.6 | 0.7 | 0.7 | 0.8 |
| CA\_n3-n7-n8-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n20-n67 | 0.5 | 0.5 | 0.3 | - |
| CA\_n3-n7-n20-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n7-n26-n78 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n7-n28-n38 | 0.5 | N/A | 0.3 | N/A |
| CA\_n3-n7-n28-n78 | 0.6 | 0.6 | 0.6 | 0.6 |
| CA\_n3-n7-n40-n105 | 0.6 | 0.6 | 0.6 | 0.5 |
| CA\_n3-n7-n67-n78 | 0.6 | 0.6 | N/A | 0.6 |
| CA\_n3-n7-n75-n78 | 0.6 | 0.6 | N/A | 0.6 |
| CA\_n3-n7-n78-n105 | 0.6 | 0.6 | 0.8 | 0.5 |
| CA\_n3-n18-n28-n41 | 0.5 | 0.4 | 0.4 | 0.33 / 0.84 |
| CA\_n3-n18-n28-n77 | 0.6 | 0.5 | 0.5 | 0.8 |
| CA\_n3-n18-n41-n77 | 0.6 | 0.4 | 0.33 / 0.84 | 0.8 |
| CA\_n3-n20-n67-n78 | 0.5 | 0.5 | - | 0.8 |
| CA\_n3-n28-n40-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n3-n28-n41-n77 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n41-n78 | 1 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n41-n79 | 0.5 | 0.5 | 0.31 / 0.82 | 0.8 |
| CA\_n3-n28-n77-n79 | 0.6 | 0.5 | 0.8 | 0.8 |
| CA\_n3-n41-n77-n79 | 0.6 | 0.31 / 0.82 | 0.8 | 0.8 |
| CA\_n5-n25-n29-n66 | 0.5 | 0.5 | N/A | 0.5 |
| CA\_n5-n25-n66-n77 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n25-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n5-n28-n78-n79 | 0.7 | 0.7 | 0.8 | 0.8 |
| CA\_n5-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n5-n48-n66-n77 | 0.6 | 0.8 | 0.6 | 0.8 |
| CA\_n7-n8-n40-n78 | 0.5 | 0.3 | 0.5 | 0.8 |
| CA\_n7-n12-n25-n66 | 0.5 | 0.3 | 0.5 | 0.5 |
| CA\_n7-n20-n67-n78 | 0.6 | 0.6 | - | 0.8 |
| CA\_n7-n25-n66-n71 | 0.5 | 0.5 | 0.5 | 0.6 |
| CA\_n7-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n25-n66-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n40-n78-n105 | 0.5 | 0.6 | 0.8 | 0.5 |
| CA\_n8-n20-n28-n75 | 0.8 | 0.7 | 0.7 | - |
| CA\_n12-n30-n66-n77 | 0.8 | 0.3 | 0.6 | 0.8 |
| CA\_n13-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n14-n30-n66-n77 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n18-n28-n41-n77 | 0.5 | 0.5 | 0.33 / 0.84 | 0.8 |
| CA\_n25-n38-n66-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n25-n41-n66-n71 | 0.5 | 0.5 | 0.5 | 0.3 |
| CA\_n25-n41-n66-n77 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n66-n78 | 0.5 | 0.83 / 1.34 | 0.5 | 0.8 |
| CA\_n25-n41-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n41-n71-n78 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n41-n77-n85 | 0.5 | 0.5 | 0.8 | 0.6 |
| CA\_n25-n66-n71-n77 | 0.5 | 0.5 | 0.6 | 0.8 |
| CA\_n25-n66-n71-n78 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n28-n41-n77-n79 | 0.5 | 0.3 | 0.8 | 0.8 |
| CA\_n29-n30-n66-n77 | N/A | 0.3 | 0.6 | 0.8 |
| CA\_n41-n66-n70-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n41-n66-n71-n77 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| CA\_n41-n66-n71-n78 | 0.33 / 0.84 | 1 | 0.5 | 0.8 |
| CA\_n41-n66-n77-n85 | 0.33 / 0.84 | 1 | 0.8 | 0.5 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz.  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz.  NOTE 5: “-” denotes ΔTIB,c = 0.  NOTE 6: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n78 the band order from left to right is n1, n3, n5 and n78. | | | | |

##### 6.2A.4.2.6 ΔTIB,c for Inter-band CA (five bands)

Table 6.2A.4.2.6-1: ΔTIB,c due to NR CA (five bands)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔTIB,c for NR bands (dB)1 | | | | |
| Component band in order of bands in configuration2 | | | | |
| CA\_n1-n3-n5-n7-n78 | 0.6 | 0.6 | 0.6 | 0.6 | 0.8 |
| CA\_n1-n3-n5-n28-n78 | 0.6 | 0.6 | 0.7 | 0.7 | 0.8 |
| CA\_n1-n3-n7-n8-n78 | 0.7 | 0.7 | 0.7 | 0.6 | 0.8 |
| CA\_n1-n3-n7-n26-n78 | 0.7 | 0.7 | 0.7 | 0.6 | 0.8 |
| CA\_n1-n3-n7-n28-n38 | 0.6 | 0.6 | N/A | 0.6 | N/A |
| CA\_n1-n3-n7-n28-n78 | 0.7 | 0.7 | 0.7 | 0.6 | 0.8 |
| CA\_n1-n3-n7-n67-n78 | 0.7 | 0.7 | 0.7 | N/A | 0.8 |
| CA\_n1-n3-n7-n75-n78 | 0.6 | 0.6 | 0.6 | N/A | 0.8 |
| CA\_ n1-n3-n28-n41-n77 | 0.6 | 1 | 0.6 | 0.63/0.84 | 0.8 |
| CA\_n1-n3-n28-n41-n79 | 0.5 | 0.5 | 0.6 | 0.63/0.84 | 0.8 |
| CA\_n1-n3-n28-n77-n79 | 0.6 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n1-n3-n40-n78-n105 | 0.6 | 0.6 | 0.6 | 0.8 | 0.6 |
| CA\_n1-n3-n41-n77-n79 | 0.6 | 0.6 | 0.53/0.84 | 0.8 | 0.8 |
| CA\_n1-n5-n28-n78-n79 | 0.6 | 0.7 | 0.7 | 0.8 | 0.8 |
| CA\_n1-n7-n40-n78-n105 | 0.6 | 0.6 | 0.6 | 0.8 | 0.6 |
| CA\_n1-n28-n41-n77-n79 | 0.6 | 0.6 | 0.6 | 0.8 | 0.8 |
| CA\_n2-n5-n30-n66-n77 | 0.6 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n2-n5-n48-n66-n77 | 0.6 | 0.3 | 0.8 | 0.6 | 0.8 |
| CA\_n2-n12-n30-n66-n77 | 0.6 | 0.8 | 0.3 | 0.6 | 0.8 |
| CA\_n2-n14-n30-n66-n77 | 0.6 | 0.6 | 0.3 | 0.6 | 0.8 |
| CA\_n2-n29-n30-n66-n77 | 0.6 | N/A | 0.3 | 0.6 | 0.8 |
| CA\_n3-n7-n20-n67-n78 | 0.6 | 0.6 | 0.6 | - | 0.8 |
| CA\_n3-n7-n40-n78-n105 | 0.6 | 0.8 | 0.6 | 0.8 | 0.6 |
| CA\_n3-n28-n41-n77-n79 | 1 | 0.5 | 0.8 | 0.8 | 0.8 |
| NOTE 1: “-” denotes ΔTIB,c = 0.  NOTE 2: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n7-n78 the band order from left to right is n1, n3, n5, n7 and n78.  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz | | | | | |

##### 6.2A.4.2.7 ΔTIB,c for Inter-band CA (six bands)

Table 6.2A.4.2.7-1: ΔTIB,c due to NR CA (six bands)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Inter-band CA combination |  | ΔTIB,c for NR bands (dB)1 | | | | |
|  | Component band in order of bands in configuration2 | | | | |
| CA\_n1-n3-n7-n28-n38-n78 | 0.7 | 0.7 | N/A | 0.6 | N/A | 0.8 |
| NOTE 1: “-” denotes ΔTIB,c = 0.  NOTE 2: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n7-n78 the band order from left to right is n1, n3, n5, n7 and n78. | | | | | | |

---Text omitted---

##### 7.3A.3.2.4 ΔRIB,c for four bands

Table 7.3A.3.2.4-1: ΔRIB,c due to CA (four bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔRIB,c for NR bands (dB)7 | | | |
| Component band in order of bands in configuration8 | | | |
| CA\_n1-n3-n5-n28 | 0.2 | 0.2 | 0.2 | 0.2 |
| CA\_n1-n3-n5-n78 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n3-n7-n8 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n26 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n28 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n67 | - | - | - | 0.2 |
| CA\_n1-n3-n7-n78 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n1-n3-n7-n79 | 0.2 | - | 0.2 | 0.5 |
| CA\_n1-n3-n8-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n18-n28 | - | - | - | 0.2 |
| CA\_n1-n3-n18-n41 | - | - | - | 05 / 0.56 |
| CA\_n1-n3-n18-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n3-n20-n67 | - | - | - | 0.2 |
| CA\_n1-n3-n26-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n38 | - | - | 0.2 | - |
| CA\_n1-n3-n28-n41 | - | - | 0.2 | 05 / 0.56 |
| CA\_n1-n3-n28-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n28-n79 | - | - | 0.2 | 0.5 |
| CA\_n1-n3-n40-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n1-n3-n40-n105 | 0.3 | 0.3 | 0.3 | 0.3 |
| CA\_n1-n3-n41-n77 | 0.2 | 0.2 | 05 / 0.56 | 0.5 |
| CA\_n1-n3-n41-n79 | - | - | 05 / 0.56 | 0.5 |
| CA\_n1-n3-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n75-n78 | - | - | - | 0.5 |
| CA\_n1-n3-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n28-n79 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n5-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n7-n8-n40 | - | - | 0.3 | 0.8 |
| CA\_n1-n7-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n7-n26-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n28-n38 | - | - | 0.2 | - |
| CA\_n1-n7-n28-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n40-n78 | 0.2 | - | 0.4 | 0.5 |
| CA\_n1-n7-n40-n105 | 0.2 | - | 0.4 | 0.3 |
| CA\_n1-n7-n67-n78 | 0.2 | 0.2 | - | - |
| CA\_n1-n7-n75-n78 | - | - | - | 0.5 |
| CA\_n1-n7-n78-n105 | 0.2 | 0.2 | 0.5 | 0.3 |
| CA\_n1-n8-n40-n78 | 0.2 | - | 0.4 | 0.5 |
| CA\_n1-n8-n78-n79 | 0.3 | 0.3 | 0.5 | - |
| CA\_n1-n18-n28-n41 | 0.2 | - | 0.2 | - |
| CA\_n1-n18-n28-n77 | 0.2 | - | 0.2 | 0.5 |
| CA\_n1-n18-n41-n77 | 0.2 | - | - | 0.5 |
| CA\_n1-n28-n38-n78 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n28-n40-n77 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n40-n78 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n41-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n1-n28-n41-n79 | - | 0.2 | 0.5 | 0.5 |
| CA\_n1-n28-n75-n78 | - | 0.2 | - | 0.5 |
| CA\_n1-n28-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n28-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n5-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n5-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n5-n48-n66 | 0.2 | - | 0.5 | 0.2 |
| CA\_n2-n5-n48-n77 | 0.2 | - | 0.5 | 0.5 |
| CA\_n2-n5-n66-n77 | 0.3 | - | 0.3 | 0.5 |
| CA\_n2-n12-n30-n66 | 0.4 | 0.5 | 0.5 | 0.4 |
| CA\_n2-n12-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n12-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n14-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n14-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n14-n66-n77 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n2-n29-n30-n66 | 0.4 | - | 0.5 | 0.4 |
| CA\_n2-n29-n30-n77 | 0.2 | 0.2 | - | 0.5 |
| CA\_n2-n30-n66-n77 | 0.2 | 0.5 | 0.4 | 0.5 |
| CA\_n2-n41-n66-n71 | 0.3 | 0.51 / 12 | 0.5 | 0.3 |
| CA\_n2-n48-n66-n77 | 0.3 | 0.5 | 0.3 | 0.5 |
| CA\_n2-n66-n71-n77 | 0.3 | 0.5 | - | 0.5 |
| CA\_n2-n66-n71-n78 | 0.3 | 0.5 | - | 0.5 |
| CA\_n3-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n5-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n5-n28-n79 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n8-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n20-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n26-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n28-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n40-n105 | 0.2 | 0.2 | 0.2 | 0.3 |
| CA\_n3-n7-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n75-n78 | - | - | - | 0.5 |
| CA\_n3-n7-n78-n105 | 0.2 | 0.2 | 0.5 | 0.3 |
| CA\_n3-n18-n28-n41 | - | - | - | 05 / 0.56 |
| CA\_n3-n18-n28-n77 | 0.2 | - | 0.2 | 0.5 |
| CA\_n3-n18-n41-n77 | 0.2 | - | 05 / 0.56 | 0.5 |
| CA\_n3-n20-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n40-n77 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n28-n41-n77 | 0.5 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n28-n41-n78 | 0.5 | 0.2 | 01 / 0.52 | 0.5 |
| CA\_n3-n28-n41-n79 | - | 0.2 | 0.5 | 0.5 |
| CA\_n3-n28-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n3-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n5-n25-n29-n66 | 0.5 | - | 0.3 | - |
| CA\_n5-n25-n66-n77 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n5-n25-n66-n78 | 0.5 | 0.3 | 0.3 | 0.5 |
| CA\_n5-n28-n78-n79 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n5-n30-n66-n77 | 0.2 | 0.4 | 0.4 | 0.5 |
| CA\_n5-n48-n66-n77 | 0.2 | 0.5 | 0.2 | 0.5 |
| CA\_n7-n8-n40-n78 | - | 0.2 | 0.4 | 0.5 |
| CA\_n7-n12-n25-n66 | 0.5 | 0.5 | 0.3 | 0.5 |
| CA\_n7-n20-n67-n78 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n7-n25-n66-n71 | 0.5 | 0.3 | 0.5 | 0.3 |
| CA\_n7-n25-n66-n77 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n25-n66-n78 | 0.5 | 0.6 | 0.6 | 0.8 |
| CA\_n7-n40-n78-n105 | 0.5 | 0.5 | 0.8 | 0.3 |
| CA\_n8-n20-n28-n75 | 0.3 | 0.2 | 0.2 | - |
| CA\_n12-n30-n66-n77 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n13-n25-n66-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n14-n30-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n18-n28-n41-n77 | - | 0.2 | 05 / 0.56 | 0.5 |
| CA\_n25-n38-n66-n78 | 0.3 | 0.4 | 0.3 | 0.5 |
| CA\_n25-n41-n66-n71 | 0.3 | 0.5 | 0.5 | - |
| CA\_n25-n41-n66-n77 | 0.3 | 0.53 / 1.04 | 0.3 | 0.5 |
| CA\_n25-n41-n66-n78 | 0.3 | 0.53 / 1.04 | 0.3 | 0.5 |
| CA\_n25-n41-n71-n77 | - | - | 0.2 | 0.5 |
| CA\_n25-n41-n77-n85 | - | - | 0.5 | 0.2 |
| CA\_n25-n41-n71-n78 | - | - | 0.2 | 0.5 |
| CA\_n25-n66-n71-n77 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n25-n66-n71-n78 | 0.3 | 0.3 | 0.3 | 0.5 |
| CA\_n28-n41-n77-n79 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n29-n30-n66-n77 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n41-n66-n70-n78 | - | 0.2 | 0.2 | 0.5 |
| CA\_n41-n66-n71-n77 | 03 / 0.54 | 0.5 | 0.2 | 0.5 |
| CA\_n41-n66-n71-n78 | 03 / 0.54 | 0.5 | 0.2 | 0.5 |
| CA\_n41-n66-n77-n85 | 03 / 0.54 | 0.5 | 0.5 | 0.2 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz  NOTE 5: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 6: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz  NOTE 7: “-” denotes ΔRIB,c = 0.  NOTE 8: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n7-n78 the band order from left to right is n1 n3, n7 and n78. | | | | |

##### 7.3A.3.2.5 ΔRIB,c for five bands

Table 7.3A.3.2.5-1: ΔRIB,c due to CA (five bands)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Inter-band CA combination | ΔRIB,c for NR bands (dB)1 | | | | |
| Component band in order of bands in configuration2 | | | | |
| CA\_n1-n3-n5-n7-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n5-n28-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n7-n26-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n7-n28-n38 | - | - | - | 0.2 | - |
| CA\_n1-n3-n7-n28-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n7-n67-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n1-n3-n7-n75-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_ n1-n3-n28-n41-n77 | 0.2 | 0.5 | 0.2 | 03/0.54 | 0.5 |
| CA\_n1-n3-n28-n41-n79 | - | - | 0.2 | 0.5 | 0.5 |
| CA\_n1-n3-n28-n77-n79 | 0.2 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n3-n40-n78-n105 | 0.2 | 0.2 | 0.2 | 0.5 | 0.2 |
| CA\_n1-n3-n41-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n1-n5-n28-n78-n79 | 0.2 | 0.2 | 0.2 | 0.5 | 0.5 |
| CA\_n1-n7-n40-n78-n105 | 0.2 | 0.2 | 0.2 | 0.5 | 0.2 |
| CA\_n1-n28-n41-n77-n79 | 0.2 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n5-n30-n66-n77 | 0.3 | 0.2 | 0.5 | 0.4 | 0.5 |
| CA\_n2-n5-n48-n66-n77 | 0.2 | - | 0.5 | 0.2 | 0.5 |
| CA\_n2-n12-n30-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n14-n30-n66-n77 | 0.2 | 0.2 | 0.5 | 0.5 | 0.5 |
| CA\_n2-n29-n30-n66-n77 | 0.2 | 0.5 | 0.5 | 0.5 | 0.5 |
| CA\_n3-n7-n20-n67-n78 | 0.2 | 0.2 | 0.2 | 0.2 | 0.5 |
| CA\_n3-n7-n40-n78-n105 | 0.2 | 0.5 | 0.2 | 0.5 | 0.2 |
| CA\_n3-n28-n41-n77-n79 | 0.5 | 0.2 | 0.5 | 0.5 | 0.5 |
| NOTE 1: “-” denotes ΔRIB,c = 0.  NOTE 2: The component band order in the configuration should be listed by the order of NR bands, such as for CA\_n1-n3-n5-n7-n78 the band order from left to right is n1 n3, n5, n7 and n78.  NOTE 3: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 4: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz | | | | | |

---End of changes---