**3GPP TSG-RAN WG4 Meeting #110 R4-24xxxxx**

**Athens, Greece, 26th February – 1st March 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **-1** | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | draft CR 38.101-1 adding UL configurations to CA\_n25-n41, CA\_n41-n66 and CA\_n41-n71 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson, Nokia | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CADC\_R18\_2BDL\_xBUL | | | | |  | ***Date:*** | | | 2024-02-19 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | adding UL configurations to CA\_n25-n41, CA\_n41-n66 and CA\_n41-n71 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Draft CR based on below TP’s:  R4-2401482, TP for 38718-02-01 adding UL CA\_n25A-n41C to DL CA\_n25(2A)-n41C  R4-2401483, TP for 38718-02-01 adding UL CA\_n41C-n66A to DL CA\_n41C-n66(2A)  R4-2401484, TP for 38718-02-01 adding UL CA\_n41C-n71A to DL CA\_n41C-n71(2A) and DL CA\_n41C-n71B | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | UL configurations are not added | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

---Start of changes---

Table 5.5A.3.1-1g: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n20A-n28A | CA\_n20A-n28A | n20 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n20 | 5, 10, 15, 20 | 1 |
|  |  | n28 | 5, 10, 15, 20, 30 |  |
|  |  | n20 | 5, 10, 15, 20 | 2 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n20A-n40A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n20A-n67A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n67 | 5, 10, 15, 20 |  |
|  |  | n20 | n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n67 | n67 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n75A | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n20 | 5, 10,15, 20 | 1 |
|  |  | n75 | 5, 10,15, 20, 25, 30, 40, 50 |  |
| CA\_n20A-n78A | CA\_n20A-n78A | n20 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n20A-n78C | - | n20 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n20A-n78(2A) | CA\_n20A-n78A  CA\_n78(2A) | n20 | See n20 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n24A-n41A | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n24A-n41(2A) | CA\_n24A-n41A | n24 | 5, 10 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 |  |
| CA\_n24A-n48A | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n24A-n48B | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48B\_BCS1 |  |
| CA\_n24A-n48(2A) | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n24A-n48(3A) | CA\_n24A-n48A | n24 | 5, 10 | 0 |
|  |  | n48 | CA\_n48(3A)\_BCS0 |  |
| CA\_n24A-n77A | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n24 | See n24 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n24A-n77C | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n24A-n77(2A) | CA\_n24A-n77A | n24 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n24 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n25A-n29A | - | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n25A-n38A | CA\_n25A-n38A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25(2A)-n38A | CA\_n25A-n38A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n25A-n41A13,14 | n418,9  CA\_n25A-n41A8, 13,14 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41A | n418,9  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n41C | n418,9  CA\_n25A-n41A8  CA\_n25A-n41C  CA\_n41C8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | CA\_n41C\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(2A) | n418,9  CA\_n25A-n41A 8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS3 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41C | n418,9  CA\_n25A-n41A8  CA\_n41C8 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  | n418,9  CA\_n25A-n41A8  CA\_n41C8  CA\_n25A-n41C | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C BCS 4 and 5 |  |
| CA\_n25A-n41(2A) | n418,9  CA\_n25A-n41A8 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS1 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | CA\_n41(2A)\_BCS3 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(3A) | n418,9  CA\_n25A-n41A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(3A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
| CA\_n25A-n41(A-C) | n418,9  CA\_n25A-n41A8  CA\_n41C8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(A-C)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(3A) | n418,9  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n41(A-C) | n418,9  CA\_n41C8  CA\_n25A-n41A8 | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 |  |
| CA\_n25A-n46A | - | n25 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
| CA\_n25A-n48A | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n25A-n48(2A) | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n25A-n48C | CA\_n25A-n48A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n48 | CA\_n48C\_BCS0 |  |
| CA\_n25A-n66A | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n66(2A) | CA\_n25A-n66A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n66A | CA\_n25A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | 10, 15, 20, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 2 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n66(2A) | CA\_n25A-n66A | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS1 | 2 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n71A | CA\_n25A-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n71B | CA\_n25A-n71A | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n71(2A) | CA\_n25A-n71A | n25 | 5, 10, 15, 20 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n71A | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n71(2A) | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n71B | CA\_n25A-n71A | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n25A-n77A | n778,9  CA\_n25A-n77A8,14 | n25 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25A-n77(3A) | n778,9  CA\_n77(2A)8  CA\_n25A-n77A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25(2A)-n77A | n778,9  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n77(2A) | n778,9  CA\_n77(2A)  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n25(2A)-n77(3A) | n778,9  CA\_n25(2A)  CA\_n77(2A)  CA\_n25A-n77A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS1 |  |
| CA\_n25A-n78A | n788,9  CA\_n25A-n78A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25A-n78(2A) | n788,9  CA\_n25A-n78A8 | n25 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  | CA\_n25A-n78A  CA\_n78(2A) | n25 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  | CA\_n25A-n78A | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n25(2A)-n78A | n788,9  CA\_n25A-n78A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n25 | CA\_n25(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n78(2A) | n788,9  CA\_n25A-n78A8 | n25 | CA\_n25(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n25 | CA\_n25(2A)\_BCS0 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n25 | CA\_n25(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n25A-n85A | CA\_n25A-n85A | n25 | See n25 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n25(2A)-n85A | CA\_n25A-n85A | n25 | CA\_n25(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |

Table 5.5A.3.1-1h: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n26A-n28A | CA\_n26-n2816 | n26 | 5, 10, 15, 20 | 0 |
|  |  | n28 | 5, 10, 15, 20 |  |
|  |  | n26 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n28 | 5, 10, 15, 20, 25, 30 |  |
| CA\_n26A-n29A | - | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n29 | 5, 10 |  |
| CA\_n26A-n48A | CA\_n26A-n48A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26A-n48(2A) | CA\_n26A-n48A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
| CA\_n26A-n66A | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n26A-n66(2A) | CA\_n26A-n66A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
| CA\_n26A-n66(3A) | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n26A-n70A | CA\_n26A-n70A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n26A-n71A | - | n26 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n26A-n77A | CA\_n26A-n77A | n26 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26A-n78A | CA\_n26A-n78A13 | n26 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26(2A)-n78A | CA\_n26A-n78A | n26 | CA\_n26(2A)\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n26A-n78(2A) | CA\_n26A-n78A | n26 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n26(2A)-n78(2A) | CA\_n26A-n78A | n26 | CA\_n26(2A)\_BCS0 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
| CA\_n28A-n34A | CA\_n28A-n34A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n34 | 5, 10, 15 |  |
| CA\_n28A-n38A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n28A-n39A | CA\_n28A-n39A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n39 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n28A-n40A | CA\_n28A-n40A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n40B | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n40 | CA\_n40B\_BCS0 |  |
| CA\_n28A-n41A | n418  CA\_n28A-n41A8, 13 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 30 | 1 |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n41B | CA\_n28A-n41A | n28 | 5, 10 | 0 |
|  |  | n41 | CA\_n41B\_BCS0 |  |
| CA\_n28A-n41C | CA\_n28A-n41A  CA\_n41C | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n28A-n46A | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | 20, 40, 60, 80 |  |
| CA\_n28A-n46C | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46C\_BCS0 |  |
| CA\_n28A-n46D | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46D\_BCS0 |  |
| CA\_n28A-n46(2A) | CA\_n28A-n46A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n46 | CA\_n46(2A)\_BCS0 |  |
| CA\_n28A-n50A | CA\_n28A-n50A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n50 | 5, 10, 15, 20, 40, 50, 60, 801 |  |
| CA\_n28A-n71A | - | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n28A-n74A | CA\_n28A-n74A | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n28A-n75A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n75 | 5, 10, 15, 20 |  |
|  |  | n28 | 5, 10, 15, 20 | 1 |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 2 |
|  |  | n75 | 5, 10, 15, 20, 25, 30, 40, 50 |  |
| CA\_n28A-n77A | n778,9  CA\_n28A-n77A8 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | See n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n77C | CA\_n28A-n77A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n28A-n77(2A) | n778,9  CA\_n77(2A)8  CA\_n28A-n77A8 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20, 25, 30 | 1 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS4 and 5 |  |
| CA\_n28A-n77(3A) | n778,9  CA\_n77(2A)  CA\_n28A-n77A8 | n28 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS4 and 5 |  |
| CA\_n28A-n78A | n788,9  CA\_n28A-n78A8,13 | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n28 | 5, 10, 15, 20, 30 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n78C | CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n28A-n78(2A) | CA\_n78(2A)  CA\_n28A-n78A | n28 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n28 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n28A-n79A | n798,9  CA\_n28A-n79A8 | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n28A-n79C | CA\_n79C | n28 | 5, 10, 15, 20, 30 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n28 | See n28 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n28A-n94A | - | n28 | 5, 10, 15, 20 | 0 |
|  |  | n94 | 5, 10, 15, 20 |  |
| CA\_n28A-n102A | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | 20, 40, 60, 80, 100 |  |
| CA\_n28A-n102(2A) | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102(2A)\_BCS0 |  |
| CA\_n28A-n102B | CA\_n28A-n102A  CA\_n28A-n102B | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102B\_BCS0 |  |
| CA\_n28A-n102C | CA\_n28A-n102A  CA\_n28A-n102C | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102C\_BCS0 |  |
| CA\_n28A-n102D | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102D\_BCS0 |  |
| CA\_n28A-n102E | CA\_n28A-n102A | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n102 | CA\_n102E\_BCS0 |  |
| CA\_n28A-n105A | - | n28 | 5, 10, 15, 20, 25, 30 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |
| CA\_n29A-n30A | - | n29 | 5, 10 | 0 |
|  |  | n30 | 5, 10 |  |
| CA\_n29A-n48A | - | n29 | 5, 10 | 0 |
|  |  | n48 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n66A | - | n29 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n29 | 5, 10 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n29A-n66B | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66B\_BCS0 |  |
| CA\_n29A-n66(2A) | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS0 |  |
|  |  | n29 | 5, 10 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n29A-n66(3A) | - | n29 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n29A-n70A | - | n29 | 5, 10 | 0 |
|  |  | n70 | 5, 10, 15, 201,, 251 |  |
| CA\_n29A-n71A | - | n29 | 5, 10 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n29A-n77A | n778, 9 | n29 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n29A-n77(2A) | n778, 9 | n29 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |

Table 5.5A.3.1-1i: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n30A-n66A | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n30A-n66(2A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n30A-n66(3A) | CA\_n30A-n66A | n30 | 5, 10 | 0 |
|  |  | n66 | CA\_n66(3A)\_BCS0 |  |
| CA\_n30A-n77A | n778, 9  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n30A-n77(2A) | n778, 9  CA\_n77(2A)  CA\_n30A-n77A8 | n30 | 5, 10 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n34A-n39A | CA\_n34A-n39A | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n40A | CA\_n34A-n40A | n34 | 5, 10, 15 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41A | CA\_n34A-n41A | n34 | 5, 10, 15 | 0 |
|  |  | n41 | 10, 15, 20, 30 ,40 ,50, 60, 70, 80, 90, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n41C | CA\_n41C  CA\_n34A-n41A  CA\_n34A-n41C | n34 | 5, 10, 15 | 0 |
|  |  | n41 | CA\_n41C\_BCS1 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n34A-n79A | CA\_n34A-n79A | n34 | 5, 10, 15 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n34A-n79C | CA\_n34A-n79A | n34 | 5, 10, 15 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n34 | See n34 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n38A-n40A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n38A-n66A | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | 5, 10, 15, 20, 30, 40 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
| CA\_n38A-n66(2A) | CA\_n38A-n66A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
| CA\_n38A-n71A | - | n38 | 5, 10, 15, 20 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
| CA\_n38A-n78A | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |
|  |  | n38 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n78(2A) | CA\_n38A-n78A | n38 | 5, 10, 15, 20 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS0 |  |
|  |  | n38 | 5, 10, 15, 20 | 1 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n38A-n79A | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n38A-n79C | - | n38 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n38 | See n38 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n39A-n40A | CA\_n39A-n40A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41A | CA\_n39A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n41C | CA\_n41C  CA\_n39A-n41A  CA\_n39A-n41C | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n39A-n41(2A) | CA\_n39A-n41A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41(2A)\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 |  |
| CA\_n39A-n79A | CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n39A-n79C | CA\_n79C  CA\_n39A-n79A | n39 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n39 | See n39 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n40A-n41A | n418  CA\_n40A-n41A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n41 | 10, 15, 20, 40, 50, 60 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n41C | CA\_n41C  CA\_n40A-n41A  CA\_n40A-n41C | n40 | 5, 10, 15, 20, 25, 30, 40 | 0 |
|  |  | n41 | CA\_n41C\_BCS0 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n41 | CA\_n41C\_BCS4 and 5 |  |
| CA\_n40A-n77A | CA\_n40A-n77A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40A-n77(2A) | CA\_n40A-n77A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40A-n77C | - | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40B-n77A | n778  CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 704,80, 904, 100 |  |
| CA\_n40B-n77(2A) | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
| CA\_n40B-n77C | CA\_n40A-n77A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n77 | CA\_n77C\_BCS1 |  |
| CA\_n40A-n78A | CA\_n40A-n78A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n78(2A) | CA\_n40A-n78A | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS1 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n40A-n78C | CA\_n40A-n78A | n40 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40B-n78A | - | n40 | CA\_n40B\_BCS0 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n40B-n78(2A) | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
| CA\_n40B-n78C | CA\_n40A-n78A | n40 | CA\_n40B\_BCS1 | 0 |
|  |  | n78 | CA\_n78C\_BCS1 |  |
| CA\_n40A-n79A | n798  CA\_n40A-n79A8 | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | 5, 10, 15, 20, 25, 30, 40 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n40A-n79C | CA\_n40A-n79A  CA\_n79C | n40 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n40 | See n40 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
| CA\_n40A-n105A | CA\_n40A-n105A | n40 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n105 | 5, 10, 15, 20, 25, 30, 35 |  |

Table 5.5A.3.1-1j: NR CA configurations and bandwidth combinations sets defined for inter-band CA (two bands)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| NR CA configuration | Uplink CA configuration or single uplink carrier10 | NR Band | Channel bandwidth (MHz) (NOTE 3) | Bandwidth combination set |
| CA\_n41A-n48A | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n48B | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41A-n48C | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41A-n48(2A) | CA\_n41A-n48A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n41C-n48A | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
| CA\_n41C-n48B | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41C-n48C | CA\_n41A-n48A | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41(2A)-n48A | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | 5, 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | See n48 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n48B | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | CA\_n48B\_BCS2 |  |
| CA\_n41(2A)-n48C | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n48 | CA\_n48C\_BCS1 |  |
| CA\_n41(2A)-n48(2A) | CA\_n41A-n48A | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n48 | CA\_n48(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS4 and 5 | 4 and 5 |
|  |  | n48 | CA\_n48(2A)\_BCS4 and 5 |  |
| CA\_n41A-n50A | CA\_n41A-n50A | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n50 | 5, 10, 15, 20, 40, 50, 60, 801 |  |
| CA\_n41A-n66A13,14 | n418,9  CA\_n41A-n66A8, 13,14 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n66A | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n66(2A) | n418, 9  CA\_n41A-n66A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n66A | n418, 9  CA\_n41A-n66A8  CA\_n41C | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 40 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  | n418, 9  CA\_n41A-n66A8  CA\_n41C  CA\_n41C-n66A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n66(2A) | n418, 9  CA\_n41A-n66A8  CA\_n41C-n66A  CA\_n41C | n41 | CA\_n41C\_BCS2 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n66(2A) | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(2A)\_BCS3 | 0 |
|  |  | n66 | CA\_n66(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(3A)-n66A | n418, 9  CA\_n41A-n66A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40, |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n66(2A) | n418,9  CA\_n41A-n66A8 | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41(A-C)-n66A | n418, 9  CA\_n41C8  CA\_n41A-n66A8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n66 | 5, 10, 15, 20, 25, 30, 40 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | n66 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n66(2A) | n418,9  CA\_n41C8  CA\_n41A-n66A8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n66 | CA\_n66(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n70A | CA\_n41A-n70A | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n70 | 5, 10, 15, 201, 251 |  |
| CA\_n41A-n71A | n418,9  CA\_n41A-n71A8, 13, 14 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n71B | n418,9  CA\_n41A-n71A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n71A | n418, 9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  | n418, 9  CA\_n41A-n71A8  CA\_n41C8  CA\_n41C-n71A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n71(2A) | n418,9  CA\_n41A-n71A8  CA\_n41C-n71A  CA\_n41C8 | n41 | CA\_n41C\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71A | n418, 9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS3 | 1 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71(2A)\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n71B | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | CA\_n41(2A)\_BCS1 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41(3A)-n71A | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n71B | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS4 and 5 |  |
| CA\_n41(3A)-n71(2A) | n418,9  CA\_n41A-n71A8 | n41 | CA\_n41(3A)\_BCS4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS4 and 5 |  |
| CA\_n41(A-C)-n71A | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n71 | 5, 10, 15, 20 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | n71 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n71B | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41(A-C)-n71(2A) | n418,9  CA\_n41A-n71A8  CA\_n41C8 | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n71B | n418,9  CA\_n41A-n71A8  CA\_n41C-n71A  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n71 | CA\_n71B\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS1 | 1 |
|  |  | n71 | CA\_n71B\_BCS2 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n71 | CA\_n71B\_BCS 4 and 5 |  |
| CA\_n41A-n74A | CA\_n41A-n74A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n74 | 5, 10, 15, 20 |  |
| CA\_n41A-n77A | n418,9  n778,9  CA\_n41A-n77A8, 13 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 1 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41B-n77A | CA\_n41A-n77A | n41 | CA\_n41B\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
| CA\_n41(2A)-n77A | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n77A | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(3A)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n77A | n418,9  n778,9  CA\_n41C8  CA\_n41A-n77A8 | n41 | CA\_n41(A-C)\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n77A | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n77 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8  CA\_n41C-n77A | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | n77 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n77(2A) | n418,9  n778,9  CA\_n77(2A)  CA\_n41A-n77A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8 | n41 | n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41C-n77(2A) | n418,9  n778,9  CA\_n41A-n77A8  CA\_n41C8 | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  |  | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A)\_BCS 4 and 5 |  |
| CA\_n41A-n77(3A) | n418,9  n778,9  CA\_n41A-n77A8 | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77(3A)\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77(3A)\_BCS 4 and 5 |  |
| CA\_n41(2A)-n77(2A) | - | n41 | CA\_n41(2A)\_BCS1 | 0 |
|  |  | n77 | CA\_n77(2A)\_BCS1 |  |
|  | n418,9  n778,9  CA\_n41A-n77A8 | n41 | CA\_n41(2A) BCS 4 and 5 | 4 and 5 |
|  |  | n77 | CA\_n77(2A) BCS 4 and 5 |  |
| CA\_n41A-n77C | CA\_n41A-n77A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n77 | CA\_n77C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n77 | CA\_n77C\_BCS 4 and 5 |  |
| CA\_n41A-n78A | CA\_n41A-n78A | n41 | 10, 15, 20, 40, 50, 60, 80, 100 | 0 |
|  |  | n78 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 1 |
|  |  | n78 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | See n78 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n78(2A) | CA\_n41A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78(2A)\_BCS2 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78(2A)\_BCS4 and 5 |  |
| CA\_n41A-n78C | CA\_n41A-n78A | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n78 | CA\_n78C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n78 | CA\_n78C\_BCS4 and 5 |  |
| CA\_n41A-n79A | n418,9  n798,9  CA\_n41A-n79A8 | n41 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | 10, 15, 20, 40, 50, 60 | 1 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | 10, 15, 20, 30, 40, 50, 60, 80, 90, 100 | 2 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41A-n79C | CA\_n41A-n79A  CA\_n79C | n41 | 10, 15, 20, 30, 40, 50, 60, 70, 80, 90, 100 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n41C-n79A | CA\_n41A-n79A  CA\_n41C | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n79 | 40, 50, 60, 80, 100 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 | 4 and 5 |
|  |  | n79 | See n79 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n79C | CA\_n41C  CA\_n79C  CA\_n41A-n79A | n41 | CA\_n41C\_BCS0 | 0 |
|  |  | n79 | CA\_n79C\_BCS0 |  |
|  |  | n41 | CA\_n41C\_BCS4 and 5 | 4 and 5 |
|  |  | n79 | CA\_n79C\_BCS4 and 5 |  |
| CA\_n41A-n85A | CA\_n41A-n85A | n41 | See n41 channel bandwidths in Table 5.3.5-1 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41C-n85A | CA\_n41A-n85A  CA\_n41C | n41 | CA\_n41C\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(2A)-n85A | CA\_n41A-n85A | n41 | CA\_n41(2A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(3A)-n85A | CA\_n41A-n85A | n25 | CA\_n41(3A)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |
| CA\_n41(A-C)-n85A | CA\_n41A-n85A  CA\_n41C | n41 | CA\_n41(A-C)\_BCS 4 and 5 | 4 and 5 |
|  |  | n85 | See n85 channel bandwidths in Table 5.3.5-1 |  |

---End of changes---