{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PUSCH 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #110",null,null,null,null,null,null,null,"R4-2401690"]
[null,"Athens, 26th Feb - 1st Mar, 2024"]
[]
[null,"Source: Huawei, HiSilicon"]
[null,"Title: Simulation summary for FR2 UL 256QAM BS Demodulation requirements"]
[null,"Agenda: 8.2.3.1"]
[null,"Document for: Information"]
[null,"Notes: Impairment results include impact or Tx EVM and Rx Phase Noise"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH 1T2R","index":2,"n_rows":14,"n_cols":25,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,13,0,14],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,17,0,18],[0,15,0,16],[2,0,13,0],[2,1,13,1],[2,2,7,2],[2,3,3,3],[4,3,5,3],[6,3,7,3],[8,2,13,2],[8,3,9,3],[10,3,11,3],[12,3,13,3],[0,11,0,12],[0,0,1,6],[0,7,1,7],[0,8,1,8],[0,9,0,10]]}
["  FR2-1 PUSCH 1T2R",null,null,null,null,null,null,"38.104 req","38.141 req","Ericsson",null,"Huawei",null,"Samsung",null,"Xiaomi",null,"ZTE",null,"Nokia",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["CP-OFDM","Mapping Type B","PT-RS Enabled","60kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",{"$f":"DerivingPerfReq(J3:U3)","v":19.600000000000001},{"$f":"IF(H3>-100,H3+0.6,H3)","v":20.200000000000003},17.09,19.79,16.8,19.399999999999999,17,19.5,16.350000000000001,19.170000000000002,16.8,null,16.48,20.37,{"$f":"MAX(J3,L3,N3,T3,P3,R3)-MIN(J3,L3,N3,T3,P3,R3)","v":0.73999999999999844},{"$f":"MAX(K3,M3,O3,U3,Q3,S3)-MIN(K3,M3,O3,U3,Q3,S3)","v":1.1999999999999993},{"$f":"AVERAGE(J3,L3,N3,T3,P3,R3)","v":16.753333333333334},{"$f":"AVERAGE(K3,M3,O3,U3,Q3,S3)","v":19.646000000000001}]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.8,20.400000000000002,17.329999999999998,19.829999999999998,17.100000000000001,19.899999999999999,17,19.5,16.309999999999999,19.100000000000001,16.600000000000001,null,16.579999999999998,20.45,{"$f":"MAX(J4,L4,N4,T4,P4,R4)-MIN(J4,L4,N4,T4,P4,R4)","v":1.0199999999999996},1.3499999999999979,{"$f":"AVERAGE(J4,L4,N4,T4,P4,R4)","v":16.819999999999997},19.756]
[null,null,null,"120kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",19.5,20.100000000000001,17.12,19.86,16.2,18.7,17.100000000000001,19.600000000000001,16.37,19.07,17.100000000000001,null,16.52,20.36,0.92000000000000171,1.6600000000000001,16.734999999999999,19.518000000000001]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.899999999999999,20.5,17.55,20.05,16.600000000000001,19.3,17.399999999999999,19.899999999999999,16.510000000000002,19.32,16.899999999999999,null,16.87,20.75,1.0399999999999991,1.4499999999999993,16.971666666666668,19.863999999999997]
[null,null,null,"120kHz, 200MHz","MCS20","TDLD30-35","DMRS 1+1",19.600000000000001,20.200000000000003,17.21,19.79,16.2,19,17.3,19.8,16.02,19.010000000000002,17,null,16.579999999999998,20.51,1.2800000000000011,1.5100000000000016,16.71833333333333,19.622000000000003]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.8,20.400000000000002,17.489999999999998,19.989999999999998,16.399999999999999,19.399999999999999,17.3,19.8,15.88,19.059999999999999,16.899999999999999,null,16.72,20.71,1.6099999999999977,1.6500000000000021,16.781666666666666,19.792000000000002]
[null,null,"PT-RS Disabled","60kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",19,{"$f":"IF(H9>-100,H9+0.6,H9)","v":19.600000000000001},16.45,19.36,16.2,18.7,16.3,18.8,15.52,18.46,15.9,null,15.73,19.66,0.92999999999999972,1.1999999999999993,16.016666666666669,18.995999999999999]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.3,19.900000000000002,16.690000000000001,19.27,16.510000000000002,19.2,16.399999999999999,18.899999999999999,15.55,18.75,15.6,null,15.88,20.260000000000002,1.1400000000000006,1.5100000000000016,16.105,19.276]
[null,null,null,"120kHz, 50MHz","MCS20","TDLD30-35","DMRS 1+1",18.8,19.400000000000002,16.5,19.18,15.5,18,16.3,18.8,15.28,18.3,16.2,null,15.67,19.489999999999998,1.2200000000000006,1.4899999999999984,15.908333333333333,18.753999999999998]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.2,19.8,16.84,19.55,15.89,18.5,16.600000000000001,19.100000000000001,15.58,18.82,15.9,null,16.010000000000002,20.149999999999999,1.2599999999999998,1.6499999999999986,16.136666666666667,19.224]
[null,null,null,"120kHz, 200MHz","MCS20","TDLD30-35","DMRS 1+1",19.100000000000001,19.700000000000003,16.579999999999998,19.559999999999999,15.5,18.2,16.600000000000001,19.100000000000001,15.32,18.77,16.3,null,15.82,19.89,1.2800000000000011,1.6900000000000013,16.02,19.103999999999999]
[null,null,null,null,"MCS20","TDLD30-35","DMRS 1+0",19.399999999999999,20,16.8,19.62,15.78,18.600000000000001,16.600000000000001,19.100000000000001,15.26,19.18,15.9,null,16.010000000000002,20.53,1.5400000000000009,1.9299999999999997,16.058333333333334,19.405999999999999]