**3GPP TSG-RAN WG4 Meeting #95-e *REV\_R4-2007043***

**Eletronic meeting, 25 May – 5 June 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-3** | **CR** | **272** | **rev** | **1** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Removal of the Annex modifiedMPR-Behaviour from the NSA specification |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-06-09 |
|  |  |  |  |  |
| ***Category:*** | **A** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Remove the Annex on ModifiedMPR-behaviour from this NR NSA specification (and move the Annex to the SA specification TS 38.101-1 instead). The *modifiedMPRbehavior* is a field of the NR band capability in the supported NR band list that is part of the *UE-NR-Capability* IE. Hence this field is intended for MPR modification in an NR band, but can also be used for the said band if part of an EN-DC band combination. The table of the NR band-specific modified MPR behaviour should therefore be moved from 38.101-3 to 38.101-1. |
|  |  |
| ***Summary of change:*** | Annex H: the Annex on ModifiedMPR-behaviour is removed (moved to TS 38.101-1).  |
|  |  |
| ***Consequences if not approved:*** | The Annex ModifiedMPR-behaviour is not part of the relevant specification. If an MPR behaviour is modified for an NR band, this modification has to be made in the *NSA* specification. |
|  |  |
| ***Clauses affected:*** | Annex H |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  TS 38.101-1 CR 351 |
| ***affected:*** |  | **X** |  Test specifications |   |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |   |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | The TS 38.101-1 CR 351 introduces the Annex on ModifiedMPR-behaviour in the TS 38.101-1.r1: reference to annex H in 38.101-1 |

*< start of changes >*

Annex H (normative):
Modified MPR behavior

The definitions of the bits in the modifiedMPRbehavior field have been moved to Annex H of 38.101-1[2].

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |
|  |  |  |  |

Annex I (normative):
Dual uplink interferer

*< end of changes >*