**3GPP TSG-RAN WG4 Meeting #95-e *DRAFT* R4-2008431**

 **Electronic Meeting , 25th May. 2020 - 5th June. 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-3** | **CR** | **draft** | **rev** | **-** | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on Introduction of NR-U EN-DC combinations in Rel-16 |
|  |  |
| ***Source to WG:*** | Charter Communication, T-Mobile US, Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_unlic-Core  |  | ***Date:*** | 2020-06-03 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Draft CR for inclusion of agreed NR-U combinations in Rel-16 |
|  |  |
| ***Summary of change:*** | This draft CR implementing the following NR-U band combinations:DC\_2\_n46DC\_48\_n46DC\_66\_n46 |
|  |  |
| ***Consequences if not approved:*** | Inclusion of agreed NR-U combinations in Rel-16 would not be possible |
|  |  |
| ***Clauses affected:*** |  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521 series |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

#### 5.5B.4.1 Inter-band EN-DC configurations within FR1 (two bands)

Table 5.5B.4.1-1: Inter-band EN-DC configurations within FR1 (two bands)

| EN-DCconfiguration | Uplink EN-DCconfiguration(NOTE 1) | Single UL allowed |
| --- | --- | --- |
| DC\_1A\_n3ADC\_1C\_n3A | DC\_1A\_n3ADC\_1C\_n3A | DC\_1\_n3 |
| DC\_1A\_n5A | DC\_1A\_n5A | No |
| DC\_1A\_n7ADC\_1A\_n7B | DC\_1A\_n7A | No |
| DC\_1A-1A\_n7ADC\_1A-1A\_n7B | DC\_1A\_n7A | No |
| DC\_1A\_n8A | DC\_1A\_n8A | No |
| DC\_1A\_n28A | DC\_1A\_n28A | No |
| DC\_1A\_n38ADC\_1C\_n38A | DC\_1A\_n38A | No |
| DC\_1A\_n40A | DC\_1A\_n40A | No |
| DC\_1A\_n41A | DC\_1A\_n41A | No |
| DC\_1A\_n50A | DC\_1A\_n50A | No |
| DC\_1A\_n51A | DC\_1A\_n51A | No |
| DC\_1A\_n77A7DC\_1A\_n77C7 | DC\_1A\_n77A | DC\_1\_n77 |
| DC\_1A\_n77(2A) | DC\_1A\_n77A | DC\_1\_n77 |
| DC\_1A\_n78A7DC\_1A\_n78C7 | DC\_1A\_n78A | No |
| DC\_1A\_n78(2A)7 | DC\_1A\_n78A | No |
| DC\_1A\_n79A7DC\_1A\_n79C7 | DC\_1A\_n79A | No |
| DC\_2A\_n5A | DC\_2A\_n5A | No |
| DC\_2A-2A\_n5A | DC\_2A\_n5A | No |
| DC\_2A\_n7A | DC\_2A\_n7A | No |
| DC\_2A\_n7(2A) | DC\_2A\_n7A | No |
| DC\_2A\_n12A | DC\_2A\_n12A | No |
| DC\_2A\_n38A | DC\_2A\_n38A | No |
| DC\_2A-2A\_n38A | DC\_2A\_n38A | No |
| DC\_2A\_n41ADC\_2A\_n41CDC\_2C\_n41A | DC\_2A\_n41ADC\_2C\_n41A | No |
| DC\_2A-2A\_n41ADC\_2A\_n41(2A) | DC\_2A\_n41A | No |
| DC\_2A\_n46A | DC\_2A\_n46A | No |
| DC\_2A\_n48ADC\_2A\_n48B | DC\_2A\_n48A | No |
| DC\_2A\_n66A | DC\_2A\_n66A | DC\_2\_n66 |
| DC\_2A-2A\_n66A | DC\_2A\_n66A | DC\_2\_n66 |
| DC\_2A\_n71ADC\_2A\_n71BDC\_2C\_n71A | DC\_2A\_n71ADC\_2C\_n71A | No |
| DC\_2A-2A\_n71A | DC\_2A\_n71A | No |
| DC\_2A\_n78A | DC\_2A\_n78A | DC\_2\_n78 |
| DC\_2A\_n78(2A) | DC\_2A\_n78A | DC\_2\_n78 |
| DC\_2A-2A\_n78A | DC\_2A\_n78A | DC\_2\_n78 |
| DC\_3A\_n1ADC\_3C\_n1A | DC\_3A\_n1ADC\_3C\_n1A | DC\_3\_n1 |
| DC\_3A-3A\_n1A | DC\_3A\_n1A | DC\_3\_n1 |
| DC\_3A\_n5ADC\_3C\_n5A | DC\_3A\_n5ADC\_3C\_n5A | DC\_3\_n5 |
| DC\_3A\_n7ADC\_3A\_n7BDC\_3C\_n7ADC\_3C\_n7B | DC\_3A\_n7ADC\_3A\_n7BDC\_3C\_n7A | No |
| DC\_3A-3A\_n7ADC\_3A-3A\_n7B | DC\_3A\_n7A | No |
| DC\_3A\_n8A | DC\_3A\_n8A | No |
| DC\_3A\_n20A | DC\_3A\_n20A | No |
| DC\_3A\_n28ADC\_3C\_n28A | DC\_3A\_n28ADC\_3C\_n28A | No |
| DC\_3A\_n34A | DC\_3A\_n34A | No |
| DC\_3A\_n38ADC\_3C\_n38A | DC\_3A\_n38A | No |
| DC\_3A\_n40A | DC\_3A\_n40A | No |
| DC\_3A\_n41ADC\_3C\_n41A | DC\_3A\_n41ADC\_3C\_n41A | DC\_3\_n41 |
| DC\_3A\_n50A | DC\_3A\_n50A | No |
| DC\_3A\_n51A | DC\_3A\_n51A | No |
| DC\_3A\_n77A7DC\_3A\_n77C7 | DC\_3A\_n77A | DC\_3\_n77 |
| DC\_3A\_n77(2A)7 | DC\_3A\_n77A | DC\_3\_n77 |
| DC\_3A-3A\_n77A | DC\_3A\_n77A | DC\_3\_n77 |
| DC\_3A\_n78A7DC\_3A\_n78C7DC\_3C\_n78A7 | DC\_3A\_n78A | DC\_3\_n78 |
| DC\_3A\_n78(2A)7DC\_3C\_n78(2A)7 | DC\_3A\_n78A | DC\_3\_n78 |
| DC\_3A-3A\_n78A | DC\_3A\_n78A | DC\_3\_n78 |
| DC\_3A\_n79A7DC\_3A\_n79C7DC\_3C\_n79A7 | DC\_3A\_n79ADC\_3C\_n79A | No |
| DC\_4A\_n38A | DC\_4A\_n38A | No |
| DC\_4A\_n41A | DC\_4A\_n41A | No |
| DC\_4A\_n78A | DC\_4A\_n78A | No |
| DC\_4A\_n78(2A) | DC\_4A\_n78A | No |
| DC\_5A\_n2ADC\_5B\_n2A | DC\_5A\_n2A | No |
| DC\_5A-5A\_n2A | DC\_5A\_n2A | No |
| DC\_5A\_n7A | DC\_5A\_n7A | DC\_5\_n7 |
| DC\_5A\_n7(2A) | DC\_5A\_n7A | DC\_5\_n7 |
| DC\_5A\_n12A | DC\_5A\_n12A | No |
| DC\_5A\_n38A | DC\_5A\_n38A | DC\_5\_n38 |
| DC\_5A\_n40A | DC\_5A\_n40A | No |
| DC\_5A\_n48ADC\_5A\_n48B | DC\_5A\_n48A | No |
| DC\_5A\_n66ADC\_5B\_n66A | DC\_5A\_n66A | DC\_5\_n66 |
| DC\_5A-5A\_n66A | DC\_5A\_n66A | DC\_5\_n66 |
| DC\_5A\_n71A | DC\_5A\_n71A | No |
| DC\_5A\_n78A7 | DC\_5A\_n78A | No |
| DC\_5A\_n78(2A)7 | DC\_5A\_n78A | No |
| DC\_5A\_n79A | DC\_5A\_n79A | No |
| DC\_7A\_n1ADC\_7C\_n1A | DC\_7A\_n1ADC\_7C\_n1A | No |
| DC\_7A-7A\_n1A | DC\_7A\_n1A | No |
| DC\_7A\_n3ADC\_7C\_n3A | DC\_7A\_n3ADC\_7C\_n3A | No |
| DC\_7A\_n5ADC\_7C\_n5A | DC\_7A\_n5ADC\_7C\_n5A | DC\_7\_n5 |
| DC\_7A-7A\_n5A | DC\_7A\_n5A | DC\_7\_n5 |
| DC\_7A\_n8A | DC\_7A\_n8A | No |
| DC\_7A-7A\_n78A7 | DC\_7A\_n78A | No |
| DC\_7A\_n28ADC\_7C\_n28A | DC\_7A\_n28ADC\_7C\_n28A | No |
| DC\_7A\_n51A | DC\_7A\_n51A | No |
| DC\_7A\_n66ADC\_7C\_n66A | DC\_7A\_n66A | No |
| DC\_7A-7A\_n66A | DC\_7A\_n66A | No |
| DC\_7A\_n71A | DC\_7A\_n71A | No |
| DC\_7A\_n77A | DC\_7A\_n77A | No |
| DC\_7A-7A\_n77A | DC\_7A\_n77A | No |
| DC\_7A\_n78A7DC\_7C\_n78A7 | DC\_7A\_n78ADC\_7C\_n78A | No |
| DC\_7A\_n78(2A)7DC\_7C\_n78(2A)7 | DC\_7A\_n78ADC\_7C\_n78A | No |
| DC\_8A\_n1A | DC\_8A\_n1A | No |
| DC\_8A\_n3A | DC\_8A\_n3A | No |
| DC\_8A\_n28A | DC\_8A\_n28A | No |
| DC\_8A\_n34A | DC\_8A\_n34A | No |
| DC\_8A\_n39A | DC\_8A\_n39A | No |
| DC\_8A\_n40A7 | DC\_8A\_n40A | No |
| DC\_8A\_n41ADC\_8A\_n41C | DC\_8A\_n41A | No |
| DC\_8A\_n41(2A) | DC\_8A\_n41A | No |
| DC\_8A\_n77A7 | DC\_8A\_n77A | No |
| DC\_8A\_n77(2A)7 | DC\_8A\_n77A | No |
| DC\_8A\_n78A7 | DC\_8A\_n78A | No |
| DC\_8A\_n79A7DC\_8A\_n79C | DC\_8A\_n79ADC\_8A\_n79C | No |
| DC\_8A\_n93A | DC\_8A\_n93A\_ULSUP-TDM | N/A |
| DC\_8A\_n94A | DC\_8A\_n94A\_ULSUP-TDM | N/A |
| DC\_11A\_n3A | DC\_11A\_n3A | No |
| DC\_11A\_n77A7 | DC\_11A\_n77A | No |
| DC\_11A\_n77(2A)7 | DC\_11A\_n77A | No |
| DC\_11A\_n78A7 | DC\_11A\_n78A | No |
| DC\_11A\_n79A7 | DC\_11A\_n79A | No |
| DC\_12A\_n2A | DC\_12A\_n2A | No |
| DC\_12A\_n5A | DC\_12A\_n5A | No |
| DC\_12A\_n7ADC\_12A\_n7(2A) | DC\_12A\_n7A | No |
| DC\_12A\_n25A | DC\_12A\_n25A | No |
| DC\_12A\_n38A | DC\_12A\_n38A | No |
| DC\_12A\_n66A | DC\_12A\_n66A | No |
| DC\_12A\_n78ADC\_12A\_n78(2A) | DC\_12A\_n78A | DC\_12\_n78 |
| DC\_13A\_n7ADC\_13A\_n7(2A) | DC\_13A\_n7A | No |
| DC\_13A\_n48ADC\_13A\_n48B | DC\_13A\_n48A | No |
| DC\_13A\_n66A | DC\_13A\_n66A | No |
| DC\_13A\_n71A | DC\_13A\_n71A | No |
| DC\_13A\_n78ADC\_13A\_n78(2A) | DC\_13A\_n78A | No |
| DC\_18A\_n3A | DC\_18A\_n3A | No |
| DC\_18A\_n77A7 | DC\_18A\_n77A | No |
| DC\_18A\_n78A7 | DC\_18A\_n78A | No |
| DC\_20A\_n91A | DC\_20A\_n91A\_ULSUP-TDM | N/A |
| DC\_20A\_n92A | DC\_20A\_n92A\_ULSUP-TDM | N/A |
| DC\_18A\_n79A7 | DC\_18A\_n79A | No |
| DC\_19A\_n77A7DC\_19A\_n77C7 | DC\_19A\_n77A | No |
| DC\_19A\_n78A7DC\_19A\_n78C7 | DC\_19A\_n78A | No |
| DC\_19A\_n79A7DC\_19A\_n79C7 | DC\_19A\_n79A | No |
| DC\_20A\_n1A | DC\_20A\_n1A | No |
| DC\_20A\_n3A | DC\_20A\_n3A | No |
| DC\_20A\_n7A | DC\_20A\_n7A | DC\_20\_n7 |
| DC\_20A\_n8A | DC\_20A\_n8A | DC\_20\_n8 |
| DC\_20A\_n28A8,10,11,13 | DC\_20A\_n28A | No |
| DC\_20A\_n38A | DC\_20A\_n38A | No |
| DC\_20A\_n41A | DC\_20A\_n41A | DC\_20\_n41 |
| DC\_20A\_n50A | DC\_20A\_n50A | No |
| DC\_20A\_n51A | DC\_20A\_n51A | No |
| DC\_20A\_n77A7 | DC\_20A\_n77A | No |
| DC\_20A\_n78A7 | DC\_20A\_n78A | No |
| DC\_21A\_n77A7DC\_21A\_n77C7 | DC\_21A\_n77A | No |
| DC\_21A\_n78A7DC\_21A\_n78C7 | DC\_21A\_n78A | No |
| DC\_21A\_n79A7DC\_21A\_n79C7 | DC\_21A\_n79A | No |
| DC\_25A\_n41A | DC\_25A\_n41A | No |
| DC\_25A-25A\_n41A | DC\_25A\_n41A | No |
| DC\_26A\_n25A | DC\_26A\_n25A | No |
| DC\_26A\_n41A | DC\_26A\_n41A | No |
| DC\_26A\_n77A7 | DC\_26A\_n77A | No |
| DC\_26A\_n78A7 | DC\_26A\_n78A | No |
| DC\_26A\_n79A7 | DC\_26A\_n79A | No |
| DC\_28A\_n3A | DC\_28A\_n3A | No |
| DC\_28A\_n5A8 | DC\_28A\_n5A | No |
| DC\_28A\_n7ADC\_28A\_n7B | DC\_28A\_n7ADC\_28A\_n7B | No |
| DC\_28A\_n51A | DC\_28A\_n51A | No |
| DC\_28A\_n8A | DC\_28A\_n8A | No |
| DC\_28A\_n41A | DC\_28A\_n41A | No |
| DC\_28A\_n50A | DC\_28A\_n50A | No |
| DC\_28A\_n77A7DC\_28A\_n77C7 | DC\_28A\_n77A | No |
| DC\_28A\_n77(2A)7 | DC\_28A\_n77A | No |
| DC\_28A\_n78A7DC\_28A\_n78C7 | DC\_28A\_n78A | No |
| DC\_28A\_n79A7DC\_28A\_n79C7 | DC\_28A\_n79A | No |
| DC\_30A\_n2A | DC\_30A\_n2A | No |
| DC\_30A\_n5A | DC\_30A\_n5A | No |
| DC\_30A\_n66A | DC\_30A\_n66A | No |
| DC\_38A\_n78A7 | DC\_38A\_n78A | No |
| DC\_39A\_n40A3 | DC\_39A\_n40A | No |
| DC\_39A\_n41ADC\_39C\_n41A | DC\_39A\_n41ADC\_39C\_n41A | No |
| DC\_39A\_n78A5,7 | DC\_39A\_n78A | No |
| DC\_39A\_n79A7 | DC\_39A\_n79A | No |
| DC\_40A\_n1A | DC\_40A\_n1A | No |
| DC\_40A\_n41A3DC\_40C\_n41A3 | DC\_40A\_n41A | No |
| DC\_40A\_n77A | DC\_40A\_n77A | No |
| DC\_40A\_n78ADC\_40C\_n78A | DC\_40A\_n78ADC\_40C\_n78A | No |
| DC\_40A\_n79A7,12DC\_40C\_n79A7,12 | DC\_40A\_n79A | No |
| DC\_41A\_n77ADC\_41C\_n77A | DC\_41A\_n77ADC\_41C\_n77A | No |
| DC\_41A\_n77(2A)DC\_41C\_n77(2A) | DC\_41A\_n77ADC\_41C\_n77A | No |
| DC\_41A\_n78ADC\_41C\_n78A | DC\_41A\_n78ADC\_41C\_n78A | No |
| DC\_41A\_n79A6,7DC\_41C\_n79A6,7 | DC\_41A\_n79ADC\_41C\_n79A | No |
| DC\_42A\_n51A | DC\_42A\_n51A | No |
| DC\_42A\_n77A3,4,9,11DC\_42A\_n77C3,4,9,11DC\_42C\_n77A3,4,9,11DC\_42C\_n77C3,4,9,11DC\_42D\_n77A3,4,9,11DC\_42D\_n77CDC\_42E\_n77A3,4,9,11DC\_42E\_n77C | N/A | N/A |
| DC\_42A\_n78A3,4,9,11DC\_42A\_n78C3,4,9,11DC\_42C\_n78A3,4,9,11DC\_42C\_n78C3,4,9,11DC\_42D\_n78A3,4,9,11DC\_42D\_n78CDC\_42E\_n78A3,4,9,11DC\_42E\_n78C | N/A | N/A |
| DC\_42A\_n79A9DC\_42A\_n79C9DC\_42C\_n79A9DC\_42C\_n79C9DC\_42D\_n79A9DC\_42D\_n79CDC\_42E\_n79A9DC\_42E\_n79C | N/A | N/A |
| DC\_46A\_n78A2DC\_46C\_n78A2DC\_46D\_n78A2DC\_46E\_n78A2 | N/A | N/A |
| DC\_48A\_n5A | DC\_48A\_n5A | No |
| DC\_48A\_n12A | DC\_48A\_n12A | No |
| DC\_48A\_n46ADC\_48B\_n46ADC\_48C\_n46ADC\_48D\_n46ADC\_48E\_n46ADC\_48A\_n46BDC\_48B\_n46BDC\_48C\_n46BDC\_48D\_n46BDC\_48E\_n46BDC\_48A\_n46CDC\_48B\_n46CDC\_48C\_n46CDC\_48D\_n46CDC\_48E\_n46CDC\_48A\_n46DDC\_48B\_n46DDC\_48C\_n46DDC\_48D\_n46DDC\_48E\_n46DDC\_48A\_n46EDC\_48B\_n46EDC\_48C\_n46EDC\_48D\_n46EDC\_48E\_n46E | DC\_48A\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48A\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48A\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48A\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48A\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46ADC\_48B\_n46A | No |
| DC\_48A\_n66A | DC\_48A\_n66A | No |
| DC\_48A\_n71ADC\_48B\_n71ADC\_48C\_n71ADC\_48D\_n71A | DC\_48A\_n71A | No |
| DC\_66A\_n2A | DC\_66A\_n2A | DC\_66\_n2 |
| DC\_66A-66A\_n2A | DC\_66A\_n2A | DC\_66\_n2 |
| DC\_66A\_n5A | DC\_66A\_n5A | DC\_66\_n5 |
| DC\_66A-66A\_n5ADC\_66A-66A-66A\_n5A | DC\_66A\_n5A | DC\_66\_n5 |
| DC\_66A\_n7ADC\_66A-66A\_n7ADC\_66A-66A\_n7(2A) | DC\_66A\_n7A | No |
| DC\_66A\_n12A | DC\_66A\_n12A | No |
| DC\_66A\_n25A | DC\_66A\_n25A | DC\_66\_n25 |
| **DC\_66A\_n38A** | DC\_66A\_n38A | No |
| DC\_66A-66A\_n38A | DC\_66A\_n38A | No |
| DC\_66A\_n41ADC\_66A\_n41C | DC\_66A\_n41A | No |
| DC\_66A\_n41(2A) | DC\_66A\_n41A | No |
| DC\_66A\_n46A | DC\_66A\_n46A | No |
| DC\_66A\_n48ADC\_66A\_n48B | DC\_66A\_n48A | No |
| DC\_66A-66A\_n48ADC\_66A-66A\_n48B | DC\_66A\_n48A | No |
| DC\_66A\_n71ADC\_66C\_n71ADC\_66A\_n71B | DC\_66A\_n71A | No |
| DC\_66A-66A\_n71A | DC\_66A-66A\_n71A | DC\_66A-66A\_n71A |
| DC\_66A\_n78A | DC\_66A\_n78A | No |
| DC\_66A\_n78(2A) | DC\_66A\_n78A | No |
| DC\_66A-66A\_n78A | DC\_66A\_n78A | No |
| DC\_71A\_n5A | DC\_71A\_n5A | No |
| DC\_71A\_n38A | DC\_71A\_n38A | No |
| DC\_71A\_n48A | DC\_71A\_n48A |  |
| DC\_71A\_n66A | DC\_71A\_n66A | No |
| DC\_71A\_n78A | DC\_71A\_n78A | No |
| NOTE 1: Uplink EN-DC configurations are the configurations supported by the present release of specifications.NOTE 2: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell.NOTE 3: The minimum requirements apply only when there is non-simultaneous Tx/Rx operation between E-UTRA and NR carriers. This restriction applies also for these carriers when applicable EN-DC configuration is part of a higher order EN-DC configuration.NOTE 4: The minimum requirements for intra-band contiguous or non-contiguous EN-DC apply. The intra-band requirements also apply for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 5: The frequency range above 3600 MHz for Band n78 is not used in this combination.NOTE 6: The frequency range below 2506 MHz for Band 41 is not used in this combination.NOTE 7: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability.NOTE 8: The frequency range in band n28 is restricted for this band combination to 703 - 733 MHz for the UL and 758-788 MHz for the DL.NOTE 9: The combination is not used alone as fall back mode of other band combinations in which UL in Band 42 is not used.NOTE 10: The maximum power spectral density imbalance between downlink carriers is within [6] dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 11: The minimum requirements for inter-band EN-DC apply when the maximum power spectral density imbalance between downlink carriers is within [6] dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration.NOTE 12: Applicable for frequency range above 4800 MHz for Band n79 in this combination.NOTE 13: The minimum requirements apply for synchronized DL carriers with a maximum receive time difference ≤ 3 usec. The requirements also apply for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. |

---Text omitted---

Table 6.2B.4.2.3.1-1: ΔTIB,c due to EN-DC(two bands)

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_1\_n3 | 1 | 0.3 |
| n3 | 0.3 |
| DC\_1\_n5 | 1 | 0.3 |
| n5 | 0.3 |
| DC\_1\_n7 | 1 | 0.5 |
| n7 | 0.6 |
| DC\_1\_n8 | 1 | 0.3 |
| n8 | 0.3 |
| DC\_1\_n28 | 1 | 0.3 |
| n28 | 0.6 |
| DC\_1\_n38 | 1 | 0.5 |
| n38 | 0.5 |
| DC\_1\_n40 | 1 | 0.5 |
| n40 | 0.5 |
| DC\_1\_n50 | 1 | 0.5 |
| n50 | 0.5 |
| DC\_1\_n41 | 1 | 0.5 |
| n41 | 0.5 |
| DC\_1\_n51 | 1 | 0.6 |
| n51 | 0.6 |
| DC\_1\_n77 | 1 | 0.6 |
| n77 | 0.8 |
| DC\_1\_n78 | 1 | 0.3 |
| n78 | 0.8 |
| DC\_2\_n5 | 2 | 0.3 |
| n5 | 0.3 |
| DC\_2\_n7 | 2 | 0.5 |
| n7 | 0.5 |
| DC\_2\_n12 | 2 | 0.3 |
| n12 | 0.3 |
| DC\_2\_n38 | 2 | 0.5 |
| n38 | 0.9 |
| DC\_2\_n41 | 2 | 0.5 |
| n41 | 0.41 |
| 0.92 |
| DC\_2\_n48 | 2 | 0.6 |
| n48 | 0.8 |
| DC\_2\_n66 | 2 | 0.5 |
| n66 | 0.5 |
| DC\_2\_n71 | 2 | 0.3 |
| n71 | 0.3 |
| DC\_2\_n78 | 2 | 0.6 |
| n78 | 0.8 |
| DC\_3\_n1 | 3 | 0.3 |
| n1 | 0.3 |
| DC\_3\_n5 | 3 | 0.3 |
| n5 | 0.3 |
| DC\_3\_n8 | 3 | 0.3 |
| n8 | 0.3 |
| DC\_3\_n7 | 3 | 0.5 |
| n7 | 0.5 |
| DC\_3\_n20 | 3 | 0.3 |
| n20 | 0.3 |
| DC\_3\_n28 | 3 | 0.3 |
| n28 | 0.3 |
| DC\_3\_n34 | 3 | 0.5 |
| n34 | 0.5 |
| DC\_3\_n38 | 3 | 0.5 |
| n38 | 0.5 |
| DC\_3\_n40 | 3 | 0.5 |
| n40 | 0.5 |
| DC\_3-n41 | 3 | 0.5 |
| n41 | 0.33 |
| 0.84 |
| DC\_3\_n50 | 3 | 0.5 |
| n50 | 0.5 |
| DC\_3\_n51 | 3 | 0.3 |
| n51 | 0.3 |
| DC\_7\_n66, DC\_7-7\_n66 | 7 | 0.5 |
| n66 | 0.5 |
| DC\_3\_n77, DC\_3-3\_n77 | 3 | 0.6 |
| n77 | 0.8 |
| DC\_3\_n78, DC\_3-3\_n78 | 3 | 0.6 |
| n78 | 0.8 |
| DC\_4\_n38 | 4 | 0.5 |
| n38 | 0.8 |
| DC\_4\_n41 | 4 | 0.5 |
| n41 | [0.81] |
| [1.32] |
| DC\_4\_n78 | 4 | 0.6 |
| n78 | 0.8 |
| DC\_5\_n2,DC\_5-5\_n2 | 5 | 0.3 |
| n2 | 0.3 |
| DC\_5\_n7 | 5 | 0.3 |
| n7 | 0.3 |
| DC\_5\_n12 | 5 | 0.8 |
| n12 | 0.4 |
| DC\_5\_n38 | 5 | 0.3 |
| n38 | 0.3 |
| DC\_5\_n40 | 5 | 0.3 |
| n40 | 0.3 |
| DC\_5\_n48 | 5 | 0.3 |
| n48 | 0.3 |
| DC\_5\_n66, DC\_5-5\_n66 | 5 | 0.3 |
| n66 | 0.3 |
| DC\_5\_n71 | 5 | 0.5 |
| n71 | 0.5 |
| DC\_5\_n78 | 5 | 0.6 |
| n78 | 0.8 |
| DC\_7\_n1, DC\_7-7\_n1 | 7 | 0.6 |
| n1 | 0.5 |
| DC\_7\_n3 | 7 | 0.5 |
| n3 | 0.5 |
| DC\_7\_n5 | 7 | 0.3 |
| n5 | 0.3 |
| DC\_7\_n8 | 7 | 0.3 |
| n8 | 0.6 |
| DC\_7\_n28 | 7 | 0.3 |
| n28 | 0.3 |
| DC\_7\_n51 | 7 | 0.3 |
| n51 | 0.3 |
| DC\_7\_n71 | 7 | 0.3 |
| n71 | 0.6 |
| DC\_7\_n77, DC\_7-7\_n77 | 7 | 0.5 |
| n77 | 0.8 |
| DC\_7\_n78, DC\_7-7\_n78 | 7 | 0.5 |
| n78 | 0.8 |
| DC\_8\_n1 | 8 | 0.3 |
| n1 | 0.3 |
| DC\_8\_n3 | 8 | 0.3 |
| n3 | 0.3 |
| DC\_8\_n28 | 8 | 0.6 |
| n28 | 0.5 |
| DC\_8\_n34 | 8 | 0.3 |
| n34 | 0.3 |
| DC\_8\_n39 | 8 | 0.3 |
| n39 | 0.3 |
| DC\_8\_n40 | 8 | 0.3 |
| n40 | 0.3 |
| DC\_8\_n41 | 8 | 0.3 |
| n41 | 0.3 |
| DC\_8\_n77 | 8 | 0.6 |
| n77 | 0.8 |
| DC\_8\_n78 | 8 | 0.6 |
| n77 | 0.8 |
| DC\_11\_n3 | 11 | 0.8 |
| n3 | 0.9 |
| DC\_11\_n77 | 11 | 0.4 |
| n77 | 0.8 |
| DC\_11\_n78 | 11 | 0.4 |
| n78 | 0.8 |
| DC\_12\_n2 | 12 | 0.3 |
| n2 | 0.3 |
| DC\_12\_n5 | 12 | 0.4 |
| n5 | 0.8 |
| DC\_12\_n7 | 12 | 0.3 |
| n7 | 0.3 |
| DC\_12\_n25 | 12 | 0.3 |
| n25 | 0.3 |
| DC\_12\_n38 | 12 | 0.3 |
| n38 | 0.3 |
| DC\_12\_n66 | 12 | 0.8 |
| n66 | 0.3 |
|  |  |  |
|  |  |
| DC\_12\_n78 | 12 | 0.5 |
| n78 | 0.8 |
| DC\_13\_n7 | 13 | 0.5 |
| n7 | 0.5 |
| DC\_13\_n48 | 13 | 0.3 |
| n48 | 0.3 |
| DC\_13\_n66 | 13 | 0.3 |
| n66 | 0.3 |
| DC\_13\_n71 | 13 | 0.5 |
| n71 | 0.5 |
| DC\_13\_n78 | 13 | 0.5 |
| n78 | 0.8 |
| DC\_18\_n3 | 18 | 0.3 |
| n3 | 0.3 |
| DC\_18\_n77 | 18 | 0.3 |
| n77 | 0.8 |
| DC\_18\_n78 | 18 | 0.3 |
| n78 | 0.8 |
| DC\_19\_n77 | 19 | 0.3 |
| n77 | 0.8 |
| DC\_19\_n78 | 19 | 0.3 |
| n78 | 0.8 |
| DC\_20\_n1 | 20 | 0.3 |
| n1 | 0.3 |
| DC\_20\_n3 | 20 | 0.3 |
| n3 | 0.3 |
| DC\_20\_n7 | 20 | 0.3 |
| n7 | 0.3 |
| DC\_20\_n8 | 20 | 0.4 |
| n8 | 0.4 |
| DC\_20\_n28 | 20 | 0.5 |
| n28 | 0.5 |
| DC\_20\_n38 | 20 | 0.3 |
| n38 | 0.3 |
| DC\_20\_n41 | 20 | 0.3 |
| n41 | 0.3 |
| DC\_20\_n50 | 20 | 0.3 |
| n50 | 0.4 |
| DC\_20\_n51 | 20 | 0.5 |
| n51 | 0.5 |
| DC\_20\_n77 | 20 | 0.6 |
| n77 | 0.8 |
| DC\_20\_n78 | 20 | 0.6 |
| n78 | 0.8 |
| DC\_21\_n77 | 21 | 0.4 |
| n77 | 0.8 |
| DC\_21\_n78 | 21 | 0.4 |
| n78 | 0.8 |
| n77 | 0.8 |
| DC\_25\_n41,DC\_25-25\_n41 | 25 | 0.5 |
| n41 | 0.41 |
| 0.92 |
| DC\_26\_n25 | 26 | 0.3 |
| n25 | 0.3 |
| DC\_26\_n41 | 26 | 0.3 |
| n41 | 0.3 |
| DC\_26\_n77 | 26 | 0.3 |
| n77 | 0.8 |
| DC\_26\_n78 | 26 | 0.3 |
| n78 | 0.8 |
| DC\_28\_n3 | 28 | 0.3 |
| n3 | 0.3 |
| DC\_28\_n5 | 28 | 0.5 |
| n5 | 0.5 |
| DC\_28\_n7 | 28 | 0.3 |
| n7 | 0.3 |
| DC\_28\_n8 | 28 | 0.5 |
| n8 | 0.6 |
| DC\_28\_n41 | 28 | 0.3 |
| n41 | 0.3 |
| DC\_28\_n50 | 28 | 0.3 |
| n50 | 0.4 |
| DC\_28\_n51 | 28 | 0.5 |
| n51 | 0.5 |
| DC\_28\_n77 | 28 | 0.5 |
| n77 | 0.8 |
| DC\_28\_n78 | 28 | 0.5 |
| n78 | 0.8 |
| DC\_30\_n2 | 30 | 0.3 |
| n2 | 0.5 |
| DC\_30\_n5 | 30 | 0.3 |
| n5 | 0.3 |
| DC\_30\_n66 | 30 | 0.5 |
| n66 | 0.8 |
| DC\_38\_n78 | n78 | 0.5 |
| DC\_39-n41 | 39 | 0.5 |
| n41 | 0.5 |
| DC\_39\_n78 | 39 | 0.3 |
| n78 | 0.8 |
| DC\_39\_n79 | 39 | 0.3 |
| n79 | 0.8 |
| DC\_40\_n1 | n1 | 0.5 |
| 40 | 0.5 |
| DC\_40\_n415 | 40 | 0.5 |
| n41 | 0.5 |
| DC\_40\_n77 | n77 | 0.5 |
| DC\_40\_n78 | n78 | 0.56 |
| DC\_40\_n79 | 40 | 0.3 |
| n79 | 0.8 |
| DC\_41\_n77 | 41 | 0.3 |
| n77 | 0.8 |
| DC\_41\_n78 | 41 | 0.3 |
| n78 | 0.8 |
| DC\_41\_n79 | 41 | 0.3 |
| n79 | 0.8 |
| DC\_42\_n51 | 42 | 0.6 |
| n51 | 0.8 |
| DC\_48\_n5 | 48 | 0.3 |
| n5 | 0.3 |
| DC\_48\_n12 | 48 | 0.3 |
| n12 | 0.3 |
| DC\_48\_n46 | 48 | 0.8 |
| DC\_48\_n66 | 48 | 0.8 |
| n66 | 0.6 |
| DC\_48\_n71 | 48 | 0.3 |
| n71 | 0.3 |
| DC\_66\_n2 | 66 | 0.5 |
| n2 | 0.5 |
| DC\_66\_n5 | 66 | 0.3 |
| n5 | 0.3 |
| DC\_66\_n7 | 66 | 0.5 |
| n7 | 0.5 |
| DC\_66\_n12 | 66 | 0.8 |
| n12 | 0.3 |
| DC\_66\_n25 | 66 | 0.5 |
| n25 | 0.5 |
| DC\_66\_n38 | 66 | 0.5 |
| n38 | 0.5 |
| DC\_66\_n41 | 66 | 0.5 |
| n41 | 0.81 |
| 1.32 |
| DC\_66\_n48,DC\_66-66\_n48 | 66 | 0.6 |
| n48 | 0.8 |
| DC\_66\_n71 | 66 | 0.3 |
| n71 | 0.3 |
| DC\_66\_n78 | 66 | 0.6 |
| n78 | 0.8 |
| DC\_71\_n5 | 71 | 0.5 |
| n5 | 0.5 |
| DC\_71\_n38 | 71 | 0.6 |
| n38 | 0.3 |
| DC\_71\_n48 | 71 | 0.3 |
| n48 | 0.3 |
| DC\_71\_n66 | 71 | 0.3 |
| n66 | 0.3 |
| DC\_71\_n78 | 71 | 0.5 |
| n78 | 0.8 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545-2690 MHz.NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496-2545 MHz.NOTE 3: Applicable for the frequency range of 2515 – 2690 MHz.NOTE 4: Applicable for the frequency range of 2496 - 2515 MHz.NOTE 5: Applicable for UE supporting inter-band EN-DC without simultaneous Rx/Tx.NOTE 6: Only applicable for UE supporting inter-band carrier aggregation with uplink in one E-UTRA band and without simultaneous Rx/Tx. |

---Text omitted---

Table 7.3B.3.3.1-1: ΔRIB,c due to EN-DC(two bands)

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_1\_n28 | n28 | 0.2 |
| DC\_1\_n51 | n51 | 0.1 |
| DC\_1\_n77 | 1 | 0.2 |
| n77 | 0.5 |
| DC\_1\_n78 | n78 | 0.5 |
| DC\_2\_n48 | 2 | 0.2 |
| n48 | 0.5 |
| DC\_2\_n66 | 2 | 0.3 |
| n66 | 0.3 |
| DC\_2\_n78 | 2 | 0.2 |
| n78 | 0.5 |
| DC\_3-n41 | n41 | 03 |
| 0.54 |
| DC\_3\_n51 | 3 | 0.2 |
| n51 | 0.2 |
| DC\_3\_n77, DC\_3-3\_n77 | 3 | 0.2 |
| n77 | 0.5 |
| DC\_3\_n78, DC\_3-3\_n78 | 3 | 0.2 |
| n78 | 0.5 |
| DC\_5\_n78 | 5 | 0.2 |
| n78 | 0.5 |
| DC\_4\_n38 | 4 | 0.5 |
| n38 | 0.5 |
| DC\_4\_n41 | 4 | 0.5 |
| n41 | [0.51] |
| [12] |
| DC\_4\_n78 | 4 | 0.2 |
| n78 | 0.5 |
| DC\_5\_n12 | 5 | 0.5 |
| n12 | 0.3 |
| DC\_7\_n8 | n8 | 0.2 |
| DC\_7\_n51 | n51 | 0.2 |
| DC\_7\_n66, DC\_7-7\_n66 | 7 | 0.5 |
| n66 | 0.5 |
| DC\_7\_n71 | n71 | 0.2 |
| DC\_7\_n77, DC\_7-7\_n77 | n77 | 0.5 |
| DC\_7\_n78, DC\_7-7\_n78 | n78 | 0.5 |
| DC\_8\_n28 | 8 | 0.2 |
| n28 | 0.1 |
| DC\_8\_n77 | 8 | 0.2 |
| n77 | 0.5 |
| DC\_8\_n78 | 8 | 0.2 |
| n78 | 0.5 |
| DC\_11\_n3 | 11 | 0.3 |
| n3 | 0.5 |
| DC\_11\_n77 | n77 | 0.5 |
| DC\_11\_n78 | n78 | 0.5 |
| DC\_12\_n5 | 12 | 0.3 |
| n5 | 0.5 |
| DC\_12\_n66 | 12 | 0.5 |
| DC\_12\_n78 | 12 | 0.2 |
| n78 | 0.5 |
| DC\_13\_n7 | 13 | 0.5 |
| n7 | 0.5 |
| DC\_13\_n78 | 13 | 0.2 |
| n78 | 0.5 |
| DC\_18\_n77 | n77 | 0.5 |
| DC\_19\_n77 | n77 | 0.5 |
| DC\_19\_n78 | n78 | 0.5 |
| DC\_20\_n51 | n51 | 0.2 |
| DC\_20\_n77 | n77 | 0.5 |
| DC\_20\_n78 | n78 | 0.5 |
| DC\_21\_n77 | n77 | 0.5 |
| DC\_21\_n78 | n78 | 0.5 |
| DC\_25\_n41,DC\_25-25\_n41 | n41 | 01 |
| 0.52 |
| DC\_26\_n77 | n77 | 0.5 |
| DC\_26\_n78 | n78 | 0.5 |
| DC\_28\_n8 | 28 | 0.1 |
| n8 | 0.2 |
| DC\_28A\_n51 | n51 | 0.2 |
| DC\_28\_n77 | 28 | 0.2 |
| n77 | 0.5 |
| DC\_28\_n78 | 28 | 0.2 |
| n78 | 0.5 |
| DC\_30\_n66 | 30 | 0.5 |
| n66 | 0.4 |
| DC\_38\_n78 | 38 | 0.4 |
| n78 | 0.5 |
| DC\_39\_n40 | 39 | 0.3 |
| n40 | 0.3 |
| DC\_39-n41 | 39 | 0.2 |
| n41 | 0.2 |
| DC\_39\_n78 | n78 | 0.5 |
| DC\_39\_n79 | n79 | 0.5 |
| DC\_40\_n77 | 40 | 0.4 |
| n77 | 0.5 |
| DC\_40\_n78 | 40 | 0.45 |
| n78 | 0.55 |
| DC\_40\_n79 | n79 | 0.5 |
| DC\_41\_n77 | n77 | 0.5 |
| DC\_41\_n78 | n78 | 0.5 |
| DC\_41\_n79 | n79 | 0.5 |
| DC\_42\_n51 | n51 | 0.2 |
| DC\_48\_n46 | 48 | 0.5 |
| DC\_48\_n66 | 48 | 0.5 |
| n66 | 0.2 |
| DC\_66\_n2 | 66 | 0.3 |
| n2 | 0.3 |
| DC\_66\_n7 | 66 | 0.5 |
| n7 | 0.5 |
| DC\_66\_n12 | 66 | 0.5 |
| DC\_66\_n25 | 66 | 0.3 |
| n25 | 0.3 |
| DC\_66\_n38 | 66 | 0.5 |
| n38 | 0.5 |
| DC\_66\_n41 | 66 | 0.5 |
| n41 | 0.51 |
| 12 |
| DC\_66\_n48,DC\_66-66\_n48 | 66 | 0.2 |
| n48 | 0.5 |
| DC\_66\_n78 | 66 | 0.2 |
| n78 | 0.5 |
| DC\_71\_n38 | 71 | 0.2 |
| DC\_71\_n78 | 71 | 0.2 |
| n78 | 0.5 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545 – 2690 MHz.NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496 – 2545 MHz.NOTE 3: Applicable for the frequency range of 2515 – 2690 MHz.NOTE 4: Applicable for the frequency range of 2496 – 2515 MHz.NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one E-UTRA band and without simultaneous Rx/Tx. |

---Text omitted---

Table 7.3B.2.3.1-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1

|  |  |
| --- | --- |
|  | E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band |
| UL band | DL band | 5MHz(LCRB) | 10 MHz(LCRB) | 15 MHz(LCRB) | 20 MHz(LCRB) | 25 MHz(LCRB) | 30 MHz(LCRB) | 40 MHz(LCRB) | 50 MHz(LCRB) | 60 MHz(LCRB) | 80 MHz(LCRB) | 90 MHz(LCRB) | 100 MHz(LCRB) |
| 1 | n77 |  | 25 | 36 | 50 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| 2 | n48 | 12 | 25 | 36 | 50 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| 2 | n78 |  | 25 | 36 | 50 |  |  | 50 | 50 | 50 | 50 | 50 | 50 |
| 3 | n77, n78 |  | 25 | 36 | 50 |  |  | 50 | 50 | 50 | 50 | 50 | 50 |
| 4 | n78 |  | 25 | 36 | 50 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| 5 | n78 | 8 | 16 | 25 | 25 |  |  | 25 |  |  |  |  |  |
| 8 | n41 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 8 | n77n78 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 8 | n79 |  |  |  |  |  |  | 25 | 25 | 25 | 25 |  | 25 |
| n8 | 3 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |
| n8 | 7 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |
| 12 | n66 | 8 | 16 | 20 | 20 |  |  | 20 |  |  |  |  |  |
| 12 | n78 |  | 10 | 15 | 20 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| n12 | 48 | 5 | 10 | 15 | 20 |  |  |  |  |  |  |  |  |
| 18 | n77 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 19 | n77 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 20 | n38 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |
| 20 | n77, n78 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 26 | n41 |  | 16 | 25 | 25 |  |  | 25 | 25 |  |  |  |  |
| 26 | n77,n78 |  | 16 | 25 | 25 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| n28 | 1 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |
| 28 | n77,n78 |  | 10 | 15 | 20 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| 66 | n48 | 12 | 25 | 36 | 50 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| 66 | n78 |  | 25 | 36 | 50 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| n66 | 48 | 12 | 25 | 36 | 50 |  |  |  |  |  |  |  |  |
| n71 | 2 | 25485 | 25485 | 20485 | 20485 |  |  |  |  |  |  |  |  |
| n71 | 7 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |
| 71 | n78 |  | 10 | 15 | 20 |  |  | 25 | 25 | 25 | 25 | 25 | 25 |
| NOTE 1: The UL configuration applies regardless of the channel bandwidth of the UL band unless the UL resource blocks exceed that specified in Table 7.3.1-2 in TS 36.101 [4] or Table 7.3.2-3 in TS 38.101-1 [2] for the uplink bandwidth in which case the allocation according to Table 7.3.1-2 in TS 36.101 [4] or Table 7.3.2-3 in TS 38.101-1 [2] appliesNOTE 2: VoidNOTE 3: Unless stated otherwise, UL resource blocks shall be centred within the transmission bandwidth configuration for the channel bandwidth.NOTE 4: These requirements apply when the lower edge frequency of the 5 MHz uplink channel in Band 71 is located at or below 668 MHz and the downlink channel in Band 2 is located with its upper edge at 1990 MHz.NOTE 5: These requirements apply when the lower edge frequency of the 10 MHz, 15 MHz, or 20 MHz uplink channel in Band 71 is located at or below 668 MHz and the downlink channel in Band 2 is located with its upper edge at 1990 MHz. |

**Table 7.3B.2.3.1-3: Reference sensitivity QPSK PREFSENS (EN-DC with n46)**

|  |
| --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD |
| UL band | DL band | 5MHz(dB) | 10 MHz(dB) | 15 MHz(dB) | 20 MHz(dB) | 25 MHz(dB) | 40 MHz(dB) | 50 MHz(dB) | 60 MHz(dB) | 80 MHz(dB) | 90 MHz(dB) | 100 MHz(dB) |
| 2 | n461 |  |  |  | N/A |  | N/A |  | N/A | N/A |  |  |
| n46 | 22,3 | 28 | 28 | 28 | 28 |  |  |  |  |  |  |  |
| 66 | n46 |  |  |  | N/A |  | N/A |  | N/A | N/A |  |  |
| NOTE 1: These requirements apply when there is at least one individual RE within the downlink (victim) transmission bandwidth which falls into the reference sensitivity exclusion region as specified in Table 6.x.1.7-2 and Table 6.x.1.7-3.NOTE 2: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the aggressor (higher) band and when the frequency range of relative higher band’s uplink channel bandwidth or uplink 1st adjacent channel bandwidth is fully or partially overlapped with the downlink transmission bandwidth of a victim (lower) band.NOTE 3:   The requirements for a victim (lower) band apply for UL EARFCN of the aggressor (higher) band (superscript HB) such that cid:image004.png@01D629D8.2A3DDB60  in MHz with cid:image005.png@01D629D8.2A3DDB60  the DL carrier frequency in the lower band and $f\_{UL}^{HB}$ the UL carrier frequency in the higher band, both in MHz. . |

**Table 7.3B.2.3.1-4: n46 Reference sensitivity measurement exclusion region in MHz**

|  |
| --- |
| Licensed Component Carriers / E-UTRA Band / Harmonic order / Channel BW in UL |
| Band | Harmonic order | 5MHz | 10MHz | 15MHz | 20MHz |
| 2 | 3 | +/- 15 | +/- 23 | +/- 35 | +/- 45 |
| 66 | 3 | +/- 15 | +/- 23 | +/- 35 | +/- 45 |
| NOTE 1: Even though UL harmonic does not fall directly into n46 the exclusion region still applies.NOTE 2: The center of the exclusion region is obtained by multiplying the uplink channel center frequency by the harmonic order. |

**Table 7.3B.2.3.1-5: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC paring with n46**

|  |
| --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band |
| UL band | DL band | SCS of UL band(kHz) | 5 MHz(LCRB) | 10 MHz(LCRB) | 15 MHz(LCRB) | 20 MHz(LCRB) | 25 MHz(LCRB) | 40 MHz(LCRB) | 50 MHz(LCRB) | 60 MHz(LCRB) | 80 MHz(LCRB) | 90 MHz(LCRB) | 100 MHz(LCRB) |
| n46 | 2 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |

---Text omitted---

Table 7.3B.2.3.5.1-1: MSD test points for PCell due to dual uplink operation for EN-DC in NR FR1 (two bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DCConfiguration | EUTRA or NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL LCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_1\_n3 | 1 | 1950 | 5 | 25 | 2140 | 23 | IMD3 |
| n3 | 1760 | 5 | 25 | 1855 | N/A | N/A |
| DC\_1A-n5A | 1 | 1965 | 5 | 25 | 2155 | 6 | IMD4 |
| n5 | 836.5 | 5 | 25 | 876.5 | N/A | N/A |
| DC\_1A\_n8A | 1 | 1965 | 5 | 25 | 2155 | 6.0 | IMD4 |
| n8 | 887.5 | 5 | 25 | 932.5 | N/A | N/A |
| DC\_1A\_n77A,DC\_1A\_SUL\_n77A-n84A, DC\_1A\_n77(2A), | 1 | 1950 | 5 | 25 | 2140 | 29.8 | IMD23 |
| 32.54 |
| n77 | 4090 | 10 | 50 | 4090 | N/A | N/A |
| DC\_1A\_n77A,DC\_1A-SUL\_n77A-n84A,DC\_1A\_n77(2A),DC\_1A\_n78A,DC\_1A\_SUL\_n78A-n84A, DC\_1A\_n78(2A) | 1 | 1950 | 5 | 25 | 2140 | 8.0 | IMD43 |
| 10.74 |
| n77 | 3710 | 10 | 50 | 3710 | N/A | N/A |
| DC\_2A\_n46A | 2 | 1880 | 5 | 25 | 1960 | 12.0 | IMD3 |
| n46 | 5720 | 20 | 100 | 5720 | N/A | N/A |
| DC\_2A\_n48A | 2 | 1852.5 | 5 | 25 | 1932.5 | [12] | IMD4 |
| n48 | 3625 | 20 | 100 | 3625 | N/A | N/A |
| DC\_2A\_n66A, DC\_2A-2A\_n66A | 2 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
| n66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| DC\_2A\_n66A, DC\_2A-2A\_n66A | 2 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| n66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
| DC\_2A\_n78ADC\_2A\_n78(2A) | 2 | 1855 | 5 | 25 | 1935 | 26 | IMD23 |
| 28.74 |
| n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |
| DC\_2A\_n78ADC\_2A\_n78(2A) | 2 | 1885 | 5 | 25 | 1965 | 8.0 | IMD43 |
| 10.74 |
| n78 | 3690 | 10 | 50 | 3690 | N/A | N/A |
| DC\_3\_n1 | 3 | 1760 | 5 | 25 | 1855 | N/A | N/A |
| n1 | 1950 | 5 | 25 | 2140 | 23 | IMD3 |
| DC\_3\_n5 | 3 | 1771 | 10 | 50 | 1866 | 4 | IMD4 |
| n5 | 838 | 5 | 25 | 883 | N/A | N/A |
| 3 | 1721 | 10 | 50 | 1816 | N/A | N/A |
| n5 | 838 | 5 | 25 | 883 | 24 | IMD23 |
| DC\_3A\_n7ADC\_3C\_n7A | 3 | 1730 | 5 | 25 | 1825 | N/A | N/A |
| n7 | 2535 | 10 | 50 | 2655 | 10.2 | IMD4 |
| DC\_3\_n8 | n8 | 900 | 5 | 25 | 945 | 8 | IMD43 |
| 3 | 1755 | 10 | 50 | 1850 | N/A | N/A |
| n8 | 897.5 | 5 | 25 | 942.5 | N/A | N/A |
| 3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | IMD5 |
| CA\_3A-n20A | 3 | 1775 | 5 | 25 | 1870 | 4 | IMD4 |
| n20 | 840 | 5 | 25 | 799 | N/A | N/A |
| 3 | 1735 | 5 | 25 | 1830 | N/A | N/A |
| n20 | 847 | 5 | 25 | 806 | 9 | IMD4 |
| DC\_3A\_n38A | 3 | 1713 | 5 | 25 | 1808 | 8.2 | IMD4 |
| n38 | 2617 | 5 | 25 | 2617 | N/A | N/A |
| DC\_3A\_n41ADC\_3C\_n41ADC\_3A\_SUL\_n41A-n80A, DC\_3C\_SUL\_n41A-n80A | 3 | 1740 | 5 | 25 | 1835 | 8.2 | IMD4 |
| n41 | 2657.5 | 10 | 50 | 2657.5 | N/A | N/A |
| DC\_3A\_n77A,DC\_3A\_n77(2A),DC\_3A\_SUL\_n77A-n80A,DC\_3A\_n78A,DC\_3A-SUL\_n78A-n80A,DC\_3A\_n78(2A),DC\_3C\_n78ADC\_3C\_n78(2A) | 3 | 1740 | 5 | 25 | 1835 | 26 | IMD23 |
| 28.74 |
| n77, n78 | 3575 | 10 | 50 | 3575 | N/A | N/A |
| DC\_3A\_n77A,DC\_3A\_n77(2A),DC\_3A\_SUL\_n77A-n80A,DC\_3A\_n78A, DC\_3A-SUL\_n78A-n80A,DC\_3A\_n78(2A),DC\_3C\_n78ADC\_3C\_n78(2A) | 3 | 1765 | 5 | 25 | 1860 | 8.0 | IMD43 |
| 10.74 |
| n77, n78 | 3435 | 10 | 50 | 3435 | N/A | N/A |
| DC\_5\_n7 | n7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
| 5 | 834 | 5 | 25 | 879 | 12 | IMD33 |
| DC\_5\_n38 | 5 | 844 | 5 | 25 | 889 | 12 | IMD33 |
| n38 | 2577 | 10 | 50 | 2577 | N/A | N/A |
| DC\_5A\_n66A | 5 | 838 | 5 | 25 | 883 | 30 | IMD23 |
| n66 | 1721 | 5 | 25 | 2121 | N/A | N/A |
| DC\_5A\_n78ADC\_5A\_n78(2A) | 5 | 844 | 5 | 25 | 889 | 8.3 | IMD4 |
| n78 | 3421 | 10 | 50 | 3421 | N/A | N/A |
| DC\_7\_n3 | 7 | 2535 | 10 | 50 | 2655 | 13 | IMD4 |
| n3 | 1730 | 5 | 25 | 1825 | N/A | N/A |
| DC\_7\_n5 | 7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
| n5 | 834 | 5 | 25 | 879 | 12 | IMD33 |
| DC\_7A\_n66ADC\_7A-7A\_n66ADC\_7C\_n66A | 7 | 2535 | 10 | 50 | 2655 | 15 | 4th IMD |
| n66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| DC\_7A\_n77A | 7 | 2540 | 5 | 25 | 2660 | 7.1 | IMD4 |
| n77 | 3870 | 10 | 50 | 3870 | N/A | N/A |
| DC\_8A\_n1A | 8 | 887.5 | 5 | 25 | 932.5 | N/A | N/A |
| n1 | 1965 | 5 | 25 | 2155 | 6 | IMD4 |
| DC\_8A\_n3A | 8 | 900 | 5 | 25 | 945 | 8 | IMD43 |
| n3 | 1755 | 10 | 50 | 1850 | N/A | N/A |
| 8 | 897.5 | 5 | 25 | 942.5 | N/A | N/A |
| n3 | 1747.5 | 10 | 50 | 1842.5 | 6.4 | IMD5 |
| DC\_8A\_n41ADC\_8A\_SUL\_n41A-n81A | 8  | 882.5 | 5 | 25  | 927.5 | 12.1 | IMD33 |
| n41 | 2685 | 10 | 50  |  2685 | N/A  | N/A |
| DC\_8A\_n77A,DC\_8A\_n78A, DC\_8A-SUL\_n78A-n81A | 8 | 897.5 | 5 | 25 | 942.5 | 8.3 | IMD4 |
| n77, n78 | 3635 | 10 | 50 | 3635 | N/A | N/A |
| DC\_8A\_n79A,DC\_8A-n79C,DC\_8A-SUL\_n79A-n81A | 8 | 897.5 | 5 | 25 | 942.5 | 4.8 | IMD5 |
| n79 | 4532.5 | 40 | 216 | 4532.5 | N/A | N/A |
| DC\_12\_n78 | 12 | 710 | 5 | 25 | 740 | 5.5 | IMD5 |
| n78 | 3580 | 10 | 50 | 3580 | N/A | N/A |
| DC\_13A\_n7ADC\_13A\_n7(2A) | 13 | 784.5 | 5 | 25 | 753.5 | N/A | N/A |
| n7 | 2520 | 40 | 216 | 2640 | 2.5 | IMD5 |
| DC\_18A\_n3A | 18 | 823 | 5 | 25 | 868 | N/A | N/A |
| n3 | 1721 | 5 | 25 | 1816 | 4 | IMD4 |
| DC\_20A\_n3A | 20 | 840 | 5 | 25 | 799 | N/A | N/A |
| n3 | 1775 | 5 | 25 | 1870 | 4 | IMD4 |
| 20 | 847 | 5 | 25 | 806 | 9 | IMD4 |
| n3 | 1735 | 5 | 25 | 1830 | N/A | N/A |
| DC\_20\_n7 | 20 | 851 | 5 | 25 | 810 | 12 | IMD33 |
| n7 | 2512 | 10 | 50 | 2632 | N/A | N/A |
| DC\_20A\_n8A | 20 | 849.5 | 5 | 25 | 808.5 | 25 | IMD3 |
| n8 | 892.5 | 5 | 25 | 937.5 | 25 | IMD3 |
| DC\_20\_n41 | 20 | 851 | 5 | 25 | 810 | 12.1 | IMD3 |
| n41 | 2512 | 10 | 50 | 2512 | N/A | N/A |
| DC\_20\_n41 | 20 | 841 | 5 | 25 | 800 | 8.1 | IMD5 |
| n41 | 2564 | 10 | 50 | 2564 | N/A | N/A |
| DC\_20A\_n77A,DC\_20A\_n78A, DC\_20A-SUL\_n78A-n82A | 20 | 850 | 5 | 25 | 809 | 11 | IMD4 |
| n77, n78 | 3359 | 10 | 50 | 3359 | N/A | N/A |
| DC\_20A\_n77A | 20 | 840 | 5 | 25 | 799 | 6.5 | IMD5 |
| n77 | 4159 | 10 | 50 | 4159 | N/A | N/A |
| DC\_21A\_n79A | 21 | 1457.5 | 5 | 25 | 1505.5 | 18.4 | IMD3 |
| n79 | 4420.5 | 40 | 216 | 4420.5 | N/A | N/A |
| DC\_26A\_n41A | 26 | 839 | 5 | 25 | 884 | 15.6 | IMD33 |
| n41 | 2562 | 10 | 50 | 2562 | N/A | N/A |
| DC\_28\_n50 | 28 | 730 | 10 | 50 | 775 | 15.3 | IMD 2 |
| n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
| 28 | 740 | 10 | 50 | 785 | 6 | IMD 4 |
| n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
| 28 | 740 | 10 | 50 | 785 | 0.5 | IMD 5 |
| n50 | 1500 | 10 | 50 | 1500 | N/A | N/A |
| DC\_28A\_n51A | 28 | 742.3 | 5 | 25 | 797.3 | 5 | IMD4 |
| n51 | 1429.5 | 5 | 25 | 1429.5 | N/A | N/A |
| DC\_26A\_n77A,DC\_26A\_n78A | 26 | 836.5 | 5 | 25 | 881.5 | 11.1 | IMD4 |
| n77, n78 | 3391 | 10 | 50 | 3391 | N/A | N/A |
| DC\_28A\_n77A,DC\_28A\_n78A, DC\_28A-SUL\_n78A-n83A | 28 | 705.5 | 5 | 25 | 760.5 | 5.5 | IMD5 |
| n77, n78 | 3582.5 | 10 | 50 | 3582.5 | N/A | N/A |
| DC\_48A\_n12A | 48 | 3557.5 | 10 | 50 | 3557.5 | N/A | N/A |
| n12 | 705.5 | 5 | 25 | 735.5 | 5.5 | IMD5 |
| DC\_48A\_n66A | 48 | 3630 | 20 | 100 | 3630 | N/A | N/A |
| n66 | 1715 | 5 | 25 | 2115 | 4 | IMD5 |
| DC\_66A\_n2A, DC\_66A-66A\_n2A | 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| n2 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
| 66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
| n2 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| DC\_66A\_n5A | n5 | 838 | 5 | 25 | 883 | 30 | IMD23 |
| 66 | 1721 | 5 | 25 | 2121 | N/A | N/A |
| DC\_66A\_n7ADC\_66A-66A\_n7ADC\_66A-66A\_n7(2A) | 66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| n7 | 2535 | 10 | 50 | 2655 | 15 | IMD4 |
| DC\_66A\_n25A | 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| n25 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
| 66 | 1712.5 | 5 | 25 | 2112.5 | 23 | IMD3 |
| n25 | 1912.5 | 5 | 25 | 1992.5 | N/A | N/A |
| 66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |
| n25 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| DC\_66A\_n46A | 66 | 1735 | 5 | 25 | 2135 | 12.0 | IMD3 |
| n46 | 5605 | 20 | 100 | 5605 | N/A | N/A |
| DC\_66A\_n48A | 66 | 1715 | 5 | 25 | 2115 | 4 | IMD5 |
| n48 | 3630 | 20 | 100 | 3630 | N/A | N/A |
| DC\_66A\_n71A | 66 | 1750 | 5 | 25 | 2150 | 5 | IMD4 |
| n71 | 675 | 5 | 25 | 629 | N/A | N/A |
| DC\_71A\_n38A | 71 | 665 | 5 | 25 | 619 | 11 | IMD4 |
| n38 | 2614 | 5 | 25 | 2614 | N/A | N/A |
| DC\_71A\_n66A | 71 | 675 | 5 | 25 | 629 | N/A | N/A |
| n66 | 1750 | 5 | 25 | 2150 | 5 | IMD4 |
| DC\_71A\_n78A | 71 | 681.5 | 5 | 25 | 635.5 | 5.5 | IMD5 |
| n78 | 3361.5 | 10 | 50 | 3582.5 | N/A | N/A |
| NOTE 1: Both of the transmitters shall be set min(+20 dBm, PCMAX\_L,c) as defined in clause 6.2.5A.NOTE 2: RBstart = 0NOTE 3: This band is subject to IMD5 also which MSD is not specified.NOTE 4: Applicable only if operation with 4 antenna ports is supported in the band with EN-DC configured.NOTE 5: Void |

---Text omitted---

Table 7.3B.2.3.4-1: Reference sensitivity exceptions (MSD) due to cross band isolation for EN-DC in NR FR1

|  |  |
| --- | --- |
|  | E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD |
| UL band | DL band | 5 MHz(dB) | 10 MHz(dB) | 15 MHz(dB) | 20 MHz(dB) | 25 MHz(dB) | 30 MHz(dB) | 40 MHz(dB) | 50 MHz(dB) | 60 MHz(dB) | 80 MHz(dB) | 90 MHz(dB) | 100 MHz(dB) |
| n13 | 3 | 3 | 2.3 | 2 | 1.8 |  |  |  |  |  |  |  |  |
| n1 | 40 | 6.6 | 6.6 | 6.6 | 6.6 |  |  |  |  |  |  |  |  |
| 13 | n3 | 3 | 2.2 | 1.9 | 1.7 | 1.6 |  |  | 1.5 |  |  |  |  |
| 1 | n41 |  | 6.1 | 6.1 | 6.1 |  |  | 6.1 | 6.1 | 6.1 | 6.1 | 6.1 | 6.1 |
| 3 | n41 |  | 0.7 | 0.7 | 0.7 |  |  | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7 |
| n38 | 1 | 1.9 | 1.9 | 1.9 | 1.9 |  |  |  |  |  |  |  |  |
| n38 | 2 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |  |
| n38 | 4 | 1.9 | 1.9 | 1.9 | 1.9 |  |  |  |  |  |  |  |  |
| n38 | 66 | 1.9 | 1.9 | 1.9 | 1.9 |  |  |  |  |  |  |  |  |
| n41 | 4 | 3.5 | 3.5 | 3.5 | 3.5 |  |  |  |  |  |  |  |  |
| 40 | n1 | 8.3 | 8.3 | 8.3 | 8.3 |  |  |  |  |  |  |  |  |
| n41 | 1 | 9.1 | 9.1 | 9.1 | 9.1 |  |  |  |  |  |  |  |  |
| n41 | 2 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |  |
| n41 | 3 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |  |
| n41 | 661 | 3.5 | 3.5 | 3.5 | 3.5 |  |  |  |  |  |  |  |  |
| n41 | 25 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |  |
| n50 | 3 | 2.5 | 1.9 | 1.6 | 1.5 |  |  |  |  |  |  |  |  |
| n77 | 71 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |  |  |  |
| n77 | 411 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |  |  |  |
| 41 | n77 |  | 8.3 | 8.3 | 8.3 |  |  | 6.3 | 5.3 | 4.5 | 4.0 | 3.9 | 3.8 |
| n78 | 71 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |  |  |  |
| n78 | 38 | 3.3 | 3.3 | 3.3 | 3.3 |  |  |  |  |  |  |  |  |
| n78 | 411 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |  |  |  |
| 41 | n78 |  | 8.3 | 8.3 | 8.3 |  |  | 6.3 | 5.3 | 4.5 | 4.0 | 3.9 | 3.8 |
| n843 | 3 | 3 | 2.3 | 2 | 1.8 |  |  |  |  |  |  |  |  |
| 48 | n46 | - | - | - | 7 | - | - | 5.7 | - | 5.1 | 4.7 | - | - |
| n46 | 48 | 13.3 | 10.4 | 8.8 | 7.8 | - | - | 7.8 | 7 | 6.5 | 5.7 | 5.4 | 5.1 |
| NOTE 1: Applicable only when harmonic mixing MSD for this combination is not applied.NOTE 2: The B41 requirements are modified by -0.5dB when carrier frequency of the assigned E-UTRA channel bandwidth is within 2515 – 2690 MHz. NOTE 3: These requirements apply when the uplink is active in Band n84 and the separation between the lower edge of the uplink channel in Band n84 and the upper edge of the downlink channel in Band 3 is < 60 MHz. For each channel bandwidth in Band 3, the requirement applies regardless of channel bandwidth in Band n84.NOTE 4: The DL victim band should be configured using the lowest SCS that is compatible with the highest CBW for which an MSD is specified |

Table 7.3B.2.3.4-2: Uplink configuration for reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1

|  |
| --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band |
| UL band | DL band | SCS of UL band (kHz) | 5 MHz(LCRB) | 10 MHz(LCRB) | 15 MHz(LCRB) | 20 MHz(LCRB) | 25 MHz(LCRB) | 30 MHz(LCRB) | 40 MHz(LCRB) | 50 MHz(LCRB) | 60 MHz(LCRB) | 80 MHz(LCRB) | 90 MHz(LCRB) | 100 MHz(LCRB) |
| n1 | 3 | 15 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |  |  |
| n1 | 40 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |
| 1 | n3 | 15 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |
| 1 | n41 | 15 |  | 100 | 100 | 100 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| 3 | n41 | 15 | 50 | 502 | 502 | 502 |  |  | 502 | 502 | 502 | 502 | 502 | 502 |
| n38 | 1 | 15 | 100 | 100 | 100 | 100 |  |  |  |  |  |  |  |  |
| n38 | 2 | 15 | 100 | 100 | 100 | 100 |  |  |  |  |  |  |  |  |
| n38 | 4 | 15 | 100 | 100 | 100 | 100 |  |  |  |  |  |  |  |  |
| n38 | 66 | 15 | 100 | 100 | 100 | 100 |  |  |  |  |  |  |  |  |
| 40 | n1 | 15 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |
| n41 | 1 | 30 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |  |  |
| n41 | 2 | 30 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |  |
| n41 | 3 | 30 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |  |
| n41 | 4 | 30 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |  |  |
| n41 | 25 | 30 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |  |
| n41 | 66 | 30 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |  |  |
| n50 | 3 | 30 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |  |
| n77 | 7 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |
| n77 | 41 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |
| 41 | n77 | 15 |  | 100 | 100 | 100 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| n78 | 7 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |
| n78 | 38 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |
| n78 | 41 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |
| 41 | n78 | 15 |  | 100 | 100 | 100 |  |  | 100 | 100 | 100 | 100 | 100 | 100 |
| n84 | 3 | 15 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |  |  |
| 48 | n46 | 15 |  |  |  | 216 |  |  | 216 |  | 216 | 216 |  |  |
| n46 | 48 | 30 | 216 | 216 | 216 | 216 |  |  | 216 | 216 | 216 | 216 | 216 | 216 |
| NOTE 1: The UL configuration applies regardless of the channel bandwidth of the UL band. UL resource blocks allocation in the table shall be further limited to that specified in Table 7.3.1-2 in TS 36.101 [4] or Table 7.3.2-3 in TS 38.101-1 [2].NOTE 2: The UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth. NOTE 3: When the maximum UL RB allocation “LCRB” value is less than the maximum transmission bandwidth configuration “NRB” defined in Table 5.3.2-1 in 38.101-1 [2] for the specified UL band SCS, the UL band should be configured using the lowest CBW that is compatible with the maximum specified LCRB value. |

---End of changes---