3GPP TSG-RAN WG4 Meeting # 95-e Revised R4-2006708

Electronic Meeting, 25 May – 5 June, 2020

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-2** | **CR** |  | **rev** | **-** | **Current version:** | **16.3.1** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to 38.101-2: Conrrection of aggregated bandwidth for CA\_n261(2A-G) in Table 5.5A.2-2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Verizon, Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_CA\_R16\_Intra | | | | |  | ***Date:*** | | | 2020-05-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The total aggregated bandwidth for CA\_n261(2A-G) is incorrectely specifid | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Corrected the aggregated bandwidth for CA\_n261(2A-G) from the Table 5.5A.2-2 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrected requirement in the spec for the aggregated channel bandwidth | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5A | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **x** |  | Test specifications | | | | 38.521-3 | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

5.5A Configurations for CA

5.5A.1 Configurations for intra-band contiguous CA

## **<< Start of changes >>**

**Table 5.5A.2-2: NR CA configurations and bandwidth combination sets for intra-band non-contiguous CA**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NR CA configuration / Bandwidth combination set** | | | | | | | | | | | | | | | | | | | | | | | | |
| **CA configuration** | **Uplink CA configurations** | **Sub-block** | **Sub-block** | **Sub-block** | **Sub-block** | **Sub-block** | **Sub-block** | | **Sub-block** | | **Sub-block** | | **Sub-block** | | **Sub-block** | | **Sub-block** | | **Sub-block** | | **(BWChannel,block) (MHz)** | | **BCS** | |
|
| CA\_n260(A-D) | - | n260 | CA\_n260D |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(2A-D) | - | CA\_n260(2A) | | CA\_n260D |  |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(A-2D) | - | n260 | CA\_n260(2D) | |  |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-2D) | - | CA\_n260(2A) | | CA\_n260(2D) | |  |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(A-D-O) | - | n260 | CA\_n260D | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(2A-D-O) | - | CA\_n260(2A) | | CA\_n260D | CA\_n260O |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(A-D-2O) | - | n260 | CA\_n260D | CA\_n260(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-D-2O) | - | CA\_n260(2A) | | CA\_n260D | CA\_n260(2O) | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(A-G) | - | n260 | CA\_n260G |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n260(2A-G) | - | CA\_n260(2A) | | CA\_n260G |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(A-2G) | - | n260 | CA\_n260(2G) | |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(2A-2G) | - | CA\_n260(2A) | | CA\_n260(2G) | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-2G-O) | - | CA\_n260(2A) | | CA\_n260(2G) | | CA\_n260O |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(2A-2G-2O) | - | CA\_n260(2A) | | CA\_n260(2G) | | CA\_n260(2O) | | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(3A-2G) | - | CA\_n260(3A) | | | CA\_n260(2G) | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(4A-G) | - | CA\_n260(4A) | | | | CA\_n260G |  | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(4A-2G) | - | CA\_n260(4A) | | | | CA\_n260(2G) | | |  | |  | |  | |  | |  | |  | | 2000 | | 0 | |
| CA\_n260(A-2G-2O) | - | n260 | CA\_n260(2G) | | CA\_n260(2O) | |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-G-2O) | - | CA\_n260(2A) | | CA\_n260G | CA\_n260(2O) | |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(3A-G) | - | CA\_n260(3A) | | | CA\_n260G |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(A-2H) | - | n260 | CA\_n260(2H) | |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(2A-H) | - | CA\_n260(2A) | | CA\_n260H |  |  |  | |  | |  | |  | |  | |  | |  | | 1100 | | 0 | |
| CA\_n260(2A-2H) | - | CA\_n260(2A) | | CA\_n260(2H) | |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(A-H) | - | n260 | CA\_n260H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n260(A-O) | - | n260 | CA\_n260O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n260(A-O-P) | - | n260 | CA\_n260O | CA\_n260P |  |  |  | |  | |  | |  | |  | |  | |  | | 900 | | 0 | |
| CA\_n260(A-O-2P) | - | n260 | CA\_n260O | CA\_n260(2P) | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-O-P) | - | CA\_n260(2A) | | CA\_n260O | CA\_n260P |  |  | |  | |  | |  | |  | |  | |  | | 1300 | | 0 | |
| CA\_n260(2A-O-2P) | - | CA\_n260(2A) | | CA\_n260O | CA\_n260(2P) | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(2A-2O-P) | - | CA\_n260(2A) | | CA\_n260(2O) | | CA\_n260P |  | |  | |  | |  | |  | |  | |  | | 1500 | | 0 | |
| CA\_n260(A-O-Q) | - | n260 | CA\_n260O | CA\_n260Q |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(A-O-2Q) | - | n260 | CA\_n260O | CA\_n260(2Q) | |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(2A-O-Q) | - | CA\_n260(2A) | | CA\_n260O | CA\_n260Q |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(2A-O-2Q) | - | CA\_n260(2A) | | CA\_n260O | CA\_n260(2Q) | |  | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(2A-2O-Q) | - | CA\_n260(2A) | | CA\_n260(2O) | | CA\_n260Q |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(2A-O) | - | CA\_n260(2A) | | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(A-2O) | - | n260 | CA\_n260(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(A-2O-P) | - | n260 | CA\_n260(2O) | | CA\_n260P |  |  | |  | |  | |  | |  | |  | |  | | 1100 | | 0 | |
| CA\_n260(A-2O-2P) | - | n260 | CA\_n260(2O) | | CA\_n260(2P) | |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(A-2O-Q) | - | n260 | CA\_n260(2O) | | CA\_n260Q |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(A-2O-2Q) | - | n260 | CA\_n260(2O) | | CA\_n260(2Q) | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(2A-2O) | - | CA\_n260(2A) | | CA\_n260(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-2O-2P) | - | CA\_n260(2A) | | CA\_n260(2O) | | CA\_n260(2P) | | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(2A-2O-2Q) | - | CA\_n260(2A) | | CA\_n260(2O) | | CA\_n260(2Q) | | |  | |  | |  | |  | |  | |  | | 2000 | | 0 | |
| CA\_n260(2A-3O) | - | CA\_n260(2A) | | CA\_n260(3O) | | |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(3A-2O) | - | CA\_n260(3A) | | | CA\_n260(2O) | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(4A-O) | - | CA\_n260(4A) | | | | CA\_n260O |  | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(4A-3O) | - | CA\_n260(4A) | | | | CA\_n260(3O) |  | |  | |  | |  | |  | |  | |  | | 2200 | | 0 | |
| CA\_n260(5A-O) | - | CA\_n260(5A) | | | | | CA\_n260O | |  | |  | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(6A-O) | - | CA\_n260(6A) | | | | | | | CA\_n260O | |  | |  | |  | |  | |  | | 27002 | | 0 | |
| CA\_n260(7A-O) | - | CA\_n260(7A) | | | | | | | | | CA\_n260O | |  | |  | |  | |  | | 26502 | | 0 | |
| CA\_n260(8A-O) | - | CA\_n260(8A) | | | | | | | | | | | CA\_n260O | |  | |  | |  | | 26002 | | 0 | |
| CA\_n260(4A-2O) | - | CA\_n260(4A) | | | | CA\_n260(2O) | | |  | |  | |  | |  | |  | |  | | 2000 | | 0 | |
| CA\_n260(4A-2Q) | - | CA\_n260(4A) | | | | CA\_n260(2Q) | | |  | |  | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(3A-3O) | - | CA\_n260(3A) | | | CA\_n260(3O) | | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(A-G-O) | - | n260 | CA\_n260G | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(A-G-2O) | - | n260 | CA\_n260G | CA\_n260(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(2A-G-O) | - | CA\_n260(2A) | | CA\_n260G | CA\_n260O |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(A-2G-O) | - | n260 | CA\_n260(2G) | | CA\_n260O |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(A-3O) | - | n260 | CA\_n260(3O) | | |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(3A-O) | - | CA\_n260(3A) | | | CA\_n260O |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(3A-O-P) | CA\_n260O CA\_n260P | CA\_n260(3A) | | | CA\_n260O | CA\_n260P |  | |  | |  | |  | |  | |  | |  | | 1700 | | 0 | |
| CA\_n260(A-4O) | - | n260 | CA\_n260(4O) | | | |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-4O) | - | CA\_n260(2A) | | CA\_n260(4O) | | | | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(3A-4O) | - | CA\_n260(3A) | | | CA\_n260(4O) | | | | |  | |  | |  | |  | |  | | 2000 | | 0 | |
| CA\_n260(4A-4O) | - | CA\_n260(4A) | | | | CA\_n260(4O) | | | | | | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(5A-4O) | - | CA\_n260(5A) | | | | | CA\_n260(4O) | | | | | | | |  | |  | |  | | 26002 | | 0 | |
| CA\_n260(A-P) | - | n260 | CA\_n260P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n260(A-3P) | - | n260 | CA\_n260(3P) | | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(A-4P) | - | n260 | CA\_n260(4P) | | | |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(A-P-Q) | CA\_n260P CA\_n260Q | n260 | CA\_n260P | CA\_n260Q |  |  |  | |  | |  | |  | |  | |  | |  | | 1100 | | 0 | |
| CA\_n260(2A-P) | - | CA\_n260(2A) | | CA\_n260P |  |  |  | |  | |  | |  | |  | |  | |  | | 1100 | | 0 | |
| CA\_n260(3A-P) | - | CA\_n260(3A) | | | CA\_n260P |  |  | |  | |  | |  | |  | |  | |  | | 1300 | | 0 | |
| CA\_n260(4A-P) | - | CA\_n260(4A) | | | | CA\_n260P |  | |  | |  | |  | |  | |  | |  | | 1900 | | 0 | |
| CA\_n260(5A-P) | - | CA\_n260(5A) | | | | | CA\_n260P | |  | |  | |  | |  | |  | |  | | 2300 | | 0 | |
| CA\_n260(6A-P) | - | CA\_n260(6A) | | | | | | | CA\_n260P | |  | |  | |  | |  | |  | | 2700 | | 0 | |
| CA\_n260(A-2P) | - | n260 | CA\_n260(2P) | |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(2A-2P) | - | CA\_n260(2A) | | CA\_n260(2P) | |  |  | |  | |  | |  | |  | |  | |  | | 1400 | | 0 | |
| CA\_n260(2A-3P) | - | CA\_n260(2A) | | CA\_n260(3P) | | |  | |  | |  | |  | |  | |  | |  | | 1700 | | 0 | |
| CA\_n260(2A-4P) | - | CA\_n260(2A) | | CA\_n260(4P) | | | | |  | |  | |  | |  | |  | |  | | 2000 | | 0 | |
| CA\_n260(3A-2P) | - | CA\_n260(3A) | | | CA\_n260(2P) | |  | |  | |  | |  | |  | |  | |  | | 1800 | | 0 | |
| CA\_n260(4A-2P) | - | CA\_n260(4A) | | | | CA\_n260(2P) | | |  | |  | |  | |  | |  | |  | | 2200 | | 0 | |
| CA\_n260(5A-2P) | - | CA\_n260(5A) | | | | | CA\_n260(2P) | | | |  | |  | |  | |  | |  | | 2600 | | 0 | |
| CA\_n260(5A-2O) | - | CA\_n260(5A) | | | | | CA\_n260(2O) | | | |  | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(6A-2O) | - | CA\_n260(6A) | | | | | | | CA\_n260(2O) | | | |  | |  | |  | |  | | 24502 | | 0 | |
| CA\_n260(5A-3O) | - | CA\_n260(5A) | | | | | CA\_n260(3O) | | | | | |  | |  | |  | |  | | 2600 | | 0 | |
| CA\_n260(6A-3O) | - | CA\_n260(6A) | | | | | | | CA\_n260(3O) | | | | | |  | |  | |  | | 26002 | | 0 | |
| CA\_n260(7A-2O) | - | CA\_n260(7A) | | | | | | | | | CA\_n260(2O) | | | |  | |  | |  | | 25002 | | 0 | |
| CA\_n260(7A-3O) | - | CA\_n260(7A) | | | | | | | | | CA\_n260(3O) | | | | | |  | |  | | 25502 | | 0 | |
| CA\_n260(6A-2P) | - | CA\_n260(6A) | | | | | | | CA\_n260(2P) | | | |  | |  | |  | |  | | 26502 | | 0 | |
| CA\_n260(8A-2O) | - | CA\_n260(8A) | | | | | | | | | | | CA\_n260(2O) | | | |  | |  | | 25502 | | 0 | |
| CA\_n260(A-Q) | - | n260 | CA\_n260Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(A-2Q) | - | n260 | CA\_n260(2Q) | |  |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-Q) | - | CA\_n260(2A) | | CA\_n260Q |  |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(2A-2Q) | - | CA\_n260(2A) | | CA\_n260(2Q) | |  |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(3A-Q) | - | CA\_n260(3A) | | | CA\_n260Q |  |  | |  | |  | |  | |  | |  | |  | | 1600 | | 0 | |
| CA\_n260(3A-2Q) | - | CA\_n260(3A) | | | CA\_n260(2Q) | |  | |  | |  | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(4A-Q) | - | CA\_n260(4A) | | | | CA\_n260Q |  | |  | |  | |  | |  | |  | |  | | 2400 | | 0 | |
| CA\_n260(D-2G) | - | CA\_n260D | CA\_n260(2G) | |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(2D-O) | - | CA\_n260(2D) | | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(D-2O) | - | CA\_n260D | CA\_n260(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(A-I) | CA\_n260I | n260 | CA\_n260I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(D-G) | CA\_n260D CA\_n260G | CA\_n260D | CA\_n260G |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
|
| CA\_n260(D-H) | CA\_n260D CA\_n260H | CA\_n260D | CA\_n260H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
|
| CA\_n260(D-I) | CA\_n260D CA\_n260I | CA\_n260D | CA\_n260I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n260(D-O) | CA\_n260D CA\_n260O | CA\_n260D | CA\_n260O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
|
| CA\_n260(D-P) | CA\_n260D CA\_n260P | CA\_n260D | CA\_n260P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
|
| CA\_n260(D-Q) | CA\_n260D CA\_n260Q | CA\_n260D | CA\_n260Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n260(E-O) | CA\_n260E CA\_n260O | CA\_n260O | CA\_n260E |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n260(E-P) | CA\_n260E CA\_n260P | CA\_n260E | CA\_n260P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 8001 | | 0 | |
|
| CA\_n260(E-Q) | CA\_n260E CA\_n260Q | CA\_n260E | CA\_n260Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
|
| CA\_n260(G-H) | CA\_n260G | CA\_n260G | CA\_n260H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 500 | | 0 | |
| CA\_n260(G-I) | CA\_n260G CA\_n260I | CA\_n260G | CA\_n260I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
|
| CA\_n260(G-O) | - | CA\_n260G | CA\_n260O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 400 | | 0 | |
| CA\_n260(G-2O) | - | CA\_n260G | CA\_n260(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n260(2G-O) | - | CA\_n260(2G) | | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n260(2G-2O) | - | CA\_n260(2G) | | CA\_n260(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(G-3O) | - | CA\_n260G | CA\_n260(3O) | | |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(3G-O) | - | CA\_n260(3G) | | | CA\_n260O |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(2G-3O) | - | CA\_n260(2G) | | CA\_n260(3O) | | |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(G-4O) | - | CA\_n260G | CA\_n260(4O) | | | |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(2G-4O) | - | CA\_n260(2G) | | CA\_n260(4O) | | | | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(4G-O) | - | CA\_n260(4G) | | | | CA\_n260O |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(H-O) | - | CA\_n260H | CA\_n260O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 500 | | 0 | |
| CA\_n260(2H-O) | - | CA\_n260(2H) | | CA\_n260O |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(O-2P) | - | CA\_n260O | CA\_n260(2P) | |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(O-2Q) | - | CA\_n260O | CA\_n260(2Q) | |  |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(O-P) | - | CA\_n260O | CA\_n260P |  |  |  |  | | | |  | | | |  | | | |  | | 500 | | 0 | |
| CA\_n260(2O-P) | - | CA\_n260(2O) | | CA\_n260P | |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n260(2O-2P) | - | CA\_n260(2P) | | CA\_n260(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 1000 | | 0 | |
| CA\_n260(O-Q) | - | CA\_n260O | CA\_n260Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n260(2O-Q) | - | CA\_n260(2O) | | CA\_n260Q |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n260(2O-2Q) | - | CA\_n260(2O) | | CA\_n260(2Q) | |  |  | |  | |  | |  | |  | |  | |  | | 1200 | | 0 | |
| CA\_n260(P-Q) | - | CA\_n260P | CA\_n260Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n261(A-D) | - | n261 | CA\_n261D |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n261(A-2D) | - | n261 | CA\_n261(2D) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-D-H) | - | n261 | CA\_n261D | CA\_n261H |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-D-O) | - | n261 | CA\_n261D | CA\_n261O |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-D-2O) | - | n261 | CA\_n261D | CA\_n261(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-G) | - | n261 | CA\_n261G |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n261(A-G-H) | - | n261 | CA\_n261G | CA\_n261H |  |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-G-I) | - | n261 | CA\_n261G | n261I |  |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-G-O) | - | n261 | CA\_n261G | CA\_n261O |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-G-2O) | - | n261 | CA\_n261G | CA\_n261(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-2G-O) | - | n261 | CA\_n261(2G) | | CA\_n261O |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-2G-2O) | - | n261 | CA\_n261(2G) | | CA\_n261(2O) | |  | |  | |  | |  | |  | |  | |  | | 6501 | | 0 | |
| CA\_n261(A-3G) | - | n261 | CA\_n261(3G) | | | CA\_n261O |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-3G-O) | - | n261 | CA\_n261(3G) | | |  |  | |  | |  | |  | |  | |  | |  | | 6501 | | 0 | |
| CA\_n261(A-2G) | - | n261 | CA\_n261(2G) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | |  | |
| CA\_n261(A-4G) | - | n261 | CA\_n261(4G) | | | |  | |  | |  | |  | |  | |  | |  | | 6501 | | 0 | |
| CA\_n261(A-H) | - | n261 | CA\_n261H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n261(A-2H) | - | n261 | CA\_n261(2H) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-H-I) | - | n261 | CA\_n261H | CA\_n261I |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-I) | - | n261 | CA\_n261I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n261(A-2I) | - | n261 | CA\_n261(2I) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-J) | - | n261 | CA\_n261J |  |  |  |  | |  | |  | |  | |  | |  | |  | | 8001 | | 0 | |
| CA\_n261(A-K) | - | n261 | CA\_n261K |  |  |  |  | |  | |  | |  | |  | |  | |  | | 8001 | | 0 | |
| CA\_n261(A-O) | - | n261 | CA\_n261O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n261(A-2O) | - | n261 | CA\_n261(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-3O) | - | n261 | CA\_n261(3O) | | |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(A-4O) | - | n261 | CA\_n261(4O) | | | |  | |  | |  | |  | |  | |  | |  | | 6501 | | 0 | |
| CA\_n261(A-5O) | - | n261 | CA\_n261(5O) | | | | | |  | |  | |  | |  | |  | |  | | 6001 | | 0 | |
| CA\_n261(A-6O) | - | n261 | CA\_n261(6O) | | | | | | | |  | |  | |  | |  | |  | | 5501 | | 0 | |
| CA\_n261(A-7O) | - | n261 | CA\_n261(7O) | | | | | | | | | |  | |  | |  | |  | | 5001 | | 0 | |
| CA\_n261(A-P) | - | n261 | CA\_n261P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| CA\_n261(A-2P) | - | n261 | CA\_n261(2P) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(A-Q) | - | n261 | CA\_n261Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n261(A-2Q) | - | n261 | CA\_n261(2Q) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(2A-G) | - | CA\_n261(2A) | | CA\_n261G |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
| CA\_n261(2A-H) | - | CA\_n261(2A) | | CA\_n261H |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(2A-I) | - | CA\_n261(2A) | | CA\_n261I |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(3A-G) | - | CA\_n261(3A) | | | CA\_n261G |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(D-G) | CA\_n261D CA\_n261G | CA\_n261D | CA\_n261G |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
|
| CA\_n261(D-H) | CA\_n261D CA\_n261H | CA\_n261D | CA\_n261H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
|
| CA\_n261(D-I) | CA\_n261D CA\_n261I | CA\_n261D | CA\_n261I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n261(D-O) | CA\_n261D CA\_n261O | CA\_n261D | CA\_n261O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
|
| CA\_n261(D-2O) | - | CA\_n261D | CA\_n261(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 7501 | | 0 | |
| CA\_n261(D-P) | CA\_n261D CA\_n261P | CA\_n261D | CA\_n261P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
|
| CA\_n261(D-Q) | CA\_n261D CA\_n261Q | CA\_n261D | CA\_n261Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n261(E-O) | CA\_n261E CA\_n261O | CA\_n261E | CA\_n261O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 800 | | 0 | |
|
| CA\_n261(E-P) | CA\_n261E CA\_n261P | CA\_n261E | CA\_n261P |  |  |  |  | |  | |  | |  | |  | |  | |  | | 900 | | 0 | |
|
| CA\_n261(E-Q) | CA\_n261E CA\_n261Q | CA\_n261E | CA\_n261Q |  |  |  |  | |  | |  | |  | |  | |  | |  | | 8001 | | 0 | |
|
| CA\_n261(G-I) | - | CA\_n261G | CA\_n261I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n261(G-H) | - | CA\_n261G | CA\_n261H |  |  |  |  | |  | |  | |  | |  | |  | |  | | 500 | | 0 | |
| CA\_n261(2G-2O) | - | CA\_n261(2G) | | CA\_n261(2O) | |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(G-O) | - | CA\_n261G | CA\_n261O |  |  |  |  | |  | |  | |  | |  | |  | |  | | 400 | | 0 | |
| CA\_n261(G-2O) | - | CA\_n261G | CA\_n261(2O) | |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n261(2G-O) | - | CA\_n261(2G) | | CA\_n261O |  |  |  | |  | |  | |  | |  | |  | |  | | 600 | | 0 | |
| CA\_n261(3G-O) | - | CA\_n261(3G) | | | CA\_n261O |  |  | |  | |  | |  | |  | |  | |  | | 7001 | | 0 | |
| CA\_n261(H-I) | - | CA\_n261H | CA\_n261I |  |  |  |  | |  | |  | |  | |  | |  | |  | | 700 | | 0 | |
| NOTE 1: Void  NOTE 2: Void  NOTE 3: Channel bandwidth per operating band defined in Table 5.3.5-1  NOTE 4: Configurations for intra-band contiguous CA defined in Table 5.5A.1-1  NOTE 5: Configurations for intra-band non-contiguous CA defined in Table 5.5A.2-1  NOTE 6: Void  NOTE 7: Unless otherwise stated, BCS0 is referred in each constituent CA configuration | | | | | | | | | | | | | | | | | | | | | | | | |

## **<< End of changes >>**