**3GPP TSG-RAN WG4 Meeting # 95-e R4-2007605**

**Electronic Meeting, 25 May – 5 June, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **DRAFT CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** | **0360** | **rev** |  | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to add NR intra-band FR1 in TS 38.101-1 |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CA\_R16\_intra-Core |  | ***Date:*** | 2020-06-09 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Adding approved NR Intra-band FR1 combinations |
|  |  |
| ***Summary of change:*** | Approved NR Intra-band FR1 combinations at RAN4 94bis-e:CA\_n41B\_UL\_n41BCA\_n48(3A)CA\_n48(4A)CA\_n71B BCS1Approved NR Intra-band FR1 combinations at RAN4 95:CA\_n79C\_UL\_n79CCorrections:CA\_n48(2A) configurationCorrection of table header for Table 5.3.5-1Adding missing space after comma in channel BW tables |
|  |  |
| ***Consequences if not approved:*** | Approved NR Intra-band FR1 combinations are not added |
|  |  |
| ***Clauses affected:*** | 5.3, 5.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521 series |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

Table 5.3.5-1 Channel bandwidths for each NR band

|  |  |  |
| --- | --- | --- |
| NR band / SCS / UE Channel bandwidth |
| NR Band | SCSkHz | 5 MHz | 10 MHz | 15 MHz | 20MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70 MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n2 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n3 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n5 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n8 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n26 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n28 | 15 | Yes | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n38 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n39 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n40 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| n41 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n48 | 15 | Yes5 | Yes | Yes | Yes |  |  | Yes | Yes6 |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| 60 |  | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| n50 | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| n51 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n53 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n66 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n70 | 15 | Yes | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| n71 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n75 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n76 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| n78 | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| n79 | 15 |  |  |  |  |  |  | Yes | Yes |  |  |  |  |  |
| 30 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| n80 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n81 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n82 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n83 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n84 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n86 | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n89 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n90 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n91 | 15 | Yes | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | Yes | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n95 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: Void.NOTE 2: Void.NOTE 3: This UE channel bandwidth is applicable only to downlink.NOTE 4: This UE channel bandwidth is optional in this release of the specification.NOTE 5: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.NOTE 6: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration.NOTE 7: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.NOTE 8: This UE channel bandwidth is applicable only to uplink. |

---Text omitted---

Table 5.5A.1-1: NR CA configurations and bandwidth combination sets defined for intra-band contiguous CA

|  |
| --- |
| NR CA configuration / Bandwidth combination set |
| NR CA configuration | Uplink CA configurations | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Channel bandwidths for carrier (MHz) | Maximum aggregated bandwidth (MHz) | Bandwidth combination set |
| CA\_n1B | - | 10 | 10, 15 |  |  |  | 40 | 0 |
| 15 | 15, 20 |  |  |  |
| 20 | 20 |  |  |  |
| CA\_n7B | CA\_n7B | 10, 15, 20 | 10, 15, 20, 30, 35, 40 |  |  |  | 50 | 0 |
| CA\_n40B | - | 20 | 80 |  |  |  | 100 | 0 |
| 50 | 50 |  |  |  |
| CA\_n41B | CA\_n41B | 10, 20, 30, 40, 50 | 10, 20, 30, 40, 50 |  |  |  | 100 | 0 |
| CA\_n41C | - | 40 | 80, 100 |  |  |  | 180 | 0 |
| 50, 60, 80 | 60, 80, 100 |  |  |  |
| 10, 15, 20, 40, 50, 60, 80, 90 | 15, 20, 40, 50, 60, 80, 90, 100 |  |  |  | 190 | 1 |
| CA\_n48B | CA\_n48B | 5, 10 | 10, 15, 20 |  |  |  | 40 | 0 |
| 15, 20 | 5, 10, 15, 20 |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| - | 10 | 50, 60, 80, 90 |  |  |  | 100 | 1 |
| 15, 20 | 40, 50, 60, 80 |  |  |  |
| 40 | 40, 50, 60 |  |  |  |
| 50 | 50 |  |  |  |
| CA\_n48C | - | 10, 15 | 90, 100 |  |  |  | 150 | 0 |
| 20 | 80, 90, 100 |  |  |  |
| 40 | 60, 80, 90, 100 |  |  |  |
| 50 | 50, 60, 80, 90, 100 |  |  |  |
| 60 | 40, 50, 60, 80, 90 |  |  |  |
| 80 | 20, 40, 50, 60 |  |  |  |
| 90 | 10, 15, 20, 40, 50, 60 |  |  |  |
| 100 | 10, 15, 20, 40, 50 |  |  |  |
| CA\_n66B | - | 5 1 | 20, 40 |  |  |  | 50 | 0 |
| 10 | 15, 20, 40 |  |  |  |
| 15 | 10, 15, 20 |  |  |  |
| 20 | 5 1, 10, 15 |  |  |  |
| 40 | 5 1, 10 |  |  |  |
| CA\_n71B | - | 5 | 20 |  |  |  | 25 | 0 |
| 10 | 15 |  |  |  |
| 15 | 10 |  |  |  |
| 20 | 5 |  |  |  |
| 10 | 20 |  |  |  | 35 | 1 |
| 15 | 15, 20 |  |  |  |
| 20 | 10, 15 |  |  |  |
| CA\_n77C | - | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
| 60 | 60, 80, 100 |  |  |  |
| 80 | 80, 100 |  |  |  |
| 100 | 100 |  |  |  |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  |  | 200 | 1 |
| CA\_n78C | - | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
| 60 | 60, 80, 100 |  |  |  |
| 80 | 80, 100 |  |  |  |
| 100 | 100 |  |  |  |
| 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 | 10, 15, 20, 25, 30, 40, 50, 60, 70, 80, 90, 100 |  |  |  | 200 | 1 |
| CA\_n78B | - | 20 | 50 |  |  |  | 70 | 0 |
| CA\_n77DCA\_n78DCA\_n79D | - | 100 | 100 | 100 |  |  | 300 | 0 |
| CA\_n79C | CA\_n79C | 50 | 60, 80, 100 |  |  |  | 200 | 0 |
| 60 | 60, 80, 100 |  |  |  |
| 80 | 80, 100 |  |  |  |
| 100 | 100 |  |  |  |
| NOTE 1: 5 MHz is not applicable for 30/60 kHz SCS. |

Table 5.5A.1-2: Void

### 5.5A.2 Configurations for intra-band non-contiguous CA

Table 5.5A.2-1: NR CA configurations and bandwidth combination sets defined for intra-band non-contiguous CA

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NR CA Configuration | Uplink Configurations | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | Channel bandwidths for carrier(MHz) | MaximumAggregated bandwidth(MHz) | Bandwidth combination set |
| CA\_n3(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n7(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n25(2A) | - | 5, 10, 15, 20 | 5, 10, 15, 20 |  |  | 40 | 0 |
| CA\_n41(2A) | - | 40, 50, 60, 80, 100 | 40, 50, 60, 80, 100 |  |  | 180 | 0 |
| 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 190 | 1 |
| CA\_n48(2A) | - |  |  |  |  |  | 0 |
| 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 |  |  | 1402 |
| CA\_n48(3A) | - | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 | 10, 15, 20, 40,50, 60, 80, 90, 100 |  | 1402 | 0 |
| CA\_n48(4A) | - | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 10, 15, 20, 40, 50, 60, 80, 90, 100 | 1352 | 0 |
| CA\_n66(2A) | - | 5, 10, 15, 20, 40 | 5, 10, 15, 20, 40 |  |  | 60 | 0 |
| CA\_n77(2A) | - | 20, 40, 80, 100 | 20, 40, 80, 100 |  |  | 200 | 0 |
| CA\_n78(2A) | - | 10, 20, 40, 50, 60, 80, 90, 100 | 10, 20, 40, 50, 60, 80, 90, 100 |  |  | 200 | 0 |
| 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 | 10, 20, 25, 30, 40, 50, 60, 80, 90, 100 |  |  | 200 | 1 |
| NOTE 1: Void.NOTE 2: Parameter value accounts for both, the maximum frequency range of band n48 (150 MHz), and the minimum frequency gaps in between NR non-contiguous component carriers. |

---End of changes---