**3GPP TSG-RAN WG4 Meeting #** **95-eR4-2008722**

**Electronic Meeting, 25 May – 5 June, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.124** | **CR** | **0019** | **rev** | **1** | **Current version:** | **15.2.0** |  |
|  |
| *For* ***[HELP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.124: Electrostatic discharge requirements, Rel-15 |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-05-15 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | There is no electrostatic discharge requirements for UE. |
|  |  |
| ***Summary of change:*** | Add electrostatic discharge test requirements . |
|  |  |
| ***Consequences if not approved:*** | Electrostatic discharge test requirements missing.  |
|  |  |
| ***Clauses affected:*** | 9.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

**--------------Start of text change-------------**

## 9.3 Electrostatic discharge

### 9.3.0 General

The test shall be performed on a representative configuration of the equipment or a representative configuration of the combination of UE and ancillary equipment.

### 9.3.1 Definition

This test assesses the ability of UE and ancillary equipment to operate as intended in the event of an electrostatic discharge.

### 9.3.2 Test method and level

The test method shall be in accordance with IEC 61000‑4‑2 [11]:

- for contact discharge, the equipment shall pass at ±2 kV and ±4 kV;

- for air discharge the equipment shall pass at ±2 kV, ±4 kV and ±8 kV (only for non-conducting surfaces, see IEC 61000‑4‑2 [11]).

NOTE: The EUT shall be fully discharged between each ESD exposure by connecting its ground point (where applicable) to the HCP by a resistive wire with a 470 kΩ. resistor in either end.

### 9.3.3 Performance criteria

The performance criteria of clause 6.2 shall apply.

**-------------End of change-------------**