TSG-RAN Working Group 4 (Radio) meeting #95-ER4-2008786

Electronic Meeting, May25th – June 5 th 2020

**Source:** Ericsson

**Title:** WF on IAB-MT In-band selectivity and blocking

**Agenda item:** 6.5.2.2.2

**Document for:** Approval

# Introduction

At RAN4#94-E meeting a way-forward for IAB-MT In-Band Blocking and blocking was created based on the discussion [1].

# Way-Forward

There is strong dependency on this WF and the WF on REFSENS, so right now, there are three options :

Option 1: If only OTA sensitivity is defined for 1-O, only EISminSENS will be used for ACS and IBB

Option 2: If only OTA REFSENS is defined for 1-O, , Only EIS\_REFSENS will be used for ACS and IBB

Option 3: If both OTA REFSENS and OTA sensitivity are defined for 1-O, both EIS\_minSENS and EIS\_REFSENS will be used for IBB, but only both EIS\_minSENS is used for ACS, this is the same as BS ACS type 1-O

This WF takes consideration of the WF on REFSENS and lists the options that could be make later when REFSENS is agreed on IAB-MT type 1-O. This will apply both WA IAB-MT and LA IAB-MT.

The Below WF options for IAB-MT Type 1-O will be decided according to above options once WF of REFSENS is agreed.

1. ACS and IBB of FR1 WA IAB-MT Type 1-H:

|  |  |  |  |
| --- | --- | --- | --- |
| WA IAB-MT | Wanted signal level[dBm] | Interference signal level [dBm] | **Interference signal bandwidth and offset** |
| ACS(45dB) | REFSENS+6dB | -52 | CP-OFDM, others the same with BS spec |
| In-band blocking  | REFSENS+6dB | -43 | CP-OFDM, others the same with BS spec |

1. ACS of FR1 WA IAB-MT Type 1-O:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| WA IAB-MT |  | Wanted signal level[dBm] | Interference signal level [dBm] | Interference signal bandwidth and offset |
| ACS(45dB) | Option 1 | EISminSENS +6dB | -52 – ΔminSENS | CP-OFDM, others the same with BS spec |
| Option 2 | EISREFSENS +6dB |  -52 - ΔOTAREFSENS |
| Option 3 | EISminSENS +6dB | -52 – ΔminSENS |

1. IBB of FR1 WA IAB-MT Type 1-O:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| WA IAB-MT |  | Wanted signal level[dBm] | Interference signal level [dBm] | Interference signal bandwidth and offset |
| In-band blocking  | Option 1 | EISREFSENS +6dB | -43 - ΔOTAREFSENS | CP-OFDM, others the same with BS spec |
| Option 2 |  EISminSENS + 6 dB | -43 – ΔminSENS |
| Option 3 | EISREFSENS +6dB | -43 - ΔOTAREFSENS |
|  EISminSENS + 6 dB | -43 – ΔminSENS |

1. FR1 LA IAB-MT Type 1-H with below candidate options

|  |  |  |
| --- | --- | --- |
| LA IAB-MT | Wanted signal level[dBm] | Interference signal level [dBm] |
| Option 1: ACS 33dB | ACS | REFSENS+14dB | Case: [-45.5]Necessity on case 2 is FFS since the dynamic range for FR1 IAB-MT is open too.  |
| In-band blocking  | REFSENS+6dB | Case 1:-56Case 2:-44 |
| Option 2: ACS 45dB | ACS(45dB) | REFSENS+6dB | -44 |
| In-band blocking  | REFSENS+6dB | -35 |

Note: in option 1 for LA IAB-MT is based on the NF of 9/10dB, if the NF is agreed as 13dB the interference level should be adjusted accordingly.

1. ACS of FR1 LA IAB-MT Type 1-O:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| WA IAB-MT |  | Wanted signal level[dBm] | Interference signal level [dBm] | Interference signal bandwidth and offset |
| ACS(45dB) | Option 1 | EISminSENS +6dB | -44 – ΔminSENS | CP-OFDM, others the same with BS spec |
| Option 2 | EISREFSENS +6dB | -44 - ΔOTAREFSENS |
| Option 3 | EISminSENS +6dB | -44 – ΔminSENS |

1. IBB of FR1 LA IAB-MT Type 1-O:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| WA IAB-MT |  | Wanted signal level[dBm] | Interference signal level [dBm] | Interference signal bandwidth and offset |
| In-band blocking  | Option 1 | EISREFSENS +6dB |  -35 - ΔOTAREFSENS | CP-OFDM, others the same with BS spec |
| Option 2 |  EISminSENS + 6 dB | -35 – ΔminSENS |
| Option 3 | EISREFSENS +6dB |  -35 - ΔOTAREFSENS |
|  EISminSENS + 6 dB | -35 – ΔminSENS |

# References

[1] R4-2008699, Email discussion summary for [95e][310] NR\_IAB\_RF\_Part\_3, Samsung