**3GPP TSG-RAN WG4 Meeting #95-e *R4-2008751***

**Electronic Meeting, 25 May – 5 June, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | 0051 | **rev** | **1** | **Current version:** | **15.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR: Clarification on EPRE ratio for DL channel signal |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Perf |  | ***Date:*** | 2020-04-10 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The definition of EPRE power ratio for downlink physical channels or reference signals are unclear due to the pre-coding or beamforming. |
|  |  |
| ***Summary of change:*** | Add the clarification to make the definition of EPRE power ratio clear. |
|  |  |
| ***Consequences if not approved:*** | Ambiguous specifications. |
|  |  |
| ***Clauses affected:*** | Annex C |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.521-4 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<< Start of change >>

Annex C (normative):
Downlink physical channels

C.1 General

This annex specifies the downlink physical channels that are needed for setting a connection and channels that are needed during a connection.

C.2 Setup (Conducted)

Table C.2-1 describes the downlink Physical Channels that are required for connection set up.

**Table C.2-1: Downlink Physical Channels required for connection set-up**

|  |
| --- |
| **Physical Channel** |
| PBCH |
| SSS  |
| PSS |
| PDCCH |
| PDSCH |
| PBCH DMRS |
| PDCCH DMRS |
| PDSCH DMRS |
| CSI-RS  |

C.3 Connection (Conducted)

The following clauses, describes the downlink Physical Channels that are transmitted during a connection i.e., when measurements are done.

C.3.1 Measurement of Performance requirements

*<Editor*'*s note: OCNG for DMRS is FFS in Annex A.>*

Table C.3.1-1 is applicable for measurements in which uniform RS-to-EPRE boosting for all downlink physical channels, unless otherwise stated.**Table C.3.1-1: Downlink Physical Channels transmitted during a connection (FDD and TDD)**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value (Note 2)** |
| SSS transmit power  | W | Test specific |
| EPRE ratio of PSS to SSS | dB | 0 |
| EPRE ratio of PBCH to SSS | dB | 0 |
| EPRE ratio of PBCH to PBCH DMRS | dB | 0 |
| EPRE ratio of PDCCH to SSS | dB | 0 |
| EPRE ratio of PDCCH to PDCCH DMRS | dB | 0 |
| EPRE ratio of PDSCH to SSS | dB | 0 |
| EPRE ratio of PDSCH to PDSCH DMRS | dB | Test specific (Note 1) |
| EPRE ratio of NZP CSI-RS to SSS | dB | -10\*log(L) (Note 3) |
| EPRE ratio of PDSCH OCNG to SSS | dB | 0 |
| EPRE ratio of PDCCH OCNG to SSS | dB | 0 |
| Note 1: Value is derived from Table 4.1-1 in TS 38.214 [12] based on "Number of DM-RS CDM groups without data" and "DMRS Type" parameters specified for each testNote 2: The value is the energy of per RE for a single antenna port before pre-coding.Note 3:  is the CDM group size of NZP CSI-RS specified for each test. |

C.4 Setup (Radiated)

Table C.4-1 describes the downlink Physical Channels that are required for connection set up.

**Table C.4-1: Downlink Physical Channels required for connection set-up**

|  |
| --- |
| **Physical Channel** |
| PBCH |
| SSS  |
| PSS |
| PDCCH |
| PDSCH |
| PBCH DMRS |
| PDCCH DMRS |
| PDSCH DMRS |
| CSI-RS  |
| PTRS |

C.5 Connection (Radiated)

The following clauses, describes the downlink Physical Channels that are transmitted during a connection i.e., when measurements are done.

C.5.1 Measurement of Receiver Characteristics

*<Editor*'*s note: OCNG for DMRS is FFS in Annex A.>*

Table C.5.1-1 is applicable for measurements in which uniform RS-to-EPRE boosting for all downlink physical channels, unless otherwise stated.

**Table C.5.1-1: Downlink Physical Channels transmitted during a connection (TDD)**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value (Note 2)** |
| SSS transmit power  | W | Test specific |
| EPRE ratio of PSS to SSS | dB | 0 |
| EPRE ratio of PBCH to SSS | dB | 0 |
| EPRE ratio of PBCH to PBCH DMRS | dB | 0 |
| EPRE ratio of PDCCH to SSS | dB | 0 |
| EPRE ratio of PDCCH to PDCCH DMRS | dB | 0 |
| EPRE ratio of PDSCH to SSS | dB | 0 |
| EPRE ratio of PDSCH to PDSCH DMRS | dB | Test specific (Note 1) |
| EPRE ratio of NZP CSI-RS to SSS | dB | -10\*log(L) (Note 3) |
| EPRE ratio of PTRS to PDSCH | dB | Test specific (Note 4) |
| EPRE ratio of PDSCH OCNG to SSS | dB | 0 |
| EPRE ratio of PDCCH OCNG to SSS | dB | 0 |
| Note 1: Value is derived from Table 4.1-1 in TS 38.214 [12] based on "Number of DM-RS CDM groups without data" and "DMRS Type" parameters specified for each testNote 2: The value is the energy of per RE for a single antenna port before pre-coding.Note 3:  is the CDM group size of NZP CSI-RS specified for each test.Note 4: Value is derived from Table 4.1-2 in TS 38.214 [12] based on “The number of PDSCH layers” and “*epre-Ratio*” parameters specified for each test. |

<< End of change >>