**3GPP TSG-RAN WG4 Meeting # 95-e draftR4-2008711**

**Electronic Meeting, 25 May - 5 June, 2020**

**Agenda item:** 6.17.2.2

**Source:** Moderator (Nokia, Nokia Shanghai Bell)

**Title:** Email discussion summary for [95e][322] NR\_HST\_Demod\_BS

**Document for:** Information

# Introduction

*Briefly introduce background, the scope of this email discussion and provide some guidelines for email discussion if necessary.*

*List of candidate target of email discussion for 1st round and 2nd round*

* 1st round: TBA
* 2nd round: TBA

## Background and scope

This T-doc will be used to guide and summarize the email discussion for the topic of Rel-16 NR HST BS demodulation requirements (AI 6.17.2.2), with the email thread identifier “[95e][322] NR\_HST\_Demod\_BS”.

The scope of this email discussion are Rel-16 NR HST BS demodulation requirements, and in particular the agenda items:

6.17.2.2 BS demodulation requirements (38.104)

6.17.2.2.1 PUSCH requirements

6.17.2.2.2 PRACH requirements

6.17.2.2.3 UL timing adjustment requirements

In general, the 1st round of the email discussion mainly aims to collect the companies’ views on the open issues, while the 2nd round aims achieve consensus on remaining controversial issues.

In addition to this general split between round 1 and round 2, we aim to focus the following candidate targets:

List of candidate targets of email discussion for 1st week and 2nd week

* 1st week:
  + Collect (updated) company views on all topics.
  + Give feedback on Moderator proposed agreements.
  + Align on ITU submission related specification cleaning way forward. See sub-topic 1-6.
  + PUSCH
    - Reach agreement on DFT-s-OFDM and manufacturer declaration.
  + PRACH
    - Decide if previous agreements need to be revisited and agree on manufacturer declaration.
  + UL TA
    - Reach agreement on scenario “X”, addition CBW/SCS, and progress on manufacturer declarations.
* 2nd week:
  + TBA.

## Email discussion guidelines

Unless different guidance is received from the session chairs, the moderator would like to ask companies to adhere to the following guidelines, when taking part in [95e][322] NR\_HST\_Demod\_BS.

Please also check the “RAN4#95-e E-meeting Arrangements and Guidelines”, available on the reflector, for fundamental guidelines and deadlines.

The preferred method of commenting is to add/update your company’s view directly in this email summary document (use change marks if appropriate) and upload it to the [95e][322] NR\_HST\_Demod\_BS.

* Draft folder:   
   [322](ftp://3gpp.org/tsg_ran/WG4_Radio/TSGR4_95_e/Inbox/Drafts/322/)  
  ftp://3gpp.org/tsg\_ran/WG4\_Radio/TSGR4\_95\_e/Inbox/Drafts/322/
* It is expected delegates will download the latest version (including other companies’ versions) of the summary document, insert comments and upload it again.  
  To ensure the comments are captured timely and correctly, delegates are encouraged to:
  + Rename the file by adding your company name.  
    Example: “Summary\_322\_1st round Rev**1\_CATT\_Nok**.docx”
  + Send an email on the reflector informing that comments are made with new correct file name.
  + Please check for possibly updated base document versions, right before uploading your updates.
* Company views can be updated, e.g., based on comments from other companies
  + The revised comments should be easy to identify, for example, by marking them as “after seeing comments from …/ or intermediate proposal, our position/comment now is …”, while the initial comments remain unchanged in the template file.
  + Asking direct questions to other companies is possible in their views, but often overlooked in the first round/week.
* Please do not hesitate to mark your company as supporting a certain option directly in this document.  
  Please refrain from rewriting existing options and proposed WFs; ask the moderator to modify/add.
* It is encouraged to give a short reasoning for each view expressed (1-2 sentences are recommended).  
  Please avoid statements like “Option X”, without further explication or reasoning.
* Moderator is trying to provide a new “cleaned” revision of the base document once a day.   
  Example: “Summary\_322\_1st round Rev**2**.docx”
  + Comments only received by email will merged into the summary document by the moderator on a best effort basis.

# Topic #1: PUSCH requirements (6.17.2.2.1)

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

This section contains T-docs with corresponding proposals and observations submitted to the agenda item “6.17.2.2.1 PUSCH requirements”, as well as, any PUSCH requirement related observations and proposals submitted to other agenda items.

## Companies’ contributions summary

Ordering: 1st by agenda item, 2nd by Tdoc number.

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-20xxxxx | Company A | Proposal 1:  Observation 1: |
| R4-2006254 (AI 6.17.2.2) | CATT | Moderator: Simulation summary. |
| R4-2006266 | CATT | PUSCH high speed support declaration  **Proposal 1: To avoid the test redundancy and align with implicit test passing, it is proposed to declare category of supported maximum speed (Option 1).**   * + Option 1:  Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Which tests need to be passed, if 500kph is declared, is discussed separately under “High speed implicit test passing” |
| R4-2006267 | CATT | PUSCH multi-path fading channel model  Observation: Multi-path fading channel is very rare in HST scenarios (open area or tunnel) (Option 1).  **Proposal 1: Do not specify requirements for multi-path fading channel models with high Doppler values (Option 1).**   * Option 1: Do not specify requirements for multi-path fading channel models with high Doppler values. |
| R4-2006270 | CATT | Moderator: CR TS 38.141-1  PUSCH manufacturer declaration   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | x | x | |
| R4-2006271 | CATT | Moderator: CR TS 38.141-2  PUSCH manufacturer declaration   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | D.109 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | c | x | n/a | |
| R4-2006769 | CMCC | Multi-path fading channel under high Doppler value  **Proposal 1: it is proposed to specify PUSCH requirements for multi-path fading channel with maximum doppler shift of 600Hz and 1200Hz for 15kHz SCS and 30kHz SCS, respectively.** |
| R4-2006052 (AI 6.17.2.2.1) | Nokia, Nokia Shanghai Bell | PUSCH implicit test passing applicability rule  **Proposal 1: RAN4 to capture the following applicability rule in test specifications: “Unless otherwise stated, a BS that declares to support 500kph (see D.XXX in table 4.6-1), and passes the tests for 500kph, can also consider the tests for 350kph as passed.”**  PUSCH high speed support declaration for HST  Observation 1: There are algorithmic differences between a BS deployed in “500kph only” scenarios and “350/500kph mixed” scenarios.  **Proposal 2: RAN4 to allow the distinction between “500kph only” scenarios and “350/500kph mixed” scenarios in manufacturer declarations.**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.10X | PUSCH high speed train supported target speeds | Declaration of the supported high speed train target speeds, i.e., not declared (no high speed train support), 350km/h, 500km/h, or 350km/h and 500km/h. | x | x |   1T1R requirements for the tunnel scenario - Applicability rule  **Proposal 3: RAN4 to allow foregoing testing for 1T1R, when 1T2R is tested. This to be captured in applicability rule by changing previous rule as follows: “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”**  1T1R requirements for the tunnel scenario - Configuration  **Proposal 4: RAN4 to have requirements for both MCS2 and MCS16.**  DFT-s-OFDM waveform  Observation 2: In high speed 70%TPUT requirements, dft-s-OFDM improves coverage by less than 0.4dB in MCS2 and loses coverage (within simulation uncertainty) for MCS16.  **Proposal 5: RAN4 to not add dft-s-OFDM to minimum requirements, since coverage of re-farming LTE bands is not impacted.**  Multi-path fading channel under high Doppler value  Observation 3: The highest proposed value (2400Hz) corresponds to 650kph@2.1GHz or 375kph@3.6GHz, which does not correspond to any categories considered up until now. Neither does the proposed lower value of 1200Hz.  **Proposal 6: RAN4 to not consider multi-path fading channels under high Doppler value. The minimum test coverage is already achieved and senseful Doppler values would require extensive further studies.**  Agreeing on SNR values  **Proposal 7: Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the PUSCH CRs.**  HST test setup figures and TTS  Observation 4: RAN4 should verify, if further HST PUSCH additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272. |
| R4-2006053 | Nokia, Nokia Shanghai Bell | Moderator: CR TS 38.104 |
| R4-2006054 | Nokia, Nokia Shanghai Bell | Moderator: CR TS 38.104 |
| R4-2006258 | CATT | Moderator: Simulation results  PUSCH Additional SCS/CBW  **Proposal 1: add 5MHz CBW/15kHz SCS, 10MHz CBW/30kHz SCS for PUSCH to simulation results summary.** |
| R4-2006265 | CATT | 1T1R for tunnel scenario for NR HST PUSCH  **Proposal 1: The tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors. (Option 4)**   * Option 4: Define test applicability rule in the section 8.1.2.0 of TS 38.141-1 as:   + “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”   **Proposal 2: If 1T1R requirement is introduced, only have MCS 2 requirements (Option 1).**   * Option 1: If 1T1R requirement is introduced, only have MCS 2 requirements. |
| R4-2006268 | CATT | DFT-s-OFDM for NR HST PUSCH  **Proposal 1: Do not introduce PUSCH HST requirements for DFT-s-OFDM (Option 2).** |
| R4-2006323 | Samsung | 1T1R requirements for the tunnel scenario  **Proposal 1: only MCS 2 requirement is preferred to introduce for 1T1R requirement.**  Test applicability rule for 1T1R requirement  **Proposal 2: Define test applicability rule in the section 8.1.2.0 of TS 38.141-1 as: “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”**  Other requirements - DFT-s-OFDM  **Proposal 3: No HST PUSCH requirement with DFT-s-OFDM waveform.**  **Proposal 4: If agreed to introduce HST PUSCH requirement with DFT-s-OFDM waveform, only 500kph requirement is preferred to introduce.**  Other requirements - fading channel environment  **Proposal 5: If agreed to introduce the related requirement, the high Doppler with 600Hz and 1200Hz for 15 KHz and 30 KHz SCS can be regarded as the starting point for the feasibility study with HST requirement with high Doppler**  Initial results for fading channel  Observation 1: The fading channel with high Doppler 600Hz is feasible for MCS2 with configured 3 DMRS symbols.  Observation 2: The performance of MCS 16 under fading channel with large Doppler value suffers large degradation as Doppler increasing.  Observation 3: PUSCH with CP-OFDM waveform and DFT-s-OFDM waveform under fading channel high Doppler value have the similar results.  **Proposal 6: If agreed to introduce PUSCH requirement with multi-path fading under high Doppler value, focus on the requirements with CP-OFDM waveform.** |
| R4-2006666 | ZTE Wistron Telecom AB | Manufacturer declaration maximum supported speed for HST  **Proposal 1:** **Introduce a new declaration item (Option 1) shown in Table -1.**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x |     DFT-s-OFDM  **Proposal 2: Focus on completion of Rel-16 performance requirements at this stage and do not introduce DFT-s-OFDM requirements for HST PUSCH (Option 2).**  Multi-path fading channel under high Doppler value  **Proposal 3: Multi-path fading in high speed train may lead to non-coherence within the same slot, therefore support of HST scenarios requires a non-multi-path fading deployment, and no requirement should be introduced for multi-path fading channel under high Doppler value (Option 1).** |
| R4-2006833 | Ericsson | High speed support declaration for HST PUSCH  **Proposal 1:** **Declare category of supported maximum speed. This can be either 350km/h or 500km/h. Only the corresponding requirements are tested.**  If 1T1R requirements is introduced: MCS configuration  **Proposal 2: Agree with Option 2 that introduce MCS2 and MCS16 requirements for 1T1R.**  DFT-s-OFDM waveform  **Proposal 3: Do not introduce DFT-s-OFDM requirements for HST scenarios.**  Multi-path fading channel under high Doppler value  **Proposal 4: Do not introduce multi-path fading channel under high Doppler shift requirements to HST scenario.** |
| R4-2006836 | Ericsson | Moderator: CR TS 38.141-2 |
| R4-2006837 | Ericsson | Moderator: CR TS 38.141-2 |
| R4-2007182 | NTT DOCOMO, INC. | Declaration and applicability  **Proposal 1: Allow to declare category of supported design target speed(s) from “no HST”, “HST for 350km/h”, “HST for 500km/h” or “HST for both 350km/h and 500km/h” and introduce the following declaration:**   | Declaration identifier | Declaration | Description | Applicability | | | | --- | --- | --- | --- | --- | --- | | *BS type 1-C* | *BS type 1-H* | *BS type 1-O* | | D.1xx | PUSCH for HST | Declaration of the supported HST scenarios: no HST, HST for 350km/h, HST for 500km/h or HST for both 350km/h and 500km/h. | x | x | x |     Requirement for 1T1R  **Proposal 2: Define test applicability rule in the section 8.1.2.0 of TS 38.141-1 as below:  “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”**  **Proposal 3: Define MCS 2 and MCS16 requirements for 1T1R.**  Requirement for DFT-s-OFDM  **Proposal 4: Introduce PUSCH HST requirements for DFT-s-OFDM.**  **Proposal 5: The following configuration and applicability rule for DFT-s-OFDM are considered.  Antenna configuration: Only 1T2R  MCS: Only MCS2  CBW and SCS: Only 5MHz CBW/15kHz SCS and 10MHz CBW/ 30kHz SCS  Velocity: Only 350km/h  Applicability rule:   If BS that declare to support HST for DFT-s-OFDM, BS vendor can chose either DFT-s-OFDM or CP-OFDM for the test with 1T2R, MCS2, 5MHz CBW/15kHz SCS or 10MHz CBW/30kHz SCS and 350km/h HST scenarios. (The number of tests is kept)**  Requirement for Multi-path fading scenario  Observation 1: In NR UE HST, it was agreed to introduce PDSCH performance requirements for multi-path fading condition with 600Hz and 1200Hz Doppler frequency for 15kHz and 30kHz SCS, respectively.  Observation 2: In LTE HST, it was agreed to introduce multi-path fading channel as one of the high speed scenarios and to define ETU600 for PDSCH/PUSCH.  **Proposal 6: Multi-path fading is a typical HST scenario.**  **Proposal 7: Introduce PUSCH for multipath fading scenarios with Doppler frequency 600Hz for 15 kHz SCS and 1200Hz for 30 kHz SCS**  **Proposal 8: Introduce new PUSCH requirements for multi-path fading conditions in non-HST PUSCH section.** |
| R4-2007183 | NTT DOCOMO, INC. | Moderator: CR TS 38.141-1 |
| R4-2007184 | NTT DOCOMO, INC. | Moderator: CR TS 38.141-1 |
| R4-2007231 | Huawei, HiSilicon | Applicability rules and declarations for PUSCH  **Proposal 1: Option 1 can be applied for high speed support declaration for HST PUSCH.**   * Option 1:  Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Which tests need to be passed, if 500kph is declared, is discussed separately under “High speed implicit test passing”   Applicability rules for antenna configuration  **Proposal 2: In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for either the minimum or the sub-minimum number of supported connectors, in addition to the maximum numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.**  Performance requirements for DFT-s-OFDM  **Proposal 3: Do not introduce PUSCH HST requirements for DFT-s-OFDM.**  Performance requirements for fading channel  **Proposal 4: Do not specify requirements for multi-path fading channel models with high Doppler values.** |
| R4-2007422 | Intel Corporation | HST multi-path fading channel conditions  Observation #1: Practical channel estimation leads to small demodulation performance degradation compare to scenario with perfect channel estimation. Performance loss is limited by 1dB for at least up to MCS 17.  **Proposal #1: Specify PUSCH requirements for multi-path fading channel with maximum doppler shift of 600Hz and 1200Hz for 15kHz SCS and 30kHz SCS respectively.** |
| R4-2007423 | Intel Corporation | Moderator: Simulation results. |
| R4-2008206 | Huawei, HiSilicon | Moderator: Simulation results. |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 1-1: 1T1R requirements

*Sub-topic description:*

In the last meeting (RAN4#94-e-Bis), it was agreed to introduce 1T1R requirements for the tunnel scenario, but the applicability rules, and some other configurations, are FFS:

|  |
| --- |
| **Configurations to be tested**   * Introduce 1T1R requirements for the tunnel scenario   Previous applicability rule wording options (Informative):   * + Option 3 : Define test applicability rule in the section 8.1.2.0 of TS 38.141-1 as:     - Unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the ~~lowest and~~ highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.   + Option 4: Define test applicability rule in the section 8.1.2.0 of TS 38.141-1 as:     - “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”   Agreement 2nd round (online session)  RAN4 will introduce 1T1R for the tunnel scenario requirements only for conducted requirements, FFS for the test applicability rule   * Agreements from 1st round   + If 1T1R requirement is introduced: 1T1R requirement configuration     - Re-use the 1T2R requirement configuration.   + Slot allocation     - Only capture to use TDD pattern according to the previous WF agreement [R4-1915886]: Reuse the existing TDD configurations. 15 kHz SCS: 3D1S1U, S=10D:2G:2U 30 kHz SCS: 7D1S2U, S=6D:4G:4U * If 1T1R requirement is introduced: MCS configuration   + Option 1: If 1T1R requirement is introduced, only have MCS 2 requirements.   + Option 2: If 1T1R requirement is introduced, have MCS 2 and MCS16 requirements.   Proposed WF:  TBD after 1T1R introduction agreed.   * If 1T1R requirement is introduced with OTA testing: 1T1R requirement configuration   Agreement 2nd round:  Do not introduce OTA testing. |

This sub-topic will **exclude the discussion on 1T1R applicability rules**, which will be treated in the PUSCH applicability rules sub-topic.

*Open issues and candidate options before e-meeting:*

**Issue 1-1-1: 1T1R requirements for the tunnel scenario - MCS configuration**

* Proposals
  + Option 1 (CATT, Samsung, Huawei, ZTE): Only have MCS 2 requirements.
  + Option 2 (DoCoMo, Ericsson, Nokia): Have MCS 2 and MCS16 requirements.
* Recommended WF
  + Collect further company views during 1st round.

### Sub-topic 1-2: Multi-path fading channel under high Doppler

*Sub-topic description*

In RAN4#94-bis-e, the discussion on multi-path fading channel under high Doppler value was postponed until RAN4#95-e [2]:

|  |
| --- |
| * Multi-path fading channel under high Doppler value   + Option 1: Do not specify requirements for multi-path fading channel models with high Doppler values.   + Option 2: Specify PUSCH requirements for multi-path fading channel with maximum doppler shift of 1200Hz and 2400Hz for 15kHz SCS and 30kHz SCS, respectively.   + Option 3: Specify PUSCH requirements for multi-path fading channel with maximum doppler shift of 600Hz and 1200Hz for 15kHz SCS and 30kHz SCS, respectively.   Proposed WF:  FFS until next meeting.   * Is multi-path fading channel under high Doppler value a common scenario?   + Option 1: Multi-path fading channel is very rare in HST scenarios (open area or tunnel).   + Option 2: Fading channel is also typical condition in the real propagation under high speed.   Proposed WF:  FFS until next meeting. |

*Open issues and candidate options before e-meeting:*

**Issue 1-2-1: Is multi-path fading channel under high Doppler value a common scenario?**

* Proposals
  + Option 1 (DoCoMo): Multi-path fading is a typical HST scenario.
  + Option 2 (Huawei, Ericsson, Nokia, ZTE): Multi-path fading is not a typical HST scenario.
  + Option 3 (Samsung): Multi-path fading should be a specific HST scenario and relevant requirements if introduced should be optional and BS declared basis.
* Recommended WF
  + Collect further company views during 1st round.

**Issue 1-2-2: Specification of multi-path fading channel under high Doppler**

* Proposals
  + Option 1 (Huawei, Ericsson, ZTE, CATT, Nokia): Do not specify requirements for multi-path fading channel models with high Doppler values.
  + Option 2 (Intel, DoCoMo, CMCC): Specify PUSCH requirements for multi-path fading channel with maximum doppler shift of 600Hz and 1200Hz for 15kHz SCS and 30kHz SCS, respectively.
  + Option 3 (Samsung): If agreed to introduce the related requirement, the high Doppler with 600Hz and 1200Hz for 15 kHz and 30 kHz SCS can be regarded as the starting point for the feasibility study with HST requirement with high Doppler.
* Recommended WF
  + Collect further company views during 1st round.

**Issue 1-2-3: Where to specify multi-path fading channel under high Doppler.**

* Proposals
  + Option 1 (DoCoMo, Ericsson): If specified, introduce new PUSCH requirements for multi-path fading conditions in non-HST PUSCH section.
* Recommended WF
  + Deprioritize discussion until inclusion of multi-path fading channel decided (see issue 1-2-2).

**Issue 1-2-4: Waveform, if multi-path fading channel under high Doppler is specified.**

* Proposals
  + Option 1 (Samsung): Focus on the requirements with CP-OFDM waveform.
* Recommended WF
  + Deprioritize discussion until inclusion of multi-path fading channel decided (see issue 1-2-2).

### Sub-topic 1-3: DFT-s-OFDM waveform

*Sub-topic description*

In RAN4#94-bis-e, it was not agreed whether to introduce DFT-s-OFDM or not:

|  |
| --- |
| * Dft-s-OFDM waveform   + Option 1: Introduce PUSCH HST requirements for DFT-s-OFDM.   + Option 2: Do not introduce PUSCH HST requirements for DFT-s-OFDM   + Option 3: Define DFT-s-OFDM only for 350km/h scenario, 1T2R and minimum channel bandwidth   Proposed WF:  Discuss in next meeting. Clarify how/if implicit test passing is still applicable. |

*Open issues and candidate options before e-meeting:*

**Issue 1-3-1: Include requirements for DFT-s-OFDM waveform**

* Proposals
  + Option 1 (DoCoMo): Introduce PUSCH HST requirements for DFT-s-OFDM.
  + Option 2 (Huawei, Ericsson, ZTE, Samsung, CATT, Nokia): Do not introduce PUSCH HST requirements for DFT-s-OFDM.
* Recommended WF
  + Collect further company views during 1st round.  
    Explore if compromise to option 2 is possible.

**Issue 1-3-2: If DFT-s-OFDM waveform is introduced, target speed.**

* Proposals
  + Option 1 (Samsung): Only 500kph requirement.
* Recommended WF
  + Come back to this issue, once DFT-s-OFDM inclusion is decided (issue 1-3-1).

**Issue 1-3-3: If DFT-s-OFDM waveform is introduced, configuration.**

* Proposals
  + Option 1 (DoCoMo): The following configuration and applicability rule for DFT-s-OFDM:
    - Antenna configuration: Only 1T2R
    - MCS: Only MCS2
    - CBW and SCS: Only 5MHz CBW/15kHz SCS and 10MHz CBW/ 30kHz SCS
    - Velocity: Only 350km/h
    - Applicability rule:
      * If BS that declare to support HST for DFT-s-OFDM, BS vendor can choose either DFT-s-OFDM or CP-OFDM for the test with 1T2R, MCS2, 5MHz CBW/15kHz SCS or 10MHz CBW/30kHz SCS and 350km/h HST scenarios. (The number of tests is kept).
* Recommended WF
  + Come back to this issue, once DFT-s-OFDM inclusion is decided (issue 1-3-1).

### Sub-topic 1-4: PUSCH applicability rules

*Sub-topic description*

In RAN4#94-bis-e, it was agreed to allow implicit test passing for PUSCH:

|  |
| --- |
| * High speed implicit test passing   Agreement 2nd round (online session):  Allow implicit test passing. A BS that declares to support 500kph, and passes the tests for 500kph, can also consider the tests for 350kph as passed. |

This agreement now requires a corresponding applicability rule.

*Open issues and candidate options before e-meeting:*

**Issue 1-4-1: PUSCH implicit test passing applicability rule**

* Proposals
  + Option 1 (Nokia, ZTE, Samsung, Huawei): Capture the following applicability rule in test specifications:
    - “Unless otherwise stated, a BS that declares to support 500km\h (see D.1XX in table 4.6-1) and passes the tests for 500km\h, can also consider the tests for 350kph as passed.”
* Recommended WF
  + Collect further company views during 1st round.

**Issue 1-4-2: PUSCH 1T1R applicability rule**

* Proposals
  + Option 1 (DoCoMo, Samsung, CATT, Nokia, ZTE): Allow foregoing testing for 1T1R, when 1T2R is tested. This to be captured in applicability rule by changing previous rule (in the section 8.1.2.0 of TS 38.141-1) as follows:
    - “In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for the lowest number or two supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.”
  + Option 2 (Huawei):
    - In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for one of the lowest two number of supported connectors, in addition to the highest numbers of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.
  + Option 3 (Nokia, Ericsson, Samsung):
    - In high speed train requirements, unless otherwise stated, for a BS supporting different numbers of antenna connectors (for BS type 1-C) or TAB connectors (for BS type 1-H) (see D.37 in table 4.6-1), the tests with low MIMO correlation level shall apply only for either the lowest number of supported connectors or two connectors, in addition to the highest number of supported connectors, and the specific connectors used for testing are based on manufacturer declaration.
* Recommended WF
  + Moderator remark: In the moderator’s opinion, both option 1 and 2 capture the same meaning, but with different wording.
  + The moderator has tried to suggest a grammatically acceptable option 3, which more closely follows option 2’s goal of emphasising that only one of the two options for low numbers of connecters is applicable.
  + Companies are encouraged to state during the first round, which options are acceptable to them, or propose new exact wording options, or both.

### Sub-topic 1-5: Manufacturer declaration

*Sub-topic description*

In RAN4#94-bis-e, it was not agreed what categories companies can declare to support, how such categories would impact the test applicability and what choices each category should offer:

|  |
| --- |
| * High speed support declaration for HST PUSCH   + Option 1:  Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Which tests need to be passed, if 500kph is declared, is discussed separately under “High speed implicit test passing”   + Option 2: Declare category of supported design target speed(s). This can be 350 or 500 or 350&500kph (or no HST support).  Only the corresponding requirements are tested (only 350&500kph tests both).   Proposed WF  Companies are encouraged to bring specific manufacturer declaration proposals in a form that could be included in the manufacturer declaration table, i.e., all declaration groups, all choices per group, and explanation of each choice. |

*Open issues and candidate options before e-meeting:*

**Issue 1-5-1: PUSCH high speed support declaration for HST**

* Proposals
  + Option 1a (CATT, Ericsson, Nokia, ZTE, Samsung): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Shared for PUSCH/UL TA.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | x | x |

* + Option 1b (ZTE): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Shared for PUSCH/PRACH/UL TA.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x |

* + Option 1c (Ericsson, CMCC, ZTE, Samsung): Declare category of supported maximum speed. This can be either 350km/h or 500km/h. Only the corresponding requirements are tested.
  + Option 1d (Huawei): Declare category of supported maximum speed. This can be either 350km/h or 500km/h. Only the corresponding requirements are tested.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | High speed train | Declaration of high speed train scenario support. | x | x |
| D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x |
| D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |

* + Option 2a (Nokia): Allow the distinction between “500kph only” scenarios and “350/500kph mixed” scenarios in manufacturer declarations:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.10X | PUSCH high speed train supported target speeds | Declaration of the supported high speed train target speeds, i.e., not declared (no high speed train support), 350km/h, 500km/h, or 350km/h and 500km/h. | x | x |

* + Option 2b (DoCoMo): Declare category of supported design target speed(s) from “no HST”, “HST for 350km/h”, “HST for 500km/h” or “HST for both 350km/h and 500km/h” and introduce the following declaration:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| D.1xx | PUSCH for HST | Declaration of the supported HST scenarios: no HST, HST for 350km/h, HST for 500km/h or HST for both 350km/h and 500km/h. | x | x | x |

* Recommended WF
  + Collect further company views during 1st round.
  + Companies are encouraged to give feedback on
    - Which of the two main options (350/500 vs. 350/500/350&500) they see the most advantageous solution and why?
    - Which declaration wording option they see as best or propose new exact wording options.

### Sub-topic 1-6: Specification writing

*Sub-topic description*

With the PUSCH requirement organization and simulation contributions having become quite stable, RAN4 can go ahead and finalize the specifications.  
However, it remains to verify the additional need for additions for HST in the measurement set-up and test tolerance definition.

Additionally, the cleaning of the specification TS 38.**104** ahead of ITU submission, will have an impact on the HST PUSCH CR treatment in this meeting, as indicated in the following guidance provided by the RAN4 Chair (Steven) and Demod co-chair (Haijie) to the moderators of the relevant email discussions:

|  |
| --- |
| **From:** Haijie Qiu <haijie.qiu@samsung.com>  **Sent:** Monday, May 18, 2020 4:21 AM **To:** 'Steven Chen' <steven.chen@futurewei.com>; Mueller, Axel (Nokia - FR/Paris-Saclay) <axel.mueller@nokia-bell-labs.com>; 'Johan Sköld' <johan.skold@ericsson.com> **Cc:** zhangxiaoran@CHINAMOBILE.COM; andrey.chervyakov@intel.com; Angelow, Iwajlo (Nokia - US/Naperville) <iwajlo.angelow@nokia.com>; Kai-Erik.Sunell@etsi.org; 'Nicholas Pu' <nicholas.pu@ericsson.com>; 'Thomas Chapman' <thomas.chapman@ericsson.com>; 'Yang Shan' <yangshan@chinatelecom.cn>; 'Yuan Gao' <gaoyuan@catt.cn>; 'Kazuyoshi Uesaka' <kazuyoshi.uesaka@ericsson.com>; chuhsian@QTI.QUALCOMM.COM; 'Belov, Dmitry' <dmitry.belov@INTEL.COM>; 'Chervyakov, Andrey' <andrey.chervyakov@intel.com> **Subject:** RE: ITU submission - Demod part in core specifications (36.101/36.104/38.104)  Hello All  (I change the email title to be precise)  Many thanks for the discussion. As Steven pointed out, even ITU submission target for core requirements, it is still desirable we aim to clean the entire specification including performance part in TS 36.101/36.104 and 38.104.  Based on my initial review on t-doc submission, it’s hard to give a generic rules as some CRS aims to remove [ ] on requirements; some CRs modify requirements (still keep  [ ] ); some CRs add requirements with [ ] to replace TBD; also as Axel mentioned below there are different situations for different WIs.  Considering current stage, I would like to suggest “Technical endorse if CRs agreeable as requirements still TBD  in CRs and corresponding test CRs  if any”. To be more specific for each impacted topics areas/WIs (which already indicated in the file shared by Steven for email discussion assignment):   * [95e][313] LTE\_eMTC5\_Demod: Suggest to technical endorse if CRs agreeable as requirements still TBD in CRs * [95e][315] LTE\_terr\_bcast\_Demod: Suggest to technical endorse if CRs agreeable as requirements still TBD in CRs * [95e][322] NR\_HST\_Demod\_BS: Suggest to technical endorse if CRs agreeable as requirements still TBD in CRs  for 38.104 including R4-2006053,R4-2007204 and corresponding 38.141-1,38.141-2 CR if any * [95e][324] NR\_perf\_enh\_Demod\_BS: Suggest to technical endorse if CRs agreeable as requirements still TBD or with [ ] in CR  for 38.104 of  R4-2006251 and corresponding 38.141-1,38.141-2 CR if any * For 38.104 clean-up CR: R4-2008100/2008099: suggest to treat the changes of performance part in email thread “  [95e][312] Demod\_Maintenance” to check by demod experts  and avoid the duplicated changes with other demod CRs   Hope above suggestion fine to everyone.  BR, Haijie |

*Open issues and candidate options before e-meeting:*

**Issue 1-6-1: Removal of TBD and []**

* Proposals
  + Option 1 (Nokia): Agreeing on SNR values.  
    Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the PUSCH CRs
  + Option 2: (RAN4 chair and demod session chair):   
     Submitted TS 38.104 CRs could be technically endorsed.  
     Submitted TS 38.141-1/2 CRs could be agreed.  
     Try to resolve TBDs and [].
  + Option 3 (Huawei)  
    Firstly check if some companies have plan to submit new results or update their results in next meeting, if no, just agree CRs endorsed in last meeting and add SNR the requirements based on the latest results summary. All other newly submitted CRs for this meeting can only be endorsed if agreeable.
* Recommended WF
  + Do not agree TS 38.104 CRs that introduce new TBDs or [], either postpone, or technically endorse, or change to no longer add new TBDs or [].
    - Discuss, if [] can be removed and TBDs can be replaced in the draftCRs endorsed last meeting.
    - Change all remaining [TBD] to TBD.
    - Consider removing requirements with remaining TBD.
  + For PUSCH in particular: Do not introduce minimum CBW requirements in CRs this meeting.

**Issue 1-6-2: HST test setup figures and test tolerances**

* Proposals
  + Option 1 (Nokia): Verify if further HST PUSCH additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272.
* Recommended WF
  + Test specification CR authors to verify the need for new measurement setup figures and TTs.
    - Remark: LTE has re-used the measurement setup figure for PUSCH in PUSCH HST (TS 36.141 I.3.2) by adding “HST” to heading and caption, as well as adding a note.  
      LTE also added new PUSCH HST TTs (36.141 G.3).
  + Other delegates to check, if the additions in the CR are technically correct and sufficient.

### Sub-topic 1-7: Simulation summary management

*Sub-topic description*

Following recent agreements, for example on additional SCS/CBW combination, the simulation summary collection needs to be updated

|  |
| --- |
| Agreement 2nd round:  Keep previous agreement.  Add requirements for 5MHz CBW/15kHz SCS, 10Mhz CBW/30kHz SCS for CP-OFDM with applicability rule as for Rel-15 (i.e., only largest CBW per SCS needs to be tested). |

*Open issues and candidate options before e-meeting:*

**Issue 1-7-1: Additional SCS/CBW combinations in the simulation summary**

* Proposals
  + Option 1 (CATT, Nokia, ZTE, Huawei): Add 5MHz CBW/15kHz SCS, 10MHz CBW/30kHz SCS for PUSCH to simulation results summary.
* Recommended WF
  + Add 5MHz CBW/15kHz SCS, 10MHz CBW/30kHz SCS for PUSCH to simulation results summary.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| XXX | Issue 1-1-1:  Issue 1-1-2:  ….  Others: |
| Ericsson | **Issue 1-1-1: 1T1R requirements for the tunnel scenario - MCS configuration**  Agree with Option 2. Based on simulation results, we see MCS16 is feasible fo1 1T1R. And we don’t think multi-path fading channel with high Doppler shift is a suitable assumption for HST, especially for tunnel scenario. In that case, we prefer have both MCS2 and MCS16 as other requirements.  **Issue 1-2-1: Is multi-path fading channel under high Doppler value a common scenario?**  We still don’t think it is a typical scenario for HST. In LTE TR36.878, ETU600 was taken as an assumption for high speed train, but it just considered a possible maximum speed (300~350km/h) and didn’t consider the BS PUSCH HST deployment. Since the HST BS are normally deployed close to the railway, there is rare buildings and obstacles between BS and UE when train is at a very high speed. Furthermore, multi-path fading requirement is separate from HST requirements even in LTE spec. We think it implicitly shows that multi-path channel under high Doppler is not considered as a typical HST scenario in LTE discussion. Furthermore, this scenario is not even a normal NR scenario because vehicles can’t reach so high speed in dense urban. In summary, we think it is not expected in real life that multi-path fading is combined with high Doppler.  But we also see this requirement has been introduced on UE side, so we want companies to decide should we also introduce it on BS side even we can’t figure out a realistic scenario for it.  **Issue 1-2-2: Specification of multi-path fading channel under high Doppler**  Agree with Option 1.  **Issue 1-2-3: Where to specify multi-path fading channel under high Doppler**  If it is in a non-HST section, then it should be considered as a normal NR requirement not HST since we have agreed to introduce a separate section for HST PUSCH.  But as we are mentioned in Issue 1-2-1, this scenario is not even a realistic normal NR scenario since there is no such fast vehicle in dense urban.  **Issue 1-3-1: Include requirements for DFT-s-OFDM waveform**  Agree with Option 2. There is very small performance difference between DFT-s-OFDM and CP-OFDM when discuss Rel-15 requirements. And some companies also deliver their comparing simulation results for HST. The difference is still very small. So we don’t think we need more requirements.  **Issue 1-4-2: PUSCH 1T1R applicability rule**  We have a question on this issue if we go for these two options. If a BS supports 2/4/8 Rx, then it can be allowed to test 4 and 8 Rx? Is it really aligned with our previous agreement?  Nokia: All three option would require the testing of 2 and 8 Rx in this example.  Ericsson: We can agree with Option 3 because it is more precise  **Issue 1-5-1: PUSCH high speed support declaration for HST**  Agree with 1a. No need to declare support 350&500km/h since implicit test passing is agreed for HST PUSCH and there should be no much algorithm difference between 2 target speed.  **Issue 1-6-2: HST test setup figures and test tolerances**  We need some further check, but for now, we just think new TT is not needed. |
| CMCC | Issue 1-2-1: One consideration is that different operators may have different deployment, it cannot preclude that multi-path fading channel will be used in high speed scenario by some operators. The other consideration is that in LTE, ETU600 is introduced in high speed scenario. In rel-15, the supported maximum doppler shift is only 400Hz, it is not expected that NR has worse performance than that in LTE. Taking above into considerations, it is preferred to introduce multi-path fading channel under high doppler value (i.e. 600Hz for 15KHz SCS and 1300Hz for 30KHz).  Moderator: Thank you for explaining your thinking. I cannot decipher if CMCC sees multi-path fading channel under high Doppler value a common scenario, though.  Could you please add your company name to your preferred option (or don’t if you prefer that)?  Issue 1-2-2: support option 2. Same comments as in Issue 1-2-1.  Issue 1-5-1: for the two main options (350/500 vs. 350/500/350&500), we prefer 350/500, which is aligned with the agreements in the last meeting, which is “A BS that declares to support 500kph, and passes the tests for 500kph, can also consider the tests for 350kph as passed”.  Issue 1-7-1: we are OK with the recommended WF. |
|  |  |
| ZTE | Issue 1-1-1 MCS for 1T1R requirements  For 1T1R, a high data rate should not be expected under 1T1R deployment. It seems to us that the coding rate of MCS 16 is a bit high for such deployment and UE battery may not last long, thus we think a low MCS is a proper choice (Option 1, MCS2)  Issue 1-2-1 Multipath fading channel under high Doppler value  In our understanding, multipath fading under high Doppler value may lead to non-coherence even within a slot, which may lower the achievable performance under HST. So a practical HST deployment should avoid such scenarios.  Issue 1-2-2 Specification of multi-path fading channel under high Doppler  As stated above, it is not necessary to introduce such requirements (Option 1)  Issue 1-2-3 Where to specify multipath fading channel under high Doppler  As stated abvoe, there should be no such requirements.  Issue 1-2-4 Waveform, if multi-path fading channel under high Doppler is specified  As stated above, there should be no such requirements introduced.  Issue 1-3-1 Include requirements for DFT-s-OFDM waveform  Completion of the current works defined should have higher priority. For the time being, we don’t see the urgency to include requirements for DFT-s-OFDM waveform (Option 2)  Issue 1-3-2 Target speed for DFT-s-OFDM if introduced  As stated above, there should be no such requirements introduced for the time being.  Issue 1-3-3 Configuration for DFT-sOFDM if introduced  As stated above, there should be no such requirements introduced for the time being.  Issue 1-4-1 PUSCH implicit test passing applicability rule  As a generic rule, it is reasonable to have the implicit test passing rule proposed in Option 1.  Issue 1-4-2 PUSCH 1T1R applicability rule  Option 1 is a good balance between test coverage and test efforts.  Issue 1-5-1 PUSCH high speed support declaration for HST  In our proposal, the proposed supported maximum speed for HST include HST PUSCH, HST PRACH and UL TA, though there are different preamble formats for 350km/h and 500km/h. But if companies have different opinion on HST PRACH, it is ok for us to compromise to HST PUSCH and UL TA only, leaving HST PRACH a different testing rule. So Option 1a/1b/1c is fine with us. For Option 2a and 2b, it is out of imaginary that there is a BS supporting 500km/h does not support 350km/h.  Issue 1-6-1 Removal of TBD and []  Not sure why we were outside the limited loop on this topic. The recommended WF by Moderator is fine with us.  Issue 1-6-2 HST test setup figures and test tolerance  The recommended WF by Moderator looks reasonable.  Issue 1-7-1 Additional SCS/CBW combinations in the simulation summary  Fine with Option 1, but if we have not had enough inputs to derive the requirements in this meeting, then it may not be included in the specs to avoid new TBDs. |
| Nokia, Nokia Shanghai Bell | **Issue 1-1-1: 1T1R requirements for the tunnel scenario - MCS configuration**  Considering that the 1T1R constraint comes from the leaky cable antennas in the tunnel scenario, we expect the observed SNR values to be quite high. Hence high MCS are commonly observed, and we should include requirements for MCS16.  **Issue 1-2-1: Is multi-path fading channel under high Doppler value a common scenario?**  We don’t see multi-path fading as a typical HST scenario. A train can only go at high speeds, if it is either far away from obstacles/people (i.e., open space) or if it is in a tunnel. Both environments are not multi-path environments. As soon as the train enters urban areas, it needs to slow down to normal vehicular speeds, i.e., no high Doppler shift is expected in combination with multi-path fading.  **Issue 1-2-2: Specification of multi-path fading channel under high Doppler**  As we don’t see multi-path fading as a common scenario, we don’t think it necessary to specify such requirements.  **Issue 1-2-3: Where to specify multi-path fading channel under high Doppler.**  Postpone until after decision on 1-2-2.  **Issue 1-2-4: Waveform, if multi-path fading channel under high Doppler is specified.**  Postpone until after decision on 1-2-2. But we are sympathetic to option1.  **Issue 1-3-1: Include requirements for DFT-s-OFDM waveform**  Nokia has presented simulation results that for high speed 70%TPUT requirements, dft-s-OFDM improves coverage by less than 0.4dB in MCS2 and loses coverage (within simulation uncertainty) for MCS16. Hence we prefer to not add dft-s-OFDM to minimum requirements, since coverage of re-farming LTE bands is not impacted.  **Issue 1-3-2: If DFT-s-OFDM waveform is introduced, target speed.**  Postpone until after decision on 1-3-1.  **Issue 1-3-3: If DFT-s-OFDM waveform is introduced, configuration.**  Postpone until after decision on 1-3-1.  **Issue 1-4-1: PUSCH implicit test passing applicability rule**  Option 1 is our best attempt at translating last meetings agreement into an applicability rule text proposal. We are open to changing the text.  **Issue 1-4-2: PUSCH 1T1R applicability rule**  All three options convey the same meaning. We prefer the text in option 3, followed by option 1.  **Issue 1-5-1: PUSCH high speed support declaration for HST**  In Nokia’s opinion the declaration of supported speeds should consider the product deployment scenario first and foremost. Products are created and deployed with a certain scenario in mind, i.e., 350kph trains, 500kph train, or both mixed. A 500kph declare cell will still support 350kph, but not as well as a 350&500kph BS, as the configuration and algorithms used in a 500kph and 350&500kph deployed cell will differ (see our contribution R4-2006052 for details and examples (configuration and filtering). However, at this point we are open to compromise to 350 and 500 only, and in particular option 1a (preferably with a “i.e. 350km/h, 500km/h**, or neither**” extension).  **Issue 1-6-1: Removal of TBD and []**  Each CR should be considered separately in the corresponding section of this document. But the recommended WF seems like a good starting point for this evaluation.  **Issue 1-6-2: HST test setup figures and test tolerances**  N/A to Nokia’s CRs.  **Issue 1-7-1: Additional SCS/CBW combinations in the simulation summary**  Option 1 is fine for Nokia. |
| Samsung | **Issue 1-1-1: 1T1R requirements for the tunnel scenario - MCS configuration**  We prefer option 1, only introduce MCS 2. Meanwhile we are open to further evaluate and analyse whether MCS 16 SNR requirements is achievable under 1T1R. **Issue 1-2-1: Is multi-path fading channel under high Doppler value a common scenario?**  Similar as LTE, we believe it should be a specific HST scenario and relevant requirements if introduced should be optional and BS declared basis.  Moderator: Thank you for explaining your thinking. I cannot decipher if Samsung sees multi-path fading channel under high Doppler value a common scenario, though.  Could you please add your company name to your preferred option (or don’t if you prefer that)? For now I copy pasted the text above as option 3.  **Issue 1-2-2: Specification of multi-path fading channel under high Doppler**  **I**n current stage, we are open to discuss. Our suggestion is we first agree some tentative values for further evaluations i.e. Doppler value, waveform assumption. We can defer the discussion on introducing requirements and how to organize the specification if introduced later.  **Issue 1-2-3: Where to specify multi-path fading channel under high Doppler**  Not sure what’s the difference with issue 1-2-2. Probably we should focus on issue 1-2-2.  **Issue 1-3-1: Include requirements for DFT-s-OFDM waveform**  Taking Rel-15 NR requirements experience, no much performance difference foreseen, Considering work load and test effort, prefer not to introduce test case for DFT-s-OFDM.  Suggest to defer the discussion on issue 1-3-1 and 1-3-2 pending on the progress on issue 1-3-1.  **Issue 1-4-1: PUSCH implicit test passing applicability rule**  Fine with the proposal (option1)  **Issue 1-4-2: PUSCH 1T1R applicability rule**  Support the recommended WF.  **Issue 1-5-1: PUSCH high speed support declaration for HST**  Support option 1a/1c, we didn’t see the logic if BS declared support 500km/h why such BS cannot support 300km/h. Performance optimization around certain point is BS implementation issues which out of RAN4 scope, RAN4 define minimum performance requirements which assumed no specific optimization. Meanwhile from test aspect, we also didn’t see the necessity to require BS pass both 350km/h and 500km/h test cases, as 500km/h related test cases should be choosed.  **Issue 1-6-1: Removal of TBD and []**  Fine with the recommendation, but we should align with test CRs and core spec CRs for both changes and decision to avoid misalignment and unnecessary confusion. The normal procedure would be, we first introduce performance requirements into core specification first, then we can introduce corresponding test cases into test specification. |
| Huawei, HiSilicon | **Issue 1-1-1: MCS for 1T1R requirements**  We prefer Option 1. Only MCS 2 is enough.  **Issue 1-2-1: Is multi-path fading channel under high Doppler value a common scenario**  We prefer Option 2. We don’t think that it is a common scenario in real field that have both multi-path spread and high Doppler shift.  **Issue 1-2-2: Specification of multi-path fading channel under high Doppler**  Still prefer Option 1 considering the concern on Issue 1-2-1.  **Issue 1-3-1: Include requirements for DFT-s-OFDM waveform**  Still prefer Option 2 that not introduce PUSCH HST requirements for DFT-s-OFDM  **Issue 1-4-1: PUSCH implicit test passing applicability rule**  Generally the wording is fine for us. But need to adopt the format of velocity 500km/h to keep alignment with the CR R4-2006053.  **Issue 1-4-2: PUSCH 1T1R applicability rule**  As per the previous agreement, e.g. if BS supports both 1T1R, 1T2R, 1T8R, performance requirements for either (1T1R or 1T8R) or (1T2R and 1T8R) can be tested, how to describe this applicability rule by using plain language to make the specification clearer to reader. We think that Option 2 is clearer.  We really cannot understand “either the lowest number of supported connectors or two connectors, in addition to the highest number of supported connectors”, how to understand “or two”?  Moderator: The way the proposed WF text would work is best explained at examples:  BS declares to support 1,2,8 => BS needs to test 8, and can chose to test either 1 or 2.  BS declares to support 4,8 => BS needs to test 8 and either 4 or 2.  BS declares to support 1,4 => BS needs to test 4 and either 1 or 2. It remains to be said that this is not about “the lowest two numbers”, it is really about the fixed 2RX case. A BS that declares to support (surreal numbers) 54, 53, 52, and 51 antenna connectors, would still only need to test 54 and either 51 or 2.  **Issue 1-5-1: PUSCH high speed support declaration for HST**  “Which of the two main options (350/500 vs. 350/500/350&500) they see the most advantageous solution and why?”  In last meeting RAN4#94-e-Bis, RAN4 has agreed the implicit testing for 350km/h and 500km/h “A BS that declares to support 500kph, and passes the tests for 500kph, can also consider the tests for 350kph as passed.”, we really do not think that BS needs to declare 350&500 and test both, it is very easy to bring confusion to specification reader who did not join in this discussion. If some company wants to commit performances for both 350 and 500, it can be conducted in the real testing, no needs to set such constraints for all BS vendors from the specification point of view.  The declaration is designed for HST, but from all the available options for specific declaration wording except 1a, there is one declaration description option item “No HST” or “No HST support”, it is contradictory to the declaration title. Maybe one additional declaration for support HST or not can be added:   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | High speed train | Declaration of high speed train scenario support. | x | x | | D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x | | D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |   **Issue 1-6-1: Removal of TBD and []**  Firstly check if some companies have plan to submit new results or update their results in next meeting, if no, just agree CRs endorsed in last meeting and add SNR the requirements based on the latest results summary. All other newly submitted CRs for this meeting can only be endorsed if agreeable.  **Issue 1-6-2: HST test setup figures and test tolerances**  As per the CR work assignment, the respective CR editors are responsible for the corresponding parts of HST test setup figures and test tolerances, or one company will take all of the work?  Moderator: It was my intention for the respective spec section responsible to take over this task.  **Issue 1-7-1: Additional SCS/CBW combinations in the simulation summary**  Option 1 is ok for us. |
|  |  |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| R4-2006053 (Nokia) | [Moderator]: - Please observe the outcome of the chair guidance captured and discussed in sub-topic 1-6. - Depending on sub-topic 1-6, consider adding new minimum CBW requirements and FRCs (see R4-2007183 and R4-2007184) and other changes. |
| Ericsson   * Cover sheet: RAN4 should be R4.   Nokia: Not sure about this. Downlink the prefilled cover sheet does not fill this part, so it might not matter. Is there any reference on how to fill this? (RAN5 PRD 16 Version 1.1, points towards R4.)   * It might be good to add a statement, such as “subject to declaration”, after “… shall only apply to Wide Area Base Stations and Medium Range Base Stations”, otherwise, it would make HST requirements mandatory for all WA and MR BS.   Nokia: 38.104 does not contain a manufacturer declaration section, unlike 38.141-1/2. Hence, we followed the LTE approach of not making a specific reference to a declaration. Since this was endorsed in last meeting, we would ask Ericsson, if this presents a large point of contention, or if we can continue with the endorsed text?  Ericsson: We reviewed the text agreed last time regarding the fact that the requirement is only applied to WA and MR BS: “The performance requirements for PUSCH for high speed train shall only apply to Wide Area Base Stations and Medium Range Base Stations.”. The text risks implying that the PUSCH HST requirements are mandatory for those classes (“The requirements… shall apply…”). Although other text states that the requirement is optional, there could be some risk of perceived conflicting text or ambiguity in the specification. We propose a small fix to remove any ambiguity:  The performance requirements for PUSCH for high speed train ~~shall~~ only apply to Wide Area Base Stations and Medium Range Base Stations (subject to declaration).  Hopefully this is clearer and more acceptable to everyone,  A question: how to consider the tunnel scenario, is it a Local area deployment?  Nokia: Every manufacturer is free to declare the BS type as they please. However, given the strict RF power constraints for local area base stations (as well as other more strict RF requirements) it is probably not advantageous for a manufacturer to do so.  Ericsson: Thanks for the clarification. We just feel the tunnel scenario is kind of a Local area due to the small distance between BS and the train. But just like you said, vendors might not declare for it because of more strict requirements. |
|  |
| R4-2006054 (Nokia) | [Moderator]: - Please observe the outcome of the chair guidance captured and discussed in sub-topic 1-6. - Depending on sub-topic 1-6, consider adding new minimum CBW requirements and FRCs (see R4-2007183 and R4-2007184) and other changes. |
| Ericsson  Cover sheet: RAN4 should be R4 |
|  |
| R4-2006836 (Ericsson) | [Moderator]: - Depending on sub-topic 1-6, consider adding new minimum CBW requirements and FRCs. (See R4-2007183 and R4-2007184.)  Ericsson: Yes, we’ll update it. |
| Company B |
|  |
| R4-2006837 (Ericsson) | [Moderator]: - Depending on sub-topic 1-6, consider adding new minimum CBW requirements and FRCs. (See R4-2007183 and R4-2007184.) |
|  |
|  |
| R4-2007183 (DoCoMo) | [Moderator]: - Depending on sub-topic 1-6, consider removing new minimum CBW requirements and FRCs. (See R4-2007183 and R4-2007184.) |
| Ericsson:   * Cover sheet: rev should be “-“ not 0 * We reviewed the text agreed last time regarding the fact that the requirement is only applied to WA and MR BS: “The performance requirements for PUSCH for high speed train shall only apply to Wide Area Base Stations and Medium Range Base Stations.”. The text risks implying that the PUSCH HST requirements are mandatory for those classes (“The requirements… shall apply…”). Although other text states that the requirement is optional, there could be some risk of perceived conflicting text or ambiguity in the specification. We propose a small fix to remove any ambiguity:   The performance requirements for PUSCH for high speed train ~~shall~~ only apply to Wide Area Base Stations and Medium Range Base Stations (subject to declaration).  Hopefully this is clearer and more acceptable to everyone, |
|  |
| R4-2007184 (DoCoMo) | [Moderator]: - Depending on sub-topic 1-6, consider removing new minimum CBW requirements and FRCs. (See R4-2007183 and R4-2007184.) |
| Ericsson:  Cover sheet: rev should be “-“ not 0 |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: PRACH requirements (6.17.2.2.2)

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

This section contains T-docs with corresponding proposals and observations submitted to the agenda item “6.17.2.2.2 PRACH requirements”, as well as, any PRACH requirement related observations and proposals submitted to other agenda items.

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-20xxxxx | Company A | Proposal 1:  Observation 1: |
| R4-2006270 (AI 6.17.2.2) | CATT | Moderator: CR  PRACH   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.109 | PRACH format for HST | Declaration of restricted set type A and/or restricted set type B and/or A2 for high speed mode and/or B4 for high speed mode and/or C2 for high speed mode for HST PRACH. | x | x | |
| R4-2006271 | CATT | Moderator: CR  PRACH   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | D.110 | PRACH format for HST | Declaration of restricted set type A and/or restricted set type B and/or A2 for high speed mode and/or B4 for high speed mode and/or C2 for high speed mode for HST PRACH. | c | x | n/a | |
| R4-2006666 (AI 6.17.2.2.1) | ZTE Wistron Telecom AB | Manufacturer declaration maximum supported speed for HST  **Proposal 1: Introduce a new declaration item (Option 1) shown in Table -1.**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x | |
| R4-2006055 (AI 6.17.2.2.2) | Nokia, Nokia Shanghai Bell | High speed support declaration  **Proposal 1: RAN4 to include the two new manufacturer declarations “PRACH high speed train long format support” and “PRACH high speed train short format support”, as detailed above.**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.10X | PRACH high speed train long format support | Declaration of the supported long PRACH format restricted set configurations for high speed train categories, i.e., not declared (no high speed train support), restricted set type A, restricted set type B, or both. | x | x | | D.10X | PRACH high speed train short format support | Declaration of high speed train support for each supported short PRACH format. I.e., declare for each of the supported formats of the set {A2, B4, C2}, if high speed mode is supported. | x | x |     TDLC300-100 propagation conditions for long preamble formats  Observation 1: Performance differences in LTE specifications are only due to the usage of different sequences and not different demodulation implementation performances.  **Proposal 2: It is not necessary to repeat testing of TDLC300-100 FO=400Hz for restricted set long formats.**  Agreeing on SNR values  **Proposal 3: Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the PRACH CRs.**  HST test setup figures and TTs  Observation 2: RAN4 should verify, if HST PRACH additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272. |
| R4-2006667 | ZTE Wistron Telecom AB | Multipath fading channel  Observation 1: Non-LOS propagation should be avoided in a high speed train scenario from performance aspect.  Observation 2: A multipath fading channel plus a fixed frequency offset is not a proper model on a radio propagation with parital LOS and partial fading channel. Some other model, e.g., a Rician channel model may be more applicable.  **Proposal 1: There is no practical meaning to introduce requirements under TDLC300-100 plus 400Hz frequency offset for HST scenarios, thus such requirements should not be introduced before any further study.** |
| R4-2006834 | Ericsson | Table organization of high-speed train requirement sections for PRACH 350kph in specifications  Observation 1: The purpose of including long format 0 restricted sets is to have a smooth transition from LTE to NR  **Proposal 1: Add format 0 in the table caption to clarify confusion and modify the agreement accordingly as “add new table for long format 0 restricted set type A/B”**  High speed support declaration 350kph PRACH  Observation 2: A BS cannot declare support of 350kph short format PRACH. No remarkable performance degradation by employing PRACH short formats with 500kph HST is observed from previous simulation results, when comparing to the normal mode PRACH short formats. Note that the test configurations differ only in Doppler shift.  **Proposal 2: Consider explicitly explaining format-speed mapping for PRACH HST.**  **Proposal 3: RAN4 to consider adding requirements of 350kph on short format PRACH with preliminary condition that, allow implicit test passing for short format 350kph when declaring support of short format PRACH HST.**  Section organization of high-speed train requirements for PRACH in specifications  Observation 3: If the fading channels with 400Hz frequency offset were to be included (which we think is not reasonable), there will be confusion whether to include it in the new section or not, due to the wording of agreement.  **Proposal 4: Delay the discussion on “Section organization of high-speed train requirements for PRACH in specifications” to after the fading cases are decided.**  Multi-path fading channel test cases  Observation 4: No reasoning is provided to link multi-path fading with high speed scenario.  **Proposal 5: There is no need for RAN4 to include multi-path fading test cases in PRACH HST.** |
| R4-2007185 | NTT DOCOMO, INC. | Propagation conditions for long preamble format  **Proposal 1: RAN4 introduces TDLC300-100 for PRACH restricted set type A and B (Keep original agreement made in RAN4 #92bis).**  Declaration for PRACH high speed support  **Proposal 2: RAN4 introduces the following new declaration for PRACH high speed support:**   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | D.1xx | High speed support for PRACH | Declaration of high speed support for PRACH: restricted set type A, restricted set type B, format A2 for high speed, format B4 for high speed or/and format C2 for high speed. | x | x | x | |
| R4-2007204 | Huawei, HiSilicon | Moderator: CR TS 38.104 |
| R4-2007205 | Huawei, HiSilicon | Moderator: CR TS 38.141-1 |
| R4-2007206 | Huawei, HiSilicon | Moderator: CR TS 38.141-2 |
| R4-2007207 | Huawei, HiSilicon | Propagation conditions for long preamble format  **Proposal 1: Prefer not to define TDLC300-100 fading channel with frequency offset of 400Hz requirements for long preamble formats.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 2-1: TDLC300-100 propagation conditions for long preamble formats

*Sub-topic description:*

In RAN4#94-bis-e, no conclusion was reached with respect to testing TDLC300-100 FO=400Hz with restricted sets:

|  |
| --- |
| * TDLC300-100 propagation conditions for long preamble formats   + Option 1: Do not to introduce TDLC300-100 fading channel with frequency offset of 400Hz requirements for long preamble formats for HST requirements.   + Option 2: Introduce TDLC300-100 fading channel with frequency offset of 400Hz requirements for long preamble formats for HST requirements. |

*Open issues and candidate options before e-meeting:*

**Issue 2-1-1: TDLC300-100 propagation conditions for long preamble formats**

* Proposals
  + Option 1 (ZTE): Do not to introduce TDLC300-100 fading channel with frequency offset of 400Hz requirements for long preamble formats for HST requirements, before any further study.
  + Option 2 (Huawei, Ericsson,, ZTE): Do not to introduce TDLC300-100 fading channel with frequency offset of 400Hz requirements for long preamble formats for HST requirements.
  + Option 3 (DoCoMo): Introduce TDLC300-100 for PRACH restricted set type A and B.
* Recommended WF
  + Collect further company views during 1st round.  
    Please give feedback on how strong the respective request is.

### Sub-topic 2-2: Manufacturer declaration

*Sub-topic description:*

In RAN4#94-bis-e, it was agreed to declare high speed support based on restricted set support in long formats and based on high speed mode for short format (instead of declaration by target speed):

|  |
| --- |
| * High speed support declaration for HST PRACH - speed or feature based   + Allow BS to declare support for HST including [restricted set type A] and/or [restricted set type B] and/or [A2 for high speed mode] and/or [B4 for high speed mode] and/or [C2 for high speed mode] |

It now remains to define the specific manufacturer declaration categories and clarify the corresponding testing.

*Open issues and candidate options before e-meeting:*

**Issue 2-2-1: PRACH high speed support declaration for HST**

* Proposals
  + Option 1a (CATT, CMCC): One declaration table entry for short and long format

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.109 | PRACH format for HST | Declaration of restricted set type A and/or restricted set type B and/or A2 for high speed mode and/or B4 for high speed mode and/or C2 for high speed mode for HST PRACH. | x | x |

* + Option 1b (DoCoMo): One declaration table entry for short and long format

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| D.1xx | High speed support for PRACH | Declaration of high speed support for PRACH: restricted set type A, restricted set type B, format A2 for high speed, format B4 for high speed or/and format C2 for high speed. | x | x | x |

* + Option 1c (Huawei): One declaration table entry for short and long format.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | High speed train | Declaration of high speed train scenario support. | x | x |
| D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x |
| D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |

* + Option 2 (Nokia, Ericsson): Include the two new manufacturer declarations “PRACH high speed train long format support” and “PRACH high speed train short format support”,

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.10X | PRACH high speed train long format support | Declaration of the supported long PRACH format restricted set configurations for high speed train categories, i.e., not declared (no high speed train support), restricted set type A, restricted set type B, or both. | x | x |
| D.10X | PRACH high speed train short format support | Declaration of high speed train support for each supported short PRACH format. I.e., declare for each of the supported formats of the set {A2, B4, C2}, if high speed mode is supported. | x | x |

* + Option 3 (ZTE): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). Shared for PUSCH/PRACH/UL TA.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x |

* Recommended WF
  + Collect further company views during 1st round.
  + Companies are encouraged to give feedback on
    - Which of the three main options (long&short vs. long/short vs. PUSCH&PRACH&ULTA) they see the most advantageous solution and why?
    - Which declaration wording option they see as best or propose new exact wording options.

**Issue 2-2-2 (new): Test applicability for long PRACH format restricted set type A and B**

* Proposals
  + Option 1 (Huawei): Additionally, test applicability for long PRACH format restricted set type A and B needs to be defined if BS supports both types.

|  |
| --- |
| 8.1.2.1.x Applicability of requirements for different restricted set types of long PRACH format 0  Unless otherwise stated, PRACH requirement tests for long PRACH format 0 with restricted set Type A and B shall apply only for the restricted set type declared to be supported (see D.110 in table 4.6-1). If both restricted set type A and type B are declared to be supported, the tests shall be done for type B; the same chosen mapping type shall then be used for all tests. |

* + Option 2: No applicability rule required
* Recommended WF
  + Collect further company views during 1st round.

### Sub-topic 2-3: Revisiting of previous agreements

*Sub-topic description*

One company raised several requests for clarification of some of the previous PRACH agreements.

*Open issues and candidate options before e-meeting:*

**Issue 2-3-1: Table organization of high-speed train requirement sections for PRACH 350kph in specifications**

* Proposals
  + Option 1 (Ericsson, ZTE, Huawei): Add format 0 in the table caption to clarify confusion and modify the agreement accordingly as “add new table for long format 0 restricted set type A/B”.
    - Add new table for long format 0 restricted set type A.  
      Add new table for long format 0 restricted set type B
  + Option 2: Keep previous agreement:
    - Add new table for long format restricted set type A.  
      Add new table for long format restricted set type B.
* Recommended WF
  + Collect further company views during 1st round.

**Issue 2-3-2: High speed support declaration 350kph PRACH - Explicit format-speed mapping**

* Proposals
  + Option 1a (ZTE): Explicitly explain format-speed mapping for PRACH HST in specification.
  + Option 1b (Ericsson): Explicitly explain format-speed mapping for PRACH HST in specification.  
    Capture the following text:
    - No implicit test passing.  
      A BS claiming to support short format high speed must test all the requirements of long format 0 high speed, even if it has passed the tests for short format high speed.
  + Option 2: Explicit explanation of format-speed mapping for PRACH HST in specification is not required.
* Recommended WF
  + Collect further company views during 1st round.

**Issue 2-3-3: High speed support declaration 350kph PRACH - 350kph short format requirements**

* Proposals
  + Option 1 (Ericsson, CMCC): Add requirements of 350kph on short format PRACH with preliminary condition that, allow implicit test passing for short format 350kph when declaring support of short format PRACH HST.
  + Option 2 (Nokia, ZTE, Huawei): Keep previous agreement:
    - No implicit test passing.  
      A BS claiming to support 350kph must test all the requirements of 350kph, even if it has passed the tests for 500kph.
    - For 350km/h velocity, use PRACH format 0  
      For 500km/h velocity, use PRACH format A2/B4/C2
      * FFS if PRACH format 0 shall be used.
    - For 500km/h velocity, no extra requirements for PRACH format 0.
* Recommended WF
  + Collect further company views during 1st round.

**Issue 2-3-4: Section organization of high-speed train requirements for PRACH in specifications**

* Proposals
  + Option 1 (): Delay the discussion on “Section organization of high-speed train requirements for PRACH in specifications” to after the fading cases are decided.
  + Option 2 (Ericsson, Huawei): Keep previous agreement:
    - New section for requirements specified with frequency offset >=625Hz.  
      Example, 8.4.2.3 Minimum requirements for high speed train
* Recommended WF
  + Collect further company views during 1st round.

### Sub-topic 2-4: Specification writing

*Sub-topic description*

With the PRACH requirement organization and simulation contributions having become quite stable, RAN4 can go ahead and finalize the specifications.  
However, it remains to verify the additional need for additions for HST in the measurement set-up and test tolerance definition.

Additionally, the cleaning of the specification TS 38.**104** ahead of ITU submission, will have an impact on the HST PRACH CR treatment in this meeting, as indicated in the following guidance provided by the RAN4 Chair (Steven) and Demod co-chair (Haijie) to the moderators of the relevant email discussions:

[See email in sub-topic 1-6.]

*Open issues and candidate options before e-meeting:*

**Issue 2-4-1: Removal of TBD and []**

* Proposals
  + Option 1 (Nokia): Agreeing on SNR values.  
    Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the PRACH CRs
  + Option 2: (RAN4 chair and demod session chair):   
     Submitted TS 38.104 CRs could be technically endorsed.  
     Submitted TS 38.141-1/2 CRs could be agreed.  
     Try to resolve TBDs and [].
  + Option 3 (Huawei)  
    Firstly check if some companies have plan to submit new results or update their results in next meeting, if no, just agree CRs endorsed in last meeting and add SNR the requirements based on the latest results summary. All other newly submitted CRs for this meeting can only be endorsed if agreeable.
* Recommended WF
  + Do not agree TS 38.104 CRs that introduce new TBDs or [], either postpone, or technically endorse, or change to no longer add new TBDs or [].
    - Discuss, if [] can be removed and TBDs can be replaced in the draftCRs endorsed last meeting.
    - Change all remaining [TBD] to TBD.
    - Consider removing requirements with remaining TBD.
  + For PUSCH in particular: Do not introduce minimum CBW requirements in CRs this meeting.

**Issue 2-4-2: HST test setup figures and test tolerances**

* Proposals
  + Option 1 (Nokia): Verify if further HST PUSCH additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272.
* Recommended WF
  + Test specification CR authors to verify the need for new measurement setup figures and TTs.
    - Remark: LTE has re-used the measurement setup figure for PRACH in PRACH HST (TS 36.141 I.3.2) by adding “HST” to heading and caption, as well as adding a note.   
      Please work together with the PUSCH test specification CR authors.  
      LTE also added new PRACH HST TTs (36.141 G.3).
  + Other delegates to check, if the additions in the CR are technically correct and sufficient.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| XXX | Issue 2-1-1:  Issue 2-1-2:  ….  Others: |
| Ericsson | **Issue 2-1-1: TDLC300-100 propagation conditions for long preamble formats**  Agree with Option 2. Similar to the discussion on HST PUSCH, at the first, we don’t think multi-path fading is a typical HST scenario. At the second, the proposed multi-path fading channel test cases have already been included in the normal modes, i.e., the long format 0 multi-path fading test configurations are the same for normal mode and HST scenario. To be specific, the performance difference is quite negligible that the allowed range size for ideal results from different companies is even larger.  **Issue 2-2-1: PRACH high speed support declaration for HST**  We can go for Option 2. It would be better to declare separately to avoid too many “and/or”. But “high speed mode” could be “high speed train”?  **Issue 2-3-1: Table organization of high-speed train requirement sections for PRACH 350kph in specifications**  It just to clarify which long format is used in the table.  **Issue 2-3-2: High speed support declaration 350kph PRACH - Explicit format-speed mapping**  Since our agreements on “No implicit test passing for HST PRACH” is stated by speed, then it will cause confusion about the PRACH format and the speed. It would be good to modify the wording of “No implicit test passing for HST PRACH” to “format” based.  **Issue 2-3-3: High speed support declaration 350kph PRACH - 350kph short format requirements**  An interesting scenario will be a BS only supporting short format could not declare the support of 350kph since there is no corresponding requirement. In another words, how to handle a BS can pass 350km/h HST PUSCH test but only support short format? Yes, it is discussed in the last meetings, but it seems have no good solution for this situation. We don’t have strong opinion to introduce this requirement. We just want to bring up this question again and wait for a better explanation and solution from companies.  **Issue 2-3-4: Section organization of high-speed train requirements for PRACH in specifications**  We can agree with Option 2 after second thinking.  **Issue 2-4-2: HST test setup figures and test tolerances**  Similar to HST PUSCH, we need further check. But for now, we don’t think new TTs are needed. |
| CMCC | Issue 2-1 (exactly, it is Issue 2-2-1): Option 1a, which is aligned with the agreements in the last meeting.  Issue 2-3-3: we are OK with option 1. |
| ZTE | Issue 2-1-1 TDLC300-100 for long preamble formats  In our views, Option 1 and 2 are the same, which is our preference.  Issue 2-2-1 PRACH high speed support declaration for HST  For declaration, Option 3 is the simplest solution and with future proof when more speeds are added. The tricky part is for HST PRACH since requirements with different preamble formats are specified for different speeds, so our proposal is to take this option for declaration, but for test applicability for HST PRACH we can exclude implicit tests for HST PRACH for 350km/h and 500km/h. In other words, if maximum supported speed is declared to be 500km/h, an additional tests for HST PRACH are required for 350km/h.  Issue 2-3-1 Table organization of HST requirement sections for PRACH 350kph in specs.  Indicating which exact long format preamble is more clear, so Option 1 is ok to us.  Issue 2-3-2 High speed support declaration 350kph PRACH – explicit format-speed mapping  Clarifying format-speed mapping is helpful.  Issue 2-3-3 High speed support declaration 350kph PRACH – 350kph short format requirements  For the time being, we don’t see the necessity of adding 350kph short format requirements (Option 2).  Issue 2-3-4 Section organization of HST requirements for PRACH in specs  We agree with Ericsson’s observation that there may be a confusion on multi-path fading channel.  Issue 2-4-1 Removal of TBD and []  WF recommended by Moderator seems reasonable to us.  Issue 2-4-2 HST test setup figures and test tolerances  WF recommended by Moderator seems reasonable to us. |
| Nokia, Nokia Shanghai Bell | **Issue 2-1-1: TDLC300-100 propagation conditions for long preamble formats**  Following Huawei’s contribution [R4-2007207] we were surprised to learn about possible issues with choosing restricted sets, resulting in performance gaps of up to 1.5dB. Hence we remove our support for “not define”, albeit we still prefer to not define. In case TDLC is specified, it should be in the HST section, as we previously decided to split HST and non-HST along feature lines, and not along speed lines.  **Issue 2-2-1: PRACH high speed support declaration for HST**  Since we decided in the previous meeting to split HST and non-HST along feature lines, and not along speed lines, it seems logical to us also split the declaration. This will also make it easier to read, as we don’t merge different features in one declaration.  The request from Ericsson to capture the “0” for long format 0 seems reasonable to us.  **Issue 2-3-1: Table organization of high-speed train requirement sections for PRACH 350kph in specifications**  Both options are fine for Nokia.  **Issue 2-3-2: High speed support declaration 350kph PRACH - Explicit format-speed mapping**  We are fine with both options. We would request to have a text proposal from Ericsson on how option 1 is to be captured.  **Issue 2-3-3: High speed support declaration 350kph PRACH - 350kph short format requirements**  We object to having short format requirements for 350kph. We have previously explicitly agreed to not have such requirements. During simulation delivery and the surround discussions, it was also generally recognized that short format PRACH is not an issue at 500kph. Any BS that supports short formats should not have an issue to achieve 500kph, thus fallback to 350kph is not necessary.  **Issue 2-3-4: Section organization of high-speed train requirements for PRACH in specifications**  Nokia thinks that the previous agreement should be upheld, until a specific conflict is identified. In which case we can re-examine the previous agreement. However, we don’t expect for such a scenario to arise.  **Issue 2-4-1: Removal of TBD and []**  Each CR should be considered separately in the corresponding section of this document. But the recommended WF seems like a good starting point for this evaluation.  **Issue 2-4-2: HST test setup figures and test tolerances**  Each CR should be considered separately in the corresponding section of this document. But the recommended WF seems like a good starting point for this evaluation. |
| Huawei, HiSilicon | **Issue 2-1-1: TDLC300-100 propagation conditions for long preamble formats**  Still prefer Option 2. It is not practical scenario for NR HST.  **Issue 2-1: PRACH high speed support declaration for HST**  By considering the declaration proposal in Topic #1 for PUSCH requirements, overall our proposals are as following:   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | High speed train | Declaration of high speed train scenario support. | x | x | | D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x | | D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |   Additionally test applicability for long PRACH format restricted set type A and B needs to be defined if BS supports both types:   |  | | --- | | 8.1.2.1.x Applicability of requirements for different restricted set types of long PRACH format 0  Unless otherwise stated, PRACH requirement tests for long PRACH format 0 with restricted set Type A and B shall apply only for the restricted set type declared to be supported (see D.110 in table 4.6-1). If both restricted set type A and type B are declared to be supported, the tests shall be done for type B; the same chosen mapping type shall then be used for all tests. |   **Issue 2-3-1: Table organization of high-speed train requirement sections for PRACH 350kph in specifications**  Considering that restricted sets type A and type B are applicable for several long PRACH formats: format 0/1/2/3, it is ok for us to add format 0 to avoid confusion.  **Issue 2-3-2: High speed support declaration 350kph PRACH – Explicit format-speed mapping**  By using our proposal about the declaration, no need for explicit format-speed mapping.  **Issue 2-3-3: High speed support declaration 350kph PRACH – 350kph short format requirements**  Keep previous agreements: No additionally define 350k/h related requirements for short PRACH formats. Especially the implicitly testing for 350km/h and 500km/h.  **Issue 2-3-4: Section organization of high-speed train requirements for PRACH in specifications**  Keep previous agreements. No need to delay this agreed part because of undecided issues for other test cases.  Issue 2-4-2:  As per the agreed work split, Huawei is responsible for this part work, we are sorry for missing this part, based on our current investigation, we think that the existing “Measurement system and set-up” defined in TS 38.141-1 Annex D.5 and D.6 can be reused for HST. Discussion about TT = 0.3dB is needed. If agreements can be reached during this meeting, either prepare CR during this meeting or for next meeting is fine for us. |
|  |  |
|  |  |
|  |  |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| R4-2007204 (Huawei) | [Moderator]: - Please observe the outcome of the chair guidance captured and discussed in sub-topic 2-4. |
| Ericsson   * Cover sheet:   + rev should be “-“   + category should B   “RAN4” should be “R4” |
|  |
| R4-2007204 (Huawei) | Ericsson: same as R4-2007204, could delete the void tables as well? |
| Company B |
|  |
| R4-2007206 (Huawei) | Ericsson: same as R4-2007204 |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #3: UL timing adjustment requirements (6.17.2.2.3)

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

This section contains T-docs with corresponding proposals and observations submitted to the agenda item “6.17.2.2.3 UL timing adjustment requirements”, as well as, any UL timing adjustment requirement related observations and proposals submitted to other agenda items.

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-20xxxxx | Company A | Proposal 1:  Observation 1: |
| R4-2006266 | CATT | PUSCH UL TA  **Proposal 2: For PUSCH UL TA, it is proposed to declare category of supported maximum speed (Option 1).**   * Option 1: If 500kph UL TA scenarios are defined, Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested.   **Proposal 3: No declaration for scenario X is needed (Same approach as LTE) (Option 3)**   * Option 3: No declaration for scenario X is needed. (Same approach as LTE).   **Proposal 4: If UL TA and PUSCH high speed declaration possibilities match, then they should be shared between PUSCH UL TA and PUSCH HST (Option 2).**   * Option 2: If UL TA and PUSCH high speed declaration possibilities match, then they should be shared between PUSCH UL TA and PUSCH HST. |
| R4-2006267 | CATT | UL TA  **Proposal 2: Do not specify scenario “X” (Option 3).**  Option 3: Do not specify scenario “X”. |
| R4-2006270 | CATT | Moderator: CR  PUSCH UL TA   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | x | x | |
| R4-2006271 | CATT | Moderator: CR  PUSCH UL TA   |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | D.109 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | c | x | n/a | |
| R4-2006769 | CMCC | UL TA additional scenario “X”  **Proposal 2: for UL timing adjustment, it is proposed to specify requirements for scenario X, and no declaration for scenario X is needed.** |
| R4-2006666 | ZTE Wistron Telecom AB | Manufacturer declaration maximum supported speed for HST  **Proposal 1: Introduce a new declaration item (Option 1) shown in Table -1.**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x | |
| R4-2006056 | Nokia, Nokia Shanghai Bell | Organization of HST requirements for UL TA 500kph in specs  Observation 1: High speed scenarios over 250kph should be captured together.  **Proposal 1: RAN4 to** **capture the 500kph UL TA scenario in the same table as the 350kph UL TA scenario.**  High speed support declaration  Observation 2: In RAN4#94-bis-e, there was a general consensus for option 1 captured in the 2nd round summary.  **Proposal 2: RAN4 to adapt the following high speed support declaration for UL TA: If 500kph UL TA scenarios are defined, Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested.**  High speed support declaration and applicability for 120kph HST UL TA  Observation 3: It is our general understanding that UL TA requirements for 120kph are applicable to all BS, even those that do not support high speed train. In this case, option 2 and 3 are equal.  **Proposal 3: RAN4 to agree that scenario X (120kph) needs to be tested independently of the [PUSCH UL timing alignment high speed train support] manufacturer declaration.**  Re-use of high speed support declaration for HST UL TA  Observation 4: Both options, re-use of PUSCH declaration and separate UL TA support declaration, technically feasible. Neither impacts the BS test procedure negatively.  Additional scenario X  N/A  Additional SCS/CBW combinations  **Proposal 4: RAN4 to not add new SCS/CBW combinations for UL TA, as the performance does not sufficiently differ.**  Agreeing on SNR values  **Proposal 5: Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the UL TA CRs.**  HST test setup figures and TTs  Observation 6: RAN4 should verify, if HST UL TA additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272. |
| R4-2006255 | CATT | Moderator: CR TS 38.141-2 |
| R4-2006256 | CATT | Moderator: CR TS 38.141-2 |
| R4-2006257 | CATT | Moderator: Simulation results.  **Proposal 1: add 500kph UL TA scenraio Z to simulation results summary.** |
| R4-2006269 | CATT | Requirement organization  **Proposal 1: Requirements for different scenarios can be organised in the same table (Option 1).**  Additional simulation assumptions  **Proposal 2: Add simulation assumptions for 5MHz CBW/15KHz SCS and 10Mhz CBW/30KHz SCS to simulation summary for agreed UL timing adjustment scenarios (Option 1)** |
| R4-2006321 | Samsung | Moderator: CR TS 38.141-1 |
| R4-2006322 | Samsung | Moderator: CR TS 38.141-1 |
| R4-2006324 | Samsung | Organization of UL timing requirement  **Proposal 1: Captured the requirements for different scenarios in separable tables**  High speed support declaration for HST UL TA  **Proposal 2: If 500kph UL TA scenarios are defined, Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested**  High speed support declaration and applicability for 120kph HST UL TA  **Proposal 3: No requirement for UL TA requirement for scenario X.**  **Proposal 4: No declaration for scenario X is needed.**  Additional SCS/BW combinations  **Proposal 5: No additional SCS/BW combinations are required for UL TA requirement.** |
| R4-2006664 | ZTE Wistron Telecom AB | Moderator: CR TS 38.104 |
| R4-2006665 | ZTE Wistron Telecom AB | Organisation of high-speed train requirement sections for UL TA 500kph in specifications  **Proposal 1: Capture requirements for different scenarios in the same table (Option 1).**  High speed support declaration for HST UL TA  **Proposal 3: New declaration item “Maximum supported speed” can override the declaration of 120kph, no separate declaration for 120kph (Option 3).**  Re-use of high speed support declaration for HST UL TA  **Proposal 4: The new declaration item “Maximum supported speed” should cover HST PUSCH, HST PRACH and UL TA (Option 1).**  Additional SCS/CBW combinations and New scenario X  **Proposal 5: Neither introduce new scenario X (option 3), nor any additional SCS/CBW combinations (Option 2).** |
| R4-2006835 | Ericsson | Organisation of high-speed train requirement sections for UL TA 500kph in specifications  **Proposal 1: Agree with Option 1 to capture different scenarios requirements in same table.**  High speed support declaration for HST UL TA  **Proposal 2: Agree with Option 1 to declare by the supported maximum speed, 350kph or 500kph (or no HST support), and 350kph does not need to be tested if 500kph test is passed.**  New scenarios  **Proposal 3: Do not include Scenario X in the scope of HST scenario discussion.**  Additional SCS/CBW combinations  **Proposal 4: Agree with Option 1 to add requirements for 5MHz CBW/15kHz SCS and 10MHz CBW/30kHz SCS for agreed UL TA scenarios.** |
| R4-2007186 | NTT DOCOMO, INC. | Organization of HST requirements for UL TA 500kph in specs  **Proposal 1: RAN4 adopts Option 1 or 2 based on pros and cons consideration.**  Declaration  Thus, we prefer to declare category of supported design target speed for HST UL TA and to share the declaration with PUSCH HST.  **Proposal 1: Allow to declare category of supported design target speed(s) from “no HST”, “HST for 350km/h”, “HST for 500km/h” or “HST for both 350km/h and 500km/h” and introduce the following declaration:**   | Declaration identifier | Declaration | Description | Applicability | | | | --- | --- | --- | --- | --- | --- | | *BS type 1-C* | *BS type 1-H* | *BS type 1-O* | | D.1xx | PUSCH for HST | Declaration of the supported HST scenarios: no HST, HST for 350km/h, HST for 500km/h or HST for both 350km/h and 500km/h. | x | x | x |     Scenario X for UL timing adjustment  **Proposal 3: RAN4 introduces UL timing adjustment requirements under scenario X without any applicability rules (Option 1).**  **Proposal 4: No declaration for Scenario X is needed (Option 3).**  Channel bandwidth  **Proposal 5: RAN4 introduces the PUSCH UL TA performance requirements for 5/10MHz CBW with 15kHz SCS and 10/40MHz CBW with 30kHz SCS (Option 1).** |
| R4-2007232 | Huawei, HiSilicon | Organization of HST requirements for UL TA 500kph in specs  **Proposal 1: Requirements for different scenarios captured in same table for UL TA.**  High speed support declaration  **Proposal 2: Choose Option 1, i.e. For UL TA, declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested.**  Re-use of high speed support declaration for HST UL TA  **Proposal 3: No need to introduce new declared item.**  New scenarios  **Proposal 4: Do not specify scenario “X”.**  Additional SCS/CBW combinations  **Proposal 5: Option 2, i.e. No additional SCS/CBW combinations are required for UL TA requirements.** |

## Open issues summary

*Before e-Meeting, moderators shall summarize list of open issues, candidate options and possible WF (if applicable) based on companies’ contributions.*

### Sub-topic 3-1: UL TA additional scenario “X”

*Sub-topic description:*

In RAN4#94-bis-e several additional UL TA requirements were discussed, but not agreed upon, e.g., new scenarios:

|  |
| --- |
| * New scenarios   + Option 1: Additionally, specify scenario “X”, with the following parameters: 15KHz SCS: A= 10us, Δω =0.04 s-1; 30KHz SCS: A= 5us, Δω =0.08 s-1.   + Option 2: Additionally, specify scenario “X”, with the following parameters: 15KHz SCS: A= 10us, Δω =0.04 s-1; 30KHz SCS: A= 5us, Δω =0.08 s-1. with the applicability rule: BS can declare support for either [no HST/default/no declaration], [350kmp] or [500kmp]. If BS declare supporting of 500km/h，only scenario Z is considered. If BS declare supporting of 350km/h，only scenario Y is considered. If BS declare [no HST/default/no declaration], scenario X is considered.   + Option 3: Do not specify scenario “X”. |

*Open issues and candidate options before e-meeting:*

**Issue 3-1-1: Additional scenario “X”**

* Proposals
  + Option 1 (DoCoMo, CMCC): Specify requirements for scenario X.
  + Option 2 (Huawei, Ericsson, ZTE, Samsung, CATT): Do not specify scenario “X”.
* Recommended WF
  + Collect further company views during 1st round.  
    Please give feedback on how strong the respective request is.
  + Deprioritize the following issues that rely on a decision here.

**Issue 3-1-2: Scenario “X” implicit test passing**

* Conditions
  + Additional scenario “X” is introduced.
  + Support for scenario “X” is not explicitly declared.
* Proposals
  + Option 1 (Nokia, CMCC, CATT, Ericsson): No implicit test passing.  
    The requirements for scenario “X” need to be tested, independent of passing requirements for “Y” or “Z”.
  + Option 2 (ZTE): Allow implicit test passing.  
    The requirements for scenario “X” do not need to be tested, only if the requirements for “Y” **or** “Z” have been passed.
  + Option 3 (Huawei): Postpone after 3-1-1.
* Recommended WF
  + Collect further company views during 1st round.

### Sub-topic 3-2: UL TA additional SCS/CBW

*Sub-topic description:*

In RAN4#94-bis-e several additional UL TA requirements were discussed, but not agreed upon, e.g., additional SCS/CBW combinations:

|  |
| --- |
| * Additional SCS/CBW combinations   + Option 1: Add simulation assumptions for 5MHz CBW/15KHz SCS and 10Mhz CBW/30KHz SCS to simulation summary for agreed UL timing adjustment scenarios   + Option 2: No additional SCS/CBW combinations are required for UL TA requirements. |

*Open issues and candidate options before e-meeting:*

**Issue 3-2-1: Additional SCS/CBW combinations**

* Proposals
  + Option 1 (DoCoMo, Ericsson, CATT, CMCC): Add simulation assumptions for 5MHz CBW/15KHz SCS and 10Mhz CBW/30KHz SCS to requirements for agreed UL timing adjustment scenarios
  + Option 2 (Huawei, ZTE, Samsung, Nokia): No additional SCS/CBW combinations are required for UL TA requirements.
  + Option 3 (Nokia): Add simulation assumptions for 5MHz CBW/15KHz SCS and 10Mhz CBW/30KHz SCS to requirements for agreed UL timing adjustment scenarios and use applicability rule to only test supported SCS/CBW combinations.
* Recommended WF
  + Collect further company views during 1st round.  
    Please give feedback on how strong the respective request is.

### Sub-topic 3-3: UL TA applicability rules

*Sub-topic description:*

In RAN4#94-bis-e it was not agreed how to handle the applicability rules 120kph UL TA:

|  |
| --- |
| * High speed support declaration and applicability for 120kph HST UL TA (Pending on decision on Scenario X)   + Option 1: If performance requirement for scenario X is defined, the corresponding performance requirements should be tested when BS declares to support scenario X.   + Option 2: BS can declare support for either [no HST/default/no declaration], [350kmp] or [500kmp]. If BS declare [no HST/default/no declaration], scenario X is considered.   + Option 3: No declaration for scenario X is needed. (Same approach as LTE). |

*Open issues and candidate options before e-meeting:*

**Issue 3-3-1: Applicability for 120kph HST UL TA**

* Proposals
  + Option 1 (DoCoMo): No applicability rule is needed.
  + Option 2 (ZTE): Hold on until the decision on “X” is made.
* Recommended WF
  + Deprioritise until introduction of scenario “X” (issue 3-1-1) is decided.  
    Collect further company views during 1st round.

### Sub-topic 3-4: Manufacturer declaration

*Sub-topic description:*

In RAN4#94-bis-e it was not agreed how to declare high speed support for UL TA:

|  |
| --- |
| * High speed support declaration for HST UL TA   + Option 1: If 500kph UL TA scenarios are defined, Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested.   + Option 2: If 500kph UL TA scenarios are defined, Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported, both 350kph and 500kph need to be tested for compliance.   + Option 3: If 500kph UL TA scenarios are defined, Declare category of supported design target speed(s). This can be 350 or 500 or 350&500kph (or no HST support).  Only the corresponding requirements are tested. |

Furthermore, it is also open how to declare support for 120kph UL TA:

|  |
| --- |
| * High speed support declaration and applicability for 120kph HST UL TA (Pending on decision on Scenario X)   + Option 1: If performance requirement for scenario X is defined, the corresponding performance requirements should be tested when BS declares to support scenario X.   + Option 2: BS can declare support for either [no HST/default/no declaration], [350kmp] or [500kmp]. If BS declare [no HST/default/no declaration], scenario X is considered.   + Option 3: No declaration for scenario X is needed. (Same approach as LTE). |

*Open issues and candidate options before e-meeting:*

**Issue 3-4-1: UL TA supported speed declaration for 120kph/Scenario X**

* Proposals
  + Option 1 (Nokia, CMCC, CATT, Ericsson): No declaration for scenario X is needed; testing scenario X is always required.
  + Option 2 (Samsung): No declaration for scenario X is needed; no requirements for scenario X.
  + Option 3 (ZTE): No declaration for scenario X is needed; testing scenario X is only required, if 350 or 500kph UL TA is not declared to be supported (“overwritten”).
  + Option 3 (Huawei): Postpone to after 3-1-1.
* Recommended WF
  + Proposed agreement:   
    No explicit declaration for scenario X.
  + Proposed WF (deprioritised until introduction of scenario “X” decided):   
    Companies are encouraged to give feedback on Issue 3-1-2: Scenario “X” implicit test passing to answer the second part of the proposals.

**Issue 3-4-2: UL TA supported speed declaration for [120kph], 350kph, and 500kph**

* Proposals
  + Option 1a (CATT, Ericsson, Nokia, CMCC, Samsung): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support).   
    If 500kph is supported and successfully tested, then 350kph does not need to be tested.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | Supported maximum speed | Declaration of supported maximum speed (i.e. 350km/h, 500km/h) for PUSCH and UL timing adjustment for HST. | x | x |

* + Option 1b (ZTE): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support).   
    If 500kph is supported and successfully tested, then 350kph does not need to be tested.  
    Shared for PUSCH/PRACH/UL TA.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | Maximum supported speed for High Speed Train | Declaration of the maximum supported speed for High Speed Train scenarios. The declaration is chosen from the set {No HST support, 350 km/h, 500 km/h} and applicable to HST PUSCH, UL TA and HST PRACH. Speed(s) less than the declaration shall also be supported under this declaration. | x | x |

* + Option 1c (Ericsson, Samsung, Nokia, CMCC, ZTE): Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support).   
    If 500kph is supported and successfully tested, then 350kph does not need to be tested.
  + Option 1d (Huawei): Declare category of supported maximum speed. This can be either 350km/h or 500km/h. Only the corresponding requirements are tested.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D.108 | High speed train | Declaration of high speed train scenario support. | x | x |
| D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x |
| D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |

* + Option 2 (DoCoMo): Declare category of supported design target speed(s) from “no HST”, “HST for 350km/h”, “HST for 500km/h” or “HST for both 350km/h and 500km/h” and introduce the following declaration:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| D.1xx | PUSCH for HST | Declaration of the supported HST scenarios: no HST, HST for 350km/h, HST for 500km/h or HST for both 350km/h and 500km/h. | x | x | x |

* Recommended WF
  + Proposed agreement:  
    Declare category of supported maximum speed. This can be either 350 or 500kph (or no HST support). If 500kph is supported and successfully tested, then 350kph does not need to be tested.
  + Proposed WF:   
    Companies are encouraged to give feedback on which declaration wording option they see as best or propose new exact wording options.

**Issue 3-4-3: Re-use of high speed declaration for UL TA**

* Proposals
  + Option 1 (Nokia): No re-use. Independent support declaration for UL TA.
  + Option 2 (Huawei, DoCoMo, CATT, Nokia, Ericsson, CMCC, ZTE, Samsung): Re-use of the PUSCH HST declaration, if they match.
  + Option 3 (ZTE): Re-use of a common HST declaration for PUSCH/UL TA/PRACH.
* Recommended WF
  + Proposed agreement:  
    Re-use of the PUSCH HST declaration for UL TA, if they match.
  + Proposed WF:  
    Come back to this topic once the final wording for PUSCH declaration decided.  
    Take proposed PUSCH/UL TA re-use into account, when decision PUSCH declaration wording.

### Sub-topic 3-5: Specification writing

*Sub-topic description*

With the UL TA requirement organization and simulation contributions having become quite stable, RAN4 can go ahead and finalize the specifications.  
However, it remains to verify the additional need for additions for HST in the measurement set-up and test tolerance definition.

Additionally, the cleaning of the specification TS 38.**104** ahead of ITU submission, will have an impact on the HST UL TA CR treatment in this meeting, as indicated in the following guidance provided by the RAN4 Chair (Steven) and Demod co-chair (Haijie) to the moderators of the relevant email discussions:

[See email in sub-topic 1-6.]

Furthermore, in RAN4#94-bis-e, no conclusion was reached with respect the organization of HST requirements for UL TA 500kph in specs [2]:

|  |
| --- |
| * Organisation of high-speed train requirement sections for UL TA 500kph in specifications.   + Option 1: Requirements for different scenarios captured in same table.   + Option 2: Requirements for different scenarios captured in separate tables. |

*Open issues and candidate options before e-meeting:*

**Issue 3-5-1: Organization of HST requirements for UL TA 500kph in specifications**

* Proposals
  + Option 1 (Huawei, DoCoMo, ZTE, CATT): Requirements for different scenarios captured in same table.
  + Option 2 (DoCoMo, Samsung): Requirements for different scenarios captured in separate tables.
  + Option 3 (Nokia, Ericsson, Samsung[second choice]): Capture the 500kph UL TA scenario in the same table as the 350kph UL TA scenario.
* Recommended WF
  + Collect further company views during 1st round.  
    Explore if compromise to option 1 is possible.

**Issue 3-5-2: Removal of TBD and []**

* Proposals
  + Option 1 (Nokia): Agreeing on SNR values.  
    Unless new simulation results are received, capture the SNR values summarized in R4-2005573 in the UL TA CRs
  + Option 2: (RAN4 chair and demod session chair):   
     Submitted TS 38.104 CRs could be technically endorsed.  
     Submitted TS 38.141-1/2 CRs could be agreed.  
     Try to resolve TBDs and [].
  + Option 3 (Huawei)  
    Firstly check if some companies have plan to submit new results or update their results in next meeting, if no, just agree CRs endorsed in last meeting and add SNR the requirements based on the latest results summary. All other newly submitted CRs for this meeting can only be endorsed if agreeable.
* Recommended WF
  + Do not agree TS 38.104 CRs that introduce new TBDs or [], either postpone, or technically endorse, or change to no longer add new TBDs or [].
    - Discuss, if [] can be removed and TBDs can be replaced in the draftCRs endorsed last meeting.
    - Change all remaining [TBD] to TBD.
    - Consider removing requirements with remaining TBD.

**Issue 3-5-3: HST test setup figures and test tolerances**

* Proposals
  + Option 1 (Nokia): Verify if further HST UL TA additions to “Measurement of performance requirements” (TT definitions in TS 38.131-1/2 appendix C.3) and “Measurement system set-up” for “performance requirements” (appendix D) are required; similar to R4-2003272.
* Recommended WF
  + Test specification CR authors to verify the need for new measurement setup figures and TTs.
    - Remark: LTE has separate measurement setup figure (TS 36.141 I.3.4) and TTs (36.141 G.3) for UL TA.
    - Remark: The initially submitted CR for TS 38.141-2 (R4-2006256) has proposed a new figure for measurement setup for UL TA.
  + Other delegates to check, if the additions in the CR are technically correct and sufficient.

### Sub-topic 3-6: Simulation summary management

*Sub-topic description*

*Open issues and candidate options before e-meeting:*

**Issue 3-6-1: Additional SCS/CBW combinations in the simulation summary**

* Proposals
  + Option 1 (CATT): Add 500kph UL TA scenario Z to simulation results summary.
* Recommended WF
  + Add 500kph UL TA scenario Z to simulation results summary.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| XXX | Issue 3-1-1:  Issue 3-1-2:  ….  Others: |
| Ericsson | **Issue 3-1-1: Additional scenario “X”**  Option 2. Since scenario X is not a HST scenario.  **Issue 3-1-2: Scenario “X” implicit test passing**  Option 1.  **Issue 3-4-1: UL TA supported speed declaration for 120kph/Scenario X**  Agree with Option 1, but we think scenario X requirement is a normal scenario and should not be included in HST discussion.  **Issue 3-4-2: UL TA supported speed declaration for [120kph], 350kph, and 500kph**  Agree with Option 1a for now.  **Issue 3-4-3: Re-use of high speed declaration for UL TA**  Can agree with Option 2.  **Issue 3-5-1: Organization of HST requirements for UL TA 500kph in specifications**  Agree with Option 3 since it looks clearer and is aligned with PUSCH.  **Issue 3-5-3: HST test setup figures and test tolerances**  We need further check. But for now, we don’t think new TTs are needed. |
| CMCC | Issue 3-1-1: Considering the channel model of scenario X is different from scenario Y and scenario Z, it is necessary to introduce scenario X.  Issue 3-1-2: option 1. In LTE, requirements are specified for scenario X and no declaration for scenario X. We would like to know the reason why in Rel-15, scenario X is not considered for NR.  Issue 3-2-1: OK with option 1  Issue 3-4-2: it seems that option 1a and option 1c are the same? We are OK with both.  Issue 3-4-3: we are OK with option 2. |
| ZTE | Issue 3-1-1 Additional scenario “X”  Option 2  Issue 3-1-2 “X” implicit test passing  Option 2.  Issue 3-2-1 Additional SCS/CBW combinations  Option 2.  Issue 3-3-1 Applicability for 120kmph HST UL TA  Hold on until the decision on “X” is made.  Issue 3-4-1 UL TA supported speed declaration for 120kmph/Scenario X  Option 3 is simple and future proof.  Issue 3-4-2 UL TA supported speed declaration for [120],350, 500  Option 1c is simple and future proof.  Issue 3-4-3 Re-use of high speed declaration for UL TA  Option 2 and 3 are similar for ULTA, which is our preference.  Issue 3-5-1 Organization of HST requirements for UL TA 500kmph in specs  Option 1.  Issue 3-5-2 Removal of TBD and []  WF recommended by Moderator is reasonable.  Issue 3-5-3 HST test setup figures and test tolerances  WF recommended by Moderator is reasonable. |
| Samsung | **Issue 3-1-1: Additional scenario “X”**  Option 2. Didn’t see the benefit and necessity of introduce additional test case for scenario X.  **Issue 3-1-2: Scenario “X” implicit test passing**  Suggest to defer the discussion and pending on issue 1-3-1.  **Issue 3-2-1: Additional SCS/CBW combinations**  Prefer option 2. No additional test considering work load.  **Issue 3-4-2: UL TA supported speed declaration for [120kph], 350kph, and 500kph**  Support option 1a/1c. we didn’t see the logic if BS declared support 500km/h why such BS cannot support 300km/h. Performance optimization around certain point is BS implementation issues which out of RAN4 scope, RAN4 define minimum performance requirements which assumed no specific optimization. Meanwhile from test aspect, we also didn’t see the necessity to require BS pass both 350km/h and 500km/h test cases, as 500km/h related test cases should be choosed.  **Issue 3-4-3: Re-use of high speed declaration for UL TA**  Can agree with Option 2.  **Issue 3-5-1: Organization of HST requirements for UL TA 500kph in specifications**  Agree with option 2, option 3 also fine for us considering to keep consistent with PUSCH requirements. |
| Nokia, Nokia Shanghai Bell | **Issue 3-1-1: Additional scenario “X”**  No strong opinion from our side, we have a slight preference for option 3, but we can compromise option 1.  **Issue 3-1-2: Scenario “X” implicit test passing**  It is our general understanding that UL TA requirements for 120kph are applicable to all BS, even those that do not support high speed train. As such we don’t think that scenario X is in the same category of BS implementations as HST. And thus, it should need to be tested in all cases. Hence, no implicit test passing (option 1).  **Issue 3-2-1: Additional SCS/CBW combinations**  The UL TA implementation and performance should not differ between SCS/CBW combinations; hence we do not need additional requirements/tests. However, under the condition that there will be an applicability rule to only test supported SCS/CBWs, our opinion on this topic is not very strong.  **Issue 3-3-1: Applicability for 120kph HST UL TA**  We don’t agree with DoCoMo statement that no applicability rule is required. At least for SCS/CBW combinations an applicability rule is required. However, we agree with the our suspected intention of DoCoMo that no applicability rule is required w.r.t. being able to chose a single scenario to be tested, when more than one is declared to be supported.  **Issue 3-4-1: UL TA supported speed declaration for 120kph/Scenario X**  It is our general understanding that UL TA requirements for 120kph are applicable to all BS, even those that do not support high speed train. Hence no matter the declaration (including absent UL TA speed declaration), scenario X will need to be tested and, in particular, we don’t need a separate declaration for scenario X support.  **Issue 3-4-2: UL TA supported speed declaration for [120kph], 350kph, and 500kph**  Unlike for PUSCH, we don’t think that differing implementations can exist for UL TA command handling, that distinguish 500 from 350&500 kph deployed BS. Hence we agree with both option 1a and 1c.  **Issue 3-4-3: Re-use of high speed declaration for UL TA**  No strong opinion on this topic. Both option 1 and 2 are fine for us, assuming that PUSCH and UL TA declarations categories match formally.  **Issue 3-5-1: Organization of HST requirements for UL TA 500kph in specifications**  Option 1 and 3 are the same, assuming no scenario X introduced, or scenario X is taken to be a high speed requirement. To protect against the latter case, we proposed the wording of the agreement in option 3.  **Issue 3-5-2: Removal of TBD and []**  Each CR should be considered separately in the corresponding section of this document. But the recommended WF seems like a good starting point for this evaluation.  **Issue 3-5-3: HST test setup figures and test tolerances**  Each CR should be considered separately in the corresponding section of this document. But the recommended WF seems like a good starting point for this evaluation. |
| Huawei | **Issue 3-1-1: Additional scenario “X”**  We prefer Option 2. Do not specify scenario “X”. Fading channel with large Doppler is not the typical application scenario. We don’t see any necessary to introduce such scenario.  **Issue 3-1-2: Scenario “X” implicit test passing**  Discuss this issue after the agreement for Issue 3-1-1 is achieved.  **Issue 3-2-1: Additional SCS/CBW combinations**  We prefer Option 2. No additional SCS/CBW combinations are required for UL TA requirements. We do not think there is NR BS that only supports the smallest CBW of 5MHz/15kHz and 10MHz/30kHz SCS, and do not support the typical bandwidth of 10MHz/15kHz and 40MHz/30kHz.  **Issue 3-3-1: Applicability for 120kph HST UL TA**  Discuss this issue after the agreement for Issue 3-1-1 is achieved.  **Issue 3-4-1: UL TA supported speed declaration for 120kph/Scenario X**  Discuss this issue after the agreement for Issue 3-1-1 is achieved.  **Issue 3-4-2: UL TA supported speed declaration for [120kph], 350kph, and 500kph**  Same as Issue 1-5-1, we provide our declaration for HST.   |  |  |  |  |  | | --- | --- | --- | --- | --- | | D.108 | High speed train | Declaration of high speed train scenario support. | x | x | | D.109 | Maximum speed of high speed train for PUSCH | Declaration of supported maximum speed for high speed train scenario, i.e. 350 km/h or 500 km/h.  This declaration is applicable to PUSCH for high speed train and UL timing adjustment only if UE declares to support high speed train in D.108. | x | x | | D.110 | PRACH format for high speed train | Declaration of supported PRACH format(s) for high speed train scenario, i.e. format 0 restricted set type A, format 0 restricted set type B, format A2, format B4, format C2.  This declaration is applicable to HST PRACH only if UE declares to support high speed train in D.108. | x | x |   **Issue 3-4-3: Re-use of high speed declaration for UL TA**  We prefer Option 2. Re-use of the PUSCH HST declaration, if they match.  **Issue 3-5-1: Organization of HST requirements for UL TA 500kph in specifications**  We prefer Option 1 to make the specification more clear.  **Issue 3-5-2: Removal of TBD and []**  Same as Issue 1-6-1. Firstly check if some companies have plan to submit new results or update their results in next meeting, if no, just agree CRs endorsed in last meeting and add SNR the requirements based on the latest results summary. All other newly submitted CRs for this meeting can only be endorsed if agreeable.  **Issue 3-6-1: Additional SCS/CBW combinations in the simulation summary**  We agree with the recommended WF. |
|  |  |
|  |  |
|  |  |

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| R4-2006255 (CATT) | Ericsson:   * Cover sheet: Other specs impacted field should be filled in * Test procedure: We think the procedure is different for HST and we might need to deliver CR for this part according to our understand. * RB assignment and Starting PRB index: Adding SCS would make it clearer. |
| Company B |
|  |
| R4-2006256 (CATT) | Company A |
| Company B |
|  |
| R4-2006321 (Samsung) | Ericsson:   * Cover sheet: CR number is missing * Test procedure: We think the procedure is different for HST and we might need to deliver CR for this part according to our understand. |
| Company B |
|  |
| R4-2006322 (Samsung) | Ericsson: CR number is missing, and the TT value should be 0.6dB. |
| Company B |
|  |
| R4-2006664 (ZTE) | [Moderator]: - Please observe the outcome of the chair guidance captured and discussed in sub-topic 3-5. |
| Ericsson:   * Cover sheet: “RAN4” should be “R4” * Should not be highlighting for the changes. |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |