**3GPP TSG-RAN WG4 Meeting #96-eR4-201XXXXX**

Electronic Meeting, 17-28 Aug., 2020

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** | **0425** | **rev** | **1** | **Current version:** | **15.10.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.101-1: corrections on narrow band blocking for intra-band contiguous CA |
|  |  |
| ***Source to WG:*** | Xiaomi |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-08-07 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In the existing spec, the narrow band blocking for intra-band contiguous CA is specified only for the component carrier with 15 kHz SCS. This will case only 50MHz +50 MHz case can be tested for CA class C since there are no requirements for all other cases that one component carrier bandwidth is more than 50MHz. |
|  |  |
| ***Summary of change:*** | Add the interferer offset value for 30 kHz SCS case for narrow band blocking for CA bandwidth class C |
|  |  |
| ***Consequences if not approved:*** | The narrow band blocking for intra-band contiguous CA is incomplete. |
|  |  |
| ***Clauses affected:*** | 7.6A.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS38.521-1  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

## **--------------Start of change-------------**

### 7.6A.4 Narrow band blocking for CA

#### 7.6A.4.1 Narrow band blocking for Intra-band contiguous CA

For intra-band contiguous carrier aggregation, the downlink SCC(s) shall be configured at nominal channel spacing to the PCC. For FDD, the PCC shall be configured closest to the uplink band. All downlink carriers shall be active throughout the test. The uplink output power shall be set as specified in Table 7.6A.4.1-1 with the uplink configuration. For UE(s) supporting one uplink, the uplink configuration of the PCC shall be in accordance with Table 7.3.2-3. The UE shall fulfil the minimum requirement in presence of an interfering signal specified in Table 7.6A.4.1-1 being on either side of the aggregated signal. The throughput of each carrier shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in Annexes A.2.2, A.2.3, A3.2 and A.3.3 (with one sided dynamic OCNG Pattern OP.1 FDD/TDD for the DL-signal as described in Annex A.5.1.1/A.5.2.1) with parameters specified in Table 7.6A.4.1-1.

Table 7.6A.4.1-1: Narrow-band blocking for intra-band contiguous CA

|  |  |  |  |
| --- | --- | --- | --- |
| NR band | Parameter | Unit | NR CA bandwidth class |
| C |
| n41 | Pw in Transmission Bandwidth Configuration, per CC | dBm | REFSENS + NA CA Bandwidth Class specific value below |
| 16 |
| Puw (CW) | dBm | -55 |
| Fuw (offset for*f* = 15 kHz, 30 kHz) | MHz | - Foffset – 0.2/+ Foffset + 0.2 |
|  |  |  |
| NOTE 1: The transmitter shall be set a 4 dB below PCMAX\_L,f,c at the minimum UL configuration specified in Table 7.3.2-3 with PCMAX\_L,f,c defined in clause 6.2.4.NOTE 2: Reference measurement channel is specified in Annexes A.3.2 and A3.2 with one sided dynamic OCNG Pattern OP.1 FDD/TDD as described in Annex A.5.1.1/A.5.2.1.NOTE 3: The PREFSENS power level is specified in Table 7.3.2-1 and Table 7.3.2-2 for two and four antenna ports, respectively.NOTE 4: The Fuw (offset) is the frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer and shall be further adjusted to MHz to be offset from the sub-carrier raster. |

#### 7.6A.4.2 Void

## **-------------End of change-------------**