**3GPP TSG-RAN WG4 Meeting #96-e *R4-2012601***

**Electronic Meeting, 17- 28 Aug, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.141** | **CR** | **1271** | **rev** | **1** | **Current version:** | **16.6.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR: Introduce NPUSCH format 1 test requirements for multi-TB interleaved transmission for TS 36.141 |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NB\_IOTenh3-Perf |  | ***Date:*** | 2020-08-04 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | RAN 4 has agreed to introduce the performance requirements for NPUSCH format 1 with multi-TB interleaved transmission and WF R4-2008759 has been approved. |
|  |  |
| ***Summary of change:*** | 1. Add the new test requirments for NPUSCH format 1 with multi-TB interleaved transmission to clause 8.5.1.5.
2. Add the new FRC for NPUSCH format 1 related to this feature to clause

A.16.1 1. Add the appcability rules of the test requirements in clause 8.5.1.1
 |
|  |  |
| ***Consequences if not approved:*** | The performance requirements will still be incompleted |
|  |  |
| ***Clauses affected:*** | 8.5.1.5, A.16.1, 8.5.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*<Start of change>*

#### 8.5.1.1 Definition and applicability

The performance requirement of NPUSCH format 1 is determined by a minimum required throughput for a given SNR. The required throughput is expressed as a fraction of maximum throughput for the FRCs listed in Annex A. The performance requirements assume HARQ re-transmissions.

The tests for 3.75KHz subcarrier spacing are applicable to the base stations supporting 3.75 kHz subcarrier spacing requirements. The tests for single-subcarrier/multi-subcarrier of 15KHz subcarrier spacing are applicable to the base stations supporting the number of subcarriers of 15 kHz subcarrier spacing requirements.

The tests defined in Table 8.5.1.5-4 are applicable to the base stations supporting two HARQ processes, multiple TBs scheduling with interleaved transmission when multiple TBs are scheduled.

#### 8.5.1.5 Test Requirement

The throughput measured according to subclause 8.5.1.4.2 shall not be below the limits for the SNR levels specified in Table 8.5.1.5-1 for 3.75KHz subcarrier spacing tests, not be below the limits for the SNR levels specified in Table 8.5.1.5-2 for 15KHz subcarrier spacing with single subcarrier tests and not be below the limits for the SNR levels specified in Table 8.5.1.5-3 for 15KHz subcarrier spacing with the supported number of subcarrier tests.

Table 8.5.1.5-1 Required SNR for NPUSCH format 1 test, 200KHz Channel Bandwidth, 3.75KHz subcarrier spacing, 1Tx

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas | Number of RX antennas | Subcarrier spacing | Number of allocated subcarriers | Propagation conditions and correlation matrix (Annex B) | FRC(Annex A) | Repetition number | Fraction of maximum throughput | SNR[dB] |
| 1 | 2 | 3.75KHz | 1 | ETU 1Hz Low | A16-1 | 1 | 70% | -1.3 |
| 16 | 70% | -8.6 |
| 64 | 70% | -11.6 |

Table 8.5.1.5-2 Required SNR for NPUSCH format 1 test, 200KHz Channel Bandwidth, 15KHz subcarrier spacing, single subcarrier, 1Tx

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas | Number of RX antennas | Subcarrier spacing | Number of allocated subcarriers | Propagation conditions and correlation matrix (Annex B) | FRC(Annex A) | Repetition number | Fraction of maximum throughput | SNR[dB] |
| 1 | 2 | 15KHz | 1 | ETU 1Hz Low | A16-2 | 1 | 70% | -1.5 |
| 16 | 70% | -8.2 |
| 64 | 70% | -12 |

Table 8.5.1.5-3 Required SNR for NPUSCH format 1 test, 200KHz Channel Bandwidth, 15KHz subcarrier spacing, multiple subcarriers, 1Tx

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas | Number of RX antennas | Subcarrier spacing | Number of allocated subcarriers | Propagation conditions and correlation matrix (Annex B) | FRC(Annex A) | Repetition number | Fraction of maximum throughput | SNR[dB] |
| 1 | 2 | 15KHz | 3 | ETU 1Hz Low | A16-3 | 2 | 70% | -2.4 |
| 16 | 70% | -7.5 |
| 64 | 70% | -10.8 |
| 6 | ETU 1Hz Low | A16-4 | 2 | 70% | 0 |
| 16 | 70% | -6.2 |
| 64 | 70% | -9.9 |
| 12 | ETU 1Hz Low | A16-5 | 2 | 70% | -0.1 |
| 16 | 70% | -5.8 |
| 64 | 70% | -9.5 |

**Table 8.5.1.5-4: Required SNR for NPUSCH format 1 with two HARQ processes and multiple TBs with interleaved transmission**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Number of TX antennas | Number of RX antennas | Subcarrier spacing | Number of allocated subcarriers | Propagation conditions and correlation matrix (Annex B) | FRC(Annex A) | Repetition number | Fraction of maximum throughput | SNR[dB] |
| 1 | 2 | 15KHz | 12 | ETU 1Hz Low | A16-6 | 64 | 70% | [-13.3] |

NOTE: If the above Test Requirement differs from the Minimum Requirement then the Test Tolerance applied for this test is non-zero. The Test Tolerance for this test and the explanation of how the Minimum Requirement has been relaxed by the Test Tolerance is given in Annex G.

*<Next change>*

## A.16.1 One PRB

Table A.16.1-1: FRC parameters for NB-IoT NPUSCH format 1

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Reference channel | A16-1 | A16-2 | A16-3 | A16-4 | A16-5 | A16-6 |
| Subcarrier spacing (kHz) | 3.75 | 15 | 15 | 15 | 15 | 15 |
| Number of allocated subcarriers | 1 | 1 | 3 | 6 | 12 | 12 |
| Diversity | No | No | No | No | No | No |
| Modulation | BPSK | BPSK | QPSK | QPSK | QPSK | QPSK |
| ITBS / IRU | 0 / 1 | 0 / 1 | 3 / 0 | 7 / 0 | 9 / 0 | 5/4 |
| Payload size (bits) | 32 | 32 | 40 | 104 | 136 | 424 |
| Allocated resource unit | 2 | 2 | 1 | 1 | 1 | 5 |
| Code rate (target) | 1/3 | 1/3 | 1/3 | 1/3 | 2/3 | 1/3 |
| Code rate (effective) | 0.29 | 0.29 | 0.22 | 0.44 | 0.56 | 0.34 |
| Transport block CRC (bits) | 24 | 24 | 24 | 24 | 24 | 24 |
| Code block CRC size (bits) | 0 | 0 | 0 | 0 | 0 | 0 |
| Number of code blocks - C | 1 | 1 | 1 | 1 | 1 | 1 |
| Total number of bits per resource unit | 96 | 96 | 288 | 288 | 288 | 1440 |
| Total symbols per resource unit | 96 | 96 | 144 | 144 | 144 | 720 |
| Channel estimation length (ms) Note 1 | 16 | 4 | 4 | 4 | 2 (when repetition = 2)4 (when repetition > 2) | 4 |
| Note 1: Channel estimation lengths are included in the table for information only. |

*<End of change>*