**3GPP TSG-RAN WG4 Meeting # 97-e *R4-2016803***

**Electronic Meeting, 2 - 13 November, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** | **0498** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction on 5G V2X UE RF requirements in TS38.101-1 in rel-16 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | LG Electronics, Huawei, CATT | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core | | | | |  | ***Date:*** | | | 2020-10-17 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | This CR is to update UE-to-UE coexistence requirmeents for 5G V2X UE in TS38.101-1. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | This CR is to treat the Protect band list in UE-to-UE coexistence requirements for 5G NR V2X UE | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | NR V2X UE do not protect some adjacent UE with the additional NR operating band list. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.5.3.2, 6.5E.3.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-1 | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## *<< Start of changes >>*

#### 6.5.3.2 Spurious emissions for UE co-existence

This clause specifies the requirements for NR bands for coexistence with protected bands.

Table 6.5.3.2-1: Requirements for spurious emissions for UE co-existence

| NR Band | Spurious emission for UE co-existence | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| n1, n84 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 40, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76,  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 15, 27 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 15, 26, 27 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 15, 26, 27 |
| n2 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 43,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n3, n80 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 38, 39, 40, 41, 43, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73,74, 75, 76.  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 22, 42, 52,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n5, n89 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 18, 19, 24, 25, 26, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 50, 51, 53, 65, 66, 70, 71, 73, 74, 85  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 52,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n7 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 20, 22, 26, 27, 28, 29, 30, 31, 32, 33, 34, 40, 42, 43, 50, 51, 52, 65, 66, 67, 68, 72, 74, 75, 76, 85,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 15, 21, 26 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 15, 21, 26 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 15, 21 |
| n8, n81 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 52,  NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA 8 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n12 | E-UTRA Band 2, 5, 13, 14, 17, 24, 25, 26, 27, 30, 41, 48, 50, 51, 53, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 66, 70,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| n14 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 23, 24, 25, 26, 27, 29, 30, 41, 48, 53, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 769 | - | 775 | -35 | 0.00625 | 12, 15 |
| Frequency range | 799 | - | 805 | -35 | 0.00625 | 11, 12, 15 |
| n18 | E-UTRA Band 1, 3, 11, 21, 34, 42, 65  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 |  |
| Frequency range | 860 | - | 890 | -40 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| n20, n82 | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 33, 34, 40, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 38, 42, 52, 69,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| n25 | E-UTRA Band 4, 5, 10,12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 42, 48, 53, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 25 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 43,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n26 | E-UTRA Band 1, 2, 3, 4, 5, 10, 11, 12, 13, 14, 17, 18,19, 21, 24, 25, 26, 29, 30, 31, 34, 39, 40, 42, 43, 48, 50, 51, 53, 65, 66, 70, 71, 73,74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 15 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n28, n83 | E-UTRA Band 1, 4, 10, 22, 32, 42, 43, 50, 51, 52, 65, 66, 73, 74, 75, 76,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 19, 25 |
| E-UTRA Band 2, 3, 5, 7, 8, 18, 19, 20, 25, 26, 27, 31, 34, 38, 39, 40, 41, 72,  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 19, 24 |
| Frequency range | 470 | - | 694 | -42 | 8 | 15, 35 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 34 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 15 |
| Frequency range | 758 | - | 773 | -32 | 1 | 15 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8, 19 |
| n30 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 38, 41, 48, 53, 66, 70, 71, 85,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n34 | E-UTRA Band 1, 3, 7, 8, 11, 18, 19, 20, 21, 22, 26, 28, 31, 32, 33, 38,39, 40, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 69, 72, 74, 75, 76,  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n38 | E-UTRA Band 1, 2, 3, 4, 5, 8, 10, 12, 13, 14, 17, 20, 22, 27, 28, 29, 30, 31, 32, 33, 34, 40, 42, 43, 50, 51, 52, 65, 66, 67, 68, 72, 74, 75, 76, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2620 | - | 2645 | -15.5 | 5 | 15, 22, 26 |
| Frequency range | 2645 | - | 2690 | -40 | 1 | 15, 22 |
| n39 | E-UTRA Band 1, 8, 22, 26, 28, 34, 40, 41, 42, 44, 45, 50, 51, 52, 74,  NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 33 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 15, 26, 33 |
| n40 | E-UTRA Band 1, 3, 5, 7, 8, 20, 22, 26, 27, 28, 31, 32, 33, 34, 38, 39, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 74, 75, 76,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n41 | E-UTRA Band 1, 2, 3, 4, 5, 8, 10, 12, 13, 14, 17, 24, 25, 26, 27, 28, 29, 30, 34, 39, 42, 44, 45, 48, 50, 51, 52, 65, 66, 70, 71, 73, 74, 85,  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 8 |
| n47 | E-UTRA Band 1, 3, 5, 7, 8, 22, 26, 28, 34, 39, 40, 41, 42, 44, 45, 65, 68, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n71, n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n48 | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n50 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 65, 66, 67, 68 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n51 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 52, 65, 66, 67, 68, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n53 | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 48, 66, 70, 71, 85,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n65 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 40, 41, 42, 43, 50, 51, 65, 68, 69, 72, 74, 75, 76,  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 43 |
| Frequency range | 1900 | - | 1915 | -15.5 | 5 | 15, 26, 27 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 15, 26, 27 |
| n66, n86 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 25, 26, 27, 28, 29, 30, 38, 41, 43, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 48,  NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n70 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 48, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 30, 48, 53, 66, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70,  NR Band n47, n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 15 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| n74 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 18, 19, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 52, 65, 66, 67, 68, 85  NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| Frequency range | 1400 | - | 1427 | -32 | 27 | 15, 41 |
| Frequency range | 1475 | - | 1488 | -50 | 1 | 42 |
| Frequency range | 1488 | - | 1518 | -50 | 1 | 15 |
| n77 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 11, 12, 13, 14, 17, 18, 19, 20, 21, 24, 25, 26, 27, 28, 29, 30, 34, 39, 40, 41, 53, 65, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n95 | E-UTRA Band 1, 3 , 5, 8, 28, 39, 40, 41,  NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| NOTE 1: FDL\_low and FDL\_high refer to each frequency band specified in Table 5.2-1 in TS 38.101-1 or Table 5.5-1 in TS 36.101  NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.5.3.1-2 are permitted for each assigned NR carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x RBsize kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.  NOTE 3: 15 kHz SCS is assumed when RB is mentioned in the note when channel bandwidth is less than or equal to 50 MHz, lowest SCS is assumed when channel bandwidth is larger than 50 MHz. The transmission bandwidth in terms of RB position and range is not limited to 15 kHz SCS and shall scale with SCS accordingly.  NOTE 4: Void  NOTE 5: For non-synchronised TDD operation to meet these requirements some restriction will be needed for either the operating band or protected band  NOTE 6: N/A  NOTE 7: Void  NOTE 8: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHz.  NOTE 9: Void  NOTE 10: Void  NOTE 11: Void  NOTE 12: The emissions measurement shall be sufficiently power averaged to ensure a standard deviation < 0.5 dB  NOTE 13: Void  NOTE 14: Void  NOTE 15: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.  NOTE 16: Void  NOTE 17: Void  NOTE 18: Void  NOTE 19: Applicable when the assigned NR carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.  NOTE 20: Void  NOTE 21: This requirement is applicable for any channel bandwidths within the range 2500 - 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 - 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.  NOTE 22: This requirement is applicable for power class 3 UE for any channel bandwidths up to 20 MHz. For channel bandwidth within the range 2570 - 2615 MHz with the following restriction: for carriers of 15 MHz bandwidth when the carrier centre frequency is within the range 2605.5 - 2607.5 MHz and for carriers of 20 MHz bandwidth when the carrier centre frequency is within the range 2597 - 2605 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB. . For carriers overlapping the frequency range 2615 - 2620 MHz the requirement applies with the maximum output power configured to +19 dBm in the IE P-Max.  NOTE 23: Void  NOTE 24: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned NR carrier used in the measurement due to 2nd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.3.1-1) for which the 2nd harmonic totally or partially overlaps the measurement bandwidth (MBW).  NOTE 25: As exceptions, measurements with a level up to the applicable requirement of -36 dBm/MHz is permitted for each assigned NR carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.3.1-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).  NOTE 26: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.  NOTE 27: This requirement is applicable for channel bandwidths up to 20 MHz within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when the carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when the carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.  NOTE 28: Void  NOTE 29: Void  NOTE 30: Void  NOTE 31: Void  NOTE 32: Void  NOTE 33: This requirement is only applicable for carriers with bandwidth up to 20MHz and confined within 1885-1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz.  NOTE 34: This requirement is applicable for 5 and 10 MHz NR channel bandwidth allocated within 718-728 MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and RBstart < 48.  NOTE 35: This requirement is applicable in the case of a 10 MHz NR carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.  NOTE 36: Void  NOTE 37: Void  NOTE 38: Void  NOTE 39: Void  NOTE 40: Void  NOTE 41: Applicable for cases and when the lower edge of the assigned NR UL channel bandwidth frequency is greater than or equal to 1427 MHz + the channel BW assigned for 5 and 10 MHz bandwidth, and when the lower edge of the assigned NR UL channel bandwidth frequency is greater than or equal to 1440 MHz for 15 and 20 MHz bandwidth.  NOTE 42: Applicable for 5 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1467 MHz assigned for 10 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1463.8 MHz for 15 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1460.8 MHz for 20 MHz bandwidth.  NOTE 43: This requirement is applicable for NR channel bandwidth allocated within 1920-1980 MHz. | | | | | | | |

NOTE: To simplify Table 6.5.3.2-1, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

## *<< Unchanged sections are omitted >>*

#### 6.5E.3.3 Spurious emissions for UE co-existence for V2X con-current operation

For the inter-band con-current NR V2X operation, the UE-coexistence requirements in Table 6.5E.3.3.1-1 apply for the corresponding inter-band con-current operation with transmission assigned to both uplink in licensed band and sidelink in Band n47.

Table 6.5E.3.3.1-1: Requirements for inter-band con-current V2X operation

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| V2X con-current operating band cofiguration | Spurious emission | | | | | | |
| Protected band | Frequency range (MHz) | | | Maximum Level (dBm) | MBW (MHz) | NOTE |
| V2X\_n71A-n47A | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 30, 48, 66, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 1 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 2 |
| NR Band n71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 5925 | - | 5950 | -30 | 1 | 3, 4 |
| Frequency range | 5815 | - | 5855 | -30 | 1 | 3 |
| NOTE 1:As exceptions, measurements with a level up to the applicable requirements defined in Table 6.6.3.1-2 are permitted for each assigned E-UTRA carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. In case the exceptions are allowed due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2MHz + N x LCRB x 180kHz), where N is 2, 3 or 4 for the 2nd, 3rd or 4th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.  NOTE 2: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.6.3.1-1 and Table 6.6.3.1A-1 from the edge of the aggregated channel bandwidth.  NOTE 3: Applicable when NS\_33 is configured by the pre-configured radio parameters for power class 3 V2X UE.  NOTE 4: In the frequency range x-5950MHz, SE requirement of -30dBm/MHz should be applied; where x = max (5925, fc + 15), where fc is the channel centre frequency. | | | | | | | |

## *<< End of Changes >>*