**3GPP TSG-RAN WG4 Meeting # 97-e R4-20xxxxx**

**Electronic Meeting, Nov 2nd – 13th, 2020**

**Agenda item:** 7.19.3

**Source:** Moderator (OPPO)

**Title:** Email discussion summary for [97e][116] NR\_R16\_Maintenance

**Document for:** Information

# Introduction

This document summarizes the email discussions for agenda item 7.19.3 which is intended for R16 maintenance.

The discussions of this email thread are divided into the following four areas, i.e. papers for 38.101-1, for 38.101-2, for 38.101-3 and for other specs.

# Topic #1: Papers for 38.101-1

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| **R4-2014167**Type: CRCAT: F | Qualcomm | ***Title:*** CR CatF n7 NS\_46 AMPR and coexistence***WIC: NR\_n7\_BW******Reason for change:*** Missing the additional spurious requirement for NS\_46 large channel BWs > 20MHz.***Summary of change:***1. Add reference to the missing additional requirement sub-clause for channel BWs > 20MHz.
2. Remove AMPR for 15MHz and 20MHz channel BWs for NS\_46.
3. Modify note 21 in coexistence table to refer to coexistence requirements only apply for channel BWs up to 20MHz with RB restriction for 15MHz and 20MHz channel BWs.
4. Add the missing additional requirement sub-clause for all channel BWs for NS\_46.
 |
| **R4-2014517**Type: CRCAT: F | Nokia | ***Title:*** n53 bracket removal***WIC: NR\_n53-Core******Reason for change:*** RAN5 is developping test cases for n53 but this band has A-MPR values and OOB table note 6 still in brackets which means that these requriements are untestable. Furthermore some references and numbering is corrected***Summary of change:***1. Brackets removed and errors corrected
 |
| **R4-2014520**Type: CRCAT: B | Nokia, AT&T | ***Title:*** TS 38.101-3: Addition of missing lower order fallbacks***WIC: TEI16******Reason for change:*** These configurations have relating higher order configurations already in REL16 specs. It is important to add these as a correction inorder to retain specification intergity.DC\_2A-30A\_n2ADC\_2A-66A\_n2ADC\_29A-30A\_n2ADC\_29A-30A\_n66ADC\_30A-66A\_n66A***Summary of change:***Missing lower order configurations are added. MSD for DC\_2A-66A\_n2A is reused from DC\_2A-66A\_n25A.MSD for DC\_29A-30A\_n66A is reused from DC\_1A-28A\_n7A |
| R4-2014521 | Nokia, AT&T | ***Title:*** TR 37.716-21-11: Addition of missing lower order fallbacks |
| **R4-2015033**Type: CRCAT: F | ZTE | ***Title:*** CR to TS38.101-1: Correction on the general requirement and configured transmitted power requirement for inter-band DC***WIC: NR\_newRAT-Core******Reason for change:*** For the general requirement (subclause 4.3)1. The sentence agreed in R4-2006997 was not implemented in the latest spec.For Pcmax: (subclause 6.2B.4.1)1. According to the configured transmitted power single carrier, the total power reduction is (MPR+ ∆MPR) dB.2. The feature of PC2 inter-band NR-DC combination is not supported in Rel-16, therefore it is no need to consider ΔPPowerClass in the formulas.3. The explanation for some inter-band DC specfied terms in the formulas are missing..***Summary of change:***1. Add the sentence agreed in R4-2006997 in sub-clause 4.3
2. Add ∆MPR in the term of MAX(MPRc A-MPRc), i.e. MAX(MPRc+∆MPRc, A-MPRc) and delete ΔPPowerClass in the PCMAX\_L,f,c,MCG and PCMAX\_L,f,c,SCG formulas
3. Add the explanations for some inter-band DC specfied terms.
 |
| **R4-2015299**Type: CRCAT: F | Huawei | ***Title:*** Editorial correction on section 5.2C to 38.101-1 R16***WIC: TEI16******Reason for change:*** This CR corrects title for 5.2C***Summary of change:***This CR corrects title for 5.2C |
| **R4-2015339**Type: CRCAT: F | OPPO | ***Title:*** CR on sum of power for multiple transmit connectors***WIC: TEI16******Reason for change:*** In R4-2011768, below agreements have been reached in changing the description of how to sum powers from multiple connectors. The agreement is reproduced below. Even the agreements are made for UL MIMO/TxD, it is also applicable to other cases which require summing of powers from multiple connectors.

|  |
| --- |
| * RAN4 agree to define requirements for MOP and emission so that power is measured correctly for all implementations, including UE with transparent TxD:
	+ Use “requirements are defined as the sum of powers from both connectors”.
		- This shall be interpreted as: Measure the power and emissions per connector and then sum them up afterwards.
		- RAN4 will clean-up all requirements related to summing the powers and emissions, including UL MIMO, UL full power transmission requirement.
 |

***Summary of change:***Change the description from “measured as the sum of maximum output power at each UE antenna connector” to “defined as the sum of maximum output power from both UE antenna connectors”. |
| **R4-2015553**Type: Discussion paper for approval | Huawei, HiSilicon, CMCC | **Title:** Discussion on spurious emission about UE co-existence between band n40 and n41Proposal 1: To introduce -50dBm/MHz spurious emission requirements for band n41 frequency range when band n40 transmitting power.Proposal 2: To introduce -40dBm/MHz spurious emission requirements for band n40 frequency range when band n41 transmitting power. |
| **R4-2015554**Type: CRCAT: F | Huawei, HiSilicon, CMCC | ***Title:*** CR on spurious emission about UE co-existence between band n40 and n41***WIC: NR\_RF\_FR1-Core******Reason for change:*** 1. The operators in China has a plan to use the asynchronized deployment between band n40 and n41. It’s necessary to specify the spurious emission about UE co-existence between band n40 and n41.***Summary of change:**** To add protected band n41 for band n40 spurious emissions for UE co-existence.
* To add protected band n40 for band n41 spurious emissions for UE co-existence.
 |
| **R4-2015699**Type: CRCAT: F | Huawei, HiSilicon | ***Title:*** Reference measurement channels for 70 MHz CBW***WIC: TEI16******Reason for change:*** 70 MHz CBW is introduced in Rel-16 for band n77/n78, but the reference measurement channels for 70 MHz CBW are not defined.***Summary of change:***1. RMC for 70 MHz CBW is added |
| **R4-2015914**Type: CRCAT: F | Keysight | ***Title:*** Correction to supported channel bandwidths per SUL\_n41A-n81A***WIC: NR\_SUL\_combos\_R16-Core******Reason for change:*** SUL\_n41A-n81A ban combination includes 25 MHz and 30 MHz channel bandwiths for frequency band n81 but they are not supported according to table 5.3.5-1.***Summary of change:***Removing channel bandwidths 25 MHz and 30 MHz |
| **R4-2016341**Type: CRCAT: F | Ericsson | ***Title:*** CR for editorial corrections 38.101-1***WIC: NR\_CA\_R16\_Intra******Reason for change:*** Editorial corrections 38.101-1.***Summary of change:***Adding space between BW’s in the 2nd channel BW column for CA\_n1BRemoving 35 MHz for CA\_n7B in configuration table since 35 MHz is not yet defined.Removing empty rows for CA\_n48B and CA\_n48C in Table 5.5A.1-1 (highlighted red)Remove emply first row of CA\_n48(2A) in Table 5.5A.2-1 (highlighted red)Adding missing SCS for CA\_n20A-n78A, CA\_n41C-n79A, CA\_n46B-n48A, CA\_n46C-n48A, CA\_n46D-n48A, CA\_n46E-n48ACorrecting references from CA\_7(2A) to CA\_n7(2A) insteadCorrecting references from CA\_25(2A) to CA\_n25(2A) insteadFor the n41 row for CA\_n41(2A)-n71A, the SCS column and the CA\_n41(2A) BW column is merged (highlighted yellow)For the n78 row for CA\_n7A-n66A-n78(2A), the SCS column and the CA\_n78(2A) BW column is merged (highlighted yellow)Format the SCS values to the center for CA\_n25A-n41A-n71ADelete the emply rows between CA\_n25A-n66A-n78A and CA\_n28A-n40A-n78A (highlighted red) |
| **R4-2016442**Type: CRCAT: D | Qualcomm | ***Title:*** Replacement of void sub-clauses***WIC: NR\_newRAT-Core******Reason for change:*** Sub-clauses were incorrect marked as “Void” when the intention was to reserve them for future usage.***Summary of change:***Void sub-clauses are replaced with “Reserved”. Reserved sub-clauses are added to maintain clause numbering continuity. 7.3F is moved to 7.3B and 7.3G is moved to 7.3F. |
| **R4-2016451**Type: CRCAT: F | T-Mobile USA | ***Title:*** CR to for 38.101-1: CA uplink power clarification***WIC: TEI16******Reason for change:*** Some of the wording on UE maximum output power for carrier aggregation is unclear***Summary of change:***Clarify the wording for UE maximum output power for carrier aggregation |
| **R4-2016458**Type: CRCAT: F | T-Mobile USA | ***Title:*** CR for 38.101-1: Editorial corrections***WIC: TEI16******Reason for change:*** Many editorial errors exist in 38.101-1***Summary of change:***Corrects editorial errors |
| **R4-2016483**Type: CRCAT: F | Huawei, HiSilicon | ***Title:*** CR for TS 38.101-1 harmonic MSD for CA\_n41-n79***WIC: TEI16******Reason for change:*** For CA\_n41-n79, the frequency range below 2506 MHz for Band n41 is not used, it is assumed before that there is no 2nd order harmonic issue due to the applicable frequency range. However, since n41 supports larger CBW, considering the spectrum regrowth for the harmonics, the interference would still cause REFSENS degradation for n79 especially for the DL channel close to 5000MHz.***Summary of change:***Add harmonic MSD for CA\_n41-n79 |
| **R4-2016592**Type: CRCAT: F | Qualcomm | ***Title:*** Editorial CR to change 'Void" section to reserved***Note: Paper did not submitted before meeting.*** |
| **R4-2014327**Type: CRCAT: F | Reliance Jio | ***Title:*** LTE/NR spectrum sharing in Band 40/n40***WIC: DSS\_LTE\_B40\_NR\_Bn40\_Core******Reason for change:*** To enable dynamic spectrum sharing between LTE and NR in B40/n40 band***Summary of change:***Section 5.4.2.1, Introduction of 7.5 KHz UL shift (FREF, shift) for TDD band n40 |
| **R4-2014899**Type: CRCAT: F | Apple | ***Title:*** Coexistence cleanup for 38.101-1 Rel16***WIC: TEI16******Reason for change:*** Rel-16 features several band protection requirements which are not technical possible or contain contradicting protection requirements.***Summary of change:***Duplicate protections with contradicting requirements are corrected for several single bands and CA. |

## Open issues summary

### Sub-topic 1-1 UE co-existence between n40 and n41

*Moderator notes: UE co-existence requirements between n40 and n41 was removed from spec due to the assumption that the two bands will be synchronized and same UL/DL configuration. Now operator demands on the asynchronized NWs are shown, thus requirements are proposed in R4-2015553. The -50dBm/MHz for n40 Tx is same as removed requirement, and -40dBm/MHz is new for n41 Tx. CR is R4-2015554.*

**Issue 1-1-1: Whether following proposals from R4-2015553 is acceptable to define spurious emission requirements?**

* + **Proposal 1: To introduce -50dBm/MHz spurious emission requirements for band n41 frequency range when band n40 transmitting power.**
	+ **Proposal 2: To introduce -40dBm/MHz spurious emission requirements for band n40 frequency range when band n41 transmitting power.**
* Option 1: Yes
* Option 2: No

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LGE | For both aggressor cases, we prefer -40dBm/MHz as spurious emission requirement. The filter characteristic is quite aggressive to satisfy the 30dB isolation when we consider normal B40 filter performance. |
| ZTE | We think both synchronize and asynchronize operation should be considered for band n40 and n41. |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014167 | Title: CR CatF n7 NS\_46 AMPR and coexistence |
|  |
| R4-2014517 | Title: n53 bracket removal |
|  |
| R4-2014520 | Title: TS 38.101-3: Addition of missing lower order fallbacks |
| ZTE: Strange to see the high order configurations have already completed before lower order fallbacks are not included. But we are ok to make up the ‘hole’. |
| R4-2014521 | Title: TR 37.716-21-11: Addition of missing lower order fallbacks*Moderator note: same changes as 4520.* |
| ZTE: The contents are for TP, but the Tdoc type is for CR. This Tdoc cannot be approved. Instead, we can focus on 2014520. |
| R4-2015033 | CR to TS38.101-1: Correction on the general requirement and configured transmitted power requirement for inter-band DC |
|  |
| R4-2015299 | Editorial correction on section 5.2C to 38.101-1 R16 |
|  |
| R4-2015339 | CR on sum of power for multiple transmit connectors |
|  |
| R4-2015554 | CR on spurious emission about UE co-existence between band n40 and n41*Moderator note: This CR depends on the conclusion in R4-2015553* |
| ZTE: It should be clarified that this requirements is only for asynchronize operation between band n40 and band n41. i.e. a note is needed. |
| R4-2015699 | Reference measurement channels for 70 MHz CBW |
|  |
| R4-2015914 | Correction to supported channel bandwidths per SUL\_n41A-n81A |
|  |
| R4-2016341 | Rel-16 CR editorial corrections 38.101-1 |
|  |
| R4-2016442 | Replacement of void sub-clauses |
|  |
| R4-2016451 | CR to for 38.101-1: CA uplink power clarification |
| ZTE: Actually the sentence in current spec is the similar with LTE. Does it need to do the same correction for LTE? In addition, similar corrections should be done for the last sentence. |
| R4-2016458 | CR for 38.101-1: Editorial corrections |
|  |
| R4-2016483 | CR for TS 38.101-1: harmonic MSD for CA\_n41-n79 |
| ZTE: When RAN4 define the harmonic MSD value, MSD caused by the spectrum regrowth is not considered. We are not sure why n41-n79 needs to consider. ( also no such issue for ENDC 41-n79?) Also if we consider the harmonic spectrum regrow,then it seems there may exist some other completed combination who have the same problem need to be revisited. |
| R4-2016592 | Editorial CR to change 'Void" section to reserved |
|  |
| R4-2014327 | LTE/NR spectrum sharing in Band 40/n40 |
|  |
| R4-2014899 | Coexistence cleanup for 38.101-1 Rel16 |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |

## Discussion on 2nd round (if applicable)

The following WF and revised CR will be discussed in 2nd round to seek for approval and agreement.

|  |  |
| --- | --- |
|  | **Title:**  |
|  |
|  | **Title:**  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| CR/TP/WF number | CRs/TPs/WFs Status update recommendation  |
|  |  |
|  |  |

# Topic #2: Papers for 38.101-2

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| **R4-2014957**Type: CRCAT: F | ZTE | ***Title:*** CR to TS 38.101-2 on fallback group for intra-band contiguous CA (Rel-16)***WIC: TEI16******Reason for change:*** The fallback groups for intra-band contiguous CA classes CA\_n259G and CA\_n261D in the configuration table are incorrect groups.***Summary of change:***(1) Move CA\_n259G and CA\_n261D to the corresponding fallback groups.(2) Remove the empty row for CA\_n261H. |
| **R4-2015980**Type: CRCAT: F | ZTE | ***Title:*** Correction to modified MPR behaviour***WIC: TEI16******Reason for change:*** Incorrect conditions for the bits in the field modifiedMPRbehavior (all defined in Rel-15).Modified MPR behaviour introduced in an earlier release is mandatory in a later release.***Summary of change:***Annex H: “may set” is changed to “shall set” for the bits defined for n257, n258, n260 and n261. |
| **R4-2016342**Type: CRCAT: F | Ericsson | ***Title:*** Rel-16 CR editorial corrections 38.101-2***WIC: NR\_CA\_R16\_Intra******Reason for change:*** Editorial corrections 38.101-2***Summary of change:***Adding CA to n261I in the CA\_n261(A-G-I) row of Table 5.5A.2-2Removing references to Note 1 and Note 2 in Table 5.5A.2-2Adding A to 1CC bands in Table 5.5A.2-2 to be consistent with notation in Table 5.5A.2-1Removing not needed Note 1 in Table 5.5A.1-1 about maximum bandwidth band n261 Removing end comma not needed in the 2nd channel BW column for CA\_n260Q and n261Q |
| **R4-2016593**Type: CRCAT: F | Qualcomm | ***Title:*** Editorial CR to change 'Void" section to reserved***Note: Paper didn’t submitted before meeting.*** |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014957 | CR to TS 38.101-2 on fallback group for intra-band contiguous CA (Rel-16) |
|  |
| R4-2015980 | Correction to modified MPR behaviour |
|  |
| R4-2016342 | Rel-16 CR editorial corrections 38.101-2 |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |

## Discussion on 2nd round (if applicable)

The following WF and revised CR will be discussed in 2nd round to seek for approval and agreement.

|  |  |
| --- | --- |
|  | **Title:**  |
|  |
|  | **Title:**  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/WF number** | **CRs/TPs/WFs Status update recommendation**  |
|  |  |
|  |  |

# Topic #3: Papers for 38.101-3

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| **R4-2014170**Type: Discussion paper for approval | Qualcomm | **Title:** Handling new channel bandwidths for ENDC and NRCA band combinations with MSD**Proposal 1: Modify the UL configuration table for larger UL channel BWs as shown in section 2.3** |
| **R4-2014169**Type: CRCAT: F | Qualcomm | ***Title:*** CR CatF Cross Band Noise DC\_3\_n1\_highBW***WIC: TEI16******Reason for change:*** Missing cross band noise MSD for various interband ENDC band combinations with large NR UL BW***Summary of change:***1. Modifed UL configuration by shifting the RB starting position for the 25, 30, 40, 50MHz channel bandwidths with the allocated UL resource blocks starting at RB positions 9, 19, 42, 63 respectively.
 |
| R4-2015552Type: Discussion paper for approval | HW | **Title: Consideration on Cross band isolation impact with larger BW**Observation 1: If the NR band is a DL band or victim band, the corresponding MSD value should be specified for the new channel bandwidth. If the NR band is a UL band or aggressive band, the UL configuration and MSD values need to be further considered.Observation 2: It’s noted that UL configuration applies regardless of the channel bandwidth of the UL band and the UL resource blocks shall be located as close as possible to the downlink operating band in Table 7.3B.2.3.4-2 from TS 38.101-3.Observation 3: Even if UL configuration applies regardless of the channel bandwidth of the UL band, UL allocation such as SCS and LCRB may still restrict the channel bandwidth.Proposal 1: 15kHz SCS can be used for sub-3GHz FDD bands and sub-2.3GHz TDD/SUL bands except for n50 when RAN4 derive the UL configuration of the MSD due to cross band isolation.Proposal 2: 30kHz SCS can be used for n41, n77, n78 and n79 when RAN4 derive the UL configuration of the MSD due to cross band isolation.Proposal 3: UL SCS for n40 and n50 can be considered case by case. 15kHz or 30kHz or Both 15kHz and 30kHz can be used for n40 and n50 when RAN4 derive the UL configuration of the MSD due to cross band isolation.Observation 4: MSD due to aggressive band PA spurious emission depends on RB allocation regardless of the channel bandwidth. The maximum RB allocation is the worst case for aggressive band PA spurious emission. However, the RB allocation can be limited when deriving the UL configuration of the MSD due to cross band isolation.Observation 5: There is a difference between MSD due to spurious emission and CIM interference. The key factor for MSD due to CIM interference is whether the CIM interference falls into the DL channels. The minimum RB allocation is the worst case for CIM interference.Proposal 4: It’s proposed that RAN4 create a new MSD exception due to CIM interference. The original MSD due to cross band isolation can focus on the aggressive band PA spurious emission.Proposal 5: It’s proposed that Reference sensitivity exceptions (MSD) due to counter intermodulation interference for EN-DC in NR FR1 can be specified as table 1. |
| **R4-2015795**Type: Discussion paper for approval | CHTTL | **Title:** Discussion on handling the cross band isolation requirement for larger channel BW in Rel.16Proposal 1: for the Rel.16 combinations that face the issue on the cross band isolation with new added larger channel bandwidth, for example, DC\_3\_n1, limited UL BWs of the aggressor band for EN-DC combinations with the existing cross band noise MSD can be considered. |
| R4-2014317Type: Discussion paper for approval | LGE | **Title: Consideration on additional ILs and MSD levels for DC\_20\_n38 UE and/or V2X\_20\_n38 UE based on RF architecture**Observation1: For DC\_20\_n38 UE, RAN4 did not consider Harmonic trap filter based on the delta Tib/Rib levels for DC\_20\_n38 band combinations.Observation2: Even though DC\_20\_n38 UE did not consider HTF, the required MSD levels by 3rd harmonic problems is specified as low MSD values compared in [2]Proposal 1: RAN4 shall consider option2 or option3 to solve the RF architecture and MSD problems for DC\_20A\_n38A UE and V2X\_20A\_n38A UE.Proposal 2: Based on RAN4 consensus, the proposed contents in section 3 according to candidate option2 or option3 will be applied for DC\_20A\_n38A and V2X\_20A\_n38A UE in TS38.101-3. |
| R4-2014318Type: CRCAT: F | LGE, HW | ***Title:*** Correction on additional ILs and MSD levels for DC\_20\_n38 UE***WIC:*** NR\_newRAT-Core***Reason for change:*** This CR is to update additional ILs and MSD levels by 3rd harmonic problem for DC\_20\_n38 UE 5G V2X UE in TS38.101-3.***Summary of change:***This CR is to revise MSD level for DC\_20\_n38 UE. The specified delta Tib/Rib for DC\_20\_n38 are derived without Harmonic trap filter even though 3rd harmonic from B20 fall into n38 reception frequency. However, the MSD level is quite lower values compare to the proposed MSD values in V2X\_20\_n38 UE.So, RAN4 can update the additional ILs and MSD requirements based on RF architecture. |
| R4-2014582Type: CRCAT: F | Intel | ***Title:*** CR to 38.101-3 (Rel-16) error correntions to configurations for CA and DC***WIC:*** TEI16***Reason for change:*** There are errors in CA and DC configurations in Clause 5.5A and 5.5B***Summary of change:***Correct errors |
| **R4-2014883**Type: Discussion paper for approval | NTT DOCOMO INC. | **Title:** Clarification on RF assumption for B42\_n77 and B42\_n78Proposal 1: Conform RF assumption in Rel-15 and Rel-16 that DC\_42\_n77 and DC\_B42\_n78 have intra-band architecture.Proposal 2: Recommend that power imbalance requirements as UE demod requirements shall apply some inter-band EN-DC configuration where intra-band EN-DC requirements apply, e.g., DC\_42\_n77 and DC\_42\_n78.Proposal 3: To avoid the delay of discussion in UE demod, agree Proposal 1 and Proposal 2 in 1st round discussion in RAN#97 and give feedback to UE demod session before 2nd round. |
| **R4-2015042**Type: Discussion paper for approval | ZTE | **Title:** Discussion on the MSD of the new channel BW for EN-DC and NR CA band combinationsIn this paper, we give some discussions on the MSD of the new channel BW for EN-DC and NR CA band combinations. Comparing with the currently three options included in the WF, option 2 is reasonable from specification aspect. |
| **R4-2015264**Type: CRCAT: F | Xiaomi | ***Title:*** CR for 38.101-3 Rel16 corrections on ACS requirements for intra-band contiguous EN-DC***WIC: NR\_newRAT-Core******Reason for change:*** In release 16, the transmitter is set to 4 dB below PCMAX\_L,f,c for ACS case 2 which is not aligned with the requirement in release 15. The reason is that the agreed Cat A CR (R4-2000452) was not implemented accordingly when Cat F CR (R4-2000451) was implemented after RAN4 #94-e meeting.***Summary of change:***4dB is replaced by 24dB in the note 1 of table 7.5B.1-2. |
| **R4-2015323**Type: CRCAT: F | vivo | ***Title:*** Alignment of descritpion of the power class restriction for inter-band EN-DC***WIC: ENDC\_UE\_PC2\_TDD\_TDD******Reason for change:*** The clarification for FDD-TDD ENDC HPUE has been agreed in Note 6 in Table 6.2B.1.3-1 with improved wording which is more clear. This can be also used for Note 5 to improve the consistency and better reflect the result for TDD-TDD ENDC HPUE.***Summary of change:***Change the Note 5 wording from:““NOTE 5: The UE is not required to support PC2 within each individual cell group. Power class support within each individual cell group is signaled separately by the UE.”To: “NOTE 5: The UE supports PC3 within both E-UTRA cell group and NR cell group. Power class support within each individual cell group is signaled separately by the UE.” |
| **R4-2015324**Type: CRCAT: F | vivo | ***Title:*** Correction of delta Powerclass for Inter-band EN-DC***WIC: ENDC\_UE\_PC2\_TDD\_TDD******Reason for change:*** This is resubmission of CR R4-2010855 (CRNum: 0344). The original CR which was agreed in RAN4#96-e and also approved in RP-201504 in RAN#89, was mistakenly implemented into clause 6.2B.4.1.3a which is used for NE-DC in 38.101-3 v16.5.0. The correction for 6.2B.4.1.3 for EN-DC has to be done, and current revision to 6.2B.4.1.3a can also be kept.-------------------Power class 2 had been introduced for TDD-TDD ENDC and the fallback scheme had been defined in 6.2B.1.3. It has been clarified that under different conditions, the requirements for default or the supported power class would be applied and would “set the configured transmitted power as specified sub-clause 6.2B.4” However, no revisions had been done for section 6.2B.4.1.3 which is for inter-band EN-DC for FR1. The ∆PPowerClass,EN-DC which is used to adjust this was not updated as for other cases, thus make the specification incomplete..***Summary of change:***The condition for “∆PPowerClass,EN-DC = 3 dB” in the cofigurated transmitted power has been clarified as “for a power class 2 capable EN-DC UE when requirements of default power class had been applied as specified in sub-clause 6.2B.1”, otherwise ∆PPowerClass,EN-DC = 0 dB;This clarification aviods the duplicate condition description in this part, and effectively reduced the spec complexity.It is also general enough to applied to other inter-band EN-DC cases. |
| **R4-2015331**Type: CRCAT: F | OPPO | ***Title:*** CR on NR power class under EN-DC***WIC: TEI16******Reason for change:*** The capability signaling for NR part under EN-DC has been defined in RAN2 38.331, thus RAN4 spec shall be aligned.***Summary of change:***Align the NR power class capability with 38.331. |
| **R4-2015555**Type: Discussion paper for approval | Huawei, HiSilicon | **Title:** Discussion on asynchronous for DC\_42\_n79***Proposal 1: To introduce MSD values as below between band 42 and n79 if UE choose to support simultaneous Tx/Rx for DC\_42\_n79.*** |
| **R4-2015729**Type: CRCAT: F | Qualcomm | ***Title:*** CR to TS 38.101-3 corrections on inter-band EN-DC configurations including FR1 and FR2***WIC: DC\_R16\_xBLTE\_2BNR\_yDL2UL-Core******Reason for change:*** Few configurations in the spec are not aligned with the agreed CR, R4-2006728, “Introducing CR on new EN-DC LTE(xDL/1UL)+ NR(2DL/1UL) DC in Rel-16”.***Summary of change:***Correct the specification to be aligned with the agreed CR, R4-2006728.1. missing DC\_3A-3A\_n1A-n257A2. wrong uplink DC configurations for DC\_3A\_n40A-n258A |
| **R4-2015981**Type: CRCAT: F | Ericsson | ***Title:*** Verification of the P-MPR method for EN-DC FDD-TDD power class 2***WIC: TEI16******Reason for change:*** Introduce a test case for the P-MPR solution. The (UE-based) P-MPR solution is the default for EN-DC FDD-TDD PC2 in the absence of duty-cycle capabilities. Moreover, fallback to a lower EN-DC power class is not defined for the P-MPR solution. The total EN-DC power P\_Total^(EN-DC) is always 26 dBm for the P-MPR solution, there is not fallback behaviour (unclear if this is the case under all circumstances e.g. when the combined UL duty cycle exceeds 50% or for TDD U/D configurations up to 50% UL duty cycle ).The P-MPR method is not verified. The solution is proprietary, but it should at least make sure that the maximum power of 26 dBm can be achieved for both non-simultaneos and simultaneous (overlapping) CG transmissions when the combined duty cycle is up to 50% resulting in a 23 dBm average total EN-DC power.***Summary of change:***Clause 6.2B.4.1.3: two test case are specified for EN-DC PC2:1. For NR PC2, the UE shall meet the SA requirements when LTE and NR transmissions are not overlapping with a 60% UL duty cycle on FDD and 20% UL duty cycle on TDD. 2. For NR PC3, the UE shall meet the SA requirements when LTE and NR transmissions are overlapping with a 80% UL duty cycle on FDD and 20% UL duty cycle on TDD while the PUMAX requirement (simultaneous transmissions) is met.The UL RMC for FDD with six (60%) and eight (80%) scheduled UL subframes per radio frame and the existing UL RMC for TDD (20%) are used for this purpose. It is noted that for PC2, the test case for the PUMAX requirement only works when sub-frame p on the MCG and physical-channels q on the SCG are overlapping (this could also be the implication in general). |
| **R4-2016343**Type: CRCAT: F | Ericsson | ***Title:*** Rel-16 CR editorial corrections 38.101-3***WIC: DC\_R16\_1BLTE\_1BNR\_2DL2UL-Core******Reason for change:*** Editorial corrections 38.101-3***Summary of change:***Adding missing bands in the ΔRIB,c table for DC\_2-48\_(n)5, DC\_2-66\_(n)5Correcting band 66 DL frequency in MSD table for DC\_66A\_n7A-n78AAdding DC\_40C\_n78A to Table 6.2B.1.3-1 |
| **R4-2016498**Type: CRCAT: F | Huawei, HiSilicon | ***Title:*** Rel-16 CR editorial corrections 38.101-3***WIC: NR\_newRAT-Core******Reason for change:*** The delta TIB requirement for DC\_2-7-7-13\_n66 was missing in 38.101-3***Summary of change:***Adding delta TIB requirement for DC\_2-7-7-13\_n66 to 38.101-3 |
| **R4-2016435**Type: CRCAT: F | vivo | ***Title:*** Correction to PCMAX for contiguous intra-band EN-DC***WIC: NR\_newRAT-Core******Reason for change:*** An error seems to have been introduced into the specification during the implementation of R4-2000454. The configured maximum output power for E-UTRA cell group is not specified for contiguous intra-band EN-DC. Instead, the PCMAX for NR cell group is specified twice.***Summary of change:***Replace specifications for PCMAX,f,c,NR with specifications for PCMAX\_ E-UTRA,c. Other corrections in symbol notation according to R4-2000454 |

## Open issues summary

### Sub-topic 3-1 Larger channel BW

*Moderator notes: Paper R4-2014170, R4-2015042, R4-2015552, R4-2015795 are discussed in this sub topic which all about the handling of impact caused by new and larger CBW.*

**Issue 3-1-1: Regarding how to handle new and larger channel bandwidths introduced into NRCA and ENDC combinations which of the following options is acceptable?**

* + **Option 1: Modify the UL configuration table for larger UL channel BWs as shown below.**



* + **Option 2: RAN4 create a new MSD exception due to CIM interference as below. The original MSD due to cross band isolation can focus on the aggressive band PA spurious emission.**



* + **Option 3: For the Rel.16 combinations that face the issue on the cross band isolation with new added larger channel bandwidth, for example, DC\_3\_n1, limited UL BWs of the aggressor band for EN-DC combinations with the existing cross band noise MSD can be considered.**



*Moderator notes: Option1 is from paper R4-2014170, and the CR is R4-2014169. Option2 is from paper R4-2015552 with more proposals in issue 3-1-2. Option3 is from paper R4-2015795 and is open to other choices.*

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Option 1. Actually option 1 is consistent with our view in R4-2015042, where we use the option order in the WF. We think it is more meaningful to look for some methods to avoid big MSD values than the values themselves. |
|  |  |

**Issue 3-1-2: Regarding SCS configurations to derive the MSD due to cross band isolation whether the proposals from R4-2015552 is acceptable?**

* + **Proposal 1: 15kHz SCS can be used for sub-3GHz FDD bands and sub-2.3GHz TDD/SUL bands except for n50 when RAN4 derive the UL configuration of the MSD due to cross band isolation.**
	+ **Proposal 2: 30kHz SCS can be used for n41, n77, n78 and n79 when RAN4 derive the UL configuration of the MSD due to cross band isolation.**
	+ **Proposal 3: UL SCS for n40 and n50 can be considered case by case. 15kHz or 30kHz or Both 15kHz and 30kHz can be used for n40 and n50 when RAN4 derive the UL configuration of the MSD due to cross band isolation.**
* Option 1: Yes
* Option 2: No

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | The above three proposals are more like observations, since if we look at the table, it seems we can obverse the above three proposals.  |
|  |  |

### Sub-topic 3-2 UE architecture assumption and requirements

*Moderator notes: Two main issues will be handled under this sub-topic, one is handling of different HTF assumptions in EN-DC requirements, the other is the architecture assumption for overlapping inter-band EN-DC.*

**Issue 3-2-1: Regarding HTF assumption in defining requirements which of the following options from R4-2014317 is acceptable to update the DC\_20A\_n38A delta Tib, delta Rib, and MSD requirements? If no options acceptable, please share the views.**



*Moderator notes: The conclusion will impact CR R4-2014318.*

* Option 1
* Option 2
* Option 3
* Other view

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LGE | Prefer option2 or option3. Specially option2 is more reasonable for both DC\_20\_n38 and V2X\_20\_n38 UE. |
| ZTE | either option 2 or option 3. It seems doesn’t make sense to define huge MSD value for a combination, instead methods should be adopt to avoid such MSD value. |

**Issue 3-2-2: Regarding UE architecture for overlapping inter-band EN-DC whether the following proposals from R4-2014883 is acceptable or not?**

* + **Proposal 1: Conform RF assumption in Rel-15 and Rel-16 that DC\_42\_n77 and DC\_B42\_n78 have intra-band architecture.**
	+ **Proposal 2: Recommend that power imbalance requirements as UE demod requirements shall apply some inter-band EN-DC configuration where intra-band EN-DC requirements apply, e.g., DC\_42\_n77 and DC\_42\_n78.**

*Moderator notes: There is special request from this paper, i.e. “To avoid the delay of discussion in UE demod, agree Proposal 1 and Proposal 2 in 1st round discussion in RAN#97 and give feedback to UE demod session before 2nd round”.*

* Option 1: Yes
* Option 2: No

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LGE | For reception requirements perspective in DC\_42\_n77 or DC\_42\_n78, it is possible to operate with simultaneous reception as intra-band DC RF architecture.The power imbalance requirements for DC\_42\_n77 or DC\_42\_n77 is up to demodulation session decision. |
|  |  |

### Sub-topic 3-3 Simultaneous Tx/Rx

**Issue 3-2-3: Regarding Simultaneous Tx/Rx DC\_42\_n79 whether the following proposals from R4-2015555 is acceptable or not?**

* + **Proposal 1: To introduce MSD values as below between band 42 and n79 if UE choose to support simultaneous Tx/Rx for DC\_42\_n79.**



* Option 1: Yes
* Option 2: No

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LGE | RAN4 agreed B42 will be synchronous operation with n77 and n78. And Also we have agreements for n77 and n79 that n79 will be synchronous operation with n77 due to small frequency gap.So, we do not want to specify MSD requirements due to synchronous operation between B42 and n79. |
| ZTE | We agree with LGE.  |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014169 | Title: CR CatF Cross Band Noise DC\_3\_n1\_highBW*Moderator Note: This paper reply on whether discussion paper R4-2014170 is approved.* |
| ZTE: ‘RB position ’ is not clear. Does it from the lower edge or form upper edge? also, is note 2 applicable for large CBW MSD cases? |
| R4-2014318 | Title: Correction on additional ILs and MSD levels for DC\_20\_n38 UE*Moderator Note: This paper reply on the conclusion of discussion paper R4-2014317, i.e. which option is chosen. Now the changes are based on UEs with HTF.* |
|  |
| R4-2014582 | Title: CR to TS 38.101-3 (Rel-16) Error corrections to configurations for CA and DC*Moderator Note: Editorial changes.* |
|  |
| R4-2015264 | CR for 38.101-3 Rel16 corrections on ACS requirements for intra-band contiguous EN-DC |
|  |
| R4-2015323 | Alignment of descritpion of the power class restriction for inter-band EN-DC |
|  |
| R4-2015324 | Correction of delta Powerclass for Inter-band EN-DC*Moderator note: Content has been agreed before for EN-DC but implemented to a wrong section (NE-DC). This CR is reintroduce content for EN-DC.* |
|  |
| R4-2015331 | CR on NR power class under EN-DC*Moderator note: Align the NR power class capability with 38.331.* |
| R4-2015729 | CR to TS 38.101-3 corrections on inter-band EN-DC configurations including FR1 and FR2 |
|  |
| R4-2015981 | Verification of the P-MPR method for EN-DC FDD-TDD power class 2*Moderator note: Introduce a test case for the P-MPR* |
|  |
| R4-2016343 | Rel-16 CR editorial corrections 38.101-3 |
|  |
| R4-2016498 | CR for TS 38.101-3: Adding delta TIB requirement for DC\_2-7-7-13\_n66 (R16) |
|  |
| R4-2016435 | Correction to PCMAX for contiguous intra-band EN-DC |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |
|  |  |

## Discussion on 2nd round (if applicable)

The following WF and revised CR will be discussed in 2nd round to seek for approval and agreement.

|  |  |
| --- | --- |
|  | **Title:**  |
|  |
|  | **Title:**  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/WF number** | **CRs/TPs/WFs Status update recommendation**  |
|  |  |
|  |  |

# Topic #3: Papers for other Specs

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| **R4-2014600**Type: CRCAT: F | LGE | ***Title:*** CR for adding NR overlapping bands list in TS38.307***WIC:*** NR\_newRAT-Core***Reason for change:*** This CR is to update NR overlapping bands list in TS38.307***Summary of change:***This CR is to add NR overlapping bands list in annex A |
| **R4-2014620**Type: CRCAT: F | LGE | ***Title:*** CR for adding NR overlapping bands list in TS38.307 v16.4.0***WIC:*** NR\_newRAT-Core***Reason for change:*** This CR is to update NR overlapping bands list in TS38.307***Summary of change:***This CR is to add NR overlapping bands list in annex A |
| **R4-2015856**Type: CRCAT: B | CHTTL, ZTE Corporation, Dish, SGS Wireless | ***Title:*** CR to TS 38.307 on release independent update for the Rel.16 EN-DC and NR CA/DC***WIC:*** NR\_CA\_R16\_intra-CoreNR\_CADC\_R16\_2BDL\_xBUL-CoreDC\_R16\_1BLTE\_1BNR\_2DL2UL-CoreDC\_R16\_2BLTE\_1BNR\_3DL2UL-CoreDC\_R16\_3BLTE\_1BNR\_4DL2UL-CoreDC\_R16\_4BLTE\_1BNR\_5DL2UL-CoreDC\_R16\_5BLTE\_1BNR\_6DL2UL-CoreDC\_R16\_xBLTE\_2BNR\_yDL2UL-CoreNR\_SUL\_combos\_R16-CoreNR\_CA\_R16\_3BDL\_1BUL-CoreNR\_CA\_R16\_4BDL\_1BUL-CoreNR\_CADC\_R16\_3BDL\_2BUL-CoreDC\_R16\_LTE\_NR\_3DL3UL-Core***Reason for change:*** More Rel.16 EN-DC and NR CA/DC configurations have been introduced in latest TS 38.101-1, 38.101-2, 38.101-3, an update is needed for the release independent specification.Note that the draft CR with same content was endorsed in RAN#96-e, R4-2011781***Summary of change:***Update release-independent information for Rel.16 EN-DC and NR CA/DC configurations to be release independent from Rel.15.Note that the NR-NR DC within FR1 is release independent from Rel.16. |
| **R4-2014328**Type: CRCAT: F | Reliance Jio | ***Title:*** LTE/NR spectrum sharing in Band 40/n40***WIC:*** DSS\_LTE\_B40\_NR\_Bn40\_Core***Reason for change:*** To enable dynamic spectrum sharing between LTE and NR in B40/n40 band***Summary of change:***Section 5.4.2.1, Introduction of 7.5 KHz UL shift (FREF, shift) in TDD band n40 |
| **R4-2014329**Type: CRCAT: F | Reliance Jio | ***Title:*** LTE/NR spectrum sharing in Band 40/n40***WIC:*** DSS\_LTE\_B40\_NR\_Bn40\_Core***Reason for change:*** To enable dynamic spectrum sharing between LTE and NR in B40/n40 band***Summary of change:***Section 5.4 and B.4.7 added for UL 7.5KHz shift in n40 band |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014600 | Title: CR for adding NR overlapping bands list in TS38.307*Moderator note: This paper is for Rel-15* |
| LGE: need to specify in TS38.307 to support MFBI  |
| R4-2014620 | Title: CR for adding NR overlapping bands list in TS38.307 v16.4.0*Moderator note: This paper is same as 4600 for Rel-16.* |
| LGE: need to specify in TS38.307 to support MFBI |
| R4-2015856 | CR to TS 38.307 on release independent update for the Rel.16 EN-DC and NR CA/DC |
| ZTE: Agree. |
| R4-2014328 | LTE/NR spectrum sharing in Band 40/n40*Moderator note: CR to 38.104* |
|  |
| R4-2014329 | LTE/NR spectrum sharing in Band 40/n40*Moderator note: CR to 38.307* |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |
|  |  |
|  |  |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/WF number** | **CRs/TPs/WFs Status update recommendation**  |
|  |  |
|  |  |