**3GPP TSG-RAN WG4 Meeting # 97-e R4-201xxxx**

Electronic Meeting, 2-13 Nov., 2020

**Agenda item:** 10.22

**Source:** Moderator (Huawei)

**Title:** Email discussion summary for [97e][125] NR\_FR1\_35MHz\_45MHz\_BW

**Document for:** Information

# Introduction

The scope of this email discussion is to discuss the contributions submitted at agenda 10.22 on introduction of channel bandwidths 35MHz and 45MHz for NR. The following topics are discussed in the email discussion.

* Topic#1: General part
	+ Sub-topic 1-1: Release independence
* Topic#2: Spectrum utilization
* Topic#3: UE RF requirements
	+ Sub-topic 3-1: Expanding Specification Tables
	+ Sub-topic 3-2: UL BW limitation
	+ Sub-topic 3-3: new BW handling
	+ Sub-topic 3-4: n3 35MHz and 45MHz REFSENS
	+ Sub-topic 3-5: n8 35MHz REFSENS
	+ Sub-topic 3-6: n25 35MHz and 45 MHz REFSENS
	+ Sub-topic 3-7: n71 35MHz REFSENS
	+ Sub-topic 3-8: n7 35 MHz A-MPR
	+ Sub-topic 3-9: n25 and n66 A-MPR
	+ Sub-topic 3-10: n71 35 MHz A-MPR
* Topic #4: UE draft CRs
* Topic#5: BS draft CRs

# Topic #1: General part

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2015351 | OPPO | Proposal 1: Option 3: Release independence shall be discussed cases by case per band and bandwidths |
| R4-2015701 | Huawei, HiSilicon | The paper provide the needed changes to TS 38.307 for the options.  |
| R4-2016113 | ZTE Corporation | Observation: if 35MHz/45MHz is introduced in release independent way from earlier release, there might be potential NBC issues if the existing maximum supported channel bandwidth is less than 35MHz/45MHz.Proposal 1: sent LS to RAN2 to inform the introduction of 35MHz and 45MHz from Rel-17 onwards.Proposal 2: to explicit inform RAN2 that 35MHz/45MHz might be maximum channel bandwidth in certain bands; |
| R4-2016452 | T-Mobile USA, TELUS, Bell Mobility, AT&T | Observation 1: RAN2 has allocated spare bits in Rel-15 for adding new channel BWs to UE capabilities. Observation 2: A RAN2 CR shows how to add 35 and 45 MHz UE capability signalling to Rel-15. Observation 3: There is no protocol reason to not make 35 and 45 MHz release independent to Rel-15.Observation 4: Having the new Channel BWs release independent to RTel-15 won’t cause any backward compatibility issues. Proposal 1: RAN4 should agree to make the new 35 and 45 MHz channel BWs release independent to Rel-15, and leave the topic of release implementation to commercial rather than standards discussions. |
| R4-2015800 (Proposal 3) | Skyworks Solutions Inc. | • Release independence for band/band combination should be agreed case by case. |

## Open issues summary

### Sub-topic 1-1

**Issue 1-1: Release independence**

* Proposals
	+ Option 1: The support of 35 MHz and 45 MHz is from Rel-17 onwards
	+ Option 2: 35 MHz and 45 MHz is optional support from Rel-15
	+ Option 3: Release independence shall be discussed cases by case per band and bandwidths.
* Recommended WF
	+ It is proposed to continuously discuss the 3 options and make a decision this meeting, considering the following aspects,
		- UE signaling
		- UE hardware capability
		- backward compatibility issues
		- band specific work

## Companies views’ collection for 1st round

### Open issues

**Comments on Release independence**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | We support option 1 as this bandwidth demand is clearly from Rel-17, in addition, we could see lots of implementation efforts needed for the support of 35/45MHz, this could be treated as NBC issue. We have concerns on option 2 as this will increase BS implementation uncertainty whether to support such kind of feature due to uncertainty of UE feature. |
| Huawei | We are open on the options. We have one clarification question on R4-2015800. It propose to discuss release independence cases by case. While in R4-2015800 table 1 in clause 2.2, for all the cases it states Rel indep from R16 min. Does it mean option 3 is optional support from Rel-16? |
| Ericsson | We support the proposal in R4-2016452. |
| Qualcomm | Support for 35M, 45M BWs should not be mandatory for earlier release. It seems there is existing capability for this after checking with RAN2 colleague. We can further check if this is true for all bands mentioned in this thread as well as check that enough bits are available for BWs added in the future. |
| Skyworks | We support option 3 and would be willing to discuss cases by case if it can be before R17. But we could also agree with R17 for the cases where the 35MHz and/or 45MHz does not become the widest BW supported (especially in UL). For the cases where 35MHz and/or 45MHz becomes the highest BW one option is to have optional support from R17. Still we also need to agree whether these BW become a generic channel BW for any band which we don’t think is necessary and would result into a lot of effort in 3GPP |
|  |  |
|  |  |
|  |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |
|  |  |
|  |  |
|  |  |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |

## Discussion on 2nd round (if applicable)

|  |  |
| --- | --- |
| **WF number** | **Comments collection** |
|  |  |
|  |
|  |
|  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
|  |  |
|  |  |

# Topic #2: Spectrum utilization

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2015043 | ZTE Corporation | Remove [] for the SU values for 35MHz and 45MHz in the table.

|  |  |  |
| --- | --- | --- |
| SCS (kHz) | 35MHz | 45MHz |
| NRB | NRB |
| 15 | 188 | 243 |
| 30 | 92 | 119 |
| 60 | 44 | 58 |

 |

## Open issues summary

### Sub-topic 2-1

**Issue 2-1: Spectrum utilization**

* Proposals
	+ Remove [] for the SU values for 35MHz and 45MHz
* Recommended WF
	+ Approve the proposal to remove [].

## Companies views’ collection for 1st round

### Open issues

**Comments on spectrum utilization**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | We support the recommended WF.  |
| Huawei | We agree |
| Qualcomm | Agree to remove square brackets |
| Skyworks | Agree with SU without brackets |
|  |  |
|  |  |
|  |  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |

## Discussion on 2nd round (if applicable)

## Summary on 2nd round (if applicable)

# Topic #3: UE RF requirements

## Companies’ contributions

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Title** |
| R4-2014173 revised to R4-2016600 | Qualcomm Incorporated | 35M\_45M AMPR, MPR, REFSENS |
| R4-2015432 | Murata Manufacturing Co Ltd. | REFSENS of n3, n8, n25 and n71 for new channel bandwidth |
| R4-2015800 | Skyworks Solutions Inc. | Specification impact of additional 35&45MHz channel bandwidths |
| R4-2016010 | Skyworks Solutions Inc. | n71 35MHz AMPR and MSD Measurements |
| R4-2016011 | Skyworks Solutions Inc. | n8 35MHz AMPR and MSD Measurements |
| R4-2016027 | Skyworks Solutions Inc. | n7 35MHz AMPR and MSD Measurements |
| R4-2016060 | Ericsson | Introduction of 35MHz and 45MHz regarding CA, DC, V2x combinations |
| R4-2016295 | Apple Inc. | Introduction of 35 MHz for n8, n66, n71 and 45 MHz for n66 |
| R4-2014186 | MediaTek Inc. | REFSENS of n8 and n71 for 35MHz channel bandwidth |
|  |  |  |

## Open issues summary

### Sub-topic 3-1

**Issue 3-1: Expanding Specification Tables**

* Proposals

**Proposal 1:** SEM, ACS, In-band and Narrow band blocking, Spurious response, Intermodulation tables use equations proportional to channel BW instead of one column per channel BW.

**Observation:** There are many other specification tables that have one column per channel BW such as channel configurations for single CC and band combinations and the related REFSENS and RFSENS exceptions. Simplification or a separate table may be needed.

* Recommended WF
	+ Check whether proposal 1 above is agreeable

### Sub-topic 3-2

**Issue 3-2: UL BW limitation**

* Proposals
* UL BW limitation to 20 MHz for n8 and n71 should seriously be considered as default operation to guarantee the best DL operation in 35 MHz and reduce spec/test impact.
* UL BW limitation to 40 MHz for n25 could be further studied if justified from an MSD point of view
* Recommended WF
	+ To discuss whether UL BW limitation is adopted for the case with high MSD in DL

### Sub-topic 3-3

**Issue 3-3: new BW handling**

* Proposals

In R4-2015800

* Support of 35 and 45 MHz Channel bandwidth should be optional for bands and should use separate table for band and band specific requirements. This should apply to any new FR1 channel BW beyond Release 16.
* The introduction of new “regular” channel bandwidth or new bands using these channel bandwidths, should not be treated with a basket approach including for band combinations.

 In R4-2016060

* Proposal 1: RAN4 shall avoid adding new BCSs when introducing new bandwidths to band combinations, if really needed it should be done on a case by case basis.
* Recommended WF
	+ Comments on the proposals

### Sub-topic 3-4

**Issue 3-4: n3 35MHz and 45MHz REFSENS**

* Proposals summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)**  | **45 MHz (dBm)** | **Duplex Mode** |
|
|
|  |  | **Murata** | **Qualcomm** |  | **Murata** | **Qualcomm** |  |  |
| n3 | 15 | -86 | -85.2 | 　 | -84.2 | -80.2 | 　 | FDD |
| 30 | -86.1 | 　 | 　 | -84.3 | 　 | 　 |
| 60 | -86.2 | 　 | 　 | -84.4 | 　 | 　 |
|  |  |  |  |  |  |  |  |  |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)** | **45 MHz (dBm)** | **Duplex Mode** |
|
|
|  |  | **Murata** | **Qualcomm** |  | **Murata** | **Qualcomm** |  |  |
| n3 | 15 | 50 | 50 | 　 | 50 | 50 | 　 | FDD |
| 30 | 24 | 　 | 　 | 24 | 　 | 　 |
| 60 | 10 | 　 | 　 | 10 | 　 | 　 |

* Tentative agreements
	+ For n3 35MHz and 45MHz UL configuration, 50RB is used for 15 KHz SCS, 24RB is used for 30 KHz SCS, and10RB is used for 60 KHz SCS
* Recommended WF
	+ Agree on the UL configuration and check if companies can agree on the MSD

### Sub-topic 3-5

**Issue 3-5: n8 35MHz REFSENS**

* Proposals summary

|  |  |  |  |
| --- | --- | --- | --- |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)**  | **Duplex Mode** |
|
|
| n8 |  | **Murata R4-2015432** | **QualcommR4-2014173** | **SkyworksR4-2016011** | **AppleR4-2016295** | **MediaTek R4-2014186** |  |
| 15 | -62.2 | -69.9 (Rbend =187)-84.0 (Rbend =143)-87.9 (Rbend =123) | -66.3 | -62.3 | -69.2 | FDD |
| 30 | -62.3 | 　 | -66.4 | -63,7 | -69.5 |
| 60 | 　 | 　 | 　 | 　 | 　 |
|  |  |  |  |  |  |  |  |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)** | **Duplex Mode** |
|
|
| n8 |  | **Murata R4-2015432** | **QualcommR4-2014173** | **SkyworksR4-2016011** | **AppleR4-2016295** | **MediaTek R4-2014186** |  |
| 15 | 20 | 16 | 25 | 8 | 20 | FDD |
| 30 | 10 | 　 | 10 | 4 | 10 |
| 60 | 　 | 　 | 　 | 　 | 　 |

* Tentative agreements
* Recommended WF
	+ Agree on UL configuration firstly and check if companies can get agreement on MSD

### Sub-topic 3-6

**Issue 3-6: n25 35MHz and 45 MHz REFSENS**

* Proposals summary

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)**  | **45 MHz (dBm)** | **Duplex Mode** |
|
|
|  |  | **Murata R4-2015432** | **QualcommR4-2014173** |  | **Murata R4-2015432** | **Qualcomm****R4-2016600** |  |  |
| n25 | 15 | -85.4 | -81.7 | 　 | -70.7 | -68. | 　 | FDD |
| 30 | -85.5 | 　 | 　 | -70.8 | 　 | 　 |
| 60 | -85.6 | 　 | 　 | -70.9 | 　 | 　 |
|  |  |  |  |  |  |  |  |  |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)** | **45 MHz (dBm)** | **Duplex Mode** |
|
|
|  |  | **Murata R4-2015432** | **QualcommR4-2014173** |  | **Murata R4-2015432** | **QualcommR4-2016600** |  |  |
| n25 | 15 | 40 | 45 | 　 | 40 | 40 | 　 | FDD |
| 30 | 20 | 　 | 　 | 20 | 　 | 　 |
| 60 | 10 | 　 | 　 | 10 | 　 | 　 |

* Tentative agreements
* Recommended WF
	+ Agree on UL configuration firstly and check if companies can get agreement on MSD

### Sub-topic 3-7

**Issue 3-7: n71 35MHz REFSENS**

* Proposals summary

|  |  |  |  |
| --- | --- | --- | --- |
| **Operating Band** | **SCS kHz** | **35 MHz (dBm)**  | **Duplex Mode** |
|
|
|  |  | **Murata R4-2015432** | **QualcommR4-2014173** | **Skyworks R4-2016010**  | **AppleR4-2016295** | **MediaTek R4-2014186** |  |
| n71 | 15 | -67.6 | 69.9 | -66.5 | -62.5 | -70.5 | FDD |
| 30 | -67.7 | 　 | -66.6 | -63.9 | -70.8 |
| 60 | 　 | 　 | 　 | 　 | 　 |
|  |  |  |  |  |  |  |  |
| **Operating Band** | **SCS kHz** | **35 MHz**  | **Duplex Mode** |
|
|
|  |  | **Murata R4-2015432** | **QualcommR4-2014173** | **Skyworks R4-2016010** | **AppleR4-2016295** | **MediaTek R4-2014186** |  |
| n71 | 15 | 20 | 16 | 25 | 8 | 20 | FDD |
| 30 | 10 | 　 | 10 | 4 | 10 |
| 60 | 　 | 　 | 　 | 　 | 　 |

* Tentative agreements
* Recommended WF
	+ Agree on UL configuration firstly and check if companies can get agreement on MSD

### Sub-topic 3-8

**Issue 3-8: n7 35 MHz A-MPR**

* Proposals
* A-MPR regions for in R4-2014173,

|  |  |  |  |
| --- | --- | --- | --- |
| **Channel Bandwidth, MHz** | **Carrier Center Frequency, Fc, MHz** | **Regions** | **A-MPR** |
| **RBend\*12\*SCS** | **LCRB\*12\*SCS** |
| **MHz** | **MHz** |
| 35 MHz | 2517.5 ≤ FC ≤ 2552.5 | ≥0, <2.7 | >0 | A4 |
| ≥2.7, <13.5 | >max (0, 12\*SCS\*RBend –2.7) | A5 |
| ≥13.5, <23.76 | >9.0 | A6 |
| ≥23.76, <29.52 | >9.0 | A7 |
| ≥29.52 | >0 | A8 |

* A-MPR regions for in R4-2016027,

|  |  |  |  |
| --- | --- | --- | --- |
| Channel Bandwidth, MHz | Carrier Center Frequency, Fc, MHz | Regions | A-MPR |
| RBend\*12\*SCSMHz | LCRB\*12\*SCSMHz |
| 35 MHz | 2517.5 ≤ FC ≤ 2552.5 | ≥0, <[2.7] | >0 | A4 |
| ≥[2.7], <[15.84] | >max (0, 12\*SCS\*RBend –[3.06]) | A5 |
| ≥[15.84], <[22.68] | >[12.6] | A6 |
| ≥[22.68], <[28.8] | >[9.36] | A7 |
| ≥[28.8] | >0 | A8 |

* Recommended WF
	+ The A-MPR value for NS\_46 can be reused and check if companies can get agreement on A-MPR regions.

### Sub-topic 3-9

**Issue 3-9: n25 and n66 A-MPR**

* Proposals
* in R4-2014173,

Updated NS\_03 requirement below:

|  |  |  |
| --- | --- | --- |
| **ΔfOOB** **MHz**  | **Channel bandwidth (MHz) / Spectrum emission limit (dBm)**  | **Measurement bandwidth**  |
| **5**  | **10**  | **15**  | **20**  | **25**  | **30**  | **35**  | **40**  | **45**  |
|  0-1  | -13   | -13   | -13  | -13   | -13   | -13   | -13  | -13  | -13  | 1 % of channel BW   |
|  1-6  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | 1 MHz  |
|  6-10  | -25  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | 1 MHz  |
|  10-15  |   | -25  | -13  | -13  | -13  | -13  | -13  | -13  | -13  | 1 MHz  |
|  15-20  |   |   | -25  | -13  | -13  | -13  | -13  | -13  | -13  | 1 MHz  |
|  20-25  |   |   |   | -25  | -13  | -13  | -13  | -13  | -13  | 1 MHz  |
|  25-30  |   |   |   |   | -25  | -13  | -13  | -13  | -13  | 1 MHz  |
|  30-35  |   |   |   |   |   | -25  | -13  | -13  | -13  | 1 MHz  |
|  35-40  |   |   |   |   |   |   | -25  | -13  | -13  | 1 MHz  |
|  40-45  |   |   |   |   |   |   |  | -25  | -13  | 1 MHz  |
|  45-50  |  |  |  |  |  |  |  |  | -25 | 1 MHz  |

**Proposal 2**: Use same NS\_03 AMPR for 35MHz and 45MHz as specified in TS38.101-1.

* in R4-2016295,

**Observation 4**: Band n66 Tx with 45MHz CBW and NS\_43&NS\_43U does not seem to require additional power reduction for CP-OFDM QPSK to comply with emission requirements.

* Recommended WF
	+ Agree on the updated NS\_03 requirement for 35MHz and 45MHz
	+ Agree to use same NS\_03 AMPR for 35MHz and 45MHz as specified in TS38.101-1

### Sub-topic 3-10

**Issue 3-10: n71 35 MHz A-MPR**

* Proposals
* in R4-2014173,

SEM requirements for NS\_35

|  |  |  |
| --- | --- | --- |
| **ΔfOOB (MHz)** | **Channel bandwidth (MHz) / Spectrum emission limit (dBm)** | **Measurement bandwidth** |
| **5** | **10** | **15** | **20** | **35** |
|  0-0.1  | -15   | -18   | -20  | -21  | -23.5  | 30 kHz   |
|  0.1-6  | -13  | -13  | -13  | -13  | -13  | 100 kHz  |
|  6-10  | -251   | -13  | -13  | -13  | -13  | 100 kHz  |
|  10-15  |   | -251  | -13  | -13  | -13  | 100 kHz  |
|  15-20  |   |   | -251   | -13   | -13   | 100 kHz  |
|  20-25  |   |   |   | -251   | -13 | 100 kHz  |
|  25-35  |  |  |  |  | -13 | 100 kHz  |
|  35-40 |  |  |  |  | -25 | 1 MHz |
|  | NOTE 1: The measurement bandwidth shall be 1 MHz  |

**Observation 1**: Further measurement study is required to determine the 35MHz NS\_35 AMPR impact.

* In R4-2016295,

**Observation 3**: Band n71 Tx with 35MHz CBW and filter rejection of 9dB in protected region requires additional power reduction of roughly 10dB for CP-OFDM QPSK to comply with coexistence requirements.

**Proposal 5:** RAN4 needs to consider either introducing additional power back off for n71 with 35MHz or the usage of asymmetric UL/DL.

* Recommended WF
	+ Agree on the SEM requirements for NS\_35
	+ Further discussion on the approach for protection close 3GPP bands
	+ Further study on the required A-MPR for NS\_35

## Companies views’ collection for 1st round

### Open issues

**Issue 3-1: Expanding Specification Tables**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Thanks to the good idea by using equations proportional to channel BW. But currently we still think using one column per channel BW is more straightforward (i.e. current way). |
| Huawei | It will change the existing table for other channel bandwidth and not sure if it need to be discussed in TEI. |
| Ericsson | Interesting idea with an equation, there is a risk of reduced readability/understanding though. Would be good to see an example before any agreement. Maybe this is a larger discussion than to be agreed and implemented as part of this WI. |
| Qualcomm | I think WF is a good idea to at least study to reduce complexity of table using formula-based approach for specifications. Many new intermediary BWs could be added in the future |
| Skyworks | We support an equations based approach like described in R4-2014911 wherever feasible (possibly additional SEM for n71..also) this is also a future proof way for more cases and can handle the mandatory/optional aspect also. It may be feasible to extend to other requirements |

**Issue 3-2: UL BW limitation**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Maybe we can add a note for the RB position to avoid the large MSD for the large UL BW. The discussion here seems similar with the discussion on the MSD for combination in thread #116  |
| Huawei | One clarification question: it is about channel bandwidth limitation or it is just RB restriction? |
| Qualcomm | Consider asymmetric UL/DL BW combination set 0 and set 1 based on UE capability with set 1 having the 35MHz UL BW. The requirements would still need to be defined for both set 0 and set 1.RB restriction and position can also be considered, but this also has same effect of restricting BW. |
| Skyworks | Asymmetric Tx/Rx with associated duplex distance allows to do the RB restriction and position clear and since image does not change from existing channel BW compared to the requested larger BW we don’t need any dMPR/AMPR work. This is the advantage versus only RB restriction. This is especially advantageous for n8 and n71 performance. |

**Issue 3-3: new BW handling**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | 1. Does it mean the 35/45M for all bands are optional? We think it should be discussed with the sub-topic 1-1.

2.It seems how to treat the 35M/45M for the band combination is out of the WID scope. Usually, when a existing band combination supports a new channel bandwidth, new BCS is needed. It depends on the proponents and similar situations are happened for the other bands. RAN4 is discussing the similar issues in thread [#146]  |
| Qualcomm | At least optional support for earlier release. |
| Skyworks | We agree that this is related to 1-1 but regardless we are concerned if 35MHz/and 45MHz becomes a generic mandatory BW we will see any band (and subsequent combinations) that supports up to 40 or 50MHz requesting 35MHz or 45MHz without real justification and result in a large work in terms of MSD/MPR/AMPR. This is not just a tick in a box work. For this reason at least within this release we do not believe these BW become available to any band. we have seen many errors/missed requirements because of new BW being treated in a basket approach. |
|  |  |

**Issue 3-4: n3 35MHz and 45MHz REFSENS**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Agree with UL configuration. The REFSEN values should be averaged among companies. |
| Huawei | Agree with UL configuration |
| Ericsson | Ok to average REFSEN |
| Qualcomm | Not supporting average. Let’s discuss science.40MHz REFSENS is already approved for n3 and Murata’s 45MHz value is lower than the approved 40MHz value, which is concerning. Perhaps the PA used by Murata was not an efficiently biased ET type PA which could lower the intermodulation between the CIM3 and TX signal. QC values are more in line with the requirements defined for both 30MHz and 40MHz that have TX distortion landing in RX BW. It is recommended that Skyworks provide measurement data as well. |
| Skyworks | Ok with UL configuration proposal. Need to come back with measurements for MSD proposal. We can’t agree with a REFSENS for 35/45MHz that is not consistent with 30 and 40MHz values |

**Issue 3-5: n8 35MHz REFSENS**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm | * Apple’s analysis is pessimistic because it assumes TX signal would act like an IBB2 blocker which would be 12dB higher than the standard -44dBm, and REFSENS would be derived by the amount signal level to be raised 11.5+12=23.5dB to overcome the scaled IBB2 blocker of -32dBm.
	+ Problem with approach is that at max power, IM3 of Image and TX, causes de-sense.
	+ Also, per 36.101, the IBB2 blocker test range needs to be modified for any channel BW at the lower part of RF band.

Murata’s value for n8 should not be much different than the value for n71 |
| Skyworks | MSD:We present 3 MSD evaluations: worst case 35M UL / 35M DL, worst case 20M UL/35M DL and best case 20M UL/35M DL. Our preference is to restrict UL CBW operation to 20MHz as MSD can be moderate (worst case) to neglectable (best case ). If acceptable, our proposal 1 can be modified to propose 20MHz UL best and worst case REFSENSE.UL configuration: We show that Tx noise in Rx is nearly constant over LCRB range: 10-60RBs. So all values proposed are acceptable. We propose LCRB=25RB . In any case we believe limitation of UL BW should be seriously considered as it provides best MSD and no rework on UL side, ultimately providing the best case DL throughput and range. |
|  |  |
|  |  |

**Issue 3-6: n25 35MHz and 45 MHz REFSENS**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm | Same comments as in n3 |
| Skyworks | UL configuration: for 35MHz, we do not expect any impact between 40 or 45 LCRB. For 45MHz, we also do not expect major impact on Tx noise level but would need measurements to confirm.REFSENS: We need to come back with measurement data to confirm proposed values. |
|  |  |
|  |  |

**Issue 3-7: n71 35MHz REFSENS**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm | Same comments as in n71 |
| Skyworks | Same comment as for n8.UL configuration: We show that Tx noise in Rx is nearly constant over LCRB range: 10-60RBs. So all values proposed are acceptable. We propose LCRB=25RB .MSD:We present 3 MSD evaluations: worst case 35M UL / 35M DL, worst case 20M UL/35M DL and best case 20M UL/35M DL. Our preference is to restrict UL CBW operation to 20MHz as MSD can be moderate (worst case) to neglectable (best case). If acceptable, our proposal 1 can be modified to propose 20MHz UL best and worst case REFSENSE.We also present A-MPR measurements which show that restricting UL to 20MHz not only improves DL REFSENSE but also enhances uplink performance since no A-MPR is needed. 35MHz Uplink leads to high MSD (22dB) and high A-MPR (12 – 14 dB)In any case we believe limitation of UL BW should be seriously considered as it provides best MSD and no rework on UL side, ultimately providing the best case DL throughput and range. |
|  |  |
|  |  |

**Issue 3-8: n7 35 MHz A-MPR**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Qualcomm | Common ground between QC and SWKS:* QCOM thresholds are based on actual RB sweeps for CIM3, 5th order, and IM3 distortion except TBD1, TBD2, and TBD3.
* SWKS thresholds are based on interpolation
* Potential agreement/compromise/common ground will contain thresholds from actual RB sweeps and choose between TBDX=[SWKS, QCOM]: TBD1 = [15.84, 13.5], TBD2=[3.06, 2.7], and TBD3=[12.6, 9]
 |
| Skyworks | Both proposals are similar, we are open to discuss threshold with other companies. |
|  |  |
|  |  |

**Issue 3-9: n25 and n66 A-MPR**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Agree with the Updated NS\_03 requirement. We have the same proposals in R4-2015044. |
| Ericsson | Agreed |
| Qualcomm | Prefer to use same NS\_03 AMPR for 35MHz and 45MHz as specified in TS38.101-1 with agreed requirement |
| Skyworks | We propose to use equation based approach so that we don’t need to explicitely need to introduce 35 and 45MHz. This approach is already use fo DC and CA and is described in R4-2014911. Note that this is not needed for asymmetric UL/DL with UL limited at 20MHz |
|  |  |

**Issue 3-10: n71 35 MHz A-MPR**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| ZTE | Agree with the SEM requirement for NS\_35. We have the same proposals in R4-2015044. |
| Ericsson | Agree on the SEM requirements, support WF |
| Qualcomm | Agree on recommended WF. |
| Skyworks | Agree on SEM requirements, we provide initial A-MPR measurements that indicate at least 12dB is needed. Further measurements are needed. Same comment than for NS\_03 on using equation based table. Note that this is not needed for asymmetric UL/DL with UL limited at 20MHz |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
|  |  |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
|  |  |  |

## Discussion on 2nd round (if applicable)

|  |  |
| --- | --- |
| **WF number** | **Comments collection** |
|  |  |
|  |
|  |
|  |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
|  |  |

# Topic #4: UE draft CRs

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2015044 | ZTE Corporation | On UE RF requirement for new channel bandwidth of 35MHz and 45MHz |
| R4-2015702 | Huawei, HiSilicon | Draft CR for TS 38.101: introduction of channel bandwidths 35MHz and 45MHz for general part |
| R4-2016059 | Ericsson | Draft CR to add 35MHz and 45 MHz Bandwidth to TS38.101-1 |
|  |  |  |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2015044 | Huawei: we suggest to focus on general part for this meeting since for the discussion on band specific requirement is ongoing. |
| Ericsson: Almost complete CR (with FFS in some places), still missing CA, SUL, etc combos that are still open for discussion. |
| Skyworks: we agreed with the values but too early to agree on CRs especially depending on whether these channel BW are mandatory/optional/generic to all bands… |
| R4-2015702 | ZTE: We think we capture all the possible changes in our contribution R4-2015044 by introducing 35/45M in the spec, not only for the ‘general part’ but also for the other parts although they are FFS for now. |
| Ericsson: Some editorial comments: In Table 7.4-1: no changes seen. In Table 7.5-1 & Table 7.5-3: & Table 7.6.2-1: & Table 7.7-1: new BWs not in right place in the tables. |
| Skyworks: we agreed with the values but too early to agree on CRs especially depending on whether these channel BW are mandatory/optional/generic to all bands… |
| R4-2016059 | ZTE: Incomplete clauses. We think we capture all the possible changes in our contribution R4-2015044 by introducing 35/45M in the spec, not only for the ‘general part’ but also for the other parts although they are FFS for now. |
| Ericsson: Agree with above comment, R4-2015044 more complete but CA, SUL etc combos missingSuggestion: Combine these three papers to a common joint CR for next meeting that can be circulated in advance. |
| Skyworks: we agreed with the values but too early to agree on CRs especially depending on whether these channel BW are mandatory/optional/generic to all bands… |
|  |  |
|  |
|  |

## Summary for 1st round

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |
|  |  |

## Discussion on 2nd round (if applicable)

# Topic #4: BS draft CRs

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2015703 | Huawei, HiSilicon | draft CR on introduction of channel bandwidths 35MHz and 45MHz for BS TX |
| R4-2015718 | Ericsson | Draft CR to TS 38.104: Introduction of CBWs 35 MHz and 45 MHz |
| R4-2015719 | Ericsson | Draft CR to TS 38.141-1: Introduction of CBWs 35 MHz and 45 MHz |
| R4-2015720 | Ericsson | Draft CR to TS 38.141-2: Introduction of CBWs 35 MHz and 45 MHz |
| R4-2016114 | ZTE Corporation | Discussion on BS RF requirement for new channel bandwidth of 35MHz and 45MHz |
| R4-2016115 | ZTE Corporation | Draft CR to TS 38.104: Introduction of 35MHz and 45MHz |
| R4-2016116 | ZTE Corporation | Draft CR to TS 38.141-1: Introduction of 35MHz and 45MHz |
| R4-2016117 | ZTE Corporation | Draft CR to TS 38.141-2: Introduction of 35MHz and 45MHz |
| R4-2016118 | ZTE Corporation | Draft CR to TS 37.104: Introduction of 35MHz and 45MHz |
| R4-2016119 | ZTE Corporation | Draft CR to 37.141: Introduction of 35MHz and 45MHz |
| R4-2016120 | ZTE Corporation | Draft CR to TS 37.105: Introduction of 35MHz and 45MHz |
| R4-2016121 | ZTE Corporation | Draft CR to 37.145-1: Introduction of 35MHz and 45MHz |
| R4-2016122 | ZTE Corporation | Draft CR to 37.145-2: Introduction of 35MHz and 45MHz |

## Companies views’ collection for 1st round

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2015703 | ZTE: spec version should be 17.0.0 instead of 16.5.0. In addition, in Table 6.6.3.2-3 Note 4, 35MHz/45MHz is missing. |
| Huawei: agree with the comments above |
|  |
| R4-2015718 | ZTE:spec version should be 17.0.0 instead of 16.5.0. Table 6.6.3.2-2a and 6.6.3.2-3, 35MHz/45MHz is missing in Note 4.For dynamic range requirement, interfering signal power level is missing. For RX intermodulation, freq offse for NBB and general intermodulation is not aligned with ours, more discussion are needed.EVM window length is not added. |
|  |
|  |
| R4-2015719 | ZTE:spec version should be 17.0.0 instead of 16.5.0. For RX intermodulation, freq offse for NBB and general intermodulation is not aligned with ours, more discussion are needed. |
|  |
|  |
| R4-2015720 | ZTE: Table 6.7.3.5.1-2a and Table 6.7.3.5.1-3, 35MHz/45MHz is missing in the Note.For dynamic range requirement, interfering signal power level is missing for 45MHz.. For RX intermodulation, freq offse for NBB and general intermodulation is not aligned with ours, more discussion are needed. |
|  |
|  |
| R4-2016115 | Ericsson: missing clause 5 for transmission bandwidth configuration, guard band definition. Also a few differences in values calculated between Ericsson submitted CR on BS RF. As a suggestion, we would propose to perhaps pull out the requirements where there is a difference to assist in further discussion.  |
|  |
|  |
| R4-2016116 | Ericsson; Missing clause 6.5 EVM Test requirementAs a suggestion, we would propose to perhaps pull out the requirements where there is a difference to assist in further discussion.  |
|  |
|  |
| R4-2016117 | Ericsson: Missing updates to Table 6.6.3.5.1-2, 6.6.3.5.1-3, 6.6.3.5.1-4 including 35/45 MHz EVM window length for *BS type 1-O*.As a suggestion, we would propose to perhaps pull out the requirements where there is a difference to assist in further discussion.  |
|  |
|  |
| R4-2016118 |  |
|  |
|  |
| R4-2016119 |  |
|  |
|  |
| R4-2016120 |  |
|  |
|  |
| R4-2016121 |  |
|  |
|  |
| R4-2016122 |  |
|  |
|  |

## Summary for 1st round

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
|  |  |
|  |  |

## Discussion on 2nd round (if applicable)