**3GPP TSG-RAN4 Meeting #97-e *R4-2017088***

**Electronic Meeting, November 2-13, 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** | **1407** | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correction to timing requirements in NR-U | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_unlic-Core | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To clarify gradual timing adjustment also applied to CCA | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | It is clarified that the UE timing requirement on gradual timing adjustment is also when the reference cell is subject to CCA.  The UE initial transmission timing error requirements for CCA are explicitly defined in section 7.1.2. But gradual timing adjustment requirements are in separate section and it does not state anything about CCA. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | It may be misinterpreted that the UE timing requirement on gradual timing adjustment does not apply the when the reference cell is subject to CCA | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.1.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.533 | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**----------------------START OF CHANGES----------------------------**

7.1.2.1 Gradual timing adjustment

Requirements in this section shall apply regardless of whether the reference cell is on a carrier frequency subject to CCA or not.

When the transmission timing error between the UE and the reference timing exceeds ±Te then the UE is required to adjust its timing to within ±Te. The reference timing shall be  before the downlink timing of the reference cell. All adjustments made to the UE uplink timing shall follow these rules:

1) The maximum amount of the magnitude of the timing change in one adjustment shall be Tq.

2) The minimum aggregate adjustment rate shall be Tp per second.

3) The maximum aggregate adjustment rate shall be Tq per 200 ms.

where the maximum autonomous time adjustment step Tq and the aggregate adjustment rate Tp are specified in Table 7.1.2.1-1.

**Table 7.1.2.1-1: Tq Maximum Autonomous Time Adjustment Step and Tp Minimum Aggregate Adjustment rate**

|  |  |  |  |
| --- | --- | --- | --- |
| **Frequency Range** | **SCS of uplink signals (kHz)** | **Tq** | **Tp** |
| 1 | 15 | 5.5\*64\*Tc | 5.5\*64\*Tc |
|  | 30 | 5.5\*64\*Tc | 5.5\*64\*Tc |
|  | 60 | 5.5\*64\*Tc | 5.5\*64\*Tc |
| 2 | 60 | 2.5\*64\*Tc | 2.5\*64\*Tc |
|  | 120 | 2.5\*64\*Tc | 2.5\*64\*Tc |
| NOTE: Tc is the basic timing unit defined in TS 38.211 [6] | | | |

**----------------------END OF CHANGES----------------------------**