**3GPP TSG- RAN WG4 Meeting #97 *R4-2017361***

**Electronic Meeting, November - , 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **1373**  | **rev** | 2 | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | LTE\_NR\_DC\_CA\_enh-Perf  |  | ***Date:*** | 13 |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Introduction of accuracy requirements for MR-DC EMr idle mode measurements. |
|  |  |
| ***Summary of change:*** | Accuracy requirements for MR-DC measurements for early measurement reporting are introduced. |
|  |  |
| ***Consequences if not approved:*** | Specification of feature is incomplete |
|  |  |
| ***Clauses affected:*** | New sections: 10.1.2B, 10.1.3B, 10.1.4B, 10.1.5B, 10.1.7B, 10.1.8B, 10.1.9B, 10.1.10B, 10.2.4 and 10.2.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  |  |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Start of Change 1>

10.1.2 Intra-frequency RSRP accuracy requirements for FR1

10.1.2.1 Intra-frequency SS-RSRP accuracy requirements

10.1.2.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on the same frequency as that of the serving cell in FR1.

The accuracy requirements in Table 10.1.2.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

**Table 10.1.2.1.1-1: SS-RSRP Intra frequency absolute accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 2** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| ±4.5 | ±9 | ≥-6 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
| ±8 | ±11 | ≥-6 | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A,NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F,NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.2.1.2 Relative SS-RSRP Accuracy

The relative accuracy of SS-RSRP is defined as the SS-RSRP measured from one cell compared to the SS-RSRP measured from another cell on the same frequency, or between any two SS-RSRP levels measured on the same cell in FR1.

The accuracy requirements in Table 10.1.2.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

**Table 10.1.2.1.2-1: SS-RSRP Intra frequency relative accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot Note 2** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 4** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±2 | ±3 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| ±3 | ±3 | ≥-6 | Note 3 | Note 3 | Note 3 | N/A | Note 3 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies.NOTE 3: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 4: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.2.2 Void

10.1.2B Intra-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements

10.1.2B.1 Intra-frequency SS-RSRP accuracy requirements

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRP.

10.1.2B.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on the same frequency as that of the serving cell in FR1.

The accuracy requirements in Table 10.1.2B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

**Table 10.1.2B.1.1-1: SS-RSRP Intra frequency absolute accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 2** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| [±6] | [±10.5] | [≥-6] | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
| [±9.5] | [±12.5] | [≥-6] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A,NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F,NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.3 Intra-frequency RSRP accuracy requirements for FR2

10.1.3.1 Intra-frequency SS-RSRP accuracy requirements

10.1.3.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on the same frequency as that of the serving cell in FR2.

The accuracy requirements in Table 10.1.3.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.3.1.1-1: SS-RSRP Intra frequency absolute accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |  |
| ±6 | ±9 | ≥-6 | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | N/A | -70 |
| ±8 | ±11 |  | N/A | -70 | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

10.1.3.1.2 Relative SS-RSRP Accuracy

The relative accuracy of SS-RSRP is defined as the SS-RSRP measured from one cell compared to the SS-RSRP measured from another cell on the same frequency, or between any two SS-RSRP levels measured on the same cell in FR2.

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.3.1.2-1: SS-RSRP Intra frequency relative accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |
| ±6 | ±9 | ≥-6 | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table.Note 4: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies. |

10.1.3B Intra-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements

10.1.3B.1 Intra-frequency SS-RSRP accuracy requirements

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRP.

10.1.3B.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on the same frequency as that of the serving cell in FR2.

The accuracy requirements in Table 10.1.3B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.3B.1.1-1: SS-RSRP Intra frequency absolute accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |  |
| [±7.5] | [±10.5] | [≥-6] | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | N/A | -70 |
| [±9.5] | [±12.5] |  | N/A | -70 | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

<Start of Change 2>

10.1.4 Inter-frequency RSRP accuracy requirements for FR1

10.1.4.1 Inter-frequency SS-RSRP accuracy requirements

10.1.4.1.1 Absolute Accuracy of SS-RSRP in FR1

The requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on a frequency in FR1 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.4.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

**Table 10.1.4.1.1-1: SS-RSRP Inter frequency Absolute accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot Note 2** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 3** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| ±4.5 | ±9 | ≥-6 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
| ±8 | ±11 | ≥-6 | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A, NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F,NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: VoidNOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.4.1.2 Relative Accuracy of SS-RSRP in FR1

The relative accuracy of SS-RSRP in inter frequency case is defined as the RSRP measured from one cell on a frequency in FR1compared to the RSRP measured from another cell on a different frequency in FR1.

The accuracy requirements in Table 10.1.4.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] Clause 7.3 for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- |SSB\_RP1dBm - SSB\_RP2dBm| ≤ 27 dB

- | Channel 1\_Io ‑Channel 2\_Io | ≤ 20 dB

**Table 10.1.4.1.2-1: SS-RSRP Inter frequency relative accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot Note 2** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 3** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±4.5 | ±6 | ≥-6 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies.NOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.4.2 Void

10.1.4B Inter-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements

10.1.4B.1 Inter-frequency SS-RSRP accuracy requirements

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRP.

10.1.4B.1.1 Absolute Accuracy of SS-RSRP in FR1

The requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on a frequency in FR1 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.4B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

**Table 10.1.4B.1.1-1: SS-RSRP Inter frequency Absolute accuracy in FR1**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot Note 2** | **Io Note 1 range** |
|  |  |  | **NR operating band groups Note 3** | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** |  | **dBm / SCSSSB** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  |  | **SCSSSB = 15 kHz** | **SCSSSB = 30 kHz** |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -70 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -70 |
| [±6] | [±10.5] | [≥-6] | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -70 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -70 |
| [±9.5] | [±12.5] | [≥-6] | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A, NR\_SDL\_FR1\_A, NR\_FDD\_FR1\_B, NR\_TDD\_FR1\_C, NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D, NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E, NR\_FDD\_FR1\_F,NR\_FDD\_FR1\_G, NR\_FDD\_FR1\_H | N/A | N/A | -70 | -50 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: VoidNOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

10.1.5 Inter-frequency RSRP accuracy requirements for FR2

10.1.5.1 Inter-frequency SS-RSRP accuracy requirements

10.1.5.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on a frequency in FR2 that is on a different frequency than the serving cell.

The accuracy requirements in Table 10.1.5.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.5.1.1-1: SS-RSRP Inter frequency absolute accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |  |
| ±6 | ±9 | ≥-4 | Same value as SSB\_RP in Table B.2.3-2, according to UE Power class, operating band and angle of arrival | N/A | -70 |
| ±8 | ±11 |  | N/A | -70 | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

10.1.5.1.2 Relative SS-RSRP Accuracy

The relative accuracy of SS-RSRP is defined as the SS-RSRP measured from one cell on a frequency in FR2 compared to the SS-RSRP measured from another cell on another frequency in FR2.

The accuracy requirements in Table 10.1.5.1.2-1 are valid under the following conditions:

- Conditions defined in 38.101-2 [19] Clause 7.3 for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- |SSB\_RP1dBm - SSB\_RP2dBm| ≤ 27dB

- | Channel 1\_Io ‑Channel 2\_Io | ≤ 20 dB

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.5.1.2-1: SS-RSRP Inter frequency relative accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |
| ±6 | ±9 | ≥-4 | Same value as SSB\_RP in Table B.2.3-2, according to UE Power class, operating band and angle of arrival | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table.Note 4: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies. |

10.1.5.2 Void

10.1.5B Inter-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements

10.1.5B.1 Inter-frequency SS-RSRP accuracy requirements

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRP.

10.1.5B.1.1 Absolute SS-RSRP Accuracy

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRP in this clause apply to a cell on a frequency in FR2 that is on a different frequency than the serving cell.

The accuracy requirements in Table 10.1.5B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

**Table 10.1.5B.1.1-1: SS-RSRP Inter frequency absolute accuracy in FR2**

|  |  |
| --- | --- |
| **Accuracy** | **Conditions** |
| **Normal condition** | **Extreme condition** | **SSB Ês/Iot** | **Io Note 2 range** |
|  |  |  | **Minimum Io** | **Maximum Io** |
| **dB** | **dB** | **dB** | **dBm / SCSSSB Note 1** | **dBm/BWChannel** | **dBm/BWChannel** |
|  |  |  | **SCSSSB = 120kHz** | **SCSSSB = 240kHz** |  |  |
| [±7.5] | [±10.5] | [≥-4] | Same value as SSB\_RP in Table B.2.3-2, according to UE Power class, operating band and angle of arrival | N/A | -70 |
| [±9.5] | [±12.5] |  | N/A | -70 | -50 |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

<Start of Change 3>

### 10.1.7 Intra-frequency RSRQ accuracy requirements for FR1

#### 10.1.7.1 Intra-frequency SS-RSRQ accuracy requirements in FR1

##### 10.1.7.1.1 Absolute SS-RSRQ Accuracy in FR1

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on the same frequency as that of the serving cell in FR1.

The accuracy requirements in Table 10.1.7.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

Table 10.1.7.1.1-1: SS-RSRQ Intra frequency absolute accuracy in FR1

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range |
|  |  |  | NR operating band groups Note 3 | Minimum Io | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±2.5 | ±4 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| ±3.5 | ±4 | ≥-6 | Note 2 | Note 2 | Note 2 | Note 2 | Note 2 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

### 10.1.7B Intra-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements

#### 10.1.7B.1 Intra-frequency SS-RSRQ accuracy requirements in FR1

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRQ.

##### 10.1.7B.1.1 Absolute SS-RSRQ Accuracy in FR1

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on the same frequency as that of the serving cell in FR1.

The accuracy requirements in Table 10.1.7B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

Table 10.1.7B.1.1-1: SS-RSRQ Intra frequency absolute accuracy in FR1

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range |
|  |  |  | NR operating band groups Note 3 | Minimum Io | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| [±4] | [±5.5] | [≥-3] | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| [±5] | [±5.5] | [≥-6] | Note 2 | Note 2 | Note 2 | Note 2 | Note 2 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

### 10.1.8 Intra-frequency RSRQ accuracy requirements for FR2

#### 10.1.8.1 Intra-frequency SS-RSRQ accuracy requirements in FR2

##### 10.1.8.1.1 Absolute SS-RSRQ Accuracy in FR2

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on the same frequency as that of the serving cell in FR2.

The accuracy requirements in Table 10.1.8.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.8.1.1-1: SS-RSRQ Intra frequency absolute accuracy in FR2

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 2 range |
|  |  |  | Minimum Io | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 1 | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| ±2.5 | ±4 | ≥-3 | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| ±3.5 | ±4 | ≥-6 |  |  |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

### 10.1.8B Intra-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements

#### 10.1.8B.1 Intra-frequency SS-RSRQ accuracy requirements in FR2

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRQ.

##### 10.1.8B.1.1 Absolute SS-RSRQ Accuracy in FR2

Unless otherwise specified, the requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on the same frequency as that of the serving cell in FR2.

The accuracy requirements in Table 10.1.8B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for intra-frequency measurements are fulfilled according to Annex B.2.2 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.8B.1.1-1: SS-RSRQ Intra frequency absolute accuracy in FR2

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 2 range |
|  |  |  | Minimum Io | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 1 | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| [±4] | [±5.5] | [≥-3] | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| [±5] | [±5.5] | [≥-6] |  |  |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

<Start of Change 4>

### 10.1.9 Inter-frequency RSRQ accuracy requirements for FR1

#### 10.1.9.1 Inter-frequency SS-RSRQ accuracy requirements in FR1

##### 10.1.9.1.1 Aboslute Accuracy of SS-RSRQ in FR1

The requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on a frequency in FR1 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.9.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

Table 10.1.9.1.1-1: SS-RSRQ Inter frequency absolute accuracy in FR1

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range |
|  |  |  | NR operating band groups Note 3 | Minimum Io | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±2.5 | ±4 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| ±3.5 | ±4 | ≥-6 | Note 2 | Note 2 | Note 2 | Note 2 | Note 2 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

##### 10.1.9.1.2 Relative Accuracy of SS-RSRQ in FR1

The relative accuracy of SS-RSRQ in inter frequency case is defined as the RSRQ measured from one cell on a frequency in FR1 compared to the RSRP measured from another cell on a different frequency in FR1.

The accuracy requirements in Table 10.1.9.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- |SSB\_RP1dBm - SSB\_RP2dBm| ≤ 27 dB

- | Channel 1\_Io ‑Channel 2\_Io | ≤ 20 dB

Table 10.1.9.1.2-1: SS-RSRQ Inter frequency relative accuracy in FR1

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range |
|  |  | Note 2 | NR operating band groups Note 4 | Minimum Io | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| ±3 | ±4 | ≥-3 | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| ±4 | ±4 | ≥-6 | Note 3 | Note 3 | Note 3 | Note 3 | Note 3 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies.NOTE 3: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 4: NR operating band groups in FR1 are as defined in clause 3.5.2. |

### 10.1.9B Inter-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements

#### 10.1.9B.1 Inter-frequency SS-RSRQ accuracy requirements in FR1

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRQ.

##### 10.1.9B.1.1 Aboslute Accuracy of SS-RSRQ in FR1

The requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on a frequency in FR1 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.9B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-1 [18] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

Table 10.1.9B.1.1-1: SS-RSRQ Inter frequency absolute accuracy in FR1

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 1 range |
|  |  |  | NR operating band groups Note 3 | Minimum Io | Maximum Io |
| dB | dB | dB |  | dBm / SCSSSB | dBm/BWChannel | dBm/BWChannel |
|  |  |  |  | SCSSSB = 15 kHz | SCSSSB = 30 kHz |  |  |
|  |  |  | NR\_FDD\_FR1\_A, NR\_TDD\_FR1\_A,NR\_SDL\_FR1\_A | -121 | -118 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_B | -120.5 | -117.5 | N/A | -50 |
|  |  |  | NR\_TDD\_FR1\_C | -120 | -117 | N/A | -50 |
| [±4] | [±5.5] | [≥-3] | NR\_FDD\_FR1\_D, NR\_TDD\_FR1\_D | -119.5 | -116.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_E, NR\_TDD\_FR1\_E | -119 | -116 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_F | -118.5 | -115.5 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_G | -118 | -115 | N/A | -50 |
|  |  |  | NR\_FDD\_FR1\_H | -117.5 | -114.5 | N/A | -50 |
| [±5] | [±5.5] | [≥-6] | Note 2 | Note 2 | Note 2 | Note 2 | Note 2 |
| NOTE 1: Io is assumed to have constant EPRE across the bandwidth.NOTE 2: The same bands and the same Io conditions for each band apply for this requirement as for the corresponding highest accuracy requirement.NOTE 3: NR operating band groups in FR1 are as defined in clause 3.5.2. |

### 10.1.10 Inter-frequency RSRQ accuracy requirements for FR2

10.1.10.1 Inter-frequency SS-RSRQ accuracy requirements in FR2

10.1.10.1.1 Aboslute Accuracy of SS-RSRQ in FR2

The requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on a frequency in FR2 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.10.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.10.1.1-1: SS-RSRQ Inter frequency absolute accuracy in FR2

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 2 range |
|  |  |  | Minimum Io | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 1 | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| ±2.5 | ±4 | ≥-3 | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| ±3.5 | ±4 | ≥-4 |  |  |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

10.1.10.1.2 Relative Accuracy of SS-RSRQ in FR2

The relative accuracy of SS-RSRQ in inter frequency case is defined as the RSRQ measured from one cell on a frequency in FR2 compared to the RSRP measured from another cell on a different frequency in FR2.

The accuracy requirements in Table 10.1.10.1.2-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- |SSB\_RP1dBm - SSB\_RP2dBm| ≤ 27 dB

- | Channel 1\_Io ‑Channel 2\_Io | ≤ 20 dB

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.10.1.2-1: SS-RSRQ Inter frequency relative accuracy in FR2

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 2 range |
|  |  |  | Minimum Io | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 1 | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| ±3 | ±4 | ≥-3 | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| ±4 | ±4 | ≥-4 |  |  |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: The parameter SSB Ês/Iot is the minimum SSB Ês/Iot of the pair of cells to which the requirement applies.Note 4: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

### 10.1.10B Inter-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements

10.1.10B.1 Inter-frequency SS-RSRQ accuracy requirements in FR2

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRQ.

10.1.10B.1.1 Aboslute Accuracy of SS-RSRQ in FR2

The requirements for absolute accuracy of SS-RSRQ in this clause apply to a cell on a frequency in FR2 that has different carrier frequency from the serving cell.

The accuracy requirements in Table 10.1.10B.1.1-1 are valid under the following conditions:

- Conditions defined in clause 7.3 of TS 38.101-2 [19] for reference sensitivity are fulfilled.

- Conditions for inter-frequency measurements are fulfilled according to Annex B.2.3 for a corresponding Band for each relevant SSB.

- The measured signals are in the directions covered by the percentile EIS spherical coverage of the UE, defined in clause 7.3.4 of TS 38.101-2 [19].

Table 10.1.10B.1.1-1: SS-RSRQ Inter frequency absolute accuracy in FR2

|  |  |
| --- | --- |
| Accuracy | Conditions |
| Normal condition | Extreme condition | SSB Ês/Iot | Io Note 2 range |
|  |  |  | Minimum Io | Maximum Io |
| dB | dB | dB | dBm / SCSSSB Note 1 | dBm/BWChannel |
|  |  |  | SCSSSB = 120kHz | SCSSSB = 240kHz |  |
| [±4] | [±5.5] | [≥-3] | Same value as SSB\_RP in Table B.2.2-2, according to UE Power class, operating band and angle of arrival | -50 |
| [±5] | [±5.5] | [≥-4] |  |  |
| Note 1: Values based on Refsens and EIS spherical coverage as defined in clauses 7.3.2 and 7.3.4 of TS 38.101-2 [19]. Applicable side condition selected depending on angle of arrival.Note 2: Io specified at the Reference point, and assumed to have constant EPRE across the bandwidth.Note 3: In the test cases, the SSB Ês/Iot and related parameters may need to be adjusted to ensure Ês/Iot at UE baseband is above the value defined in this table. |

<Start of Change 5>

## 10.2 E-UTRAN measurements

### 10.2.1 Introduction

Accuracy requirements for measurements on E-UTRAN carrier frequencies are specified in clause 10.2 and apply for UE in SA or NR-DC or NE-DC operation mode, unless otherwise specified.

Unless otherwise specified, the requirements in clause 10.2 are applicable for a UE:

- in RRC\_CONNECTED state

- performing measurements with appropriate measurement gaps according to clause 9.1.2.

- that is synchronised to the cell that is measured.

The reported measurement result after layer 1 filtering shall be an estimate of the average value of the measured quantity over the measurement period. The reference point for the measurement result after layer 1 filtering is referred to as point B in the measurement model described in TS 36.300 [24].

The accuracy requirements of E-UTRA measurements in this clause are valid for the reported measurement result after layer 1 filtering. The accuracy requirements are verified from the measurement report at point D in the measurement model having the layer 3 filtering disabled.

If the UE needs measurement gaps to perform the inter-RAT NR ─ E-UTRAN FDD and NR ─ E-UTRAN TDD measurements, the relevant measurement procedure and measurement gap patterns stated in clause 9.1.2 shall apply.

### 10.2.2 E-UTRAN RSRP measurements

NOTE: This measurement is for handover between NR and E-UTRAN.

The measurement period of E-UTRA RSRP in RRC\_CONNECTED state is specified in clause 9.4.2 and 9.4.3.

The accuracy requirements of E-UTRA RSRP measurements in RRC\_CONNECTED state and the corresponding side conditions shall be the same as the inter-frequency RSRP Accuracy Requirements in clause 9.1.3 of TS 36.133 [15].

The reporting range and mapping specified for RSRP measurements in clause 9.1.4 of TS 36.133 [15] shall apply.

### 10.2.3 E-UTRAN RSRQ measurements

NOTE: This measurement is for handover between NR and E-UTRAN.

The measurement period of E-UTRA RSRQ in RRC\_CONNECTED state is specified in clause 9.4.2 and 9.4.3.

The accuracy requirements of E-UTRA RSRQ measurements in RRC\_CONNECTED state and the corresponding side conditions shall be the same as the inter-frequency RSRQ Accuracy Requirements in clause 9.1.6 of TS 36.133 [15].

The requirements for accuracy of E-UTRA RSRQ measurements in RRC\_CONNECTED state and the corresponding side conditions shall be the same as the inter-frequency RSRQ Accuracy Requirements in clause 9.1.6 of TS 36.133 [15].

The reporting range and mapping specified for RSRQ measurements in clause 9.1.7 of TS 36.133 [15] shall apply.

### 10.2.4 E-UTRAN RSRP measurements for CA/DC Idle Mode Measurements

NOTE: This measurement is for CA/DC Idle Mode measurements between NR and E-UTRAN.

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRP.

The measurement period of E-UTRA RSRP in RRC\_IDLE and RRC INACTIVE states are specified in clause 4.4.2.

The accuracy requirements of E-UTRA RSRP measurements in RRC\_IDLE and RRC INACTIVE states and the corresponding side conditions shall be as the inter-frequency RSRP Accuracy Requirements in clause 9.1.3B of TS 36.133 [15].

The reporting range and mapping specified for RSRP measurements in clause 9.1.4 of TS 36.133 [15] shall apply.

### 10.2.5 E-UTRAN RSRQ measurements for CA/DC Idle Mode Measurements

NOTE: This measurement is for CA/DC Idle Mode measurements between NR and E-UTRAN.

The requirements in this clause are applicable for a UE:

- in state RRC\_IDLE or RRC INACTIVE

- that is synchronised to the cell that is measured.

The requirements are for absolute accuracy of SS-RSRQ.

The measurement period of E-UTRA RSRQ in RRC\_IDLE and RRC INACTIVE states are specified in clause 4.4.2.

The accuracy requirements of E-UTRA RSRQ measurements in RRC\_IDLE and RRC INACTIVE states and the corresponding side conditions shall be as the inter-frequency RSRQ Accuracy Requirements in clause 9.1.6B of TS 36.133 [15].

The requirements for accuracy of E-UTRA RSRQ measurements in RRC\_IDLE and RRC INACTIVE states and the corresponding side conditions shall be the same as the inter-frequency RSRQ Accuracy Requirements in clause 9.1.6B of TS 36.133 [15].

The reporting range and mapping specified for RSRQ measurements in clause 9.1.7 of TS 36.133 [15] shall apply.

<End of Changes>