**3GPP TSG-RAN WG4 Meeting #97-e *R4-2017448***

**Electronic Meeting, 2nd – 13th Nov, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | **0116** | **rev** | **1** | **Current version:** | **15.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR: Updates to OCNG pattern reference |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** |  NR\_newRAT-Perf  |  | ***Date:*** | 2010-10-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | OCNG FDD pattern 1 and OCNG TDD pattern 2 are defined in Annex A.5, but ‘OCNG’ is wrongly configured for “Symbols for all unused REs” in the test parameters instead of OCNG pattern, it is easy to create confusion for testing. |
|  |  |
| ***Summary of change:*** | Specified the OCNG pattern to be applied for the “Symbols for all unused REs” in the test parameters |
|  |  |
| ***Consequences if not approved:*** | Confusion will still exist and wrong TE implementation will be caused. |
|  |  |
| ***Clauses affected:*** | 5.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.521-4  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | This is the revision of R4-2016424 |

*<The start of updates>*

## 5.2 PDSCH demodulation requirements

The parameters specified in Table 5.2-1 are valid for all PDSCH tests unless otherwise stated.

Table 5.2-1: Common test parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 2) | RBs | 0 |
| Subcarrier spacing | kHz | 15 or 30 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| RB offset | RBs | 0 |
| Number of contiguous PRB | PRBs | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | First SSB in Slot #0 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH | Symbols | 0, 1 |
| Number of PRBs in CORESET |  | Table 5.2-2 for tested channel bandwidth and subcarrier spacing |
| Number of PDCCH candidates and aggregation levels |  | 1/AL8 |
| CCE-to-REG mapping type |  | Non-interleaved |
| DCI format |  | 1\_1 |
| TCI state |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration |  | Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1 |
| Cross carrier scheduling |  | Not configured |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS  |  | k0=0 for CSI-RS resource 1,2,3,4 |
| First OFDM symbol in the PRB used for CSI-RS  |  |  l0 = 6 for CSI-RS resource 1 and 3l0 = 10 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | 'No CDM’ for CSI-RS resource 1,2,3,4 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | Slots | 15 kHz SCS: 20 for CSI-RS resource 1,2,3,430 kHz SCS: 40 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | Slots | 15 kHz SCS:10 for CSI-RS resource 1 and 211 for CSI-RS resource 3 and 430 kHz SCS:20 for CSI-RS resource 1 and 221 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS  |  | k0 = 0 |
| First OFDM symbol in the PRB used for CSI-RS  |  | l0 = 12 |
| Number of CSI-RS ports (X) |  | Same as number of transmit antenna |
| CDM Type |  | 'No CDM' for 1 transmit antenna'FD-CDM2' for 2 and 4 transmit antenna |
| Density (ρ) |  | 1 |
| CSI-RS periodicity | Slots | 15 kHz SCS: 2030 kHz SCS: 40 |
| CSI-RS offset | Slots | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS  |  | k0 = 4 |
| First OFDM symbol in the PRB used for CSI-RS  |  | l0 = 12 |
| Number of CSI-RS ports (X) |  | 4 |
| CDM Type |  | 'FD-CDM2' |
| Density (ρ) |  | 1 |
| CSI-RS periodicity | Slots | 15 kHz SCS: 2030 kHz SCS: 40 |
| CSI-RS offset | Slots | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| PDSCH DMRS configuration | Antenna ports indexes |  | {1000} for Rank 1 tests{1000, 1001} for Rank 2 tests{1000-1002} for Rank 3 tests{1000-1003} for Rank 4 tests |
| Position of the first DMRS for PDSCH mapping type A |  | 2 |
| Number of PDSCH DMRS CDM group(s) without data |  | 1 for Rank 1 and Rank 2 tests2 for Rank 3 and Rank 4 tests |
| TCI state #0 | Type 1 QCL information  | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | N/A |
| QCL Type |  | N/A |
| TCI state #1 | Type 1 QCL information  | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | N/A |
| QCL Type |  | N/A |
| PT-RS configuration |  | PT-RS is not configured |
| Maximum number of code block groups for ACK/NACK feedback |  | 1 |
| Maximum number of HARQ transmission |  | 4 |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| PDSCH & PDSCH DMRS Precoding configuration |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, and with PRB bundling granularity |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.Note 2: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. |

*<The next updates>*

## 5.3 PDCCH demodulation requirements

The receiver characteristics of the PDCCH are determined by the probability of miss-detection of the Downlink Scheduling Grant (Pm-dsg).

The parameters specified in Table 5.3-1 are valid for all PDCCH tests unless otherwise stated.

Table 5.3-1: Common test Parameters

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value** |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 1) |  | 0 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| RB offset | RBs | 0 |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | 1 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Number of PDCCH candidates |  | 1 |
| Frequency domain resource allocation for CORESET |  | Start from RB = 0 with contiguous RB allocation |
| TCI state |  | TCI state #1 |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (*k0*) |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | CSI-RS resource 1: 4CSI-RS resource 2: 8CSI-RS resource 3: 4CSI-RS resource 4: 8 |
| Number of CSI-RS ports (*X*) |  | 1 |
| CDM Type |  | No CDM |
| Density (*ρ*) |  | 3 |
| CSI-RS periodicity | Slots | 15 kHz SCS: 2030 kHz SCS: 40 |
| CSI-RS offset | Slots | 15 kHz SCS:10 for CSI-RS resource 1 and 211 for CSI-RS resource 3 and 430 kHz SCS:20 for CSI-RS resource 1 and 221 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| TCI state #0 | Type 1 QCL information  | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information  | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| PDCCH & PDCCH DMRS Precoding configuration |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination with REG bundling granularity for number of Tx larger than 1 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Note 1: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. |

*<The next updates>*

## 5.5A Sustained downlink data rate provided by lower layers

### 5.5A.1 FR1 CA requirements

*<Unchanged Sections Skipped>*

Table 5.5A-1: Common test parameters for FDD and TDD component carriers

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value** |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| EPRE ratio of PTRS to PDSCH | dB | N/A |
| Channel bandwidth | MHz | Channel bandwidth from selected CA bandwidth combination |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | First SSB in Slot #0 |
| SSB periodicity | ms | 20 |
| First DMRS position for Type A PDSCH mapping |  | 2 |
| Cross carrier scheduling |  | Not configured |
| Active DL BWP index |  | 1 |
| Actual carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 2) | RBs | 0 |
| Subcarrier spacing | kHz | 15 or 30 |
| DL BWP configuration #1 | RB offset | RBs | 0 |
| Number of contiguous PRB |  | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing |
| Subcarrier spacing | kHz | 15 or 30 |
| Cyclic prefix |  | Normal |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH |  | Symbols #0 |
| Number of PRBs in CORESET |  | Table 5.5A-4 |
| Number of PDCCH candidates and aggregation levels |  | 1/AL 1 for 30 kHz / 5 MHz 1/AL4 for 15 kHz / 5 MHz, 30 kHz / 10 MHz and 30 kHz / 15 MHz1/AL 8 for other combinations |
| CCE-to-REG mapping type |  | Non-interleaved |
| DCI format |  | 1\_1 |
| TCI State |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration |  | For 2Tx:Single Panel Type I, Random precoder chosen from precoder index 0 and 2, selection updated per slotFor 4Tx:Single Panel Type I, Random precoder chosen from precoders with i\_1,1 in {1,2,3,5,6,7} and i\_2 in {0,2}, selection updated per slot  |
| PDSCH configuration | Mapping type |  | Type A |
| k0 |  | 0 |
| PDSCH aggregation factor |  | 1 |
| PRB bundling type |  | Static |
| PRB bundling size |  | WB |
| Resource allocation type |  | Type 0 |
| VRB-to-PRB mapping type |  | Non-interleaved |
| VRB-to-PRB mapping interleaver bundle size |  | N/A |
| PDSCH DMRS configuration | DMRS Type |  | Type 1 |
| Number of additional DMRS |  | 1 |
| Length |  | 1 |
| Antenna ports indexes |  | {1000} for 1 Layer CCs{1000, 1001} for 2 Layers CCs{1000 – 1003} for 4 Layers CCs |
| Number of PDSCH DMRS CDM group(s) without data |  | 1 for 1 layer and 2 layers CCs2 for 4 Layers CCs |
| PTRS configuration |  | PTRS is not configured |
| CSI-RS for tracking | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 3 for CSI-RS resource 1,2,3,4 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 6 for CSI-RS resource 1 and 3l0 = 10 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2,3,4 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | Slots | 15 kHz SCS: 20 for CSI-RS resource 1,2,3,430 kHz SCS: 40 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | Slots | 15 kHz SCS:10 for CSI-RS resource 1 and 211 for CSI-RS resource 3 and 430 kHz SCS:20 for CSI-RS resource 1 and 221 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 4 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 12 |
| Number of CSI-RS ports (X) |  | Same as number of transmit antenna |
| CDM Type |  | 'FD-CDM2' |
| Density (ρ) |  | 1 |
| CSI-RS periodicity |  | 15 kHz SCS: 2030 kHz SCS: 40  |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 0 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 12 |
| Number of CSI-RS ports (X) |  | 4 |
| CDM Type |  | 'FD-CDM2' |
| Density (ρ) |  | 1 |
| CSI-RS periodicity |  | 15 kHz SCS: 2030 kHz SCS: 40 |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| TCI state #0 | Type 1 QCL information  | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | N/A |
| QCL Type |  | N/A |
| TCI state #1 | Type 1 QCL information  | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | N/A |
| QCL Type |  | N/A |
| Maximum number of code block groups for ACK/NACK feedback |  | 1 |
| Maximum number of HARQ transmission |  | 4 |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| PDSCH & PDSCH DMRS Precoding configuration |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination with PRB bundling granularity |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Propagation condition |  | Static propagation conditionNo external noise sources are applied |
| Antenna configuration | 1 layer CCs |  | 1x2 or 1x4 |
| 2 layers CCs |  | 2x2 or 2x4 |
| 4 layers CCs |  | 4x4 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmissionNote 2: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing |

*<The next updates>*

### 6.1.2 Common test parameters

Parameters specified in Table 6.1.2-1 are applied for all test cases in this clause unless otherwise stated.

Table 6.1.2-1: Test parameters for CSI test cases

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| Actual carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 3) | RBs | 0 |
| Subcarrier spacing | kHz | 15 or 30 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| RB offset | RBs | 0 |
| Number of contiguous PRB | PRBs | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing |
| Active DL BWP index |  | 1 |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | First SSB in Slot #0 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH |  | 0,1 |
| Number of PDCCH candidates and aggregation levels |  | 1/AL8 |
| DCI format |  | 1\_1 |
| TCI state |  | TCI state #1 |
| Cross carrier scheduling |  | Not configured |
| PDSCH configuration | Mapping type |  | Type A |
| *k0* |  | 0 |
| Starting symbol (S)  |  | 2 |
| Length (L) |  | 12 |
| PDSCH aggregation factor |  | 1 |
| PRB bundling type |  | Static |
| PRB bundling size |  | 2 |
| Resource allocation type |  | type 0 |
| VRB-to-PRB mapping type |  | Non-interleaved |
| VRB-to-PRB mapping interleaver bundle size |  | N/A |
| PDCCH & PDCCH DMRS Precoding configuration |  | Multi-path fading propagation conditions:Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1Static propagation conditions:Single Panel Type I, Random precoder chosen from precoder index 0 an 2, selection updated per slot |
| PDSCH DMRS configuration | DMRS Type |  | Type 1 |
| Number of additional DMRS |  | 1 |
| Maximum number of OFDM symbols for DL front loaded DMRS |  | 1 |
| DMRS ports indexes |  | {1000} for Rank1{1000,1001} for Rank2{1000,1001,1002} for Rank3{1000,1001,1002,1003} for Rank4 |
| Number of PDSCH DMRS CDM group(s) without data |  | 2 |
| PTRS configuration | Frequency density (*KPT-RS*) |  | N/A |
| Time density (*LPT-RS*) |  | N/A |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (*k0*) |  | 0 for CSI-RS resource 1,2,3,4 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | 4 for CSI-RS resource 1 and 38 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (*X*) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2,3,4 |
| Density (*ρ*) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | slot | 15 kHz SCS: 20 for CSI-RS resource 1,2,3,430 kHz SCS: 40 for CSI-RS resource |
| CSI-RS offset | slot | 15 kHz SCS:10 for CSI-RS resource 1 and 211 for CSI-RS resource 3 and 430 kHz SCS:20 for CSI-RS resource 1 and 221 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | N/A |
| QCL Type |  | N/A |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | N/A |
| QCL Type |  | N/A |
| Number of HARQ Processes |  | 4 For FDD8 for TDD |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| K1 value(PDSCH-to-HARQ-timing-indicator) |  | 2 for FDDFor FR1.30-1:8 if mod(i,10) = 06 if mod(i,10) = 25 if mod(i,10) = 35 if mod(i,10) = 44 if mod(i,10) = 53 if mod(i,10) = 6Where i is slot index per radio frame with 0~19 |
| Symbols for unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: PDSCH is not scheduled on slots containing CSI-RS or slots which are not full DL.Note 2: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.Note 3: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. |

*<The third updates>*

## 7.2 PDSCH demodulation requirements

The parameters specified in Table 7.2-1 are valid for all PDSCH demodulation tests unless otherwise stated.

Table 7.2-1: Common Test Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| PTRS *epre-Ratio* |  | 0 |
| Actual carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 2) | RBs | 0 |
| Subcarrier spacing | kHz | 60 or 120 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| RB offset | RBs | 0 |
| Number of contiguous PRB | PRBs | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | 1 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH |  | 0 |
| Number of PRBs in CORESET |  | Table 7.2-2 for tested channel bandwidth and subcarrier spacing |
| Number of PDCCH candidates and aggregation levels |  | 1/AL8 |
| CCE-to-REG mapping type |  | Non-interleaved |
| DCI format |  | 1\_1 |
| TCI state |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration |  | Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1 |
| Cross carrier scheduling |  | Not configured |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (*k0*) |  | 0 for CSI-RS resource 1,2,3,4 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | 6 for CSI-RS resource 1 and 310 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (*X*) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2,3,4 |
| Density (*ρ*) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80 for CSI-RS resource 1,2,3,4120 kHz SCS: 160 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | Slots | 60 kHz SCS: 40 for CSI-RS resource 1 and 241 for CSI-RS resource 3 and 4120 kHz SCS:80 for CSI-RS resource 1 and 281 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS (*k0*) |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | 12 |
| Number of CSI-RS ports (*X*) |  | 2 |
| CDM Type |  | FD-CDM2 |
| Density (*ρ*) |  | 1 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80120 kHz SCS: 160 |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | First subcarrier index in the PRB used for CSI-RS (k0) |  | 4 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | 12 |
| Number of CSI-RS ports (*X*) |  | 4 |
| CDM Type |  | FD-CDM2 |
| Density (*ρ*) |  | 1 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80120 kHz SCS: 160 |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| CSI-RS for beam refinement | First subcarrier index in the PRB used for CSI-RS  |  | k0=0 for CSI-RS resource 1,2 |
| First OFDM symbol in the PRB used for CSI-RS  |  | l0 = 8 for CSI-RS resource 1l0 = 9 for CSI-RS resource 2 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80 for CSI-RS resource 1,2120 kHz SCS: 160 for CSI-RS resource 1,2 |
| CSI-RS offset | Slots | 0 for CSI-RS resource 1,2 |
| Repetition |  | ON |
| QCL info |  | TCI state #1 |
| PDSCH DMRS configuration | Antenna ports indexes |  | {1000} for Rank 1 tests{1000, 1001} for Rank 2 tests |
| Position of the first DMRS for PDSCH mapping type A |  | 2 |
| Number of PDSCH DMRS CDM group(s) without data |  | 1 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| PTRS configuration | Frequency density (*KPT-RS*) |  | 2 |
| Time density (*LPT-RS*) |  | 1 |
| Resource Element Offset |  | 2 |
| Maximum number of code block groups for ACK/NACK feedback |  | 1 |
| Maximum number of HARQ transmission |  | 4 |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| PDSCH & PDSCH DMRS Precoding configuration |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination, andwith Wideband granularity |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.Note 2: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing. |

Table 7.2-2: Number of PRBs in CORESET

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SCS (kHz) | 50 MHz | 100 MHz | 200 MHz | 400 MHz |
| 60 | 66 | 132 | 264 | N.A |
| 120 | 30 | 66 | 132 | 264 |

*<The next updates>*

## 7.3 PDCCH demodulation requirements

The receiver characteristics of the PDCCH are determined by the probability of miss-detection of the Downlink Scheduling Grant (Pm-dsg).

The parameters specified in Table 7.3-1 are valid for all PDCCH tests unless otherwise stated.

Table 7.3-1: Common test Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 1) |  | 0 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | 1 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Number of PDCCH candidates |  | 1 |
| Frequency domain resource allocation for CORESET |  | Start from RB = 0 with contiguous RB allocation |
| TCI state |  | TCI state #1 |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (k0) |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | CSI-RS resource 1: 4CSI-RS resource 2: 8CSI-RS resource 3: 4CSI-RS resource 4: 8 |
| Number of CSI-RS ports (X) |  | 1 |
| CDM Type |  | No CDM |
| Density (ρ) |  | 3 |
| CSI-RS periodicity | Slots | 160 |
| CSI-RS offset | Slots | 80 for CSI-RS resource 1 and 281 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for beam management | First subcarrier index in the PRB used for CSI-RS (k0) |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (l0) |  | CSI-RS resource 1: 8CSI-RS resource 2: 9 |
| Number of CSI-RS ports (X) |  | 1 |
| CDM Type |  | No CDM |
| Density (ρ) |  | 3 |
| CSI-RS periodicity | Slots | 120 kHz SCS: 160 for CSI-RS resource 1,2 |
| CSI-RS offset | Slots | 0 for CSI-RS resource 1,2 |
| Repetition |  | ON |
| QCL info |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration |  | Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Note 1: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. |

*<The next updates>*

## 7.5A Sustained downlink data rate provided by lower layers

### 7.5A.1 FR2 CA requirements

*<Unchanged Sections Skipped>*

Table 7.5A.1-1: Test parameters for FR2 TDD

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| PTRS epre-Ratio |  | 0 |
| Channel bandwidth | MHz | Channel bandwidth from selected CA bandwidth combination |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | First SSB in Slot #0 |
| SSB periodicity | ms | 20 |
| First DMRS position for Type A PDSCH mapping |  | 2 |
| Cross carrier scheduling |  | Not configured |
| Active DL BWP index |  | 1 |
| Actual carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 3) | RBs | 0 |
| Subcarrier spacing | kHz | 60 or 120 |
| DL BWP configuration #1 | RB Offset |  | 0 |
| Number of contiguous PRB |  | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing |
| Subcarrier spacing | kHz | 60 or 120 |
| Cyclic prefix |  | Normal |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH |  | Symbols #0 |
| Number of PRBs in CORESET |  | Table 7.5A.1-2 |
| Number of PDCCH candidates and aggregation levels |  | 1/8 |
| CCE-to-REG mapping type |  | Non-interleaved |
| DCI format |  | 1-1 |
| TCI State |  | TCI state #1 |
| PDCCH &PDCCH DMRS Precoding configuration |  | Single Panel Type I, Random per slot with equal probability of precoder index 0 and 2, and with REG bundling granularity for number of Tx larger than 1 |
| PDSCH configuration | Mapping type |  | Type A |
| k0 |  | 0 |
| PDSCH aggregation factor |  | 1 |
| PRB bundling type |  | Static |
| PRB bundling size |  | WB |
| Resource allocation type |  | Type 0 |
| RBG size |  | Config2 |
| VRB-to-PRB mapping type |  | Non-interleaved |
| VRB-to-PRB mapping interleaver bundle size |  | N/A |
| Starting symbol (S)  |  | 1 |
| Length (L) |  | 13 |
| PDSCH DMRS configuration | DMRS Type |  | Type 1 |
| Number of additional DMRS |  | 1 |
| Length |  | 1 |
| Antenna ports indexes |  | {1000} for 1 Layer CCs{1000, 1001} for 2 Layers CCs |
| Number of PDSCH DMRS CDM group(s) without data |  | 1 |
| PTRS configuration | Frequency density (*KPT-RS*) |  | 2 |
| Time density (*LPT-RS*) |  | 1 |
| CSI-RS for tracking | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 3 for CSI-RS resource 1,2,3,4 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 6 for CSI-RS resource 1 and 3l0 = 10 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2,3,4 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80 for CSI-RS resource 1,2,3,4120 kHz SCS: 160 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | Slots | 60 kHz SCS:40 for CSI-RS resource 1 and 241 for CSI-RS resource 3 and 4120 kHz SCS:80 for CSI-RS resource 1 and 281 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 4 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 13 |
| Number of CSI-RS ports (X) |  | Same as number of transmit antenna |
| CDM Type |  | 'FD-CDM2' |
| Density (ρ) |  | 1 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80120 kHz SCS: 160  |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | Subcarrier indexes in the PRB used for CSI-RS |  | k0 = 0 |
| OFDM symbols in the PRB used for CSI-RS |  | l0 = 12 |
| Number of CSI-RS ports (X) |  | 4 |
| CDM Type |  | 'FD-CDM2' |
| Density (ρ) |  | 1 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80120 kHz SCS: 160 |
| CSI-RS offset |  | 0 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| CSI-RS for beam refinement | First subcarrier index in the PRB used for CSI-RS  |  | k0=0 for CSI-RS resource 1,2 |
| First OFDM symbol in the PRB used for CSI-RS  |  | l0 = 8 for CSI-RS resource 1l0 = 9 for CSI-RS resource 2 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2 |
| CSI-RS periodicity | Slots | 60 kHz SCS: 80 for CSI-RS resource 1,2120 kHz SCS: 160 for CSI-RS resource 1,2 |
| CSI-RS offset | Slots | 0 for CSI-RS resource 1,2 |
| Repetition |  | ON |
| QCL info |  | TCI state #1 |
| TCI state #0 | Tyoe 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Tyoe 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Tyoe 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Tyoe 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| Maximum number of code block groups for ACK/NACK feedback |  | 1 |
| Number of HARQ Processes |  | 10 for FR2.60-1 and 8 for FR2.120-1 |
| K1 value |  | Specific to each UL-DL pattern |
| Maximum number of HARQ transmission |  | 4 |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| TDD UL-DL pattern |  | 60 kHz SCS: FR2.60-1120 kHz SCS: FR2.120-1 |
| PDSCH & PDSCH DMRS Precoding configuration |  | Single Panel Type I, Precoder index 0 per slot with Wideband granularity for Rank 2  |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Propagation condition |  | Static propagation conditionNo external noise sources are applied |
| Antenna configuration | 1 layer CCs |  | 1x2 or 1x4 |
| 2 layers CCs |  | 2x2 or 2x4 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: PDSCH is scheduled only on full DL slots not containing SSB or TRS.Note 2: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.Note 3: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing. |

*<The Next Updates>*

### 8.1.2 Common test parameters

Parameters specified in Table 8.1.2-1 are applied for all test cases in this clause unless otherwise stated.

Table 8.1.2-1: Test parameters for CSI test cases

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Value |
| PDSCH transmission scheme |  | Transmission scheme 1 |
| Duplex Mode |  | TDD |
| PTRS *epre-Ratio* |  | 0 |
| Actual carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 3) | RBs | 0 |
| Subcarrier spacing | kHz | 120 |
| DL BWP configuration #1 | Cyclic prefix |  | Normal |
| RB offset | RBs | 0 |
| Number of contiguous PRB | PRBs | Maximum transmission bandwidth configuration as specified in clause 5.3.2 of TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing |
| Active DL BWP index |  | 1 |
| Common serving cell parameters | Physical Cell ID |  | 0 |
| SSB position in burst |  | First SSB in Slot #0 |
| SSB periodicity | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring |  | Each slot |
| Symbols with PDCCH |  | 0,1 |
| Number of PDCCH candidates and aggregation levels |  | 1/AL8 |
| DCI format |  | 1\_1 |
| TCI state |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration |  | Multi-path fading propagation conditions:Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1Static propagation conditions:Single Panel Type I, Random precoder chosen from precoder index 0 and 2, selection updated per slot |
| Cross carrier scheduling |  | Not configured |
| PDSCH configuration | Mapping type |  | Type A |
| *k0* |  | 0 |
| Starting symbol (S)  |  | 2 |
| Length (L) |  | 12 |
| PDSCH aggregation factor |  | 1 |
| PRB bundling type |  | Static |
| PRB bundling size |  | 2 |
| Resource allocation type |  | Type 0 |
| RBG size |  | Config2 |
| VRB-to-PRB mapping type |  | Non-interleaved |
| VRB-to-PRB mapping interleaver bundle size |  | N/A |
| PDSCH DMRS configuration | DMRS Type |  | Type 1 |
| Number of additional DMRS |  | 1 |
| DMRS ports indexes |  | {1000} for Rank1{1000,1001} for Rank2 |
| Maximum number of OFDM symbols for DL front loaded DMRS |  | 1 |
| Number of PDSCH DMRS CDM group(s) without data |  | 2 |
| PTRS configuration | Frequency density (*KPT-RS*) |  | 2 |
| Time density (*LPT-RS*) |  | 1 |
| Resource Element Offset |  | 2 |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (*k0*) |  | 0 for CSI-RS resource 1,2,3,4 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) |  | 4 for CSI-RS resource 1 and 38 for CSI-RS resource 2 and 4 |
| Number of CSI-RS ports (*X*) |  | 1 for CSI-RS resource 1,2,3,4 |
| CDM Type |  | No CDM for CSI-RS resource 1,2,3,4 |
| Density (*ρ*) |  | 3 for CSI-RS resource 1,2,3,4 |
| CSI-RS periodicity | slot | 120kHz SCS: 160 for CSI-RS resource 1,2,3,4 |
| CSI-RS offset | slot | 120 kHz SCS:80 for CSI-RS resource 1 and 281 for CSI-RS resource 3 and 4 |
| Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #0 |
| NZP CSI-RS for CSI acquisition | Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| QCL info |  | TCI state #1 |
| ZP CSI-RS for CSI acquisition | Frequency Occupation |  | Start PRB 0Number of PRB = BWP size |
| CSI-RS for beam refinement | First subcarrier index in the PRB used for CSI-RS  |  | k0=0 for CSI-RS resource 1,2 |
| First OFDM symbol in the PRB used for CSI-RS  |  | l0 = 8 for CSI-RS resource 1l0 = 9 for CSI-RS resource 2 |
| Number of CSI-RS ports (X) |  | 1 for CSI-RS resource 1,2 |
| CDM Type |  | 'No CDM' for CSI-RS resource 1,2 |
| Density (ρ) |  | 3 for CSI-RS resource 1,2 |
| CSI-RS periodicity | Slots | 120 kHz SCS: 160 for CSI-RS resource 1,2 |
| CSI-RS offset | Slots | 0 for CSI-RS resource 1,2 |
| Repetition |  | ON |
| QCL info |  | TCI state #1 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| Number of HARQ Processes |  | 8 |
| HARQ ACK/NACK bundling |  | Multiplexed |
| Redundancy version coding sequence |  | {0,2,3,1} |
| K1 value(PDSCH-to-HARQ-timing-indicator) |  | For FR2.120-1:3 if mod (i.5) = 0,6 if mod(i,5) = 2For FR2.120-2:11 if mod(i,8) = 0,7]if mod(i,8) = 4,6]if mod(i,8) = 5,where i is slot index per radio fame with values 0-79. |
| Symbols for unused REs |  | OP.1 FDD as defined in Annex A.5.1.1OP.1 TDD as defined in Annex A.5.2.1 |
| Physical signals, channels mapping and precoding |  | As specified in Annex B.4.1 |
| Note 1: PDSCH is not scheduled on slots containing CSI-RS or slots which are not full DL.Note 2: UE assumes that the TCI state for the PDSCH is identical to the TCI state applied for the PDCCH transmission.Note 3: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-2 [7] for tested channel bandwidth and subcarrier spacing. |

*<The Next Updates>*

### 9.1.2 E-UTRA Cell setup

This sub-clause provides the parameters for E-UTRA cell during the demodulation performance test for EN-DC unless otherwise stated. For EN-DC with multiple E-UTRA carriers or bands, randomly selected one carrier or band can be used as E-UTRA Pcell for the connection setup unless otherwise stated.

#### 9.1.2.1 FDD

The parameters specified in Table 9.1.2.1-1 and Table 9.1.2.1-2 are used to setup E-UTRA cell. One of test setup in Table 9.1.2.1-2 will be selected for the E-UTRA Cell depending on the maximum bandwidth of an E-UTRA carrier for all the EN-DC band combinations supported by the UE.

The measurement channels in Table 9.1.2.1-2 and OCNG pattern OP.1 FDD are specified in TS 36.101 [4]. The physical channel setup with downlink power allocation is according to Annex C.3.2 of TS 36.101 [4].

Table 9.1.2.1-1: Common Test Parameters (FDD)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value**  |
| Cyclic prefix |  | Normal |
| Physical Cell ID |  | 0 |
| Number of PDCCH symbols | symbols | 1 |
|  PHICH Ng (Note 1) |  | 1 |
| PHICH duration |  | Normal |
| Number of HARQ processes per component carrier | Processes | 8 |
| Maximum number of HARQ transmission |  | 4 |
| Redundancy version coding sequence |  | {0,0,1,2} for 64QAM |
| Propagation condition |  | Static propagation conditionNo external noise sources are applied |
| Transmission mode |  | 1 |
| Transmission time difference between E-UTRA cell and NR cell(s) | μs | 0 |
| Antenna configuration |  | All NR cells are in FR1: 1x2Any NR cell is in FR2: 1 TxNote 1 |
| Codebook subset restriction |  | 10 |
| Symbols for all unused REs |  | OP.1 FDD as defined in Annex A.5.1.1 |
| Note 1: As the link can be provided over the air, the UE Rx antenna configuration is not relevant for the test configuration and has no impact on the test implementation. |

Table 9.1.2.1-2: Specific Test Parameters (FDD [64QAM])

|  |  |  |
| --- | --- | --- |
| **Test setup** | **Bandwidth (MHz)** | **Downlink power allocation (dB)** |
|  |  | **σ** |
| 1 | 5 | 0 | 0 | 0 |
| 2 | 10 | 0 | 0 | 0 |
| 3 | 15 | 0 | 0 | 0 |
| 4 | 20 | 0 | 0 | 0 |

#### 9.1.2.2 TDD

The parameters specified in Table 9.1.2.2-1 and Table 9.1.2.2-2 are used to setup an E-UTRA cell. One of test setup in Table 9.1.2.2-2 will be selected for the E-UTRA Cell depending on the maximum bandwidth of an E-UTRA carrier for all the EN-DC band combinations supported by the UE.

The measurement channels in Table 9.1.2.2-2 and OCNG pattern OP.1 TDD are specified in TS 36.101 [4]. The physical channel setup with downlink power allocation is according to Annex C.3.2 of TS 36.101 [4].

Table 9.1.2.2-1: Common Test Parameters (TDD)

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Unit** | **Value**  |
| UL DL configuration |  | 2 (Note1) |
| Special subframe configuration |  | 7 |
| Number of PDCCH symbols | symbols | 1 |
| PHICH Ng (Note 3) |  | 1 |
| PHICH duration |  | Normal |
| Cyclic prefix |  | Normal |
| Cell ID |  | 0 |
| Maximum number of HARQ transmission |  | 4 |
| Redundancy version coding sequence |  | {0,0,1,2} for 64QAM |
| Propagation condition |  | Static propagation conditionNo external noise sources are applied |
| Transmission mode |  | 1 |
| Transmission time difference between E-UTRA cell and NR cell(s) | μs | 0 |
| Antenna configuration |  | All NR cells are in FR1: 1x2Any NR cell is in FR2: 1 TxNote 2 |
| Codebook subset restriction |  | 10 |
| Symbols for all unused REs |  | OP.1 TDD as defined in Annex A.5.2.1 |
| NOTE 1: The start of transmission of LTE frame is delayed by 2 LTE subframes with respect to the start of transmission of NR frame when TDD-TDD EN-DC configuration is configured during the test.NOTE 2: As the link can be provided over the air, the UE Rx antenna configuration is not relevant for the test configuration and has no impact on the test implementation. |

*<End of updates>*