**3GPP TSG-RAN WG4 Meeting # 97-e R4-20xxxxx**

**Electronic Meeting, 2 – 13 Nov., 2020**

**Agenda item:** 7.3.7.1 & 7.3.7.2

**Source:** Moderator (LG Electronics)

**Title:** Email discussion summary for [97e][317] V2X\_Demod\_Part1

**Document for:** Information

# Introduction

This email discussion is for Rel-16 NR V2X demodulation performance for single link in Agenda 7.3.7.1 and 7.3.7.2. For the information, in this meeting, email discussion will focus on finalizing the simulation assumptions, so draft CRs will be treated with low priority.

List of candidate target of email discussion for 2nd round as follows:

* 1st round:
	+ Topic#1 : Simulation assumption for performance requirements
		- Sub-topic 1-1: PSSCH demodulation
		- Sub-topic 1-2: PSCCH demodulation
		- Sub-topic 1-3: PSBCH demodulation
		- Sub-topic 1-4: PSFCH demodulation
		- Sub-topic 1-5: Resource pool configuration
	+ Topic#2 : Draft CRs for demodulation test cases
		- Sub-topic 2-1: Draft CR handling
* 2nd round:
	+ Topic#1 : Simulation assumption for performance requirements
		- Sub-topic 1-1: PSSCH demodulation
		- Sub-topic 1-2: PSCCH demodulation
		- Sub-topic 1-3: PSBCH demodulation
		- Sub-topic 1-4: PSFCH demodulation
		- Sub-topic 1-5: Resource pool configuration
	+ Topic#2: Draft CRs for demodulation test cases
		- Continue to collect comments for draft CR/CR

# Topic #1: Simulation assumptions for performance requirements

This section will treat simulation assumption for single link performance requirements.

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014417 | CATT | Observation 1: PSSCH DMRS position in time domain should not be overlapped with PSCCH when the sub-channel size is less than 20 PRB. Observation 2: it is difficult to avoid the overlapping case between PSSCH DMRS and PSCCH when sub-channel size is less than 20 RB.Proposal 1: Given that DMRS pattern is more likely to vary based on different SL UE velocities, it is proposed to increase the sub-channel size such that the sub-channel size is above 20 RB.Observation 3: The number of RE for 2nd stage SCI excluding the REs used for the 1st symbol and 2nd symbol should be multiple of PRB.Proposal 2: The number of RE for 2nd stage SCI in Option 1 should be configured as 246 where 2nd stage SCI occupies the total 13 PRB.Proposal 3: To specify the number of DMRS symbol based on the specific SL UE speed. Proposal 4: To introduce 1 S-SSB per SL period for PSBCH demodulation performance requirements (Option 1).Proposal 5: To reduce and simplify the test case, it is proposed to introduce either Case 1 or Case 2 or both.Proposal 6: It is proposed to reuse the TO and FO based on BS sync source in LTE V2X for NR V2X.Proposal 7: Do not introduce 256QAM demodulation test case in Rel-16. |
| R4-2014538 | Intel Corporation | Proposal 1: Use the following simulation assumptions for Rel-16 V2X PSSCH demodulation requirements with GNSS based synchronization:* PSFCH periodicity = 4 slots
* Test 1
	+ MCS 4
	+ PSSCH DMRS Time Pattern = {2, 4} (2 is for slots with PSFCH, 4 for slots without PSFCH)
	+ Channel model: TDLA30 – 2700
* Test 2
	+ MCS 11
	+ PSSCH DMRS Time Pattern = {2, 4} (2 is for slots with PSFCH, 4 for slots without PSFCH)
	+ Channel model: TDLA30 – 1400

Proposal 2: Use the following simulation assumptions for Rel-16 V2X PSSCH demodulation requirements with gNB based synchronization:* PSFCH periodicity = 4 slots
* MCS 17
* PSSCH DMRS Time Pattern = 2
* Channel model: TDLA30 – 180
* Proposal 3: Use the following simulation assumptions for Rel-16 V2X PSCCH demodulation requirements:
* SCI payload = 30 bits
* Channel model: TDLA30-1400

Proposal 4: Use the following simulation assumptions for Rel-16 V2X PSBCH demodulation requirements:* 1 S-SB per SL period
* Channel model: TDLA30-180

Proposal 5: Use the following simulation assumptions for Rel-16 V2X PSFCH demodulation requirements:* PSFCH periodicity 1 slot
* Channel model: TDLA30-180
* Test metrics: Pr (DTX to ACK) ≤ 1% and Pr (ACK miss) ≤ 1%.
 |
| R4-2014637 | Qualcomm, Inc. | Proposal 1: Introduce two tests for PSSCH with 64QAM MCS table with low speed 30km/h and high speed 500km/h. For high speed tests, consider the following configurations (a) TDL\_C 300ns channel (b) More subchannel allocation (c) Not configuring PSFCH. (a)+(b) is preferred in our opinion.Proposal 2: Configure 2 DMRS symbol for PSSCH low speed test.Proposal 3: PSSCH tests MCS configuration: MCS 21 for low speed, and MCS 4 for high speedProposal 4: Define the requirement based on subchannel size of 10RB for all PSSCH tests except high speed.Proposal 5: Define 256QAM PSSCH demod test with the same configuration as low speed PSSCH demod test configuration, only change the MCS to lowest one in 256QAM (MCS 20).Proposal 6: Set beta = 2.25 for all PSSCH tests.Proposal 7: Use relative speed of 260km/h and SCI 1 payload size = 28bits in PSCCH test.Proposal 8: Use 30km/h relative speed and no repetition for PSBCH test.Proposal 9: Consider 1 PSFCH in PSFCH detection performance test. Statistics to be collected:Option 2 (ACK/NACK type): Pr(NACK to ACK) < 0.1%.Option 1 (NACK only type): Pr(NACK miss) < 1%, or Pr(DTX to NACK)<1% (if we have DTX). |
| R4-2014652 | LG Electronics Inc. | Proposal 1: DMRS configuration for PSSCH demodulation should be considered depending on relative velocity as case 1 and case 3 in option 1.Proposal 2: PSFCH transmission should be considered every 4 slots.Proposal 3: QPSK and 64QAM modulation order should be considered for PSSCH demodulation requirementsProposal 4: 256QAM modulation order should be verified with applicability rule.Proposal 5: TDLA30-1350 should be used for PSCCH demodulation requirement.Proposal 6: Only ACK/NACK feedback mode should be considered for PSFCH demodulation (single link) requirement.Proposal 7: Use simulation assumptions Table 1~4 for single link tests |
| R4-2015640 | Huawei, HiSilicon | Proposal 1: Define the PSSCH performance requirements with first PSSCH DMRS FDMed with PSCCH.Proposal 2: Allocate 20 RBs for PSSCH and 10 RBs for PSCCH.Proposal 3: PSFCH is transmitted on every 4 slots for PSSCH test.Proposal 4: At least 260km/h and 500km/h should be used as candidate velocity for PSSCH performance test.Proposal 5: Use following receiver assumptions for PSSCH performance tests * CFO estimation: Cross-DMRS symbol CFO estimation.
* CE channel estimation:
	+ Frequency domain interpolation: MMSE interpolation
	+ Time domain interpolation: Linear interpolation
* RX window: CP/2 from GNSS

Proposal 6: Use following DMRS pattern for PSSCH performance test:* + Case 1: Max speed: 500km/h DMRS symbol: 4 for slots without PSFCH, 3 for slots with PSFCH.
	+ Case 2: Moderate speed: 260km/h DMRS symbol: 3 for slots without PSFCH, 2 for slots with PSFCH

Proposal 7: Use MCS 11 (16QAM, 378/1024) for 260 km/h and MCS 4 (QPSK, 308/1024) for 500km/h and not to define the 256 QAM performance requirements.Proposal 8: For 2nd-stage SCI configuration:* Set$ β\_{offset}^{SCI2}$=5 and $β\_{offset}^{SCI2}$=3.5 from Table 9.3-2 of TS 38.213 to guarantee the performance of 2nd-stage SCI for SCH\_Test1 and SCH\_Test2 of respectively.
* Use SCI format 2-A.

Proposal 9: Use 10% BLER as test metric.Proposal 10: Not introduce the case for gNB based synchronization reference sourceProposal 11: Adopt simulation assumptions in Table 2.1.2 for PSSCH performance test.Proposal 12: Use TDLA30-1350 as propagation conditions for performance requirements for PSCCH.Proposal 13: Set payloads to 28 bits for performance requirements for PSCCH.Proposal 14: Use TDLA30-180 as propagation condition for PSBCH demodulation performance Proposal 15: Use 2 S-SSBs within one period (i.e.160ms) without combining for PSBCH test.Proposal 16: Transmission of SLSS and PSBCH in the same slot during the test to keep consistent with core specificationProposal 17: Use TDLA-30-180 as propagation conditions for PSFCH performance requirements. Proposal 18: Only consider 1 CS pair for PSFCH performance requirement.Proposal 19: Only consider NACK/ACK case for single-link PSFCH performance requirement. |
| R4-2014537 | Intel Corporation | Proposal 1: Define SDR requirements with active Sidelink in the scope of Rel-16 V2X.Proposal 2: Define Rel-16 V2X demodulation requirements for different relative vehicle speeds: 30, 260 and 500 km/h.Proposal 3: Define Rel-16 V2X demodulation requirements for scenarios with gNB based synchronisation, relative vehicle speed 30 km/h, TX/RX frequency offset ±1300 Hz and TX/RX time offset ±24Ts.Proposal 4: Postpone the discussion on definition of 256QAM until simulation assumption for verification of basic V2X functionality will be stable.Proposal 5: Use the following resource pool configuration for V2X demodulation requirements with CBW 20 MHz and SCS 30 kHz: sub-channel size = 10 PRBs, number of sub-channels = 5. |
| R4-2014779 | MediaTek inc. | Proposal 1: 40MHz CBW should be configured for PSCCH/PSSCH decoding capability test.Proposal 2: The velocity configuration of NR V2X test case can reuse LTE V2X.Proposal 3: PSFCH should be transmitted on every slot and 3DMRS symbols for PSSCH test cases.Proposal 4: 1 S-SSB per SL period should be configured for 30kHz SCS.Proposal 5: Not to define 256QAM demodulation test case.Proposal 6: Not to define SDR with active sidelink test case.  |
| R4-2014419 | CATT | Initial simulation results |
| R4-2014668 | LG Electronics Inc. | Initial simulation results |
| R4-2015641 | Huawei, HiSilicon | Initial simulation results |

## Open issues summary

### Sub-topic 1-1 : PSSCH demodulation

**Issue 1-1-1: Sub-channel size**

* Proposals
	+ Option 1: 10 PRB sub-channel for low relative velocity and 20 sub-channel size for high relative velocity
	+ Option 2: 15 PRB sub-channel (with 15 PRB PSCCH)
	+ Option 3: 20 PRB sub-channel (with 10 PRB PSCCH)
	+ Option 4: lager than 20 PRB sub-channel
* Recommended WF
	+ Need further discussion.

**Issue 1-1-2: Modulation order (GNSS based sync)**

* Proposals: Introduce two test cases based on GNSS sync with
	+ Test 1: QPSK for 500km/h
	+ Test 2:
		- Option 1: 16QAM for 260km/h
		- Option 2: 64QAM for 30km/h
* Recommended WF
	+ Need further discussion

**Issue 1-1-3: PSFCH periodicity**

* Proposals:
	+ Option 1: 1 periodicity
	+ Option 2: 4 periodicity
* Recommended WF
	+ Need further discussion

**Issue 1-1-4: DMRS pattern**

* Proposals: Depending on decision of Issue 1-1-2,
	+ For 500km/h
		- Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4
		- Option 2: {3,4} DMRS symbols when PSFCH periodicity is 4
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1
	+ For 260km/h
		- Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4
		- Option 2: {2,3} DMRS symbols when PSFCH periodicity is 4
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1
	+ For 30km/h
		- Option 1: {2,3} DMRS symbols when PSFCH periodicity is 4
		- Option 2: 2 DMRS symbols when PSFCH periodicity is 1 or 4
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1

Note: {a,b} DMRS means the number of DMRS (a) with PSFCH symbol and (b) without PSFCH symbol in a slot.

* Recommended WF
	+ Need further discussion

**Issue 1-1-5: 2nd stage SCI allocation**

* Proposals:
	+ Option 1: beta = 2.25 for all test cases
	+ Option 2: beta = 5 for 16QAM test configuration and beta = 3.5 for QPSK test configuration
	+ Option 3: beta = 1.75, 2.5, and 4 for QPSK, 64QAM, and 256QAM test configuration, respectively
* Recommended WF
	+ Need further discussion

**Issue 1-1-6: gNB based sync test cases**

* Proposals:
	+ Option 1: Define performance requirement with 1300Hz FO and ±24Ts TO
	+ Option 2: Do not define performance requirement
* Recommended WF
	+ Need further discussion

**Issue 1-1-7: 256QAM test cases**

* Proposals:
	+ Option 1: Define performance requirement
	+ Option 2: Do not define performance requirement
* Recommended WF
	+ Need further discussion

**Issue 1-1-8: Propagation condition for high relative velocity**

* Proposals:
	+ Option 1: consider TDLC300ns
* Recommended WF
	+ Need further discussion

**Issue 1-1-9: Receiver assumption**

* Proposals:
	+ Option 1:
		- CFO estimation: Cross-DMRS symbol CFO estimation.
		- CE channel estimation:
			* Frequency domain interpolation: MMSE interpolation
			* Time domain interpolation: Linear interpolation
		- RX window: CP/2 from GNSS
* Recommended WF
	+ Need further discussion

### Sub-topic 1-2 : PSCCH demodulation

**Issue 1-2-1: Payload size**

* Proposals
	+ Option 1: 28 bit
	+ Option 2: 30bit
	+ Option 3: 24 bits
* Recommended WF
	+ Need further discussion.

**Issue 1-2-2: Relative velocity**

* Proposals
	+ Option 1: 260km/h
* Recommended WF
	+ Use 260km/h relative velocity (TDLA30-1400)

### Sub-topic 1-3 : PSBCH demodulation

**Issue 1-3-1: The number of S-SSB per one period**

* Proposals
	+ Option 1: 1 S-SSB
	+ Option 2: 2 S-SSBs
* Recommended WF
	+ Need further discussion.

**Issue 1-3-2: Relative velocity**

* Proposals
	+ Option 1: 30km/h
* Recommended WF
	+ Use 30km/h relative velocity (TDLA30-180)

### Sub-topic 1-4 : PSFCH demodulation

**Issue 1-4-1: Test metric**

* Proposals
	+ Option 1: Pr(DTX to ACK)<1% and Pr(ACK miss)<1%
	+ Option 2: Pr(DTX to ACK)<1% , Pr(ACK miss)<1% , and Pr(NACK to ACK) < 0.1%
	+ Option 3: Statistics to be collected:
		- ACK/NACK type: Pr(NACK to ACK) < 0.1%.
		- NACK only type: Pr(NACK miss) < 1%.
* Recommended WF
	+ Need further discussion.

**Issue 1-4-2: PSFCH periodicity**

* Proposals
	+ Option 1: 1 periodicity
	+ Option 2: 4 periodicity
* Recommended WF
	+ Need further discussion

**Issue 1-4-3: Number of Cyclic shift pairs**

* Proposals
	+ Option 1: 1
* Recommended WF
	+ Use 1 cyclic shift pair

**Issue 1-4-4: Relative velocity**

* Proposals
	+ Option 1: 30km/h
* Recommended WF
	+ Use 30km/h relative velocity (TDLA30-180)

### Sub-topic 1-5 : Resource pool configuration

**Issue 1-5-1: Resource pool configuration**

* Proposals
	+ Option 1: for V2X demodulation requirements with CBW 20 MHz and SCS 30 kHz: sub-channel size = 10 PRBs, number of sub-channels = 5
* Recommended WF
	+ Need further discussion.

## Companies views’ collection for 1st round

### Open issues

**Issue 1-1: PSSCH demodulation**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | **Issue 1-1-1: Sub-channel size**According to RAN1’s agreements for DMRS pattern limitation, to support high relative speed (500km/h), more than 3 DRMS symbols pattern should be considered, so 20 PRB sub-channel size is reasonable. For other tests, 10 or 20 PRB sub-channel size is fine for us. We support option 1 or option 3.**Issue 1-1-2: Modulation order (GNSS based sync)**We support option 2. Supporting 64QAM modulation for NR V2X is mandatory feature. So we need to consider 64QAM modulation order. And similar to LTE V2X test cases, low and high relative velocity can be considered for PSSCH test. **Issue 1-1-3: PSFCH periodicity**We prefer option 2**Issue 1-1-4: DMRS pattern**For 500km/h, we prefer option 2. For 30km/h, we prefer option 1.**Issue 1-1-5: 2nd stage SCI allocation**We don’t have strong view on these. However, it should be not affect the PSSCH coding rate due to the high beta value. **Issue 1-1-6: gNB based sync test cases**We don’t have strong view.**Issue 1-1-7: 256QAM test cases**We support option 1. This feature was first introduced in NR V2X to support high data rate and RAN4 agreed 256QAM modulation as optional feature. So, if the UE supporting 256QAM modulation should be tested. To reduce test cases, applicability rule can be considered to test 256QAM instead of 64QAM (if agreed).**Issue 1-1-8: Propagation condition for high relative velocity**We can check performance with TDLC300, but if more than 3 DMRS symbols are considered, current propagation model is available.**Issue 1-1-9: Receiver assumption** |
| QC | **Issue 1-1-1: Sub-channel size**We propose option one, since in a V2X network, in order to maximize system capacity to accommodate more SL UEs and transmissions, subchannel size of 10RB is the most common choice, especially in low speed scenario, in which usually with crowded cars. Moreover, since less RBs are allocated, less RSREs are available for channel estimation and this becomes the bottleneck scenario and need to be tested.**Issue 1-1-2: Modulation order (GNSS based sync)**For test 2, we support option 2. Since high speed is covered by 500km/h QPSK test, and highest modulation order supported needs to be tested, therefore, low speed test with 64QAM should be introduced. Otherwise 64QAM is out of test coverage.**Issue 1-1-3: PSFCH periodicity**Both options are fine for us.**Issue 1-1-4: DMRS pattern**500km/h: option 2 or option 3260km/h: option 2 and option 3 if being introduced as a test30km/h: option 2, our simulation shows that 2 DMRS performs better than 3 DMRS.**Issue 1-1-5: 2nd stage SCI allocation**We proposed option 1, but can compromise to option 2, given that better performance is shown.**Issue 1-1-6: gNB based sync test cases**We support option 2.**Issue 1-1-7: 256QAM test cases**We support option 1, since (1) optional feature still requires to be tested if UE declare support (2) if workload is an issue, this test can directly copy the 30km/h configuration, with MCS replaced by 20 in 256QAM table, the smallest MCS with 256QAM.**Issue 1-1-8: Propagation condition for high relative velocity**We propose this option, since larger delay spread can help CFO estimation in high speed scenario. But we are open to discuss other options.**Issue 1-1-9: Receiver assumption**Option 1 is good for us. |
| CATT | **Issue 1-1-1: Sub-channel size**Prefer option 3. We share the same view as LGE. Based on current DMRS patterns, it is difficult to avoid the overlapping case between PSSCH DMRS symbol and PSCCH symbol when sub-channel size is less than 20RB, especially for 3 and 4 DMRS pattern. For PSSCH test case, we prefer 20RB as sub-channel size.**Issue 1-1-2: Modulation order (GNSS based sync)**Prefer option 2. From the perspective of testing, the upper limit and lower limit are usually preferred to increase the test coverage. If 256QAM is not considered, 64QAM is expected to be tested.**Issue 1-1-3: PSFCH periodicity**Prefer Option 1. Option 2 is also acceptable.**Issue 1-1-4: DMRS pattern**If the periodicity of PSFCH is defined as 4, our preference of DMRS pattern is as follows:* For 500km/h: Option 2
* For 260km/h: Option 2
* For 30km/h: Option 2.

**Issue 1-1-5: 2nd stage SCI allocation**We don’t have strong view.**Issue 1-1-6: gNB based sync test cases**Option 1. The principle of LTE V2X can be reused.**Issue 1-1-7: 256QAM test cases**Prefer Option 2. 256QAM reception was agreed as an optional UE capability. Compared to 64QAM, 256QAM demodulation requires much higher SNR level that is difficult to be achieved in time-varying channel with different velocities.**Issue 1-1-8: Propagation condition for high relative velocity**No strong view.**Issue 1-1-9: Receiver assumption**Support Option 1. |
| Intel | **Issue 1-1-1: Sub-channel size**Our preference is to have 10 PRB sub-channel size for all tests with 20 MHz and 30 kHz, because such configuration allow to have efficient spectrum utilization. Same time, we are open to further discuss how many sub-channels will be allocated for PSSCH transmission. At current stage, our results show that performance with one sub-channel allocation is fine for different scenarios.**Issue 1-1-2: Modulation order (GNSS based sync)**We are fine to define test 2 with 16QAM or 64QAM. Same time, we suggest to have one PSSCH test with 260 km/h relative speed to show performance for medium speed conditions. Probably we can check 64QAM performance for 260 km/h scenario.**Issue 1-1-3: PSFCH periodicity**For PSSCH requirements, we prefer to consider PFSCH periodicity 4 to reduce overhead and verify correct UE processing of slots with and without PSFCH. PSFCH periodicity 1 can be considered for other tests.**Issue 1-1-4: DMRS pattern**For high and medium speed, probably further discussion is needed depending on discussion on Issues 1-1-1 and 1-1-4.For low speed, we think that 2 DMRS configuration is sufficient. (i.e. Option 2)**Issue 1-1-5: 2nd stage SCI allocation**Don’t have strong preference at current stage, we think that 2nd stage SCI configuration should be selected to balance between overhead and impact on PSSCH performance. Probably we can list several options for further analysis and decide in the next meeting. **Issue 1-1-6: gNB based sync test cases**As we showed in our General paper, FO and TO configuration will be worser in comparison to scenario with GNSS sync source. Usually, RAN4 define minimum requirements for the worst scenarios. Therefore, we think that it will be rather important to verify UE which support concurrent operation. If there is concern about number of tests, then we can further discuss the definition of applicability rule (e.g. UE can skip one test with GNSS sync source in case it passed test with gNB sync source).**Issue 1-1-7: 256QAM test cases**We prefer to keep this open or not define in Rel-16 time frame. Based on our understanding, due to this feature is optional for Tx and Rx, this feature is only applicable to unicast operation. Therefore, we suggest to focus on discussion of requirements for basic V2X features verification.**Issue 1-1-8: Propagation condition for high relative velocity**At current stage, we prefer to have same propagation conditions for scenarios with different speeds and keep agreement from previous meeting. Same time, we can further investigate if there are any issues with existing model and whether scenario with high delay spread is typical for high speed conditions.**Issue 1-1-9: Receiver assumption**We are fine to consider Option 1 for minimum requirements definition. Same time, we should not preclude any other UE implementation in case it allows to meet requirements. |
| Huawei: | **Issue 1-1-1: Sub-channel size**We support option 3. To Intel: According to the agreements of RAN 1 #102-3 meeting:

|  |
| --- |
| Agreements:* When a subchannel size is less than 20 PRBs and the size of PSCCH is less than the subchannel size, a TX UE is not expected to choose a PSSCH DMRS pattern to be transmitted in the same OFDM symbol with PSCCH.
 |

Even if we use 10 PRBs subchannel size with more than one sub-channels are allocated, only 2 DMRS symbols can be selected, it is difficult to guarantee the performance under the scenario with medium speed and high speedFor Option1, 10 RBs sub-channel allocation will cause that PSSCH is TDM with PSCCH which has been verified in Rel-15. Meanwhile, our purpose is to verify the single link demodulation performance, so spectrum utilization is not the key factors to be considered for PSCCH test. While for multi-link test such as PSCCH/PSSCH decoding capability and power imbalance test, 10 RBs sub-channel allocation can be considered.**Issue 1-1-2: Modulation order (GNSS based sync)**The suitable modulation order depends on speed. We think that at least 260km/h and 500km/h should be included, considering that 260km/h is very typical velocity for NR V2X for scenarios of vehicles platooning and advanced Driving as figured out in TS 22.186, at the same time according to our simulation results shown in R4-2015641, MCS 11 for 260km/h is feasible. If companies have strong views on 30km/h with 64QAM, we are also fine to include it.**Issue 1-1-3: PSFCH periodicity**We support option 2. We should configure PSFCH periodicity to 4 to reduce overhead. **Issue 1-1-4: DMRS pattern** According to our simulation results, we support option 2 for 500km/h and option 2 for 260km/h and option 1 or 2 for 30km/h (If agreed).To Intel, for 260km/h, according to our simulation results, we think 3 DMRS symbol is enough to guarantee the performance for slots without PSFCH. There is no need to set maximum 4 DMRS symbols.**Issue 1-1-5: 2nd stage SCI allocation**We support option 2, the principle to derive it is that the performance of 2nd stage SCI allocation should be guaranteed when the SNR satisfying 10% BLER for PSSCH is achieved. According to our simulation results in R4-2015640, 2nd stage SCI configuration in option 2 is reasonable.However, the 2nd stage SCI allocation not only depends on Beta-offset but also depends on MCS, DMRS pattern and sub-channel size. We propose to further discuss this issue after parameters such as MCS, DMRS pattern and sub-channel size have been determined.For how to select Beta-offset, we propose the following principle: the BLER of 2nd stage SCI should be lower than [1%] when SNR satisfying 10% BLER of PSSCH is achieved.**Issue 1-1-6: gNB based sync test cases**We prefer Option 2.**Issue 1-1-7:256 QAM test cases**We support option 2, 256QAM is not commonly used in group cast and broadcast scenarios. What’s more, the SNR @ 10% of BLER is very high (more than 20dB) for 256QAM and it is not possible to achieve such high in practical scenario. We prefer not define the performance requirements for 256 QAM. **Issue1-1-8: Propagation condition for high relative velocity**High speed is most used for scenarios with less obstacles, time delay shouldn’t be set such high as 300ns. From our simulation results, it is feasible to use TDLA-30, but we can further check TDL-C 300**Issue 1-1-9: Receiver assumption**Support option 1. |
| MTK | **Issue 1-1-1: Sub-channel size**Support option 3.We have the same view with CATT/HW.**Issue 1-1-2: Modulation order (GNSS based sync)**We are ok with test 1.For test 2, we prefer option 2. According to RAN1’s discussion, 64QAM modulation is mandatory for NR V2X, we suggest defining 64QAM test case. For speed configuration, we have similar view with LG.**Issue 1-1-3: PSFCH periodicity**Support option 1.If the PSFCH periodicity is 4 slots, DMRS pattern for PSSCH will be 4-symbol for most of slots. DMRS pattern for PSSCH will be always 3-symbol when PSFCH periodicity is 1 slot. To test UE’s performance in worst scenario, we suggest defining the test case with PSFCH transmission on every slot. **Issue 1-1-4: DMRS pattern**The DMRS pattern is related to velocity configuration. About PSSCH velocity configuration, we suggest reusing LTE V2X configuration, e.g., high speed (500km/h) and low speed (30km/h). Besides, as mentioned in issue 1-1-3, we think PSFCH should be configured within every slot. 3 DMRS symbols with PSFCH configuration also have the same DMRS symbol interval (3 symbols) with LTE V2X. Thus, we shall configure DMRS pattern as follows:* + For 500km/h
		- Option 3: 3 DMRS symbols and PSFCH periodicity is 1
	+ For 30km/h
		- Option 3: 3 DMRS symbols and PSFCH periodicity is 1

**Issue 1-1-5: 2nd stage SCI allocation**The beta offset of the 2nd stage SCI $β\_{offset}^{SCI2}$ should guarantee 2nd SCI have enough performance, which will not impact the PSSCH performance. From HW’s simulation results, it can be seen that beta = 3.5 for QPSK test is enough. We can further evaluate the specific beta offset value for 64QAM modulation.**Issue 1-1-6: gNB based sync test cases**Support option 2.The only difference between GNSS and gNB is timing offset, which can be guaranteed by RRM test. Besides, gNB is an optional feature. Thus, we suggest not to introduce this test.**Issue 1-1-7: 256QAM test cases**Support option 2.256QAM may need a high SNR, and it isn’t a practical NR V2X application scenarios. Especially, 256QAM performance mainly depends on RF front end and AGC other than baseband demodulation performance. Since V2X UE may use different hardware design with Uu link, it may be hard for RAN4 to discuss how to consider the additional RF margin for 256QAM.**Issue 1-1-8: Propagation condition for high relative velocity**We think that TDL-C 300ns is not a practical scenario in high speed. We have noticed QC’s concern about the PSSCH performance. we suggest to evaluate the PSSCH performance with more RBs firstly in RAN4.**Issue 1-1-9: Receiver assumption**We are Ok with the proposal. |
| QC | **Issue 1-1-8: Propagation condition for high relative velocity**We see some concerns from above comments on TDL\_C 300ns, here are a few alternatives to avoid the error floor we observed, for second round discussion:1. Lower MCS
2. Instead of TDL\_C 300ns, TDL\_B 100ns is another option, which is closer to traditional EVA channel
3. Set CCH symbol to 3: this reduce number of SCH symbols, can help performance when Doppler spread is large
 |

**Issue 1-2: PSCCH demodulation**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | **Issue 1-2-1: Payload size**We support option 1**Issue 1-2-2: Relative velocity**We support option 1 |
| QC | **Issue 1-2-1: Payload size**We support option 1**Issue 1-2-2: Relative velocity**We support option 1 |
| CATT | **Issue 1-2-1: Payload size**We support option 1.**Issue 1-2-2: Relative velocity**We support option 1. |
| Intel | **Issue 1-2-1: Payload size**At current stage, our calculation shows that PSCCH with 30 bits payload reflects the typical scenario. Same time, we are open to further discuss both options. Please find below the details of calculations from our side:* Priority – 3 bits
* Frequency resource assignment – 4 bits
* Time resource assignment – 5 bits
* Resource reservation period – 4 bits
* DMRS pattern – 1 bit
* 2nd-stage SCI format – 2 bits
* Beta\_offset indicator – 2 bits
* Number of DMRS port – 1 bits
* Modulation and coding scheme – 5 bits
* Additional MCS table indicator – 0 bits
* PSFCH overhead indication – 1 bits
* Reserved – 2 bits

**Issue 1-2-2: Relative velocity**Support Option 1 |
| Huawei | **Issue 1-2-1: Payload size**Our proposal for payload size setting:* Priority: 3
* Frequency resource assignment: 2
* Time resource assignment: 5
* Resource reservation period: 0
* DMRS pattern: 1
* 2nd-stage SCI format: 2
* Beta\_offset indicator: 2
* Number of DMRS port: 1
* Modulation and coding scheme: 5
* Additional MCS table indicator: 0
* PSFCH overhead indication: 1
* Reserved: 2

Total payload should be 24bits.To intel:We propose to set sub-channel size to 20RBs, so the number of sub-channels should be 2, the number of bits indicating frequency resource assignment should be 2.We don’t think resource reservation period is necessary since for PSSCH testing, repetition is not configured.To Qualcomm:In contribution R4-2014637, you propose to set number of sub-channel to 10, in that case, for 20MHz bandwidth, the subchannel size is 5RBs, which is not suitable. **Issue 1-2-2: Relative velocity**Support Option 1 |
| MTK | **Issue 1-2-1: Payload size**Support option 1.**Issue 1-2-2: Relative velocity** Support option 1. |

**Issue 1-3: PSBCH demodulation**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | **Issue 1-3-1: The number of S-SSB per one period**We support option 1. We think that 2 S-SSBs configuration does not affect PSBCH demodulation performance requirement.**Issue 1-3-2: Relative velocity**We support option 1. |
| QC | **Issue 1-3-1: The number of S-SSB per one period**We prefer option 1 for simplicity, but open to discuss option 2.**Issue 1-3-2: Relative velocity**We support option 1. |
| CATT | **Issue 1-3-1: The number of S-SSB per one period**Prefer Option 1. 1 S-SSB transmission per SL period brings about smaller transmission time delay and smaller overhead. In our understanding, Option 1 and Option 2 seem to have the similar performance except the simulation time. So 1 S-SSB per SL slot is preferred.**Issue 1-3-2: Relative velocity**Support Option 1 which is also aligned with LTE V2X. |
| Intel | **Issue 1-3-1: The number of S-SSB per one period**Support Option 1, because impact of 2 S-SSB on demodulation requirements is not clear taking into account that SSB combining is not considered.**Issue 1-3-2: Relative velocity**Support Option 1. |
| Huawei | **Issue 1-3-1: The number of S-SSB per one period**Prefer Option 2 considering the similar performance requirements as 1-SSB and short test time.To CATT: Could you share clarification about “1 S-SSB transmission per SL period brings about smaller transmission time delay and smaller overhead”? Based on our understanding, transmission 2-SSB without combing per SL period will bring smaller transmission delay and achieve similar performance. We cannot understand the relationship with smaller overhead.To Intel: Transmission 1 S-SSB or 2 S-SSB with suitable gap between 2 S-SSB within one SL period of 160ms, no any demodulation difference, how to understand the impact of 2 S-SSB on demodulation requirement?**Issue 1-3-2: Relative velocity**Support Option 1. |
| MTK | **Issue 1-3-1: The number of S-SSB per one period**Support option 1.**Issue 1-3-2: Relative velocity**Support option 1. |

**Issue 1-4: PSFCH demodulation**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | **Issue 1-4-1: Test metric**We prefer option 2. For clarification, final test metric for PSFCH is only Pr(ACK miss) < 1% with Pr(DTX to ACK)<1% and Pr(NACK to ACK)<0.1% being satisfied if option 2 is used. Is it the same understanding?**Issue 1-4-2: PSFCH periodicity**We don’t have strong view. If no any technical concern, we prefer option 2.**Issue 1-4-3: Number of Cyclic shift pairs**We support option 1.**Issue 1-4-4: Relative velocity**We support option 1. |
| QC | **Issue 1-4-1: Test metric**Since this test is option 2 ACK/NACK test, we support option 2, with the clarification that DTX corresponding to nothing is transmitted from SL Tx.**Issue 1-4-2: PSFCH periodicity**We support option 1.**Issue 1-4-3: Number of Cyclic shift pairs**We support option 1**Issue 1-4-4: Relative velocity**We support option 1 |
| CATT | **Issue 1-4-1: Test metric**Prefer Option 2.**Issue 1-4-2: PSFCH periodicity**Prefer Option 1.**Issue 1-4-3: Number of Cyclic shift pairs**Prefer Option 1.**Issue 1-4-4: Relative velocity**Prefer Option 1 |
| Intel | **Issue 1-4-1: Test metric**Prefer Option 1. Based on our understanding, PSFCH is same as PUCCH format 0. For PUCCH format 0, Pr(DTX to ACK) and Pr(ACK miss) are used for requirements definition. We think that this set of metrics is sufficient from testing point of view and it is not required to verify Pr(NACK to ACK) separately.**Issue 1-4-2: PSFCH periodicity**If PSFCH periodicity 4 will be used for PSSCH test then we prefer to consider periodicity 1 for PSFCH requirements to have sufficient test coverage. **Issue 1-4-3: Number of Cyclic shift pairs**Support Option 1.**Issue 1-4-4: Relative velocity**Support Option 1. |
| Huawei | **Issue 1-4-1: Test metric**Support option 1. Based our evaluation, SNR@ Pr(NACK to ACK) = 0.1% is much lower than SNR@ Pr(ACK miss) = 1%. Therefore if we check SNR@ Pr(ACK miss) = 1%, the Pr(NACK to ACK) = 0.1% can be met at the same time, but Pr(DTX to ACK)<1% needs to be checked separately, so Option 1 is enough.Company is welcome to check this observation based on your simulations. Before RAN4 derived these two test metrics of Pr(DTX to ACK)<1% and Pr(ACK miss) = 1% for PUCCH format 0 based on evaluations.**Issue 1-4-2: PSFCH periodicity**We prefer option 1, for PSFCH performance testing, shorter PSFCH period can reduce test time and is more suitable.**Issue 1-4-3: Number of Cyclic shift pairs**Support option 1**Issue 1-4-4: Relative velocity**Support Option 1 |
| MTK | **Issue 1-4-1: Test metric**Support option 2. We’re also fine with option 1.**Issue 1-4-2: PSFCH periodicity**Support option 1.To have sufficient test coverage as mentioned by Intel’s paper and align with PSFCH periodicity configuration in PSSCH Demod configuration, we can consider 1 slot PSFCH periodicity for PSFCH demodulation requirements.**Issue 1-4-3: Number of Cyclic shift pairs**Support option 1.**Issue 1-4-4: Relative velocity**Support option 1. |

**Issue 1-5: Resource pool configuration**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | It is better to discuss after sub-channel size is decided. |
| Intel | This topic is coupled with Issue 1-1-1. Based on our understanding, the only option from Issue 1-1-1, which contradicts with Option 1 from Issue 1-5-1, is Option 3. The other options can be replaced with multiple sub-channels allocation of size 10 PRBs.Based on our discussion from General paper, the following sub-channel sizes can be considered to ensure more efficient spectrum utilization for 20 MHz and 30 kHz: 10, 25 and 50. Same time, 10 PRBs sub-channel allows to have more flexibility in resource allocation. Therefore, we proposed to use this option for all scenarios with 20 MHz and 30 kHz scenario. |
| Huawei | As discussed in Issue 1-1-1. For PSSCH testing, we propose to use 20RBs sub-channel size. For other tests, 10RBs sub-channel size is OK for us. |
| MTK | We have the same comment with LG. |
|  |  |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| XXX | Company A |
| Company B |
|  |
| YYY | Company A |
| Company B |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1-1: PSSCH** | **Issue 1-1-1: Sub-channel size***Tentative agreements: Need further discussion**Candidate options:** *Option 1: 10 PRB sub-channel for low relative velocity and 20 PRB sub-channel for high relative velocity (LG, Qualcomm)*
* *Option 2: 10 PRB sub-channel size for all cases and number of allocated sub-channels is FFS (Intel)*
* *Option 3: 20 PRB sub-channel for all cases (LG, CATT, Huawei, MediaTek)*

*Recommendations for 2nd round: Select one option in 2nd round. As moderator point of view, one compromise option is option 1* **Issue 1-1-2: Modulation order (GNSS based sync)***Tentative agreements: Introduce test for QPSK with 500km/h, and additional test will be discussed in 2nd round**Candidate options:** *Option 1: 16QAM for 260km/h (Intel, Huawei)*
* *Option 2: 64QAM for 30km/h (LG, Qualcomm, CATT, MediaTek, Huawei(additionally))*
* *Option 3: Introduce tests both option 1 and option 2 (compromised option from moderator)*

*Recommendations for 2nd round: Select one option in 2nd round.* **Issue 1-1-3: PSFCH periodicity***Tentative agreements: Need further discussion**Candidate options:** *Option 1: 1 periodicity (Qualcomm, CATT, MediaTek)*
* *Option 2: 4 periodicity (LG, Qualcomm, CATT, Intel, Huawei)*

*Recommendations for 2nd round: Select one option in 2nd round.***Issue 1-1-4: DMRS pattern***Tentative agreements: Need further discussion**Candidate options:** *For 500km/h*
	+ *Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4*
	+ *Option 2: {3,4} DMRS symbols when PSFCH periodicity is 4 (LG, Qualcomm, CATT, Huawei)*
	+ *Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)*
* *For 260km/h*
	+ *Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4*
	+ *Option 2: {2,3} DMRS symbols when PSFCH periodicity is 4 (Qualcomm, CATT, Huawei)*
	+ *Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)*
* *For 30km/h*
	+ *Option 1: {2,3} DMRS symbols when PSFCH periodicity is 4 (LG, Huawei)*
	+ *Option 2: 2 DMRS symbols when PSFCH periodicity is 1 or 4 (Qualcomm, CATT, Huawei)*
	+ *Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)*

*Recommendations for 2nd round: Select one option for each relative velocity in 2nd round. This issue is related Issue 1-1-1, Issue 1-1-2, and Issue 1-1-3.* **Issue 1-1-5: 2nd stage SCI allocation***Tentative agreements: Depending on final decision of test cases, beta value will be used by 5 for 16QAM test configuration and beta = 3.5 for QPSK test configuration.**Candidate options:**Recommendations for 2nd round: Companies are encouraged to provide beta value for 64QAM modulation order if 640QAM is introduced.***Issue 1-1-6: gNB based sync test cases***Tentative agreements: Need further discussion**Candidate options:** *Option 1: Define performance requirement with 1300Hz FO and ±24Ts TO (CATT, Intel)*
* *Option 2: Do not define performance requirement (Qualcomm, Huawei, MediaTek)*

*Recommendations for 2nd round: Select one option in 2nd round.***Issue 1-1-7: 256QAM test cases***Tentative agreements: Need further discussion**Candidate options:** *Option 1: Define performance requirement (LG, Qualcomm)*
* *Option 2: Do not define performance requirement (CATT, Intel, Huawei, MediaTek)*

*Recommendations for 2nd round: Select one option in 2nd round.***Issue 1-1-8: Propagation condition for high relative velocity** *Tentative agreements: Need further discussion**Candidate options:** *Option 1: TDLA30*
* *Option 2: other conditions as following*
	+ *Lower MCS*
	+ *TDLB100*
	+ *Set PSCCH symbol to 3*

*Recommendations for 2nd round: Select one option in 2nd round. As moderator point of view, majority companies support option 1 and can further check other propagation condition in the next meeting,***Issue 1-1-9: Receiver assumption***Tentative agreements: Agree option 1**Candidate options:**Recommendations for 2nd round:* |
| **Sub-topic#1-2: PSCCH** | **Issue 1-2-1: Payload size***Tentative agreements: Need further discussion**Candidate options:** *Option 1: 28bits (LG, Qualcomm, CATT, MediaTek)*
* *Option 2: 30bit (Intel)*
* *Option 3: 24 bits (Huawei)*

*Recommendations for 2nd round: Select one option in 2nd round, and companies supporting option 1 are encouraged to re-check 28bit payload size considering Huawei comments for ‘Frequency resource assignment’ bit.***Issue 1-2-2: Relative velocity***Tentative agreements: Use 260km/h relative velocity (TDLA30-1400)**Candidate options:**Recommendations for 2nd round:* |
| **Sub-topic#1-3: PSBCH** | **Issue 1-3-1: The number of S-SSB per one period***Tentative agreements: Need further discussion**Candidate options:** *Option 1: 1 S-SSB (LG, Qualcomm, CATT, Intel, MediaTek)*
* *Option 2: 2 S-SSBs (Huawei)*

*Recommendations for 2nd round: Select one option in 2nd round, but majority view is option 1.* **Issue 1-3-2: Relative velocity***Tentative agreements: Use 30km/h relative velocity (TDLA30-180)**Candidate options:**Recommendations for 2nd round:* |
| **Sub-topic#1-4: PSFCH** | **Issue 1-4-1: Test metric***Tentative agreements: Use ACK/NACK feedback mode and Pr(DTX to ACK)<1% and Pr(ACK miss)<1% for test metric. RAN4 will discuss whether or not to consider Pr(NACK to ACK) < 0.1% for test metric**Candidate options:**Introduce additional test metric as Pr(NACK to ACK) < 0.1%** *Option 1: Yes (LG, Qualcomm, CATT, MediaTek)*
* *Option 2: No (Intel, Huawei, MediaTek)*

*Recommendations for 2nd round: Select one option in 2nd round.* **Issue 1-4-2: PSFCH periodicity***Tentative agreements: Use 1 periodicity**Candidate options:**Recommendations for 2nd round:***Issue 1-4-3: Number of Cyclic shift pairs***Tentative agreements: Use 1 cyclic shift pair**Candidate options:**Recommendations for 2nd round:***Issue 1-4-4: Relative velocity***Tentative agreements: Use 30km/h relative velocity (TDLA30-180)**Candidate options:**Recommendations for 2nd round:* |
| **Sub-topic#1-5: Resource pool** | *Tentative agreements: Need further discussion**Candidate options:**Recommendations for 2nd round: Depending on decision of sub-channel size for Sub-topic 1-1, RAN4 will continue to discuss this issue.* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 | WF on single link tests for NR V2X demodulation performance | LG Electronics |
| #2 | Simulation assumptions for NR V2X single link test case | Huawei |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

### Sub-topic 1-1 : PSSCH demodulation

**Issue 1-1-1: Sub-channel size**

* Proposals
	+ Option 1: 10 PRB sub-channel for low relative velocity and 20 PRB sub-channel for high relative velocity (LG, Qualcomm)
	+ Option 2: 10 PRB sub-channel size for all cases and number of allocated sub-channels is FFS (Intel)
	+ Option 3: 20 PRB sub-channel for all cases (LG, CATT, Huawei, MediaTek)
* Recommended WF
	+ Need further discussion, but as moderator point of view, option 1 is suggested to compromise solution.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option 1. For option 2, I don’ know why multiple sub-channels are allocated for 20 PRB test configuration. We can use simply single sub-channel size, and multiple sub-channel will be used for multiple link tests. |
|  |  |
|  |  |
|  |  |

**Issue 1-1-2: Modulation order (GNSS based sync)**

* Test 1 : QPSK for 500km/h
* Proposals for Test 2:
	+ Option 1: 16QAM for 260km/h (Intel, Huawei)
	+ Option 2: 64QAM for 30km/h (LG, Qualcomm, CATT, MediaTek, Huawei(additionally))
	+ Option 3: Introduce tests both option 1 and option 2 (compromised option from moderator)
* Recommended WF
	+ Need further discussion.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option2. 64QAM for NR V2X is mandatory feature, so option 2 should be considered. If companies want to include 16QAM, we are fine to option 3. |
|  |  |
|  |  |
|  |  |

**Issue 1-1-3: PSFCH periodicity**

* Proposals
	+ Option 1: 1 periodicity (Qualcomm, CATT, MediaTek)
	+ Option 2: 4 periodicity (LG, Qualcomm, CATT, Intel, Huawei)
* Recommended WF
	+ Need further discussion.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option 2If 1 periodicity is configured for all tests, other DMRS patterns cannot be verified. We prefer to use 4 periodicity at least one test case.  |
|  |  |
|  |  |
|  |  |

**Issue 1-1-4: DMRS pattern**

* Proposals
	+ For 500km/h
		- Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4
		- Option 2: {3,4} DMRS symbols when PSFCH periodicity is 4 (LG, Qualcomm, CATT, Huawei)
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)
	+ For 260km/h
		- Option 1: {2,4} DMRS symbols when PSFCH periodicity is 4
		- Option 2: {2,3} DMRS symbols when PSFCH periodicity is 4 (Qualcomm, CATT, Huawei)
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)
	+ For 30km/h
		- Option 1: {2,3} DMRS symbols when PSFCH periodicity is 4 (LG, Huawei)
		- Option 2: 2 DMRS symbols when PSFCH periodicity is 1 or 4 (Qualcomm, CATT, Huawei)
		- Option 3: 3 DMRS symbols when PSFCH periodicity is 1 (MediaTek)
* Recommended WF
	+ Need further discussion.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Depending on sub-channel size and PSFCH periodicity, DMRS pattern will be decided. Our preference is the same as 1st round, and option 2 is preferred if 260km/h is considered. |
|  |  |
|  |  |
|  |  |

**Issue 1-1-5: 2nd stage SCI allocation**

* beta = 3.5 for QPSK and beta = 5 for 16QAM depending on final decision of test cases
* Proposals
	+ Companies are encouraged to provide beta value for 64QAM (if 64QAM modulation is introduced)

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | We suggest 5 for beta value of 64QAM. If beta value is high, it might be impact on PSSCH coding rate. |
|  |  |
|  |  |
|  |  |

**Issue 1-1-6: gNB based sync test cases**

* Proposals
	+ Option 1: Define performance requirement with 1300Hz FO and ±24Ts TO (CATT, Intel)
	+ Option 2: Do not define performance requirement (Qualcomm, Huawei, MediaTek)
* Recommended WF
	+ Need further discussion.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | No strong view.  |
|  |  |
|  |  |
|  |  |

**Issue 1-1-7: 256QAM test cases**

* Proposals
	+ Option 1: Define performance requirement (LG, Qualcomm)
	+ Option 2: Do not define performance requirement (CATT, Intel, Huawei, MediaTek)
* Recommended WF
	+ Need further discussion.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option 1Since unicast will be typical scenario for NR V2X., high SNR for 256QAM can be achieved. So, even this feature is optional, this feature should be verified. |
|  |  |
|  |  |
|  |  |

**Issue 1-1-8: Propagation condition for high relative velocity**

* Proposals
	+ Option 1: TDLA30
	+ Option 2: other conditions as following
		- Lower MCS
		- TDLB100
		- Set PSCCH symbol to 3
* Recommended WF
	+ Need further discussion. As moderator point of view, majority companies support option 1 and can further check other propagation condition in the next meeting.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option 1. And we can check with one of option 2 in the next meeting. |
|  |  |
|  |  |
|  |  |

### Sub-topic 1-2 : PSCCH demodulation

**Issue 1-2-1: Payload size**

* Proposals
	+ Option 1: 28bits (LG, Qualcomm, CATT, MediaTek)
	+ Option 2: 30bit (Intel)
	+ Option 3: 24 bits (Huawei)
* Recommended WF
	+ Need further discussion. Companies supporting option 1 are encouraged to re-check 28bit payload size considering Huawei 1st round comments for ‘Frequency resource assignment’ bit.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Depending on sub-channel size, it can be slightly different. As Huawei was derived as follow:* Priority: 3
* Frequency resource assignment: 2
* Time resource assignment: 5
* Resource reservation period: 0
* DMRS pattern: 1
* 2nd-stage SCI format: 2
* Beta\_offset indicator: 2
* Number of DMRS port: 1
* Modulation and coding scheme: 5
* Additional MCS table indicator: 0
* PSFCH overhead indication: 1
* Reserved: 2

For ‘additional MCS table indicator’, I think 1 bit is needed. If 20 sub-channel size for PSSCH is used, payload size will be 25bit.  |
|  |  |
|  |  |
|  |  |

### Sub-topic 1-3 : PSBCH demodulation

**Issue 1-3-1: The number of S-SSB per one period**

* Proposals
	+ Option 1: 1 S-SSB (LG, Qualcomm, CATT, Intel, MediaTek)
	+ Option 2: 2 S-SSBs (Huawei)
* Recommended WF
	+ Need further discussion, but if there is no performance issue, majority view is suggested.

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Support option 1. There are no performance issue, so we prefer to set simple one. |
|  |  |
|  |  |
|  |  |

### Sub-topic 1-4 : PSFCH demodulation

**Issue 1-4-1: Test metric**

* Use ACK/NACK feedback mode and Pr(DTX to ACK)<1% and Pr(ACK miss)<1% for test metric.
* Proposals: Introduce additional test metric as Pr(NACK to ACK) < 0.1%
	+ Option 1: Yes (LG, Qualcomm, CATT, MediaTek)
	+ Option 2: No (Intel, Huawei, MediaTek)
* Recommended WF
	+ Option 2 is reasonable if companies agree with following observation
		- If SNR@ Pr(ACK miss) = 1%, the Pr(NACK to ACK) = 0.1% can be met at the same time

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | Based on the observation of recommended WF, option 2 is fine. |
|  |  |
|  |  |
|  |  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

# Topic #2: Draft CRs for demodulation test cases

This section will discuss the draft CRs for NR V2X demodulation.

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2014420 | CATT | CR for PSBCH performance requirements for NR V2X |
| R4-2014780 | MediaTek inc. | Draft CR for PSFCH test cases |

## Open issues summary

### Sub-topic 2-1: Draft CR handling

**Issue 2-1-1: Draft CR handling**

* Proposals from moderator
	+ Option 1: collect companies’ comments and postpone all draft CRs to the next meeting
* Recommended WF
	+ Postpone all draft CRs to the next meeting based on the email discussion summary in the last meeting

## Companies views’ collection for 1st round

### Open issues

Sub-topic 2-1: Draft CR handling

**Issue 2-1-1: Draft CR handling**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| LG | We prefer the moderator’s suggestion. In the last meeting, following summary was captured in Tdoc for summary 2nd round discussion.* *As moderator, final confirm for the work split with [ ] will be made in the next meeting. Given the status of this meeting, there are no need to prepare draft CRs in the next meeting.*
 |
| Intel | We are fine with Option 1 from moderator. |
| Huawei | We are fine with Option 1 from moderator. |
| MTK | We agree with moderator’s suggestion. |

### CRs/TPs comments collection

*Major close-to-finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014420 | LG : According to Big CR approach, formal CR is not allowed in early stage. Resource pool configuration should be defined. |
| CATT: Agree with moderator’s suggestion. It should be a draft CR.  |
| Huawei: 1) Mistakes for title: “CR for 38.101-1: Introduce PSBCH performance requirements for NR V2X” shall be changed to be “CR for 38.101-4: Introduce PSBCH performance requirements for NR V2X”(2) Mistakes for “Proposed change affects”: The CR should affect “ME”, not Radio Access Network. |
| R4-2014780 | LG : Do we need separate NACK to ACK and DTX to ACK requirements? Resource pool configuration should be defined. |
| - MTK: we can wait the conclusion of Issue 1-4-1 and then make final decision. |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | **Issue 2-1-1: Draft CR handling***Tentative agreements: collect companies’ comments and postpone all draft CRs to the next meeting. Companies volunteering for draft CR are encouraged to provide draft CRs in the next meeting.* *Candidate options:**Recommendations for 2nd round:* |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title**  | **Assigned Company,****WF or LS lead** |
| #1 |  |  |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation**  |
| R4-2014420 | Postpone to next meeting |
| R4-2014780 | Postpone to next meeting |

## Discussion on 2nd round (if applicable)

### Continue to collect comments for draft CR/CR

Following Tdocs have been already decided by ”postpone” in 1st round, but based on chairmna’s guidance, please add your commnets if companies have further comments for following draft CR/CR. There will be no summary on 2nd round.

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2014420 | LG : According to Big CR approach, formal CR is not allowed in early stage. Resource pool configuration should be defined. |
| CATT: Agree with moderator’s suggestion. It should be a draft CR.  |
| Huawei: 1) Mistakes for title: “CR for 38.101-1: Introduce PSBCH performance requirements for NR V2X” shall be changed to be “CR for 38.101-4: Introduce PSBCH performance requirements for NR V2X”(2) Mistakes for “Proposed change affects”: The CR should affect “ME”, not Radio Access Network. |
| R4-2014780 | LG : Do we need separate NACK to ACK and DTX to ACK requirements? Resource pool configuration should be defined. |
| - MTK: we can wait the conclusion of Issue 1-4-1 and then make final decision. |
|  |

## Summary on 2nd round (if applicable)

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation**  |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |