{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","Results"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #97-e",null,null,null,null,null,null,null,"R4-20015861"]
[null,"Electronic meeting,  2nd-13th November, 2020"]
[]
[null,"Source: Moderator (Ericsson)"]
[null,"Title: Summary of ideal and impairment results for ultra-low BLER BS"]
[null,"Agenda: 7.8.1.1.3"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"Results","index":2,"n_rows":10,"n_cols":29,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,27,0,28],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,23,0,24],[0,11,0,12],[0,6,1,6],[0,19,0,20],[0,21,0,22],[0,25,0,26],[0,0,1,0],[0,1,1,1],[0,3,1,3],[0,8,1,8],[0,9,0,10],[0,7,1,7],[0,2,1,2],[0,4,1,4],[0,5,1,5]]}
[" waveform","Tx/Rx","PUSCH mapping type","SCS and BW","MCS level","Propagation condition","DMRS","38.104 req","38.141 req","Nokia",null,"Huawei",null,"Intel",null,"Ericsson",null,"Samsung",null,null,null,null,null,null,null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["CP-OFDM","1T2R","type A","15kHz, 5MHz","MCS5","AWGN","DMRS 1+1",{"$f":"DerivingPerfReq(J3:Y3)","v":-5.0999999999999996},{"$f":"IF(H3>-100,H3+1.3,H3)","v":-3.8},-6.5,-4,-7.8,-5.3,-6.9,-5.4,-7.9,-5.4,-7.2,-5.2,null,null,null,null,null,null,{"$f":"MAX(J3,L3,N3,P3,R3,T3,V3,X3)-MIN(J3,L3,N3,P3,R3,T3,V3,X3)","v":1.4000000000000004},{"$f":"MAX(K3,M3,O3,Q3,S3,U3,W3,Y3)-MIN(K3,M3,O3,Q3,S3,U3,W3,Y3)","v":1.4000000000000004},{"$f":"AVERAGE(J3,L3,N3,P3,R3,T3,V3,X3)","v":-7.2600000000000007},-5.0600000000000005]
["CP-OFDM","1T2R","type A","15kHz, 10MHz","MCS5","AWGN","DMRS 1+1",-5.9,-4.6000000000000005,-7.3,-4.8,-8.5,-6,-8.4,-6.9,-8.1,-5.6,-7.7,-6.2,null,null,null,null,null,null,{"$f":"MAX(J4,L4,N4,P4,R4,T4,V4,X4)-MIN(J4,L4,N4,P4,R4,T4,V4,X4)","v":1.2000000000000002},{"$f":"MAX(K4,M4,O4,Q4,S4,U4,W4,Y4)-MIN(K4,M4,O4,Q4,S4,U4,W4,Y4)","v":2.1000000000000005},{"$f":"AVERAGE(J4,L4,N4,P4,R4,T4,V4,X4)","v":-8.0000000000000018},{"$f":"AVERAGE(K4,M4,O4,Q4,S4,U4,W4,Y4)","v":-5.9}]
["CP-OFDM","1T2R","type A","30kHz, 10MHz","MCS5","AWGN","DMRS 1+1",-5.4,-4.1000000000000005,-6.5,-4,-7.8,-5.3,-7.8,-6.3,-7.9,-5.4,-7.7,-6.2,null,null,null,null,null,null,{"$f":"MAX(J5,L5,N5,P5,R5,T5,V5,X5)-MIN(J5,L5,N5,P5,R5,T5,V5,X5)","v":1.4000000000000004},2.2999999999999998,-7.5400000000000009,-5.4399999999999995]
["CP-OFDM","1T2R","type A","30kHz, 40MHz","MCS5","AWGN","DMRS 1+1",-6.2,-4.9000000000000004,-7.6,-5.0999999999999996,-8.4,-5.9,-8.8000000000000007,-7.3,-8.6999999999999993,-6.2,-8,-6.5,null,null,null,null,null,null,{"$f":"MAX(J6,L6,N6,P6,R6,T6,V6,X6)-MIN(J6,L6,N6,P6,R6,T6,V6,X6)","v":1.2000000000000011},{"$f":"MAX(K6,M6,O6,Q6,S6,U6,W6,Y6)-MIN(K6,M6,O6,Q6,S6,U6,W6,Y6)","v":2.2000000000000002},{"$f":"AVERAGE(J6,L6,N6,P6,R6,T6,V6,X6)","v":-8.3000000000000007},{"$f":"AVERAGE(K6,M6,O6,Q6,S6,U6,W6,Y6)","v":-6.2}]
["CP-OFDM","1T2R"," type B","15kHz, 5MHz","MCS5","AWGN","DMRS 1+1",-5.2,-3.9000000000000004,-6.6,-4.0999999999999996,-7.9,-5.4,-6.9,-5.4,-7.9,-5.4,-7.3,-5.8,null,null,null,null,null,null,1.3000000000000007,1.7000000000000002,-7.3199999999999985,-5.2200000000000006]
["CP-OFDM","1T2R"," type B","15kHz, 10MHz","MCS5","AWGN","DMRS 1+1",-5.9,-4.6000000000000005,-7.3,-4.8,-8.5,-6,-8.4,-6.9,-8.1,-5.6,-7.7,-6.2,null,null,null,null,null,null,{"$f":"MAX(J8,L8,N8,P8,R8,T8,V8,X8)-MIN(J8,L8,N8,P8,R8,T8,V8,X8)","v":1.2000000000000002},{"$f":"MAX(K8,M8,O8,Q8,S8,U8,W8,Y8)-MIN(K8,M8,O8,Q8,S8,U8,W8,Y8)","v":2.1000000000000005},{"$f":"AVERAGE(J8,L8,N8,P8,R8,T8,V8,X8)","v":-8.0000000000000018},{"$f":"AVERAGE(K8,M8,O8,Q8,S8,U8,W8,Y8)","v":-5.9}]
["CP-OFDM","1T2R","type B","30kHz, 10MHz","MCS5","AWGN","DMRS 1+1",-5.5,-4.2,-6.6,-4.0999999999999996,-7.9,-5.4,-7.8,-6.3,-7.9,-5.4,-7.7,-6.2,null,null,null,null,null,null,1.3000000000000007,2.2000000000000002,-7.580000000000001,-5.48]
["CP-OFDM","1T2R","type B","30kHz, 40MHz","MCS5","AWGN","DMRS 1+1",-6.2,-4.9000000000000004,-7.6,-5.0999999999999996,-8.4,-5.9,-8.8000000000000007,-7.3,-8.6999999999999993,-6.2,-7.9,-6.4,null,null,null,null,null,null,{"$f":"MAX(J10,L10,N10,P10,R10,T10,V10,X10)-MIN(J10,L10,N10,P10,R10,T10,V10,X10)","v":1.2000000000000011},{"$f":"MAX(K10,M10,O10,Q10,S10,U10,W10,Y10)-MIN(K10,M10,O10,Q10,S10,U10,W10,Y10)","v":2.2000000000000002},{"$f":"AVERAGE(J10,L10,N10,P10,R10,T10,V10,X10)","v":-8.2799999999999994},{"$f":"AVERAGE(K10,M10,O10,Q10,S10,U10,W10,Y10)","v":-6.18}]